(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "Button_Switch_SMD:SW_SPST_SKQG_WithStem" (layer "F.Cu")
    (at 158.3 100)
    (descr "ALPS 5.2mm Square Low-profile Type (Surface Mount) SKQG Series, With stem, http://www.alps.com/prod/info/E/HTML/Tact/SurfaceMount/SKQG/SKQGAFE010.html")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference "REF**" (at 0 -3.6) (layer "F.SilkS") hide)
    (fp_text value "SW_SPST_SKQG_WithStem" (at 0 3.6) (layer "F.Fab") hide)
    (fp_text user "No F.Cu tracks" (at -2.5 0.2) (layer "Cmts.User"))
    (fp_text user "KEEP-OUT ZONE" (at 2.5 -0.2) (layer "Cmts.User"))
    (fp_text user "KEEP-OUT ZONE" (at -2.5 -0.2) (layer "Cmts.User"))
    (fp_text user "No F.Cu tracks" (at 2.5 0.2) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.1 -1.85) (size 1.8 1.1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "1" smd rect (at 3.1 -1.85) (size 1.8 1.1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -3.1 1.85) (size 1.8 1.1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at 3.1 1.85) (size 1.8 1.1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 154.3 98.7)
          (xy 157.3 98.7)
          (xy 157.3 101.3)
          (xy 154.3 101.3)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 159.3 98.7)
          (xy 162.3 98.7)
          (xy 162.3 101.3)
          (xy 159.3 101.3)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_SKQG_WithStem.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_SPST_SKQG_WithStem" (layer "F.Cu")
    (at 150 100)
    (descr "ALPS 5.2mm Square Low-profile Type (Surface Mount) SKQG Series, With stem, http://www.alps.com/prod/info/E/HTML/Tact/SurfaceMount/SKQG/SKQGAFE010.html")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference "REF**" (at 0 -3.6) (layer "F.SilkS") hide)
    (fp_text value "SW_SPST_SKQG_WithStem" (at 0 3.6) (layer "F.Fab") hide)
    (fp_text user "No F.Cu tracks" (at -2.5 0.2) (layer "Cmts.User"))
    (fp_text user "KEEP-OUT ZONE" (at -2.5 -0.2) (layer "Cmts.User"))
    (fp_text user "KEEP-OUT ZONE" (at 2.5 -0.2) (layer "Cmts.User"))
    (fp_text user "No F.Cu tracks" (at 2.5 0.2) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.1 -1.85) (size 1.8 1.1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "1" smd rect (at 3.1 -1.85) (size 1.8 1.1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at -3.1 1.85) (size 1.8 1.1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (pad "2" smd rect (at 3.1 1.85) (size 1.8 1.1) (layers "F.Cu" "F.Paste" "F.Mask"))
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 146 98.7)
          (xy 149 98.7)
          (xy 149 101.3)
          (xy 146 101.3)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254) (filled_areas_thickness no)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 151 98.7)
          (xy 154 98.7)
          (xy 154 101.3)
          (xy 151 101.3)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_SKQG_WithStem.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "B.Cu")
    (at 146.73 101.73 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 1.648) (layer "B.SilkS") hide)
    (fp_text value "TestPoint_Pad_D1.5mm" (at 0 -1.75) (layer "B.Fab") hide)
    (pad "1" smd circle (at 0 0 180) (size 1.5 1.5) (layers "B.Cu" "B.Mask"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "B.Cu")
    (at 154.13 98.18 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 1.648) (layer "B.SilkS") hide)
    (fp_text value "TestPoint_Pad_D1.5mm" (at 0 -1.75) (layer "B.Fab") hide)
    (pad "1" smd circle (at 0 0 180) (size 1.5 1.5) (layers "B.Cu" "B.Mask"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "B.Cu")
    (at 161.25 101.62 180)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 1.648) (layer "B.SilkS") hide)
    (fp_text value "TestPoint_Pad_D1.5mm" (at 0 -1.75) (layer "B.Fab") hide)
    (pad "1" smd circle (at 0 0 180) (size 1.5 1.5) (layers "B.Cu" "B.Mask"))
  )
  (gr_arc (start 160.445498 96.107713) (mid 164.32 99.98319) (end 160.479423 103.892288)
    (layer "Edge.Cuts"))
  (gr_arc (start 147.708297 103.892288) (mid 143.86772 99.98319) (end 147.742222 96.107713)
    (layer "Edge.Cuts"))
  (gr_line (start 147.742222 96.107713) (end 160.445498 96.107713)
    (layer "Edge.Cuts"))
  (gr_line (start 160.479423 103.892288) (end 147.708297 103.892288)
    (layer "Edge.Cuts"))
)
