(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 323)
    (zones 0)
    (modules 26)
    (nets 37)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 /XTAL1)
  (net 5 /XTAL2)
  (net 6 /BD+)
  (net 7 /BD-)
  (net 8 /AD+)
  (net 9 /AD-)
  (net 10 /Reset)
  (net 11 /D+)
  (net 12 /D-)
  (net 13 /uD+)
  (net 14 /uD-)
  (net 15 /Sel)
  (net 16 "Net-(J4-Pad4)")
  (net 17 "Net-(J4-Pad3)")
  (net 18 "Net-(J4-Pad2)")
  (net 19 "Net-(J4-Pad1)")
  (net 20 "Net-(D1-Pad1)")
  (net 21 "Net-(J4-Pad19)")
  (net 22 "Net-(J4-Pad18)")
  (net 23 "Net-(J4-Pad17)")
  (net 24 "Net-(J4-Pad16)")
  (net 25 "Net-(J4-Pad15)")
  (net 26 "Net-(J4-Pad14)")
  (net 27 "Net-(J4-Pad13)")
  (net 28 "Net-(J4-Pad12)")
  (net 29 "Net-(J4-Pad11)")
  (net 30 "Net-(J4-Pad10)")
  (net 31 "Net-(J4-Pad9)")
  (net 32 "Net-(J4-Pad8)")
  (net 33 "Net-(J4-Pad7)")
  (net 34 "Net-(J4-Pad6)")
  (net 35 "Net-(J4-Pad5)")
  (net 36 "Net-(D2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /AD+)
    (add_net /AD-)
    (add_net /BD+)
    (add_net /BD-)
    (add_net /D+)
    (add_net /D-)
    (add_net /Reset)
    (add_net /Sel)
    (add_net /XTAL1)
    (add_net /XTAL2)
    (add_net /uD+)
    (add_net /uD-)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad10)")
    (add_net "Net-(J4-Pad11)")
    (add_net "Net-(J4-Pad12)")
    (add_net "Net-(J4-Pad13)")
    (add_net "Net-(J4-Pad14)")
    (add_net "Net-(J4-Pad15)")
    (add_net "Net-(J4-Pad16)")
    (add_net "Net-(J4-Pad17)")
    (add_net "Net-(J4-Pad18)")
    (add_net "Net-(J4-Pad19)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
    (add_net "Net-(J4-Pad9)")
  )
  (module 0482580002:MOLEX_0482580002 (layer F.Cu) (tedit 5E8332BD)
    (at 155.956 94.869 270)
    (fp_text reference J2 (at 2.159 -3.556) (layer F.SilkS))
    (fp_text value USB_A (at 10.387515 -6.17344 270) (layer F.Fab))
    (fp_line (start -6.75 11.9) (end -6.75 2) (layer Edge.Cuts) (width 0.1))
    (fp_line (start -5.95 2) (end 5.95 2) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 6.75 2) (end 6.75 11.9) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 6.75 11.9) (end -6.75 11.9) (layer Edge.Cuts) (width 0.1))
    (fp_text user PCB~Edge (at 4.61444 13.2665 90) (layer F.Fab))
    (fp_arc (start -6.35 2) (end -6.35 1.6) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start -6.35 2) (end -5.95 2) (angle -90) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start 6.35 2) (end 6.35 1.6) (angle 90) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start 6.35 2) (end 5.95 2) (angle 90) (layer Edge.Cuts) (width 0.1))
    (pad 1 thru_hole rect (at 3.5 -0.85 270) (size 1.478 1.478) (drill 0.97) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 1 -0.85 270) (size 1.478 1.478) (drill 0.97) (layers *.Cu *.Mask)
      (net 9 /AD-))
    (pad 3 thru_hole circle (at -1 -0.85 270) (size 1.478 1.478) (drill 0.97) (layers *.Cu *.Mask)
      (net 8 /AD+))
    (pad 4 thru_hole circle (at -3.5 -0.85 270) (size 1.478 1.478) (drill 0.97) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad P3 smd rect (at -8 9.1 270) (size 2.4 2.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad P4 smd rect (at 8 9.1 270) (size 2.4 2.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad None np_thru_hole circle (at 0 6.95 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask))
    (pad P1 thru_hole oval (at -7.85 0 270) (size 1.458 2.916) (drill oval 0.95 2.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad P2 thru_hole oval (at 7.85 0 270) (size 1.458 2.916) (drill oval 0.95 2.35) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 162.052 86.233 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference REF** (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value PinHeader_1x02_P2.54mm_Vertical (at 3.81 0.254 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5E82C2AA)
    (at 187.452 86.233 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference JP1 (at 1.143 10.795 180) (layer F.SilkS))
    (fp_text value Jumper_NC_Dual (at 3.302 1.397 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /Sel))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 179.705 85.725 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at -2.667 0.254) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 164.719 100.076 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 12pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /XTAL2))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 164.719 92.456 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 1.778 1.27) (layer F.SilkS))
    (fp_text value 12pF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /XTAL1))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 170.561 92.964)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.43) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 168.529 99.695 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 177.546 92.837)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 1.27 -1.397) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 176.022 89.789 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /D+))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /uD+))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DFN_QFN:Texas_R-PUQFN-N10 (layer F.Cu) (tedit 5C425719)
    (at 179.705 88.011)
    (descr http://www.ti.com/general/docs/lit/getliterature.tsp?baseLiteratureNumber=MPQF186&fileType=pdf)
    (tags Texas_R-PUQFN-N10)
    (clearance 0.17)
    (attr smd)
    (fp_text reference U2 (at -2.286 -0.762) (layer F.SilkS))
    (fp_text value TS3USB221 (at 0 2.25) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 5 smd rect (at 0 1.175 90) (size 0.63 0.35) (drill (offset 0.315 0)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 0 -1.175 270) (size 0.63 0.35) (drill (offset 0.315 0)) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at -0.35 -0.25 270) (size 0.25 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask)
      (net 9 /AD-))
    (pad 3 smd rect (at -0.35 0.25 270) (size 0.25 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask)
      (net 13 /uD+))
    (pad 7 smd rect (at 0.35 0.25 90) (size 0.25 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask)
      (net 7 /BD-))
    (pad 8 smd rect (at 0.35 -0.25 90) (size 0.25 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask)
      (net 6 /BD+))
    (pad 9 smd rect (at 0.35 -0.75 90) (size 0.3 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask)
      (net 15 /Sel))
    (pad 6 smd rect (at 0.35 0.75 90) (size 0.3 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -0.35 0.75 270) (size 0.3 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask)
      (net 14 /uD-))
    (pad 1 smd rect (at -0.35 -0.75 270) (size 0.3 0.575) (drill (offset 0 0.2875)) (layers F.Cu F.Paste F.Mask)
      (net 8 /AD+))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/Texas_R-PUQFN-N10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 199.009 102.489 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0.127 1.524 90) (layer F.SilkS))
    (fp_text value 1k2 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(D2-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 "Net-(J4-Pad19)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 197.358 102.503 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at -2.399 0 180) (layer F.SilkS))
    (fp_text value 1k2 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 173.99 90.805 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at -2.2098 -0.0254 180) (layer F.SilkS))
    (fp_text value 22 (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /D-))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 /uD-))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 187.071 94.615 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 1.524 1.651 180) (layer F.SilkS))
    (fp_text value 47k (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /Reset))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_Push_1P1T-SH_NO_CK_KMR2xxG (layer F.Cu) (tedit 5D8D2A01)
    (at 193.421 102.362 180)
    (descr "CK components KMR2 tactile switch with ground pin http://www.ckswitches.com/media/1479/kmr2.pdf")
    (tags "tactile switch kmr2")
    (attr smd)
    (fp_text reference SW1 (at 0 -2.45) (layer F.SilkS))
    (fp_text value SW_Push (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 -2.45) (layer F.Fab))
    (pad 2 smd rect (at 2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J4-Pad18)"))
    (pad 2 smd rect (at -2.05 0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.05 -0.8 180) (size 0.9 1) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J4-Pad18)"))
    (pad SH smd rect (at 0 -1.425 180) (size 1.7 0.55) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_Push_1P1T-SH_NO_CK_KMR2xxG.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 199.009 99.06 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D2 (at 2.413 0 180) (layer F.SilkS))
    (fp_text value "LED Blue" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x19_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 154.432 106.553 90)
    (descr "Through hole straight pin header, 1x19, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x19 2.54mm single row")
    (fp_text reference J4 (at 2.413 -0.889 180) (layer F.SilkS))
    (fp_text value Conn_01x19_Female (at -2.794 20.193 180) (layer F.Fab))
    (fp_text user %R (at 0 22.86) (layer F.Fab))
    (pad 19 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J4-Pad19)"))
    (pad 18 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J4-Pad18)"))
    (pad 17 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J4-Pad17)"))
    (pad 16 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J4-Pad16)"))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J4-Pad15)"))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J4-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J4-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J4-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J4-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J4-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J4-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J4-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J4-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J4-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x19_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B4B45C9)
    (at 197.358 99.06 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (attr smd)
    (fp_text reference D1 (at 2.286 -0.127 180) (layer F.SilkS))
    (fp_text value "LED Green" (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.27mm:PinHeader_2x03_P1.27mm_Vertical_SMD (layer F.Cu) (tedit 59FED6E3)
    (at 183.769 94.615 90)
    (descr "surface-mounted straight pin header, 2x03, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 1.27mm double row")
    (attr smd)
    (fp_text reference J3 (at -5.207 -1.778 90) (layer F.SilkS))
    (fp_text value ATMELICE-UPDI-6-50mm (at 0 2.965 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 1.95 -1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 10 /Reset))
    (pad 4 smd rect (at 1.95 0 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at -1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.95 1.27 90) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x03_P1.27mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 194.945 95.377 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 2.413 -0.254 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 2 +5V))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical_SMD_Pin1Left (layer F.Cu) (tedit 59FED738)
    (at 190.5 90.297)
    (descr "surface-mounted straight pin header, 1x02, 1.00mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x02 1.00mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference TP1 (at -3.5052 -0.889) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 2.06) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.875 0.5) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /BD-))
    (pad 1 smd rect (at -0.875 -0.5) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /BD+))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical_SMD_Pin1Left (layer F.Cu) (tedit 59FED738)
    (at 168.783 89.154)
    (descr "surface-mounted straight pin header, 1x02, 1.00mm pitch, single row, style 1 (pin 1 left)")
    (tags "Surface mounted pin header SMD 1x02 1.00mm single row style1 pin1 left")
    (attr smd)
    (fp_text reference TP2 (at 0 -2.06) (layer F.SilkS))
    (fp_text value TestPoint_2Pole (at 0 2.06) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.875 0.5) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /AD-))
    (pad 1 smd rect (at -0.875 -0.5) (size 1.75 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /AD+))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical_SMD_Pin1Left.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_SeikoEpson_TSX3225-4Pin_3.2x2.5mm_HandSoldering (layer F.Cu) (tedit 5A0FD1B2)
    (at 164.719 96.266 90)
    (descr "crystal Epson Toyocom TSX-3225 series https://support.epson.biz/td/api/doc_check.php?dl=brief_fa-238v_en.pdf, hand-soldering, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal hand-soldering")
    (attr smd)
    (fp_text reference Y1 (at 0.889 3.175 180) (layer F.SilkS))
    (fp_text value "16.00 MHZ" (at 0 2.95 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 4 smd rect (at -1.45 -1.0875 90) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 1.45 -1.0875 90) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 4 /XTAL1))
    (pad 2 smd rect (at 1.45 1.0875 90) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.45 1.0875 90) (size 2.1 1.725) (layers F.Cu F.Paste F.Mask)
      (net 5 /XTAL2))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_SeikoEpson_TSX3225-4Pin_3.2x2.5mm_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:TQFP-32_7x7mm_P0.8mm (layer F.Cu) (tedit 5A02F146)
    (at 175.768 99.314)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at -0.127 -1.27) (layer F.SilkS))
    (fp_text value ATmega32U2-AU (at 0.127 6.731) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /XTAL1))
    (pad 2 smd rect (at -4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /XTAL2))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J4-Pad1)"))
    (pad 6 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J4-Pad2)"))
    (pad 7 smd rect (at -4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J4-Pad3)"))
    (pad 8 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J4-Pad4)"))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J4-Pad5)"))
    (pad 10 smd rect (at -2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J4-Pad6)"))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J4-Pad7)"))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J4-Pad8)"))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J4-Pad9)"))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J4-Pad10)"))
    (pad 15 smd rect (at 2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J4-Pad11)"))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J4-Pad12)"))
    (pad 17 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J4-Pad13)"))
    (pad 18 smd rect (at 4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J4-Pad14)"))
    (pad 19 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J4-Pad15)"))
    (pad 20 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J4-Pad16)"))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J4-Pad17)"))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(J4-Pad18)"))
    (pad 23 smd rect (at 4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J4-Pad19)"))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 /Reset))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /D+))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /D-))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Micro-B_Molex-105017-0001 (layer F.Cu) (tedit 5A1DC0BE)
    (at 199.39 92.7608 90)
    (descr http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf)
    (tags "Micro-USB SMD Typ-B")
    (attr smd)
    (fp_text reference J1 (at 5.2578 0.254 180) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0.3 4.3375 90) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.6875 90) (layer Dwgs.User))
    (fp_text user %R (at 0 0.8875 90) (layer F.Fab))
    (pad 6 smd rect (at 1 1.2375 90) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -2.5 -1.4625 90) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.65 -1.4625 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 7 /BD-))
    (pad 1 smd rect (at -1.3 -1.4625 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at 1.3 -1.4625 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -1.4625 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -1.4625 90) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 6 /BD+))
    (pad 6 thru_hole circle (at 2.5 -1.4625 90) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -1 1.2375 90) (size 1.5 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -3.5 1.2375 270) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 3.5 1.2375 90) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.9 1.2375 90) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.9 1.2375 90) (size 1.2 1.9) (layers F.Cu F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex-105017-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 142.24 85.344) (end 142.24 107.188) (layer Edge.Cuts) (width 0.05))
  (gr_text "ATMega32U2 USB Demo Board v1.0" (at 187.833 103.886) (layer B.SilkS))
  (gr_arc (start 143.51 85.344) (end 143.51 84.074) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 143.51 107.188) (end 142.24 107.188) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 200.787 107.188) (end 200.787 108.458) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 200.787 85.344) (end 202.057 85.344) (angle -90) (layer Edge.Cuts) (width 0.05))
  (dimension 20.32 (width 0.15) (layer Eco1.User)
    (gr_text "20.320 mm" (at 148.052 96.393 90) (layer Eco1.User))
    (feature1 (pts (xy 154.432 86.233) (xy 148.765579 86.233)))
    (feature2 (pts (xy 154.432 106.553) (xy 148.765579 106.553)))
    (crossbar (pts (xy 149.352 106.553) (xy 149.352 86.233)))
    (arrow1a (pts (xy 149.352 86.233) (xy 149.938421 87.359504)))
    (arrow1b (pts (xy 149.352 86.233) (xy 148.765579 87.359504)))
    (arrow2a (pts (xy 149.352 106.553) (xy 149.938421 105.426496)))
    (arrow2b (pts (xy 149.352 106.553) (xy 148.765579 105.426496)))
  )
  (dimension 49.657 (width 0.15) (layer Eco1.User)
    (gr_text "1.9550 in" (at 174.8155 79.98) (layer Eco1.User))
    (feature1 (pts (xy 149.987 83.82) (xy 149.987 80.693579)))
    (feature2 (pts (xy 199.644 83.82) (xy 199.644 80.693579)))
    (crossbar (pts (xy 199.644 81.28) (xy 149.987 81.28)))
    (arrow1a (pts (xy 149.987 81.28) (xy 151.113504 80.693579)))
    (arrow1b (pts (xy 149.987 81.28) (xy 151.113504 81.866421)))
    (arrow2a (pts (xy 199.644 81.28) (xy 198.517496 80.693579)))
    (arrow2b (pts (xy 199.644 81.28) (xy 198.517496 81.866421)))
  )
  (dimension 25.273 (width 0.15) (layer Eco1.User)
    (gr_text "0.9950 in" (at 206.151 96.8375 270) (layer Eco1.User))
    (feature1 (pts (xy 202.057 109.474) (xy 205.437421 109.474)))
    (feature2 (pts (xy 202.057 84.201) (xy 205.437421 84.201)))
    (crossbar (pts (xy 204.851 84.201) (xy 204.851 109.474)))
    (arrow1a (pts (xy 204.851 109.474) (xy 204.264579 108.347496)))
    (arrow1b (pts (xy 204.851 109.474) (xy 205.437421 108.347496)))
    (arrow2a (pts (xy 204.851 84.201) (xy 204.264579 85.327504)))
    (arrow2b (pts (xy 204.851 84.201) (xy 205.437421 85.327504)))
  )
  (gr_line (start 202.057 107.188) (end 202.057 85.344) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.51 108.458) (end 200.787 108.458) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 200.787 84.074) (end 143.51 84.074) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.803 97.409) (xy 196.723 97.409) (xy 196.723 92.202) (xy 199.1614 92.202) (xy 199.1614 90.932)
        (xy 196.723 90.932) (xy 196.723 88.138) (xy 201.803 88.138)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.242 104.394) (xy 144.399 104.394) (xy 144.399 85.344) (xy 158.242 85.344) (xy 158.242 90.043)
        (xy 155.575 90.043) (xy 155.575 92.71) (xy 158.242 92.71)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 196.342 104.902) (xy 158.623 104.902) (xy 158.623 84.455) (xy 196.342 84.455)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 201.803 104.902) (xy 196.215 104.902) (xy 196.215 97.663) (xy 201.803 97.663)
      )
    )
  )
)
