(kicad_pcb (version 20170123) (host pcbnew "(2017-03-27 revision c7c172d36)-makepkg")
  (general
    (links 12)
    (no_connects 0)
    (area 131.2185 91.376499 166.0965 127.082333)
    (thickness 1.6)
    (drawings 16)
    (tracks 53)
    (zones 0)
    (modules 2)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (user_trace_width 1)
    (user_trace_width 1.2)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 148.59 106.68)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x3fff3_ffffffff)
      (usegerberextensions true)
      (usegerberattributes true)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory CAM/))
  )
  (net 0 "")
  (net 1 "Net-(NX1-Pad0)")
  (net 2 "Net-(NX1-Pad1)")
  (net 3 "Net-(NX1-Pad2)")
  (net 4 "Net-(NX1-Pad3)")
  (net 5 "Net-(NX1-Pad4)")
  (net 6 "Net-(NX1-Pad5)")
  (net 7 "Net-(NX1-Pad6)")
  (net 8 "Net-(NX1-Pad7)")
  (net 9 "Net-(NX1-Pad8)")
  (net 10 "Net-(NX1-Pad9)")
  (net 11 "Net-(NX1-PadA)")
  (net 12 "Net-(NX1-PadA1)")
  (net_class Default "Dit is de standaard class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net "Net-(NX1-Pad0)")
    (add_net "Net-(NX1-Pad1)")
    (add_net "Net-(NX1-Pad2)")
    (add_net "Net-(NX1-Pad3)")
    (add_net "Net-(NX1-Pad4)")
    (add_net "Net-(NX1-Pad5)")
    (add_net "Net-(NX1-Pad6)")
    (add_net "Net-(NX1-Pad7)")
    (add_net "Net-(NX1-Pad8)")
    (add_net "Net-(NX1-Pad9)")
    (add_net "Net-(NX1-PadA)")
    (add_net "Net-(NX1-PadA1)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 58BC9807)
    (at 134.62 121.92 90)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X12 (at 0 30.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(NX1-PadA)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(NX1-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(NX1-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(NX1-Pad3)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(NX1-Pad4)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(NX1-Pad5)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(NX1-Pad6)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(NX1-Pad7)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(NX1-Pad8)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(NX1-Pad9)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(NX1-Pad0)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(NX1-PadA1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 -0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module nixie_tube:nixie_tube-ZM1042-DSUB (layer F.Cu) (tedit 200000)
    (at 148.60992 106.0831 180)
    (descr "SOCKET WITH D-SUB SOCKETS")
    (tags "SOCKET WITH D-SUB SOCKETS")
    (attr virtual)
    (fp_text reference NX1 (at -0.07366 -0.88392 180) (layer F.SilkS))
    (fp_text value ZM1042 (at 0.5588 0.61468 180) (layer F.SilkS))
    (fp_text user 2 (at 5.0038 -3.6195 180) (layer F.SilkS))
    (fp_text user 3 (at 6.32206 -1.01854 180) (layer F.SilkS))
    (fp_text user 4 (at 6.2103 1.59258 180) (layer F.SilkS))
    (fp_text user 5 (at 4.70916 4.07162 180) (layer F.SilkS))
    (fp_text user 6 (at 2.64668 5.59054 180) (layer F.SilkS))
    (fp_text user 7 (at -2.15138 5.4229 180) (layer F.SilkS))
    (fp_text user 8 (at -4.4323 4.02844 180) (layer F.SilkS))
    (fp_text user 9 (at -5.77342 1.61798 180) (layer F.SilkS))
    (fp_text user 0 (at -5.80136 -1.1303 180) (layer F.SilkS))
    (fp_text user A (at -2.32918 -5.40258 180) (layer F.SilkS))
    (fp_text user A (at 0.30734 -5.92328 180) (layer F.SilkS))
    (fp_text user IV (at 0.33528 6.10362 180) (layer F.SilkS))
    (fp_text user 1 (at -4.73202 -3.70078 180) (layer F.SilkS))
    (pad 0 thru_hole circle (at -8.18896 -1.8669 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 1 "Net-(NX1-Pad0)"))
    (pad 1 thru_hole circle (at -6.5659 -5.23494 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 2 "Net-(NX1-Pad1)"))
    (pad 2 thru_hole circle (at 6.5659 -5.23494 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 3 "Net-(NX1-Pad2)"))
    (pad 3 thru_hole circle (at 8.18896 -1.8669 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 4 "Net-(NX1-Pad3)"))
    (pad 4 thru_hole circle (at 8.18896 1.8669 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 5 "Net-(NX1-Pad4)"))
    (pad 5 thru_hole circle (at 6.5659 5.23494 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 6 "Net-(NX1-Pad5)"))
    (pad 6 thru_hole circle (at 3.6449 7.56666 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 7 "Net-(NX1-Pad6)"))
    (pad 7 thru_hole circle (at -3.6449 7.56666 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 8 "Net-(NX1-Pad7)"))
    (pad 8 thru_hole circle (at -6.5659 5.23494 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 9 "Net-(NX1-Pad8)"))
    (pad 9 thru_hole circle (at -8.18896 1.8669 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 10 "Net-(NX1-Pad9)"))
    (pad A thru_hole circle (at 0 -8.39978 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 11 "Net-(NX1-PadA)"))
    (pad A1 thru_hole circle (at -3.6449 -7.56666 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask)
      (net 12 "Net-(NX1-PadA1)"))
    (pad IV thru_hole circle (at 0 8.39978 180) (size 2.39776 2.39776) (drill 1.59766) (layers *.Cu *.Paste *.Mask))
  )
  (gr_text A2 (at 163.83 119.38) (layer F.SilkS))
  (gr_text 0 (at 160.02 119.38) (layer F.SilkS))
  (gr_text 9 (at 157.48 119.38) (layer F.SilkS))
  (gr_text 8 (at 154.94 119.38) (layer F.SilkS))
  (gr_text 7 (at 152.4 119.38) (layer F.SilkS))
  (gr_text 6 (at 149.86 119.38) (layer F.SilkS))
  (gr_text 5 (at 147.32 119.38) (layer F.SilkS))
  (gr_text 4 (at 144.78 119.38) (layer F.SilkS))
  (gr_text 3 (at 142.24 119.38) (layer F.SilkS))
  (gr_text 2 (at 139.7 119.38) (layer F.SilkS))
  (gr_text 1 (at 137.16 119.38) (layer F.SilkS))
  (gr_text A (at 133.35 119.38) (layer F.SilkS))
  (gr_line (start 165.1 124.46) (end 132.08 124.46) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 165.1 91.44) (end 165.1 124.46) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 132.08 91.44) (end 165.1 91.44) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 132.08 124.46) (end 132.08 91.44) (layer Edge.Cuts) (width 0.127))
)
