(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "D:/KICAD Projects/4272ShaftEncoder_R2/")
    )
  )
  (net 0 "")
  (net 1 "+3.3V")
  (net 2 "GND")
  (net 3 "Net-(LED3-Pad2)")
  (net 4 "/DIR")
  (net 5 "/SDA")
  (net 6 "/SCL")
  (net 7 "/OUT")
  (net 8 "/PGO")
  (footprint "import:3Pin Strain Relief 1x03 2.54mm" (layer "F.Cu")
    (tedit 0)
    (at 153.22 94.434)
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -1.37 -3.834 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Strain3" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -2.54 -2.54) (size 1.778 1.778) (drill 1.778) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -7.62 -2.54) (size 1.778 1.778) (drill 1.778) (layers F&B.Cu *.Mask))
    (pad "" np_thru_hole circle (at -5.08 -2.54) (size 1.778 1.778) (drill 1.778) (layers F&B.Cu *.Mask))
    (pad "1" thru_hole roundrect (at -7.62 -5.334) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.108696)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -5.08 -5.334) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+3.3V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at -2.54 -5.334) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/OUT") (pinfunction "Pin_3") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 144.8 75 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 2.0258 -0.02 180) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/DIR") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 153.9625 78.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0.037497 -1.300002) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 143.5 86 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "TVS1" (at 2.6714 0.3964 180) (layer "F.SilkS"))
    (fp_text value "SP0502BAHT" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/OUT") (pinfunction "K") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.2 75 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at -2.0512 0.5206 180) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/SCL") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.8 75 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at -0.849988 -1.199988 90) (layer "F.SilkS"))
    (fp_text value "137" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(LED3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_1.0x1.0mm_Drill0.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 143.7 82.4)
    (descr "THT rectangular pad as test Point, square 1.0mm side length, hole diameter 0.5mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 8 "/PGO") (pinfunction "1") (pintype "passive"))
  )
  (footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 148.125 71.5)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Description" "Lite-On LTST-C190KGKT, 571 nm Green LED, 1608 (0603) SMD package")
    (property "Height" "0.8")
    (property "Manufacturer_Name" "Lite-On")
    (property "Manufacturer_Part_Number" "LTST-C190KGKT")
    (property "Mouser Part Number" "859-LTST-C190KGKT")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Lite-On/LTST-C190KGKT?qs=205qCy6M2Q%252BAdcgwUZktqw%3D%3D")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "LED3" (at -0.125 1.3) (layer "F.SilkS"))
    (fp_text value "LTST-C190KGKT" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.875 0) (size 1.05 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(LED3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_1.0x1.0mm_Drill0.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 141.2 77.8)
    (descr "THT rectangular pad as test Point, square 1.0mm side length, hole diameter 0.5mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "/SCL") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 143 79.6375 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at -2.8625 -0.9 180) (layer "F.SilkS"))
    (fp_text value "56pF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 90) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_THTPad_1.0x1.0mm_Drill0.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 141.2 79.9)
    (descr "THT rectangular pad as test Point, square 1.0mm side length, hole diameter 0.5mm")
    (tags "test point THT pad rectangle square")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 -1.448) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "/SDA") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.4 75 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at -0.0192 -1.238 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/SDA") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.4 75.0875 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -3.1875 -1.9 180) (layer "F.SilkS"))
    (fp_text value "0" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/DIR") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 0.975 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 153.5 80.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -0.7444 1.2372) (layer "F.SilkS"))
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 147.955 78.1812 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Description" "IC SENSOR MAG ROTARY 12BIT 8SOIC")
    (property "Height" "1.75")
    (property "Manufacturer_Name" "ams")
    (property "Manufacturer_Part_Number" "AS5600-ASOM")
    (property "Mouser Part Number" "985-AS5600-ASOM")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/ams/AS5600-ASOM?qs=KTMMzrZdriG6aU1h9lJCUQ%3D%3D")
    (property "Sheetfile" "4272ShaftEncoder.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 3.4) (layer "B.SilkS"))
    (fp_text value "AS5600-ASOM" (at 0 -3.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pinfunction "VDD5V") (pintype "passive"))
    (pad "2" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pinfunction "VDD3V3") (pintype "passive"))
    (pad "3" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/OUT") (pinfunction "OUT") (pintype "passive"))
    (pad "4" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "5" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/PGO") (pinfunction "PGO") (pintype "passive"))
    (pad "6" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "/SDA") (pinfunction "SDA") (pintype "passive"))
    (pad "7" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "/SCL") (pinfunction "SCL") (pintype "passive"))
    (pad "8" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/DIR") (pinfunction "DIR") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm" (layer "B.Cu")
    (tedit 56D1B4CB)
    (at 148 83.9 180)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 12 1.2) (layer "B.SilkS") hide)
    (fp_text value "MountingHole_2.5mm" (at 0 -3.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 2.54 2.54) (drill 2.54) (layers F&B.Cu *.Mask))
  )
  (gr_line (start 155.9 76.88) (end 155.9 79.42) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 149.245 70.2) (mid 153.64504 72.471473) (end 155.9 76.88) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 154.3 93.46) (end 141.6 93.46) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 141.6 83.1222) (mid 140.568851 81.386813) (end 140 79.45) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 154.3 83.124994) (end 154.3 93.46) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 140 76.91) (end 140 79.45) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 155.9 79.42) (mid 155.335532 81.374212) (end 154.3 83.124994) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 146.705 70.2) (end 149.245 70.2) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 140 76.91) (mid 142.265552 72.468861) (end 146.705 70.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 141.6 93.46) (end 141.6 83.1222) (layer "Edge.Cuts") (width 0.1))
  (gr_text "SCL\n" (at 142.5 76.6 270) (layer "B.SilkS"))
  (gr_text "PGO" (at 145.4 82.7 -90) (layer "B.SilkS"))
  (gr_text "SDA" (at 142.6 79.9 -90) (layer "B.SilkS"))
  (gr_text "Encoder" (at 148.0566 82.042) (layer "F.SilkS"))
  (gr_text "4272 Maverick\nRobotics" (at 147.849996 77.95) (layer "F.SilkS"))
  (gr_text "GND" (at 145.75 87.55) (layer "F.SilkS"))
  (gr_text "3.3V" (at 148.4 87.7) (layer "F.SilkS"))
  (gr_text "MAG" (at 147.955 80.772) (layer "F.SilkS"))
  (gr_text "C" (at 146.0754 71.1454) (layer "F.SilkS"))
  (gr_text "OUT" (at 150.900003 87.600003) (layer "F.SilkS"))
  (gr_text "REV3\n" (at 142.8 91.2 90) (layer "F.SilkS"))
  (gr_text "Bld Date: 2022" (at 153.399998 87.2 90) (layer "F.SilkS"))
  (dimension (type aligned) (layer "User.1")
    (pts (xy 154.3 93.46) (xy 141.6 93.46))
    (height -8.04)
    (gr_text "0.5000 in" (at 147.95 100.35) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.1")
    (pts (xy 154.3 93.46) (xy 147.95 93.46))
    (height -3.69)
    (gr_text "0.2500 in" (at 151.125 96) (layer "User.1"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "User.2")
    (pts (xy 148 78) (xy 148 83.9))
    (height -14)
    (gr_text "0.2323 in" (at 160.85 80.95 90) (layer "User.2"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144 86.8)
        (xy 145.1 89.3)
        (xy 143.7 90.2)
        (xy 143 89.4)
        (xy 143.1 83.3)
        (xy 144 83.3)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.5 95)
        (xy 135 95)
        (xy 135 70)
        (xy 160.5 70)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 151.2 80)
        (xy 144.8 79.8)
        (xy 144.8 76.6)
        (xy 151.2 76.6)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.5 95)
        (xy 135 95)
        (xy 135 70)
        (xy 160.5 70)
      )
    )
  )
)
