(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 112)
    (no_connects 0)
    (area 58.728191 73.701499 117.514858 110.361801)
    (thickness 1.6)
    (drawings 62)
    (tracks 527)
    (zones 0)
    (modules 35)
    (nets 47)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.2032)
    (user_trace_width 0.508)
    (user_trace_width 0.762)
    (user_trace_width 1.016)
    (user_trace_width 1.27)
    (user_trace_width 2.54)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.0992)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x01038_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ./))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 /LOW_PWR-)
  (net 6 +5V)
  (net 7 "Net-(C6-Pad1)")
  (net 8 /AGC_STATUS-)
  (net 9 "Net-(C8-Pad1)")
  (net 10 +6V)
  (net 11 /ATR_RX_ONLY)
  (net 12 /ATR_TX_ONLY)
  (net 13 /ATR_TX+RX)
  (net 14 /ATR_IDLE)
  (net 15 /LOW_PWR)
  (net 16 /AGC_STATUS)
  (net 17 /TEST_MODE)
  (net 18 /TEST_MODE-)
  (net 19 /LOW_PWR+)
  (net 20 /TEST_MODE+)
  (net 21 /TR-)
  (net 22 /AGC_STATUS+)
  (net 23 /TR+)
  (net 24 "Net-(J3-Pad1)")
  (net 25 /TX_ONLY_LED)
  (net 26 "Net-(J3-Pad3)")
  (net 27 /IDLE_LED)
  (net 28 "Net-(J3-Pad5)")
  (net 29 /RX_LED)
  (net 30 "Net-(J3-Pad7)")
  (net 31 /TX_LED)
  (net 32 /TR_SMA)
  (net 33 /TX_ONLY_SMA)
  (net 34 /IDLE_SMA)
  (net 35 /RX_ONLY_SMA)
  (net 36 /TR)
  (net 37 /RX)
  (net 38 /TX)
  (net 39 /IDLE)
  (net 40 VCC)
  (net 41 /OUT_0)
  (net 42 /OUT_1)
  (net 43 "Net-(J3-Pad9)")
  (net 44 "Net-(J3-Pad11)")
  (net 45 /~OUT_0)
  (net 46 /~OUT_1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net +6V)
    (add_net /AGC_STATUS)
    (add_net /AGC_STATUS+)
    (add_net /AGC_STATUS-)
    (add_net /ATR_IDLE)
    (add_net /ATR_RX_ONLY)
    (add_net /ATR_TX+RX)
    (add_net /ATR_TX_ONLY)
    (add_net /IDLE)
    (add_net /IDLE_LED)
    (add_net /IDLE_SMA)
    (add_net /LOW_PWR)
    (add_net /LOW_PWR+)
    (add_net /LOW_PWR-)
    (add_net /OUT_0)
    (add_net /OUT_1)
    (add_net /RX)
    (add_net /RX_LED)
    (add_net /RX_ONLY_SMA)
    (add_net /TEST_MODE)
    (add_net /TEST_MODE+)
    (add_net /TEST_MODE-)
    (add_net /TR)
    (add_net /TR+)
    (add_net /TR-)
    (add_net /TR_SMA)
    (add_net /TX)
    (add_net /TX_LED)
    (add_net /TX_ONLY_LED)
    (add_net /TX_ONLY_SMA)
    (add_net /~OUT_0)
    (add_net /~OUT_1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad9)")
    (add_net VCC)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad locked (layer F.Cu) (tedit 5CABC069)
    (at 105.3425 77.6965)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0.258 -0.036) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0.8295 0.0275) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad locked (layer F.Cu) (tedit 5CABC072)
    (at 71.2225 90.9165)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0.342 -0.048) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at -0.1025 0.1425) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module "U.FL-R-SMT_01_:HRS_U.FL-R-SMT(01)" (layer F.Cu) (tedit 5CAF9DF3)
    (at 97.536 76.2)
    (attr smd)
    (fp_text reference J4 (at -3.048 0.254) (layer F.SilkS))
    (fp_text value TR (at 0.254 3.429) (layer F.SilkS))
    (pad 1 smd rect (at -1.475 0) (size 1.1 2.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.475 0) (size 1.1 2.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 1.55) (size 1.05 1.1) (layers F.Cu F.Paste F.Mask)
      (net 32 /TR_SMA))
  )
  (module "U.FL-R-SMT_01_:HRS_U.FL-R-SMT(01)" (layer F.Cu) (tedit 5CAF9DE7)
    (at 91.186 76.2)
    (attr smd)
    (fp_text reference J5 (at -3.048 0.254) (layer F.SilkS))
    (fp_text value TX_ONLY (at 0.254 3.429) (layer F.SilkS))
    (pad 1 smd rect (at -1.475 0) (size 1.1 2.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.475 0) (size 1.1 2.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 1.55) (size 1.05 1.1) (layers F.Cu F.Paste F.Mask)
      (net 33 /TX_ONLY_SMA))
  )
  (module "U.FL-R-SMT_01_:HRS_U.FL-R-SMT(01)" (layer F.Cu) (tedit 5CAF9DE2)
    (at 84.836 76.2)
    (attr smd)
    (fp_text reference J6 (at -3.048 0.254) (layer F.SilkS))
    (fp_text value IDLE (at 0.254 3.429) (layer F.SilkS))
    (pad 1 smd rect (at -1.475 0) (size 1.1 2.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.475 0) (size 1.1 2.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 1.55) (size 1.05 1.1) (layers F.Cu F.Paste F.Mask)
      (net 34 /IDLE_SMA))
  )
  (module "U.FL-R-SMT_01_:HRS_U.FL-R-SMT(01)" (layer F.Cu) (tedit 5CAF9DD8)
    (at 78.486 76.2)
    (attr smd)
    (fp_text reference J7 (at -3.302 0.254) (layer F.SilkS))
    (fp_text value RX_ONLY (at 0.254 3.429) (layer F.SilkS))
    (pad 1 smd rect (at -1.475 0) (size 1.1 2.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.475 0) (size 1.1 2.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 1.55) (size 1.05 1.1) (layers F.Cu F.Paste F.Mask)
      (net 35 /RX_ONLY_SMA))
  )
  (module TO_SOT_Packages_SMD:SOT-223-3_TabPin2 (layer F.Cu) (tedit 5CC8C753)
    (at 82.804 97.028 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 3.81 -4.572 180) (layer F.SilkS))
    (fp_text value MCP1755ST-5002E/DB (at 5.08 -1.524 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5CAE68B2)
    (at 99.568 93.472 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 3.3528 1.2446 180) (layer F.SilkS))
    (fp_text value BAT46W (at -0.9906 -0.0254 180) (layer F.Fab) hide)
    (fp_text user %R (at -0.0508 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 VCC))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5CC8AF45)
    (at 102.616 102.616 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.286 0.762 360) (layer F.SilkS))
    (fp_text value 1n (at 2.286 -1.524 360) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5CC9F195)
    (at 77.47 98.044 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 1.27 -1.905 180) (layer F.SilkS))
    (fp_text value 0.1u (at 2.54 -0.127 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5CC9F73A)
    (at 102.616 97.536 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 2.286 0.889 180) (layer F.SilkS))
    (fp_text value 10n (at 1.397 -2.286 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 /LOW_PWR-))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5CC8AED6)
    (at 100.076 89.408 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 2.413 -0.254 180) (layer F.SilkS))
    (fp_text value 0.1u (at 1.397 -2.413 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5CC8AF1C)
    (at 88.773 101.6 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 2.413 -0.254 180) (layer F.SilkS))
    (fp_text value 0.1u (at -2.413 0.127 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5CC8AFD7)
    (at 112.776 97.536 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 2.286 -1.778 180) (layer F.SilkS))
    (fp_text value 10n (at -0.127 2.159 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 /AGC_STATUS-))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5CC9F76A)
    (at 112.776 102.616 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 2.667 2.032 360) (layer F.SilkS))
    (fp_text value 0.1u (at 2.667 -1.016 360) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 40 VCC))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5CC8AFB2)
    (at 114.808 102.616 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -2.413 0.127 360) (layer F.SilkS))
    (fp_text value 1n (at -1.27 -1.397 360) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5CC8AEBE)
    (at 93.98 96.012)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 1.143 -1.524) (layer F.SilkS))
    (fp_text value 0.1u (at -3.302 -0.127) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5CC8ADC7)
    (at 71.12 79.248 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -2.413 0.127 360) (layer F.SilkS))
    (fp_text value 0.1u (at 2.286 -0.508 360) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5CC8AE19)
    (at 86.36 89.408 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 2.413 -0.508 180) (layer F.SilkS))
    (fp_text value 0.1u (at 1.016 -2.413 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuse_SMD1206_Reflow (layer F.Cu) (tedit 5CC8AE60)
    (at 82.804 103.124 180)
    (descr "Fuse, Sicherung, SMD1206, Littlefuse-Wickmann, Reflow,")
    (tags "Fuse Sicherung SMD1206 Littlefuse-Wickmann Reflow ")
    (attr smd)
    (fp_text reference F1 (at 1.905 -1.778 180) (layer F.SilkS))
    (fp_text value 500mA (at -2.159 -1.778 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.2 0 270) (size 2.03 1.14) (layers F.Cu F.Paste F.Mask)
      (net 10 +6V))
    (pad 2 smd rect (at 1.2 0 270) (size 2.03 1.14) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5CC8AC7C)
    (at 63.881 87.503)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.921 -0.127) (layer F.SilkS))
    (fp_text value RED (at -3.429 0.127) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5CC8AC79)
    (at 63.881 89.408)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.921 -0.127) (layer F.SilkS))
    (fp_text value YLW (at -3.429 0.127) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J3-Pad3)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5CC8AC77)
    (at 63.881 91.313)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.921 -0.127) (layer F.SilkS))
    (fp_text value GRN (at -3.429 0.127) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J3-Pad5)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5CC8AC76)
    (at 63.881 93.218)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.921 -0.127) (layer F.SilkS))
    (fp_text value BLU (at -3.429 0.127) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J3-Pad7)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module soic_narrow:SOIC-14_N_2 (layer F.Cu) (tedit 5CC9F653)
    (at 105.156 87.376 90)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 3.175 -4.572 180) (layer F.SilkS))
    (fp_text value SN75183D (at -0.635 -1.27 90) (layer F.SilkS))
    (pad 1 smd rect (at -3.81 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 36 /TR))
    (pad 2 smd rect (at -2.54 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 3 smd rect (at -1.27 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 4 smd rect (at 0 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 5 smd rect (at 1.27 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 23 /TR+))
    (pad 6 smd rect (at 2.54 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 21 /TR-))
    (pad 7 smd rect (at 3.81 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 3.81 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 18 /TEST_MODE-))
    (pad 9 smd rect (at 2.54 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 20 /TEST_MODE+))
    (pad 11 smd rect (at 0 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 12 smd rect (at -1.27 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 13 smd rect (at -2.54 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 17 /TEST_MODE))
    (pad 14 smd rect (at -3.81 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 10 smd rect (at 1.27 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module soic_narrow:SOIC-14_N_2 (layer F.Cu) (tedit 5CC8AF0D)
    (at 107.696 100.076 270)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U3 (at -5.842 0.635 360) (layer F.SilkS))
    (fp_text value SN75182DR (at -0.635 -1.27 270) (layer F.SilkS))
    (pad 1 smd rect (at -3.81 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 5 /LOW_PWR-))
    (pad 2 smd rect (at -2.54 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -1.27 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 19 /LOW_PWR+))
    (pad 4 smd rect (at 0 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 40 VCC))
    (pad 5 smd rect (at 1.27 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 6 smd rect (at 2.54 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 15 /LOW_PWR))
    (pad 7 smd rect (at 3.81 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 3.81 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 16 /AGC_STATUS))
    (pad 9 smd rect (at 2.54 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 11 smd rect (at 0 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 22 /AGC_STATUS+))
    (pad 12 smd rect (at -1.27 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 13 smd rect (at -2.54 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 8 /AGC_STATUS-))
    (pad 14 smd rect (at -3.81 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 40 VCC))
    (pad 10 smd rect (at 1.27 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 40 VCC))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module soic_narrow:SOIC-14_N_2 (layer F.Cu) (tedit 5CC8AF26)
    (at 96.012 101.092)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at -5.207 -2.794 180) (layer F.SilkS))
    (fp_text value SN74LS32DR (at 0.381 0.127) (layer F.SilkS))
    (pad 1 smd rect (at -3.81 3.048) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 11 /ATR_RX_ONLY))
    (pad 2 smd rect (at -2.54 3.048) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 /ATR_TX+RX))
    (pad 3 smd rect (at -1.27 3.048) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 37 /RX))
    (pad 4 smd rect (at 0 3.048) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 12 /ATR_TX_ONLY))
    (pad 5 smd rect (at 1.27 3.048) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 /ATR_TX+RX))
    (pad 6 smd rect (at 2.54 3.048) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 38 /TX))
    (pad 7 smd rect (at 3.81 3.048) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 3.81 -2.794) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 36 /TR))
    (pad 9 smd rect (at 2.54 -2.794) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 /ATR_TX+RX))
    (pad 11 smd rect (at 0 -2.794) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 39 /IDLE))
    (pad 12 smd rect (at -1.27 -2.794) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 14 /ATR_IDLE))
    (pad 13 smd rect (at -2.54 -2.794) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 14 /ATR_IDLE))
    (pad 14 smd rect (at -3.81 -2.794) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 10 smd rect (at 1.27 -2.794) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 13 /ATR_TX+RX))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module soic_narrow:SOIC-14_N_2 (layer F.Cu) (tedit 5CC8A6C8)
    (at 66.04 81.28 270)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U5 (at -3.683 5.207 360) (layer F.SilkS))
    (fp_text value SN7406D (at -0.635 -1.27 270) (layer F.SilkS))
    (pad 1 smd rect (at -3.81 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 12 /ATR_TX_ONLY))
    (pad 2 smd rect (at -2.54 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 25 /TX_ONLY_LED))
    (pad 3 smd rect (at -1.27 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 39 /IDLE))
    (pad 4 smd rect (at 0 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 27 /IDLE_LED))
    (pad 5 smd rect (at 1.27 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 37 /RX))
    (pad 6 smd rect (at 2.54 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 29 /RX_LED))
    (pad 7 smd rect (at 3.81 3.048 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 3.81 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 31 /TX_LED))
    (pad 9 smd rect (at 2.54 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 38 /TX))
    (pad 11 smd rect (at 0 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 42 /OUT_1))
    (pad 12 smd rect (at -1.27 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 45 /~OUT_0))
    (pad 13 smd rect (at -2.54 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 41 /OUT_0))
    (pad 14 smd rect (at -3.81 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 10 smd rect (at 1.27 -2.794 270) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 46 /~OUT_1))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module soic_narrow:SOIC-14_N_2 (layer F.Cu) (tedit 5CC8AEEB)
    (at 91.948 87.376 90)
    (descr "Module CMS SOJ 14 pins Large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U6 (at 5.715 -1.524 180) (layer F.SilkS))
    (fp_text value SN74128D (at -0.635 -1.27 90) (layer F.SilkS))
    (pad 1 smd rect (at -3.81 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 32 /TR_SMA))
    (pad 2 smd rect (at -2.54 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 36 /TR))
    (pad 3 smd rect (at -1.27 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 36 /TR))
    (pad 4 smd rect (at 0 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 33 /TX_ONLY_SMA))
    (pad 5 smd rect (at 1.27 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 12 /ATR_TX_ONLY))
    (pad 6 smd rect (at 2.54 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 12 /ATR_TX_ONLY))
    (pad 7 smd rect (at 3.81 3.048 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 3.81 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 39 /IDLE))
    (pad 9 smd rect (at 2.54 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 39 /IDLE))
    (pad 11 smd rect (at 0 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 11 /ATR_RX_ONLY))
    (pad 12 smd rect (at -1.27 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 11 /ATR_RX_ONLY))
    (pad 13 smd rect (at -2.54 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 35 /RX_ONLY_SMA))
    (pad 14 smd rect (at -3.81 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 10 smd rect (at 1.27 -2.794 90) (size 0.508 1.397) (layers F.Cu F.Paste F.Mask)
      (net 34 /IDLE_SMA))
    (model SMD_Packages.3dshapes/SOIC-14_N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.4 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5CC9C4F2)
    (at 63.881 95.123)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.921 -0.127) (layer F.SilkS))
    (fp_text value ~OUT_0 (at -3.429 0) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J3-Pad9)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5CC9C4EB)
    (at 63.881 96.901)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.921 -0.127) (layer F.SilkS))
    (fp_text value ~OUT_1 (at -3.429 0.127) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +5V))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J3-Pad11)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x12_Pitch2.54mm (layer F.Cu) (tedit 5CC9F1C3)
    (at 86.995 107.696 90)
    (descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x12 2.54mm single row")
    (fp_text reference J1 (at 0.254 -2.54 180) (layer F.SilkS))
    (fp_text value LFRX (at -0.127 13.97 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 13.97 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /OUT_0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /OUT_1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 +6V))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /ATR_RX_ONLY))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /ATR_TX_ONLY))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /ATR_TX+RX))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /ATR_IDLE))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /LOW_PWR))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /AGC_STATUS))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /TEST_MODE))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch2.54mm (layer F.Cu) (tedit 5CC9F6CE)
    (at 114.808 92.964 180)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J2 (at -1.016 -2.286 180) (layer F.SilkS))
    (fp_text value "Control Cable" (at 2.413 12.446 180) (layer F.SilkS))
    (fp_text user %R (at 5.08 11.049 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /LOW_PWR-))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /TEST_MODE-))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /LOW_PWR+))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /TEST_MODE+))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /AGC_STATUS-))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /TR-))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /AGC_STATUS+))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /TR+))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x06_Pitch2.54mm (layer F.Cu) (tedit 5CC9EFBF)
    (at 62.23 105.029 90)
    (descr "Through hole straight pin header, 2x06, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x06 2.54mm double row")
    (fp_text reference J3 (at -0.508 -2.286 180) (layer F.SilkS))
    (fp_text value LEDS (at -1.524 16.256 180) (layer F.SilkS))
    (fp_text user %R (at 1.27 6.35 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /TX_ONLY_LED))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /IDLE_LED))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /RX_LED))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /TX_LED))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J3-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /~OUT_0))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J3-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /~OUT_1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module graphics_lib:deadfly_5cm_4cm (layer B.Cu) (tedit 0)
    (at 91.44 91.3765 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_line (start 117.02288 110.28426) (end 117.03558 110.28426) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.02288 109.81182) (end 117.02288 110.28426) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.0296 110.2868) (end 59.0296 109.728) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "TXo IDLE RX  TX   ~OUT~\nRED YLW GRN BLU _0 _1" (at 60.325 99.568) (layer F.SilkS))
  (gr_text "Pin 1 | J1 LFRX Interconnect | Pin 12\nOUT_0 OUT_1 GND +6V RXo TXo TR IDLE LP AGC TM GND->" (at 72.644 108.712) (layer F.SilkS))
  (gr_text "10 TR+ AGC+\n8  TR- AGC-\n6  GND GND\n4  TM+ LP+\n2  TM- LP-" (at 108.966 76.962) (layer F.SilkS))
  (gr_text "Borealis-N200-TXIO v5.0\n-SuperDARN Canada- \n20180405 MD \n20180530 AL\n20190501 KK" (at 73.66 85.344) (layer F.SilkS))
  (gr_line (start 117.0225 110.2845) (end 59.0225 110.2845) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.0225 73.7765) (end 117.0225 109.7765) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.0225 73.7765) (end 117.0225 73.7765) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.0225 73.7765) (end 116.0225 73.7765) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.0225 109.7765) (end 59.0225 73.7765) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.967 109.728) (xy 59.055 109.728) (xy 59.055 73.787) (xy 116.967 73.787)
      )
    )
  )
  (zone (net 40) (net_name VCC) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 113.538 105.156) (xy 101.092 105.156) (xy 101.092 92.71) (xy 113.538 92.71)
      )
    )
  )
  (zone (net 6) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.838 82.169) (xy 110.871 82.169) (xy 110.871 91.948) (xy 100.33 91.948) (xy 100.33 109.728)
        (xy 59.055 109.728) (xy 59.055 73.787) (xy 100.838 73.787)
      )
    )
  )
)
