<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="43.18" x2="32.004" y2="43.18" width="0" layer="20"/>
<wire x1="32.004" y1="43.18" x2="32.004" y2="76.2" width="0" layer="20"/>
<wire x1="32.004" y1="76.2" x2="0" y2="76.2" width="0" layer="20"/>
<wire x1="0" y1="76.2" x2="0" y2="43.18" width="0" layer="20"/>
<text>Angelo DiNardi</text>
<text>GND Bare</text>
<text>PTT Blue</text>
<text>MIC White</text>
<text>SPKR Red</text>
<text>Mic + Speaker Adapter
for Anytone 868
and Elecraft MH-3</text>
</plain>
<libraries>
<library name="SJ-43514">
<packages>
<package name="CUI_SJ-43514">
</package>
</packages>
</library>
<library name="pot">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;&lt;p&gt;
Beckman, Copal, Piher, Spectrol, Schukat&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3RP/1610N">
<description>&lt;b&gt;16mm Potentiometer&lt;/b&gt; one level&lt;p&gt;
Source: http://www.alphapotentiometers.net/html/16mm_pot_2.html</description>
</package>
</packages>
</library>
<library name="54602-908LF">
<packages>
<package name="AMPHENOL_54602-908LF">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="RADIO" library="54602-908LF" package="AMPHENOL_54602-908LF" value="54602-908LF">
<attribute name="DESCRIPTION" value=" Conn Modular Jack F 8 POS 2.54mm Solder RA Thru-Hole 8 Terminal 1 Port Box Cat 3 "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="609-1046-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/amphenol-fci/54602-908LF/609-1046-ND/1001360?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Amphenol FCI"/>
<attribute name="MP" value="54602-908LF"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
</element>
<element name="MIC-MH3" library="SJ-43514" package="CUI_SJ-43514" value="SJ-43514">
<attribute name="CUI_PURCHASE_URL" value="https://www.cui.com/product/interconnect/audio-connectors/3.5-mm-jacks/sj-4351x-series?utm_source=snapeda.com&amp;utm_medium=referral&amp;utm_campaign=snapedaBOM"/>
<attribute name="DESCRIPTION" value=" SJ Series 3.5 mm 16 V 4 Conductor SMT Mid Mount Stereo Audio Jack "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="CP-43514-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/cui-inc/SJ-43514/CP-43514-ND/368146?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="CUI Inc."/>
<attribute name="MP" value="SJ-43514"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="SPEAKER" library="SJ-43514" package="CUI_SJ-43514" value="SJ-43514">
<attribute name="CUI_PURCHASE_URL" value="https://www.cui.com/product/interconnect/audio-connectors/3.5-mm-jacks/sj-4351x-series?utm_source=snapeda.com&amp;utm_medium=referral&amp;utm_campaign=snapedaBOM"/>
<attribute name="DESCRIPTION" value=" SJ Series 3.5 mm 16 V 4 Conductor SMT Mid Mount Stereo Audio Jack "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="CP-43514-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/cui-inc/SJ-43514/CP-43514-ND/368146?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="CUI Inc."/>
<attribute name="MP" value="SJ-43514"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="VOLUME" library="pot" package="3RP/1610N" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="MIC">
<contactref element="MIC-MH3" pad="2"/>
<contactref element="RADIO" pad="3"/>
</signal>
<signal name="SPKR_IN">
<contactref element="VOLUME" pad="2"/>
<contactref element="RADIO" pad="4"/>
</signal>
<signal name="GND">
<contactref element="RADIO" pad="2"/>
<contactref element="SPEAKER" pad="1"/>
<contactref element="MIC-MH3" pad="3"/>
</signal>
<signal name="SPKR-OUT">
<contactref element="SPEAKER" pad="2"/>
<contactref element="VOLUME" pad="3"/>
<contactref element="SPEAKER" pad="3"/>
</signal>
<signal name="RADIO_GND">
<contactref element="RADIO" pad="1"/>
<contactref element="MIC-MH3" pad="4"/>
<contactref element="MIC-MH3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
