(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 40)
    (no_connects 0)
    (area 106.380794 58.205 174.619407 120.904001)
    (thickness 1.6)
    (drawings 14)
    (tracks 51)
    (zones 0)
    (modules 11)
    (nets 89)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user hide)
    (45 Margin user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.00254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7272 1.7272)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P8-Pad3)")
  (net 2 "Net-(P8-Pad4)")
  (net 3 "Net-(P8-Pad5)")
  (net 4 "Net-(P8-Pad6)")
  (net 5 "Net-(P8-Pad7)")
  (net 6 "Net-(P8-Pad8)")
  (net 7 "Net-(P8-Pad9)")
  (net 8 "Net-(P8-Pad10)")
  (net 9 "Net-(P8-Pad13)")
  (net 10 "Net-(P8-Pad14)")
  (net 11 "Net-(P8-Pad15)")
  (net 12 "Net-(P8-Pad16)")
  (net 13 "Net-(P8-Pad17)")
  (net 14 "Net-(P8-Pad18)")
  (net 15 "Net-(P8-Pad19)")
  (net 16 "Net-(P8-Pad20)")
  (net 17 "Net-(P8-Pad21)")
  (net 18 "Net-(P8-Pad22)")
  (net 19 "Net-(P8-Pad23)")
  (net 20 "Net-(P8-Pad24)")
  (net 21 "Net-(P8-Pad25)")
  (net 22 "Net-(P8-Pad26)")
  (net 23 "Net-(P8-Pad27)")
  (net 24 "Net-(P8-Pad28)")
  (net 25 "Net-(P8-Pad29)")
  (net 26 "Net-(P8-Pad30)")
  (net 27 "Net-(P8-Pad31)")
  (net 28 "Net-(P8-Pad32)")
  (net 29 "Net-(P8-Pad33)")
  (net 30 "Net-(P8-Pad34)")
  (net 31 "Net-(P8-Pad35)")
  (net 32 "Net-(P8-Pad36)")
  (net 33 "Net-(P8-Pad37)")
  (net 34 "Net-(P8-Pad38)")
  (net 35 "Net-(P8-Pad39)")
  (net 36 "Net-(P8-Pad40)")
  (net 37 "Net-(P8-Pad41)")
  (net 38 "Net-(P8-Pad42)")
  (net 39 "Net-(P8-Pad43)")
  (net 40 "Net-(P8-Pad44)")
  (net 41 "Net-(P8-Pad45)")
  (net 42 "Net-(P8-Pad46)")
  (net 43 "Net-(P9-Pad11)")
  (net 44 "Net-(P9-Pad12)")
  (net 45 "Net-(P9-Pad13)")
  (net 46 "Net-(P9-Pad14)")
  (net 47 "Net-(P9-Pad15)")
  (net 48 "Net-(P9-Pad16)")
  (net 49 "Net-(P9-Pad17)")
  (net 50 "Net-(P9-Pad18)")
  (net 51 "Net-(P9-Pad19)")
  (net 52 "Net-(P9-Pad20)")
  (net 53 "Net-(P9-Pad21)")
  (net 54 "Net-(P9-Pad22)")
  (net 55 "Net-(P9-Pad23)")
  (net 56 "Net-(P9-Pad25)")
  (net 57 "Net-(P9-Pad26)")
  (net 58 "Net-(P9-Pad27)")
  (net 59 "Net-(P9-Pad28)")
  (net 60 "Net-(P9-Pad29)")
  (net 61 "Net-(P9-Pad30)")
  (net 62 "Net-(P9-Pad31)")
  (net 63 "Net-(P9-Pad33)")
  (net 64 "Net-(P9-Pad35)")
  (net 65 "Net-(P9-Pad36)")
  (net 66 "Net-(P9-Pad37)")
  (net 67 "Net-(P9-Pad38)")
  (net 68 "Net-(P9-Pad39)")
  (net 69 "Net-(P9-Pad40)")
  (net 70 "Net-(P9-Pad41)")
  (net 71 "Net-(P9-Pad42)")
  (net 72 +3V3)
  (net 73 +5V)
  (net 74 /TO_ALTO)
  (net 75 GND)
  (net 76 /COLLISION)
  (net 77 "Net-(J1-Pad6)")
  (net 78 /FROM_ALTO)
  (net 79 /P8_11)
  (net 80 /P8_12)
  (net 81 "Net-(P9-Pad7)")
  (net 82 "Net-(P9-Pad8)")
  (net 83 "Net-(P9-Pad9)")
  (net 84 "Net-(P9-Pad10)")
  (net 85 "Net-(P9-Pad32)")
  (net 86 "Net-(P9-Pad34)")
  (net 87 "Net-(U1-Pad8)")
  (net 88 "Net-(U1-Pad11)")
  (net_class Default "To jest domyślna klasa połączeń."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (add_net +3V3)
    (add_net +5V)
    (add_net /COLLISION)
    (add_net /FROM_ALTO)
    (add_net /P8_11)
    (add_net /P8_12)
    (add_net /TO_ALTO)
    (add_net GND)
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(P8-Pad10)")
    (add_net "Net-(P8-Pad13)")
    (add_net "Net-(P8-Pad14)")
    (add_net "Net-(P8-Pad15)")
    (add_net "Net-(P8-Pad16)")
    (add_net "Net-(P8-Pad17)")
    (add_net "Net-(P8-Pad18)")
    (add_net "Net-(P8-Pad19)")
    (add_net "Net-(P8-Pad20)")
    (add_net "Net-(P8-Pad21)")
    (add_net "Net-(P8-Pad22)")
    (add_net "Net-(P8-Pad23)")
    (add_net "Net-(P8-Pad24)")
    (add_net "Net-(P8-Pad25)")
    (add_net "Net-(P8-Pad26)")
    (add_net "Net-(P8-Pad27)")
    (add_net "Net-(P8-Pad28)")
    (add_net "Net-(P8-Pad29)")
    (add_net "Net-(P8-Pad3)")
    (add_net "Net-(P8-Pad30)")
    (add_net "Net-(P8-Pad31)")
    (add_net "Net-(P8-Pad32)")
    (add_net "Net-(P8-Pad33)")
    (add_net "Net-(P8-Pad34)")
    (add_net "Net-(P8-Pad35)")
    (add_net "Net-(P8-Pad36)")
    (add_net "Net-(P8-Pad37)")
    (add_net "Net-(P8-Pad38)")
    (add_net "Net-(P8-Pad39)")
    (add_net "Net-(P8-Pad4)")
    (add_net "Net-(P8-Pad40)")
    (add_net "Net-(P8-Pad41)")
    (add_net "Net-(P8-Pad42)")
    (add_net "Net-(P8-Pad43)")
    (add_net "Net-(P8-Pad44)")
    (add_net "Net-(P8-Pad45)")
    (add_net "Net-(P8-Pad46)")
    (add_net "Net-(P8-Pad5)")
    (add_net "Net-(P8-Pad6)")
    (add_net "Net-(P8-Pad7)")
    (add_net "Net-(P8-Pad8)")
    (add_net "Net-(P8-Pad9)")
    (add_net "Net-(P9-Pad10)")
    (add_net "Net-(P9-Pad11)")
    (add_net "Net-(P9-Pad12)")
    (add_net "Net-(P9-Pad13)")
    (add_net "Net-(P9-Pad14)")
    (add_net "Net-(P9-Pad15)")
    (add_net "Net-(P9-Pad16)")
    (add_net "Net-(P9-Pad17)")
    (add_net "Net-(P9-Pad18)")
    (add_net "Net-(P9-Pad19)")
    (add_net "Net-(P9-Pad20)")
    (add_net "Net-(P9-Pad21)")
    (add_net "Net-(P9-Pad22)")
    (add_net "Net-(P9-Pad23)")
    (add_net "Net-(P9-Pad25)")
    (add_net "Net-(P9-Pad26)")
    (add_net "Net-(P9-Pad27)")
    (add_net "Net-(P9-Pad28)")
    (add_net "Net-(P9-Pad29)")
    (add_net "Net-(P9-Pad30)")
    (add_net "Net-(P9-Pad31)")
    (add_net "Net-(P9-Pad32)")
    (add_net "Net-(P9-Pad33)")
    (add_net "Net-(P9-Pad34)")
    (add_net "Net-(P9-Pad35)")
    (add_net "Net-(P9-Pad36)")
    (add_net "Net-(P9-Pad37)")
    (add_net "Net-(P9-Pad38)")
    (add_net "Net-(P9-Pad39)")
    (add_net "Net-(P9-Pad40)")
    (add_net "Net-(P9-Pad41)")
    (add_net "Net-(P9-Pad42)")
    (add_net "Net-(P9-Pad7)")
    (add_net "Net-(P9-Pad8)")
    (add_net "Net-(P9-Pad9)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad8)")
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
  )
  (module Socket_BeagleBone_Black:Socket_BeagleBone_Black (layer F.Cu) (tedit 5A39FE3B)
    (at 116.3701 62.3824)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P9 (at 5.6769 0.1016) (layer F.SilkS))
    (fp_text value BeagleBone_Black_Header (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 +3V3))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 +5V))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 +5V))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(P9-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(P9-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(P9-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(P9-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(P9-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(P9-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(P9-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(P9-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P9-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(P9-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(P9-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(P9-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(P9-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(P9-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(P9-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(P9-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(P9-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 /FROM_ALTO))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(P9-Pad25)"))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(P9-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(P9-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(P9-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(P9-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(P9-Pad30)"))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(P9-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(P9-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(P9-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(P9-Pad34)"))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(P9-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(P9-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(P9-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(P9-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(P9-Pad39)"))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(P9-Pad40)"))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(P9-Pad41)"))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(P9-Pad42)"))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 GND))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 GND))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 GND))
    (pad 46 thru_hole oval (at 2.54 55.88) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 GND))
    (model ${KIPRJMOD}/Socket_BeagleBone_Black.3dshapes/Socket_BeagleBone_Black.wrl
      (at (xyz 0.05 -1.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Socket_BeagleBone_Black:Socket_BeagleBone_Black (layer F.Cu) (tedit 5A39FE30)
    (at 164.6301 62.3824)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at -3.0861 -0.0254) (layer F.SilkS))
    (fp_text value BeagleBone_Black_Header (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P8-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P8-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P8-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P8-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P8-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P8-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P8-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P8-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 /P8_11))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 /P8_12))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P8-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P8-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P8-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(P8-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(P8-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P8-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P8-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P8-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(P8-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P8-Pad22)"))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P8-Pad23)"))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P8-Pad24)"))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(P8-Pad25)"))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(P8-Pad26)"))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(P8-Pad27)"))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(P8-Pad28)"))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(P8-Pad29)"))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(P8-Pad30)"))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(P8-Pad31)"))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P8-Pad32)"))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P8-Pad33)"))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(P8-Pad34)"))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(P8-Pad35)"))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P8-Pad36)"))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(P8-Pad37)"))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P8-Pad38)"))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(P8-Pad39)"))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(P8-Pad40)"))
    (pad 41 thru_hole oval (at 0 50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(P8-Pad41)"))
    (pad 42 thru_hole oval (at 2.54 50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P8-Pad42)"))
    (pad 43 thru_hole oval (at 0 53.34) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P8-Pad43)"))
    (pad 44 thru_hole oval (at 2.54 53.34) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P8-Pad44)"))
    (pad 45 thru_hole oval (at 0 55.88) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P8-Pad45)"))
    (pad 46 thru_hole oval (at 2.54 55.88) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P8-Pad46)"))
    (model ${KIPRJMOD}/Socket_BeagleBone_Black.3dshapes/Socket_BeagleBone_Black.wrl
      (at (xyz 0.05 -1.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:RJ45_8 (layer F.Cu) (tedit 0)
    (at 138.43 104.14)
    (tags RJ45)
    (fp_text reference J1 (at 4.7 11.18) (layer F.SilkS))
    (fp_text value RJ45 (at 4.59 6.25) (layer F.Fab))
    (pad Hole np_thru_hole circle (at 10.38 6.35) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -1.49 6.35) (size 3.65 3.65) (drill 3.25) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 2 thru_hole circle (at 1.27 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 74 /TO_ALTO))
    (pad 3 thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 4 thru_hole circle (at 3.81 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 76 /COLLISION))
    (pad 5 thru_hole circle (at 5.08 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 6 thru_hole circle (at 6.35 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 77 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 8 thru_hole circle (at 8.89 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 78 /FROM_ALTO))
    (model ${KISYS3DMOD}/Connectors.3dshapes/RJ45_8.wrl
      (at (xyz 0.18 -0.25 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun:AXIAL-0.3 (layer F.Cu) (tedit 200000)
    (at 143.13662 79.22006)
    (descr AXIAL-0.3)
    (tags AXIAL-0.3)
    (attr virtual)
    (fp_text reference R1 (at 0 -1.397) (layer F.SilkS))
    (fp_text value unused (at 0 1.397) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
      (net 73 +5V) (solder_mask_margin 0.1016))
    (pad P$2 thru_hole circle (at 3.81 0) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
      (net 74 /TO_ALTO) (solder_mask_margin 0.1016))
  )
  (module SparkFun:AXIAL-0.3 (layer F.Cu) (tedit 200000)
    (at 143.13662 82.98688 180)
    (descr AXIAL-0.3)
    (tags AXIAL-0.3)
    (attr virtual)
    (fp_text reference R2 (at 0 -1.397 180) (layer F.SilkS))
    (fp_text value unused (at 0 1.397 180) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0 180) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
      (net 74 /TO_ALTO) (solder_mask_margin 0.1016))
    (pad P$2 thru_hole circle (at 3.81 0 180) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
      (net 75 GND) (solder_mask_margin 0.1016))
  )
  (module SparkFun:AXIAL-0.3 (layer F.Cu) (tedit 200000)
    (at 155.067 104.648 270)
    (descr AXIAL-0.3)
    (tags AXIAL-0.3)
    (attr virtual)
    (fp_text reference R3 (at 0 -1.397 270) (layer F.SilkS))
    (fp_text value 120 (at 0 1.397 270) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0 270) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
      (net 72 +3V3) (solder_mask_margin 0.1016))
    (pad P$2 thru_hole circle (at 3.81 0 270) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
      (net 78 /FROM_ALTO) (solder_mask_margin 0.1016))
  )
  (module SparkFun:AXIAL-0.3 (layer F.Cu) (tedit 200000)
    (at 159.258 104.648 90)
    (descr AXIAL-0.3)
    (tags AXIAL-0.3)
    (attr virtual)
    (fp_text reference R4 (at 0 -1.397 90) (layer F.SilkS))
    (fp_text value 330 (at 0 1.397 90) (layer F.SilkS))
    (pad P$1 thru_hole circle (at -3.81 0 90) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
      (net 78 /FROM_ALTO) (solder_mask_margin 0.1016))
    (pad P$2 thru_hole circle (at 3.81 0 90) (size 1.8796 1.8796) (drill 0.89916) (layers *.Cu *.Mask)
      (net 75 GND) (solder_mask_margin 0.1016))
  )
  (module Housings_DIP:DIP-14_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 152.75814 76.64704)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value 7438 (at 3.81 17.57) (layer F.Fab))
    (fp_text user %R (at 3.81 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 /P8_11))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(U1-Pad8)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 /P8_11))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 /TO_ALTO))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 /P8_12))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(U1-Pad11)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 /P8_12))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 /COLLISION))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 GND))
    (pad 14 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 +5V))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-14_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 144.272 86.36 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at 1.25 -2.11 180) (layer F.SilkS))
    (fp_text value unused (at 1.25 2.11 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 /TO_ALTO))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 597BC7C2)
    (at 155.615 97.79)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C2 (at 1.25 -2.11) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.11) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 +3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5A39FDFB)
    (at 157.607 72.009 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C3 (at 1.143 3.556 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 2.11 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Alto 3Mb Ethernet\ninterface\n\nKen Shirriff\nrighto.com/ether" (at 127.381 81.788 270) (layer F.SilkS))
  (gr_text "Warning:\nNot a standard\nEthernet port\n" (at 130.81 109.22 270) (layer F.SilkS))
  (gr_line (start 162.56 120.8151) (end 162.56 118.11) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 120.9802 120.8151) (end 114.4651 120.8151) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 120.9802 118.11) (end 120.9802 120.8151) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 162.56 118.11) (end 120.9802 118.11) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 169.0751 120.8151) (end 162.56 120.8151) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 114.4651 59.7027) (end 135.4201 59.7027) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 135.4201 64.2874) (end 135.4201 59.7027) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 153.2001 64.2874) (end 135.4201 64.2874) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 153.2001 59.7027) (end 153.2001 64.2874) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 169.0751 59.7027) (end 153.2001 59.7027) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 169.0751 120.8151) (end 169.0751 59.7027) (layer Edge.Cuts) (width 0.00254))
  (gr_line (start 114.4651 59.7027) (end 114.4651 120.8151) (layer Edge.Cuts) (width 0.00254))
  (zone (net 75) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.554 59.69) (xy 135.382 59.69) (xy 135.382 64.389) (xy 153.162 64.389) (xy 153.162 59.69)
        (xy 169.037 59.69) (xy 169.037 120.777) (xy 162.56 120.777) (xy 162.56 118.11) (xy 120.904 118.11)
        (xy 120.904 120.777) (xy 114.427 120.777) (xy 114.427 59.817)
      )
    )
  )
  (zone (net 75) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.427 59.69) (xy 135.382 59.69) (xy 135.382 64.516) (xy 153.289 64.77) (xy 153.162 59.69)
        (xy 169.037 59.69) (xy 169.037 120.777) (xy 162.56 120.904) (xy 162.433 118.11) (xy 120.904 118.237)
        (xy 120.904 120.777) (xy 114.427 120.777) (xy 114.427 59.817)
      )
    )
  )
)
