(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 154)
    (no_connects 0)
    (area 92.03 75.035 153.143811 141.945)
    (thickness 1.6)
    (drawings 56)
    (tracks 705)
    (zones 0)
    (modules 66)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.1)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.1778)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 258.8 150.2)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(C4-Pad1)")
  (net 4 "Net-(C7-Pad1)")
  (net 5 +9V)
  (net 6 "Net-(C10-Pad1)")
  (net 7 /ToCoil)
  (net 8 "Net-(C12-Pad2)")
  (net 9 /Pi5v)
  (net 10 /32u4-MISO)
  (net 11 /32u4-SCK)
  (net 12 /32u4-MOSI)
  (net 13 /32u4-Reset)
  (net 14 /Vin-Raw)
  (net 15 "Net-(D1-Pad1)")
  (net 16 "Net-(D2-Pad1)")
  (net 17 "Net-(D3-Pad2)")
  (net 18 "Net-(D3-Pad1)")
  (net 19 "Net-(D4-Pad2)")
  (net 20 "Net-(D4-Pad1)")
  (net 21 /PWR-SIG)
  (net 22 "Net-(D5-Pad1)")
  (net 23 "Net-(D6-Pad2)")
  (net 24 "Net-(D7-Pad2)")
  (net 25 "Net-(D8-Pad1)")
  (net 26 /OFF-PATH)
  (net 27 "Net-(J1-Pad3)")
  (net 28 "Net-(J1-Pad5)")
  (net 29 "Net-(J1-Pad8)")
  (net 30 "Net-(J1-Pad10)")
  (net 31 /sigFromPi)
  (net 32 /sigToPi)
  (net 33 /SNES-LATCH)
  (net 34 /SNES-DATA1)
  (net 35 /SNES-DATA2)
  (net 36 /SNES-CLK)
  (net 37 "Net-(P5-Pad1)")
  (net 38 /32u4-SCL)
  (net 39 /32u4-RXD)
  (net 40 /32u4-SDA)
  (net 41 /32u4-TXD)
  (net 42 /Front-LED)
  (net 43 /32u4-RXLED)
  (net 44 /32u4-TXLED)
  (net 45 /SW-SENSE)
  (net 46 "Net-(R17-Pad2)")
  (net 47 /Load-En)
  (net 48 /D_P)
  (net 49 /D_N)
  (net 50 /XTAL_P)
  (net 51 /XTAL_N)
  (net 52 /sigJPER)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /32u4-TXLED)
    (add_net /Front-LED)
    (add_net /Load-En)
    (add_net /OFF-PATH)
    (add_net /ToCoil)
    (add_net /sigJPER)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(R17-Pad2)")
  )
  (net_class "Diff Signal" ""
    (clearance 0.18)
    (trace_width 0.16)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D_N)
    (add_net /D_P)
    (add_net /XTAL_N)
    (add_net /XTAL_P)
  )
  (net_class "Digital Signal" ""
    (clearance 0.18)
    (trace_width 0.16)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /32u4-MISO)
    (add_net /32u4-MOSI)
    (add_net /32u4-RXD)
    (add_net /32u4-RXLED)
    (add_net /32u4-Reset)
    (add_net /32u4-SCK)
    (add_net /32u4-SCL)
    (add_net /32u4-SDA)
    (add_net /32u4-TXD)
    (add_net /SNES-CLK)
    (add_net /SNES-DATA1)
    (add_net /SNES-DATA2)
    (add_net /SNES-LATCH)
    (add_net /SW-SENSE)
    (add_net /sigFromPi)
    (add_net /sigToPi)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +9V)
    (add_net /PWR-SIG)
    (add_net /Pi5v)
    (add_net /Vin-Raw)
    (add_net GND)
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D8-Pad1)")
  )
  (module Pin_Headers:Pin_Header_Straight_2x20 (layer F.Cu) (tedit 594F7381)
    (at 146.42 84.51)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value Raspberry_Pi_2_3 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /Pi5v))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 /Pi5v))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 /sigFromPi))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /sigToPi))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x20.wrl
      (at (xyz 0.05 -0.95 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 594F74B6)
    (at 147.69 79.51)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (fp_text reference J6 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0.14) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 594F1538)
    (at 116.12 124.75)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.2 -0.5) (layer F.SilkS) hide)
    (fp_text value 1k (at 1.9 3.63) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 /32u4-TXLED))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 594F617B)
    (at 116.12 122.24 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.275 -0.825 180) (layer F.SilkS) hide)
    (fp_text value 1k (at -1.3 -1.24 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /32u4-RXLED))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 594F5EF5)
    (at 107.9 108.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -1.08 -1.41) (layer F.SilkS))
    (fp_text value 1k (at 0 0.01) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(P5-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 /Front-LED))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 594F5C61)
    (at 100.7 101.49 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value PWR (at 0.05 -2.68 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 /Vin-Raw))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 594F451F)
    (at 142.86 94.33)
    (fp_text reference J9 (at -2.145 -0.015) (layer F.SilkS) hide)
    (fp_text value TX (at -3.4 0.04) (layer F.SilkS))
    (pad 1 smd rect (at -0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 41 /32u4-TXD))
    (pad 2 smd rect (at 0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J1-Pad10)"))
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 594F4513)
    (at 142.86 91.84)
    (fp_text reference J8 (at -2.1 0.05) (layer F.SilkS) hide)
    (fp_text value RX (at -3.4 0) (layer F.SilkS))
    (pad 1 smd rect (at -0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 39 /32u4-RXD))
    (pad 2 smd rect (at 0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J1-Pad8)"))
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 594F4527)
    (at 142.86 89.3)
    (fp_text reference J7 (at -2.125 0.025) (layer F.SilkS) hide)
    (fp_text value SCL (at -3.4 0) (layer F.SilkS))
    (pad 1 smd rect (at -0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 38 /32u4-SCL))
    (pad 2 smd rect (at 0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J1-Pad5)"))
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 594F452B)
    (at 142.86 86.78)
    (fp_text reference J2 (at -2.05 0) (layer F.SilkS) hide)
    (fp_text value SDA (at -3.4 0) (layer F.SilkS))
    (pad 1 smd rect (at -0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 40 /32u4-SDA))
    (pad 2 smd rect (at 0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-Pad3)"))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F6234)
    (at 142.84 124.69 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R19 (at -0.01 3.5 180) (layer F.SilkS))
    (fp_text value 100k (at 2.19 0.94 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 32 /sigToPi))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 52 /sigJPER))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 594F5F73)
    (at 114.61 89.63 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0.03 -1.43 90) (layer F.SilkS))
    (fp_text value 10k (at 1.97 0.03 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R17-Pad2)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 594F5F2B)
    (at 114.61 92.84 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0.03 -1.43 90) (layer F.SilkS))
    (fp_text value 55k (at -2.07 0.08 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /Pi5v))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R17-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 594F61AB)
    (at 125.79 111.83 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -0.02 -1.46 90) (layer F.SilkS))
    (fp_text value 6.8k (at 2.04 0.02 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module jumper:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 594EF56F)
    (at 142.86 127.2)
    (fp_text reference JP1 (at -2.4 0.025) (layer F.SilkS) hide)
    (fp_text value SIGPI (at -2.95 0.035) (layer F.SilkS))
    (pad 1 smd rect (at -0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 52 /sigJPER))
    (pad 2 smd rect (at 0.65 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 32 /sigToPi))
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F5FAE)
    (at 126.875 86.075 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at -2.345 -0.195 360) (layer F.SilkS))
    (fp_text value 10uF (at 0.045 -1.475 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +9V))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F6293)
    (at 136.19 99.34 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 2.32 0.04 180) (layer F.SilkS))
    (fp_text value 100nF (at 0.06 1.51 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 +9V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F6254)
    (at 136.235 105.745 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -1.255 -1.525 180) (layer F.SilkS))
    (fp_text value 4.7uF (at -2.445 -0.165 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F6270)
    (at 132.845 102.965 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 2.235 0.025 180) (layer F.SilkS))
    (fp_text value 10nF (at -0.045 -1.515 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F27AD)
    (at 142.84 122.67)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -2.1) (layer F.SilkS) hide)
    (fp_text value 100k (at -3.06 -2.79) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 52 /sigJPER))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F62BE)
    (at 142.86 96.9 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R8 (at 2.5 -0.64 180) (layer F.SilkS))
    (fp_text value 100k (at -0.06 -1.58 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 /sigFromPi))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F6218)
    (at 141.33 137.82)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R7 (at 2.37 0.03) (layer F.SilkS))
    (fp_text value 1k (at 0.11 1.47) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F6215)
    (at 136.48 137.82)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R6 (at -2.4 0.21) (layer F.SilkS))
    (fp_text value 1k (at 0.1 1.5) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F61B8)
    (at 121.19 133.01 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference R1 (at -2.23 0.04 270) (layer F.SilkS))
    (fp_text value 100k (at -0.07 -1.44 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 /32u4-Reset))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F6952)
    (at 121.2 131 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -2.29 0.04 270) (layer F.SilkS))
    (fp_text value 0.1u (at -0.11 1.38 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F620F)
    (at 138.01 130.84)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 1.24 -1.42) (layer F.SilkS))
    (fp_text value 0.1u (at 0.02 1.38) (layer F.SilkS))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F6175)
    (at 120.82 124.43 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -1.36 -1.58 360) (layer F.SilkS))
    (fp_text value 1.0u (at 0 1.4 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F6158)
    (at 121.79 120.47 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 2.38 -0.06 180) (layer F.SilkS))
    (fp_text value 10uF (at 0.07 -1.44 90) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F6900)
    (at 125.345 135.435 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.255 -0.005 360) (layer F.SilkS) hide)
    (fp_text value 22p (at 2.335 -0.075 360) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 51 /XTAL_N))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F6925)
    (at 130.855 135.385 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.865 1.795 90) (layer F.SilkS) hide)
    (fp_text value 22p (at -2.275 -0.015 180) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 50 /XTAL_P))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 594F7521)
    (at 98.5 79.8)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (fp_text reference J5 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0.19 -0.15) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 594F75BA)
    (at 147.66 137.37)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (fp_text reference J4 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0.03 0.28) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad (layer F.Cu) (tedit 594F752A)
    (at 98.8 137.3)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (fp_text reference J3 (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -0.11 0.35) (size 5 5) (drill 2.5) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Crystals_Oscillators_SMD:crystal_FA238-TSX3225 (layer F.Cu) (tedit 594F61D4)
    (at 128.085 135.435 270)
    (descr "crystal Epson Toyocom FA-238 and TSX-3225 series")
    (fp_text reference Y1 (at 2.475 -0.025 360) (layer F.SilkS))
    (fp_text value 16MHz (at 4.485 -0.005 360) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0.8 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 51 /XTAL_N))
    (pad 3 smd rect (at 1.1 0.8 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.1 -0.8 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 1.1 -0.8 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 50 /XTAL_P))
    (model Crystals_Oscillators_SMD.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 594F5FDA)
    (at 129.665 90.745 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C14 (at -2.705 -0.015 360) (layer F.SilkS))
    (fp_text value 47uF (at -1.225 -1.745 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /Pi5v))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 594F5F8B)
    (at 117.51 87.86 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at -2.23 -0.39 180) (layer F.SilkS))
    (fp_text value 100nF (at 1.09 1.59 270) (layer F.SilkS))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 /ToCoil))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C12-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 594F61A6)
    (at 115.89 112.72 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R14 (at -0.04 1.64 180) (layer F.SilkS))
    (fp_text value 6.8k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 45 /SW-SENSE))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 594F5EDE)
    (at 111.49 112.72 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R11 (at 0.03 -1.68 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 45 /SW-SENSE))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /PWR-SIG))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 594F61A3)
    (at 120.29 112.72 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R10 (at -0.05 1.61 180) (layer F.SilkS))
    (fp_text value 10k (at -0.055 0.005 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 594F66C2)
    (at 122.715 86.085 180)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U3 (at -1.405 2.285 180) (layer F.SilkS))
    (fp_text value TPS563200 (at 0 2.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 /ToCoil))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 +9V))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(R17-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C12-Pad2)"))
    (pad 5 smd rect (at 1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 47 /Load-En))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 594F6260)
    (at 136.235 102.945)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 2.575 -0.125 90) (layer F.SilkS))
    (fp_text value NJM2870 (at -2.045 4.445) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C7-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 +9V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 594F5E9E)
    (at 120.19 106.6 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R16 (at -0.375 -2.4 270) (layer F.SilkS) hide)
    (fp_text value 1k (at 0.025 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 594F5E85)
    (at 112.24 106.65 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R15 (at -1.4 -1.95 270) (layer F.SilkS) hide)
    (fp_text value 1k (at 0 0.025 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206 (layer F.Cu) (tedit 594F5E98)
    (at 116.22 107.45)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R13 (at 6.22 -1.375) (layer F.SilkS) hide)
    (fp_text value 1k (at 0.02 -0.025) (layer F.SilkS))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 594F5EC8)
    (at 116.22 100.47 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 2.11 1.23 180) (layer F.SilkS))
    (fp_text value FET-Rev (at 0 2.5 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 +9V))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 /Vin-Raw))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 594F5C64)
    (at 100.7 105.01 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value SW (at -0.24 -2.62 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 5 +9V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 /PWR-SIG))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 594F5C69)
    (at 100.7 108.51 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value LED (at -0.17 -2.66 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "Net-(P5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05 (layer F.Cu) (tedit 594F651A)
    (at 100.55 120.8)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value SNES-HDR (at 4.03 -2.73) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /SNES-LATCH))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 /SNES-LATCH))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 /SNES-DATA1))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 /SNES-DATA2))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /SNES-CLK))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 /SNES-CLK))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x05.wrl
      (at (xyz 0.05 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 594F696C)
    (at 120.17 101.19 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D8 (at -0.71 2.16 90) (layer F.SilkS) hide)
    (fp_text value POWER (at 0.09 2.2 270) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 +9V))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D8-Pad1)"))
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 594F5C72)
    (at 112.24 101.31 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D7 (at -3.61 -0.025 270) (layer F.SilkS) hide)
    (fp_text value REVERSE (at 0 2 270) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 /Vin-Raw))
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 594F621A)
    (at 141.33 135.57 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D4 (at -0.01 1.7 180) (layer F.SilkS))
    (fp_text value 32u4-LED2 (at -4.52 -1.25 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad1)"))
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 594F621E)
    (at 136.33 135.57)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D3 (at -0.02 -1.72) (layer F.SilkS))
    (fp_text value 32u4-LED1 (at -2.43 -0.97) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D3-Pad1)"))
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 594F5D10)
    (at 112 124.65 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at -2.7 -2.5 180) (layer F.SilkS) hide)
    (fp_text value TX (at 3.61 -0.04 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D2-Pad1)"))
  )
  (module LEDs:LED-1206 (layer F.Cu) (tedit 594F5D0C)
    (at 112 122.15 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at -3.5 0.05 180) (layer F.SilkS) hide)
    (fp_text value RX (at 3.61 -0.03 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D1-Pad1)"))
  )
  (module freetronics_footprints:2X03 (layer F.Cu) (tedit 594EBB77)
    (at 113.77 136.96)
    (descr "<b>PIN HEADER</b>")
    (fp_text reference CON1 (at -2.54 0 90) (layer Eco1.User) hide)
    (fp_text value ISP-32u4 (at 0 3.175) (layer Eco1.User) hide)
    (pad 1 thru_hole oval (at -2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 /32u4-MISO))
    (pad 2 thru_hole oval (at -2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 /32u4-SCK))
    (pad 4 thru_hole oval (at 0 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 /32u4-MOSI))
    (pad 5 thru_hole oval (at 2.54 1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 /32u4-Reset))
    (pad 6 thru_hole oval (at 2.54 -1.27) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Capacitors_SMD:c_elec_5x5.3 (layer F.Cu) (tedit 594F614B)
    (at 132.24 110.87)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.3")
    (attr smd)
    (fp_text reference C10 (at 2.82 4.04 180) (layer F.SilkS))
    (fp_text value 10uF (at 4.89 -0.01 90) (layer F.SilkS))
    (fp_text user + (at -1.3716 -0.0762) (layer F.Fab))
    (fp_text user + (at -3.3782 2.3368) (layer F.SilkS))
    (pad 1 smd rect (at -2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 2.2 0 180) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/c_elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:c_elec_5x5.3 (layer F.Cu) (tedit 594F5FC2)
    (at 126.98 103.47 270)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.3")
    (attr smd)
    (fp_text reference C9 (at -4.61 -3.25 360) (layer F.SilkS))
    (fp_text value "47uF 10V" (at -4.39 0.98 360) (layer F.SilkS))
    (fp_text user + (at -1.3716 -0.0762 270) (layer F.Fab))
    (fp_text user + (at -3.3782 2.3368 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.2 0 90) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +9V))
    (pad 2 smd rect (at 2.2 0 90) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/c_elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module ATMEGA32U4-AU:QFP80P1200X1200X120-44N (layer F.Cu) (tedit 594F6758)
    (at 130.71 125.06)
    (solder_mask_margin 0.1)
    (attr smd)
    (fp_text reference U1 (at -5.82 -5.87) (layer F.SilkS))
    (fp_text value ATMEGA32U4-AU (at 1.7526 -11.1252) (layer F.SilkS) hide)
    (pad 1 smd rect (at -5.7404 -3.9878 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 2 smd rect (at -5.7404 -3.2004 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V) (solder_mask_margin 0.2))
    (pad 3 smd rect (at -5.7404 -2.3876 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 49 /D_N) (solder_mask_margin 0.2))
    (pad 4 smd rect (at -5.7404 -1.6002 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 48 /D_P) (solder_mask_margin 0.2))
    (pad 5 smd rect (at -5.7404 -0.7874 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.2))
    (pad 6 smd rect (at -5.7404 0 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C4-Pad1)") (solder_mask_margin 0.2))
    (pad 7 smd rect (at -5.7404 0.7874 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V) (solder_mask_margin 0.2))
    (pad 8 smd rect (at -5.7404 1.6002 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 43 /32u4-RXLED) (solder_mask_margin 0.2))
    (pad 9 smd rect (at -5.7404 2.3876 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 11 /32u4-SCK) (solder_mask_margin 0.2))
    (pad 10 smd rect (at -5.7404 3.2004 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 12 /32u4-MOSI) (solder_mask_margin 0.2))
    (pad 11 smd rect (at -5.7404 3.9878 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 10 /32u4-MISO) (solder_mask_margin 0.2))
    (pad 12 smd rect (at -3.9878 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 13 smd rect (at -3.2004 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 13 /32u4-Reset) (solder_mask_margin 0.2))
    (pad 14 smd rect (at -2.3876 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V) (solder_mask_margin 0.2))
    (pad 15 smd rect (at -1.6002 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.2))
    (pad 16 smd rect (at -0.7874 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 51 /XTAL_N) (solder_mask_margin 0.2))
    (pad 17 smd rect (at 0 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 50 /XTAL_P) (solder_mask_margin 0.2))
    (pad 18 smd rect (at 0.7874 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 38 /32u4-SCL) (solder_mask_margin 0.2))
    (pad 19 smd rect (at 1.6002 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 40 /32u4-SDA) (solder_mask_margin 0.2))
    (pad 20 smd rect (at 2.3876 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 39 /32u4-RXD) (solder_mask_margin 0.2))
    (pad 21 smd rect (at 3.2004 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 41 /32u4-TXD) (solder_mask_margin 0.2))
    (pad 22 smd rect (at 3.9878 5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 44 /32u4-TXLED) (solder_mask_margin 0.2))
    (pad 23 smd rect (at 5.7404 3.9878 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.2))
    (pad 24 smd rect (at 5.7404 3.2004 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V) (solder_mask_margin 0.2))
    (pad 25 smd rect (at 5.7404 2.3876 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 26 smd rect (at 5.7404 1.6002 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D3-Pad2)") (solder_mask_margin 0.2))
    (pad 27 smd rect (at 5.7404 0.7874 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D4-Pad2)") (solder_mask_margin 0.2))
    (pad 28 smd rect (at 5.7404 0 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 33 /SNES-LATCH) (solder_mask_margin 0.2))
    (pad 29 smd rect (at 5.7404 -0.7874 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 34 /SNES-DATA1) (solder_mask_margin 0.2))
    (pad 30 smd rect (at 5.7404 -1.6002 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 35 /SNES-DATA2) (solder_mask_margin 0.2))
    (pad 31 smd rect (at 5.7404 -2.3876 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 36 /SNES-CLK) (solder_mask_margin 0.2))
    (pad 32 smd rect (at 5.7404 -3.2004 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 33 smd rect (at 5.7404 -3.9878 270) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 34 smd rect (at 3.9878 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V) (solder_mask_margin 0.2))
    (pad 35 smd rect (at 3.2004 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.2))
    (pad 36 smd rect (at 2.3876 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 52 /sigJPER) (solder_mask_margin 0.2))
    (pad 37 smd rect (at 1.6002 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 31 /sigFromPi) (solder_mask_margin 0.2))
    (pad 38 smd rect (at 0.7874 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 47 /Load-En) (solder_mask_margin 0.2))
    (pad 39 smd rect (at 0 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 26 /OFF-PATH) (solder_mask_margin 0.2))
    (pad 40 smd rect (at -0.7874 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 45 /SW-SENSE) (solder_mask_margin 0.2))
    (pad 41 smd rect (at -1.6002 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 42 /Front-LED) (solder_mask_margin 0.2))
    (pad 42 smd rect (at -2.3876 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (solder_mask_margin 0.2))
    (pad 43 smd rect (at -3.2004 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.2))
    (pad 44 smd rect (at -3.9878 -5.7404 180) (size 0.508 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V) (solder_mask_margin 0.2))
  )
  (module freetronics_footprints:SW_PUSHBUTTON_SMD (layer F.Cu) (tedit 594EACE4)
    (at 112.93 129.65 180)
    (attr smd)
    (fp_text reference SW1 (at 0.05 -3.05 180) (layer Eco1.User) hide)
    (fp_text value RESET (at 0 3.15 180) (layer Eco1.User) hide)
    (pad 2 smd rect (at -2.667 1.905 180) (size 1.778 0.762) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.667 1.905 180) (size 1.778 0.762) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.667 -1.905 180) (size 1.778 0.762) (layers F.Cu F.Paste F.Mask)
      (net 13 /32u4-Reset))
    (pad 1 smd rect (at -2.667 -1.905 180) (size 1.778 0.762) (layers F.Cu F.Paste F.Mask)
      (net 13 /32u4-Reset))
  )
  (module Diodes_SMD:SOD-323 (layer F.Cu) (tedit 594F5EA7)
    (at 116.18 103.67 180)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D6 (at -1.61 -2.14 180) (layer F.SilkS))
    (fp_text value D_Zener (at 0.1 1.9 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.055 0 180) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 +9V))
    (pad 2 smd rect (at 1.055 0 180) (size 0.59 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D6-Pad2)"))
    (model Diodes_SMD.3dshapes/SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module "My Libraries:KT-MPLCH-0740-Hand" (layer F.Cu) (tedit 594F613B)
    (at 123.265 91.885)
    (fp_text reference L-KEMET1 (at -1.99 -4.45) (layer F.SilkS) hide)
    (fp_text value 33uH (at 4.445 3.335 90) (layer F.SilkS))
    (pad 1 smd rect (at -3.32 0) (size 3 3.5) (layers F.Cu F.Paste F.Mask)
      (net 7 /ToCoil))
    (pad 2 smd rect (at 3.07 0) (size 3 3.5) (layers F.Cu F.Paste F.Mask)
      (net 9 /Pi5v))
  )
  (module "My Libraries:POWER_JACK_PTH" (layer F.Cu) (tedit 594F6894)
    (at 92.48 89.99 270)
    (fp_text reference CON2 (at -1.016 -4.318 270) (layer Eco1.User))
    (fp_text value DC-In (at -2.5908 -3.6068 270) (layer Eco1.User))
    (pad 1 thru_hole oval (at 0 -13.69822 270) (size 4.4958 4.4958) (drill 2.9972) (layers *.Cu *.Mask)
      (net 14 /Vin-Raw))
    (pad 2 thru_hole oval (at 0 -7.69874 270) (size 4.4958 4.4958) (drill 2.9972) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 4.699 -10.69848) (size 4.4958 4.4958) (drill 2.9972) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module "My Libraries:SOD-523" (layer F.Cu) (tedit 594F7036)
    (at 120.29 114.67 180)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D9 (at -1.83 -0.01 360) (layer F.SilkS))
    (fp_text value 1SS389 (at 0 1.7 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 26 /OFF-PATH))
    (pad 1 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C10-Pad1)"))
  )
  (module "My Libraries:SOD-523" (layer F.Cu) (tedit 594F7031)
    (at 111.46 110.77 180)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D5 (at -1.83 -0.02 360) (layer F.SilkS))
    (fp_text value 1SS389 (at 0 1.7 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /PWR-SIG))
    (pad 1 smd rect (at -0.7 0) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D5-Pad1)"))
  )
  (module "My Libraries:USB-MICRO-5pin_PTHMOUNT" (layer F.Cu) (tedit 594F77EF)
    (at 99.41 114.52)
    (attr smd)
    (fp_text reference P2 (at -4.7 0 90) (layer Eco1.User) hide)
    (fp_text value USB_5PIN_SHELL (at 1.55 -0.05 90) (layer Eco1.User) hide)
    (pad SHLD thru_hole circle (at -2.57556 -3.62458) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad SHLD thru_hole circle (at -2.57556 3.62458) (size 2 2) (drill 1.1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad SHLD thru_hole circle (at 0.0762 -2.4257) (size 1.5 1.5) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad SHLD smd rect (at -2.57556 1.30048) (size 1.30048 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad SHLD smd rect (at -2.57556 -1.30048) (size 1.30048 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 0 1.30048) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0 0) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 48 /D_P))
    (pad 4 smd rect (at 0 0.65024) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 -0.65024) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask)
      (net 49 /D_N))
    (pad SHLD thru_hole circle (at 0.0762 2.4257) (size 1.5 1.5) (drill 0.71) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 smd rect (at 0 -1.30048) (size 1.34874 0.39878) (layers F.Cu F.Paste F.Mask))
  )
  (module freetronics_footprints:LOGO_OSHW_silkscreen_5mm (layer F.Cu) (tedit 0)
    (at 105.78 80.19)
    (fp_text reference LOGO_OSHW_silkscreen_5mm (at 0 2.65176) (layer F.SilkS) hide)
    (fp_text value val** (at 0 -2.65176) (layer F.SilkS) hide)
  )
  (gr_text baldengineer.com/rpspc (at 141.31 106.4 90) (layer F.SilkS))
  (gr_text "RetroPie Power Hat v2" (at 142.77 109.3 90) (layer F.SilkS))
  (gr_line (start 95.3 75.9) (end 114.8 75.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 110.1 75.9) (end 110 75.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.3 75.9) (end 95.3 140.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text RESET (at 108.55 129.6 90) (layer F.SilkS))
  (gr_text LED (at 98.12 108.86 90) (layer B.SilkS))
  (gr_text SW (at 98.16 105.28 90) (layer B.SilkS))
  (gr_text PWR (at 98.04 101.67 90) (layer B.SilkS))
  (gr_text GND (at 105.58 101.54 90) (layer B.SilkS))
  (gr_text GND (at 105.61 104.97 90) (layer B.SilkS))
  (gr_text GND (at 105.58 108.6 90) (layer B.SilkS))
  (gr_text GND (at 105.58 108.6 90) (layer F.SilkS))
  (gr_text GND (at 105.61 104.96 90) (layer F.SilkS))
  (gr_text GND (at 105.58 101.54 90) (layer F.SilkS))
  (gr_text GND (at 105.69 131.03) (layer B.SilkS))
  (gr_text CLK (at 105.77 128.46) (layer B.SilkS))
  (gr_text DATA2 (at 106.07 125.91) (layer B.SilkS))
  (gr_text Latch (at 105.95 123.37) (layer B.SilkS))
  (gr_text +5V (at 105.72 120.79) (layer B.SilkS))
  (gr_text GND (at 97.98 130.96) (layer B.SilkS))
  (gr_text CLK (at 97.98 128.41) (layer B.SilkS))
  (gr_text DATA1 (at 97.6 125.99) (layer B.SilkS))
  (gr_text Latch (at 97.58 123.54) (layer B.SilkS))
  (gr_text +5V (at 97.87 120.87) (layer B.SilkS))
  (gr_text +5V (at 105.61 120.75) (layer F.SilkS))
  (gr_text +5V (at 97.74 120.88) (layer F.SilkS))
  (gr_text Latch (at 97.61 123.51) (layer F.SilkS))
  (gr_text Latch (at 105.93 123.37) (layer F.SilkS))
  (gr_text DATA2 (at 106.06 125.91) (layer F.SilkS))
  (gr_text DATA1 (at 97.62 125.98) (layer F.SilkS))
  (gr_text CLK (at 97.97 128.4) (layer F.SilkS))
  (gr_text CLK (at 105.69 128.46) (layer F.SilkS))
  (gr_text GND (at 97.97 130.96) (layer F.SilkS))
  (gr_text GND (at 105.67 131.03) (layer F.SilkS))
  (gr_text SCK (at 113.81 140.1) (layer B.SilkS))
  (gr_text RESET (at 116.34 140.1) (layer B.SilkS))
  (gr_text GND (at 116.36 133.85 180) (layer B.SilkS))
  (gr_text MO (at 113.72 133.83 180) (layer B.SilkS))
  (gr_text +5V (at 111.08 133.83 180) (layer B.SilkS))
  (gr_text GND (at 116.36 133.85 180) (layer F.SilkS))
  (gr_text +5V (at 111.21 133.83 180) (layer F.SilkS))
  (gr_text MO (at 113.73 133.83 180) (layer F.SilkS))
  (gr_text RESET (at 116.35 140.09) (layer F.SilkS))
  (gr_text SCK (at 113.78 140.1) (layer F.SilkS))
  (gr_text MI (at 111.19 140.09) (layer F.SilkS))
  (gr_text MI (at 111.19 140.09) (layer B.SilkS))
  (gr_line (start 131.8 75.9) (end 151.8 75.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.8 80.5) (end 131.8 75.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8 80.5) (end 114.8 75.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.8 80.5) (end 131.8 80.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 95.3 140.9) (end 151.8 140.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.8 140.9) (end 151.8 75.9) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 5) (net_name +9V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 127.92 83.04) (xy 127.96 85.88) (xy 127.7 85.675319) (xy 127.7 85.77) (xy 126.05 85.78)
        (xy 126.05 85.53) (xy 123.1 85.52) (xy 123.109394 84.458438) (xy 123.03 84.46) (xy 123.09 84.22)
        (xy 112.72 84.23) (xy 112.7 95.43) (xy 112.72 96.59) (xy 121.709966 96.55104) (xy 121.71 96.55)
        (xy 121.776453 96.550752) (xy 121.95 96.55) (xy 121.949982 96.552716) (xy 134.08 96.69) (xy 134.09 96.68)
        (xy 134.109911 98.661138) (xy 134.33 98.66) (xy 134.33 99.234576) (xy 138.78 99.31) (xy 138.78 99.558795)
        (xy 138.81 99.56) (xy 138.82 102.92) (xy 136.28 102.92) (xy 136.23 101.19) (xy 134.58 101.16)
        (xy 134.58 100.69) (xy 130 100.72) (xy 130.03 103.33) (xy 130 103.57) (xy 121.83 103.49)
        (xy 122 101.15) (xy 118.86 101.22) (xy 118.86 101.094479) (xy 118.37 101.1) (xy 118.37 98.08)
        (xy 111.19 98.08) (xy 111.19 83.03)
      )
    )
    (polygon
      (pts        (xy 121.935898 98.67) (xy 121.935538 98.724095) (xy 132.396236 98.67)
      )
    )
  )
  (zone (net 7) (net_name /ToCoil) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254) (smoothing chamfer))
    (polygon
      (pts
        (xy 124.52 85.8) (xy 124.52 86.46) (xy 123.03 86.46) (xy 123.07 95.95) (xy 116.37 95.92)
        (xy 116.45 88.35) (xy 116.59 88.348822) (xy 116.59 87.85) (xy 118.38 87.86) (xy 118.382723 88.333731)
        (xy 122.39 88.3) (xy 122.41 85.77)
      )
    )
  )
  (zone (net 9) (net_name /Pi5v) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 150.68 82.48) (xy 150.69 88.1) (xy 150.24 88.09) (xy 144.57 88.13) (xy 144.6 87.87)
        (xy 139.75 87.92) (xy 139.83 95.81) (xy 123.47 95.8) (xy 123.4 88.08) (xy 128.3 88.08)
        (xy 128.28 90.97) (xy 131.5 90.97) (xy 134.46 90.95) (xy 134.46 90.35) (xy 134.5 82.44)
      )
    )
  )
  (zone (net 9) (net_name /Pi5v) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 150.68 82.48) (xy 150.69 88.1) (xy 150.24 88.09) (xy 144.57 88.13) (xy 144.6 87.87)
        (xy 139.75 87.92) (xy 139.83 95.81) (xy 123.47 95.8) (xy 123.4 88.08) (xy 128.3 88.08)
        (xy 128.28 90.97) (xy 131.5 90.97) (xy 134.46 90.95) (xy 134.46 90.35) (xy 134.5 82.44)
      )
    )
  )
  (zone (net 2) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254) (smoothing chamfer))
    (polygon
      (pts
        (xy 138.61 116.07) (xy 127.27 116.1) (xy 127.01 116.09) (xy 127.05838 120.057177) (xy 135.75 120.04)
        (xy 135.78 130.13) (xy 125.68 130.08) (xy 125.641295 122.323424) (xy 122.99 122.31) (xy 123.01 114.38)
        (xy 134.28 114.35) (xy 136.49 114.36) (xy 136.33 103.44) (xy 136.33 103.43) (xy 138.83 103.43)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254) (smoothing chamfer))
    (polygon
      (pts
        (xy 95.39 76.05) (xy 151.77 76) (xy 151.71 140.97) (xy 95.3 141.17) (xy 95.33 76.14)
      )
    )
  )
  (zone (net 14) (net_name /Vin-Raw) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 101.89 103.27) (xy 98.62 103.25) (xy 98.63 96.32) (xy 104.7 96.33) (xy 104.64 91.56)
        (xy 103.4 91.55) (xy 103.43 87.34) (xy 107.76 87.36) (xy 110.32 87.39) (xy 110.28 98.89)
        (xy 117.93 98.83) (xy 117.88 100.49) (xy 114.27 100.48) (xy 114.27 101.3) (xy 104.96 101.35)
        (xy 104.97 103.24) (xy 101.83 103.28)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254) (smoothing chamfer))
    (polygon
      (pts
        (xy 95.39 76.05) (xy 151.77 76) (xy 151.71 140.97) (xy 95.3 141.17) (xy 95.33 76.14)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254) (smoothing chamfer))
    (polygon
      (pts
        (xy 95.39 76.05) (xy 151.77 76) (xy 151.71 140.97) (xy 95.3 141.17) (xy 95.33 76.14)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.254) (smoothing chamfer))
    (polygon
      (pts
        (xy 95.39 76.05) (xy 151.77 76) (xy 151.71 140.97) (xy 95.3 141.17) (xy 95.33 76.14)
      )
    )
  )
)
