(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 15)
    (no_connects 0)
    (area 125.924999 99.924999 145.075001 110.075001)
    (thickness 1.6)
    (drawings 6)
    (tracks 106)
    (zones 0)
    (modules 7)
    (nets 11)
  )
  (page USLetter)
  (title_block
    (title PiezoBoost)
    (date 2017-01-30)
    (rev 1)
    (company "Silicognition LLC")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.16)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.7)
    (via_drill 0.35)
    (via_min_size 0.69)
    (via_min_drill 0.35)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.07)
    (pad_to_paste_clearance -0.05)
    (pad_to_paste_clearance_ratio -0.01)
    (aux_axis_origin 126 110)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VDD)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C3-Pad2)")
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(P1-Pad2)")
  (net 9 "Net-(P2-Pad1)")
  (net 10 "Net-(P2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.7)
    (via_drill 0.35)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net VDD)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 588FAA8F)
    (at 132 105 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.1 0 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 588FAAB2)
    (at 139 106 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.2 0 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 588FAA9E)
    (at 136.5 102)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -2.4 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 588FAAC1)
    (at 139 103 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -2.1 0 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03 (layer F.Cu) (tedit 588FAA83)
    (at 128.5 107.5 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at -0.7 2.7 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VDD))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 588FAE07)
    (at 142.5 104 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P2 (at -2.6 0 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0.5 -4 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "Net-(P2-Pad2)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 588FAAA4)
    (at 135.5 105.5)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U1 (at -1.3 2.9) (layer F.SilkS))
    (fp_text value PAM8904 (at 0 2.85) (layer F.Fab) hide)
    (pad 1 smd oval (at -1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 2 smd oval (at -1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 3 smd oval (at -1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P1-Pad2)"))
    (pad 4 smd oval (at -1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd oval (at -0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 6 smd oval (at -0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd oval (at 0.25 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P2-Pad2)"))
    (pad 8 smd oval (at 0.75 1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd oval (at 1.475 0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P2-Pad1)"))
    (pad 10 smd oval (at 1.475 0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C3-Pad2)"))
    (pad 11 smd oval (at 1.475 -0.25) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 12 smd oval (at 1.475 -0.75) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd oval (at 0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 14 smd oval (at 0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 15 smd oval (at -0.25 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VDD))
    (pad 16 smd oval (at -0.75 -1.475 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 17 smd rect (at 0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text PiezoBoost (at 135.5 103.7) (layer B.SilkS))
  (gr_text "\n(C) 2017 Silicognition LLC" (at 135.5 107) (layer B.SilkS))
  (gr_line (start 126 110) (end 145 110) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126 100) (end 145 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126 110) (end 126 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 100) (end 145 110) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.16)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 145 110) (xy 126 110) (xy 126 100) (xy 145 100)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.16)
    (fill yes (arc_segments 16) (thermal_gap 0.3) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 145 110) (xy 126 110) (xy 126 100) (xy 145 100)
      )
    )
  )
)
