(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 78)
    (tracks 461)
    (zones 0)
    (modules 10)
    (nets 75)
  )
  (page USLetter)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.5 5.5)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /ADDB6)
  (net 2 /ADCLK)
  (net 3 /NC34)
  (net 4 /NC33)
  (net 5 /NC32)
  (net 6 /NC31)
  (net 7 /NC30)
  (net 8 /ADDB7)
  (net 9 /ADDB5)
  (net 10 /ADDB4)
  (net 11 /ADDB3)
  (net 12 /ADDB2)
  (net 13 /ADDB1)
  (net 14 /ADDB0)
  (net 15 /NC20)
  (net 16 /NC19)
  (net 17 /NC18)
  (net 18 /NC17)
  (net 19 /NC16)
  (net 20 /NC15)
  (net 21 /NC14)
  (net 22 /DADB0)
  (net 23 /DADB1)
  (net 24 /DADB2)
  (net 25 /DADB3)
  (net 26 /DADB4)
  (net 27 /DADB5)
  (net 28 /DADB6)
  (net 29 /DADB7)
  (net 30 /DADCLK)
  (net 31 /NC4)
  (net 32 /NC3)
  (net 33 /VCC5)
  (net 34 /DCOM)
  (net 35 /OUT5V)
  (net 36 /IN5V)
  (net 37 /GP27)
  (net 38 /GN27)
  (net 39 /GP26)
  (net 40 /GN26)
  (net 41 /GP25)
  (net 42 /GN25)
  (net 43 /GP24)
  (net 44 /GN24)
  (net 45 /GP23)
  (net 46 /GN23)
  (net 47 /GP22)
  (net 48 /GN22)
  (net 49 /GP21)
  (net 50 /GN21)
  (net 51 /GP20)
  (net 52 /GN20)
  (net 53 /GP19)
  (net 54 /GN19)
  (net 55 /GP18)
  (net 56 /GN18)
  (net 57 /GP17)
  (net 58 /GN17)
  (net 59 /GN16)
  (net 60 /GN15)
  (net 61 /GN14)
  (net 62 /GND38)
  (net 63 /GND37)
  (net 64 /GND22)
  (net 65 /GND21)
  (net 66 /3VP20)
  (net 67 /3VP19)
  (net 68 /GP16)
  (net 69 /GP15)
  (net 70 /GP14)
  (net 71 /GND4)
  (net 72 /GND3)
  (net 73 /3VP2)
  (net 74 /3VP1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3VP1)
    (add_net /3VP19)
    (add_net /3VP2)
    (add_net /3VP20)
    (add_net /ADCLK)
    (add_net /ADDB0)
    (add_net /ADDB1)
    (add_net /ADDB2)
    (add_net /ADDB3)
    (add_net /ADDB4)
    (add_net /ADDB5)
    (add_net /ADDB6)
    (add_net /ADDB7)
    (add_net /DADB0)
    (add_net /DADB1)
    (add_net /DADB2)
    (add_net /DADB3)
    (add_net /DADB4)
    (add_net /DADB5)
    (add_net /DADB6)
    (add_net /DADB7)
    (add_net /DADCLK)
    (add_net /DCOM)
    (add_net /GN14)
    (add_net /GN15)
    (add_net /GN16)
    (add_net /GN17)
    (add_net /GN18)
    (add_net /GN19)
    (add_net /GN20)
    (add_net /GN21)
    (add_net /GN22)
    (add_net /GN23)
    (add_net /GN24)
    (add_net /GN25)
    (add_net /GN26)
    (add_net /GN27)
    (add_net /GND21)
    (add_net /GND22)
    (add_net /GND3)
    (add_net /GND37)
    (add_net /GND38)
    (add_net /GND4)
    (add_net /GP14)
    (add_net /GP15)
    (add_net /GP16)
    (add_net /GP17)
    (add_net /GP18)
    (add_net /GP19)
    (add_net /GP20)
    (add_net /GP21)
    (add_net /GP22)
    (add_net /GP23)
    (add_net /GP24)
    (add_net /GP25)
    (add_net /GP26)
    (add_net /GP27)
    (add_net /IN5V)
    (add_net /NC14)
    (add_net /NC15)
    (add_net /NC16)
    (add_net /NC17)
    (add_net /NC18)
    (add_net /NC19)
    (add_net /NC20)
    (add_net /NC3)
    (add_net /NC30)
    (add_net /NC31)
    (add_net /NC32)
    (add_net /NC33)
    (add_net /NC34)
    (add_net /NC4)
    (add_net /OUT5V)
    (add_net /VCC5)
  )
  (module library:PinHeader_Dual_1x2_P2.54mm_TestPoint.kicad_mod (layer F.Cu) (tedit 5CA15A2A)
    (at 139.065 86.36 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 1.27 -1.92 270) (layer F.SilkS) hide)
    (fp_text value 0 (at 1.27 1.92 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -1.92 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 63 /GND37))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 34 /DCOM))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x17_P2.54mm_Vertical (layer F.Cu) (tedit 5CA124DB)
    (at 179.07 88.9)
    (descr "Through hole straight pin header, 2x17, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x17 2.54mm double row")
    (fp_text reference J5 (at 0.635 -3.175) (layer F.SilkS))
    (fp_text value Conn_02x17_Odd_Even (at 0 -12.7) (layer F.Fab))
    (fp_text user %R (at 1.27 20.32 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /DCOM))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /VCC5))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /NC3))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /NC4))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /DADCLK))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /DADB7))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /DADB6))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /DADB5))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /DADB4))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /DADB3))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /DADB2))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /DADB1))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /DADB0))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /NC14))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /NC15))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /NC16))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /NC17))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /NC18))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /NC19))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /NC20))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /ADDB0))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /ADDB1))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /ADDB2))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /ADDB3))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /ADDB4))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /ADDB5))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /ADDB6))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /ADDB7))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /ADCLK))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /NC30))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /NC31))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /NC32))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /NC33))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /NC34))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x17_P2.54mm_Vertical (layer F.Cu) (tedit 5CA124D4)
    (at 163.83 88.9)
    (descr "Through hole straight pin header, 2x17, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x17 2.54mm double row")
    (fp_text reference J4 (at 0.635 -3.175) (layer F.SilkS))
    (fp_text value Conn_02x17_Odd_Even (at 0 -10.795) (layer F.Fab))
    (fp_text user %R (at 1.27 20.32 90) (layer F.Fab))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /NC34))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /NC33))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /NC32))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /NC31))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /NC30))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /ADCLK))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /ADDB7))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /ADDB6))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /ADDB5))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /ADDB4))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /ADDB3))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /ADDB2))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /ADDB1))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /ADDB0))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /NC20))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /NC19))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /NC18))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /NC17))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /NC16))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /NC15))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /NC14))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /DADB0))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /DADB1))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /DADB2))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /DADB3))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /DADB4))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /DADB5))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /DADB6))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /DADB7))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /DADCLK))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /NC4))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /NC3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /VCC5))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /DCOM))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x17_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 133.35 132.08 180)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J2 (at 1.27 21.59 180) (layer F.SilkS))
    (fp_text value "ULX3S HEADER" (at 1.27 52.07 180) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 270) (layer F.Fab))
    (pad 40 thru_hole oval (at 2.54 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /OUT5V))
    (pad 39 thru_hole oval (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /IN5V))
    (pad 38 thru_hole oval (at 2.54 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 /GND38))
    (pad 37 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /GND37))
    (pad 36 thru_hole oval (at 2.54 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /GP27))
    (pad 35 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /GN27))
    (pad 34 thru_hole oval (at 2.54 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /GP26))
    (pad 33 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /GN26))
    (pad 32 thru_hole oval (at 2.54 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /GP25))
    (pad 31 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /GN25))
    (pad 30 thru_hole oval (at 2.54 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /GP24))
    (pad 29 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /GN24))
    (pad 28 thru_hole oval (at 2.54 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /GP23))
    (pad 27 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /GN23))
    (pad 26 thru_hole oval (at 2.54 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /GP22))
    (pad 25 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /GN22))
    (pad 24 thru_hole oval (at 2.54 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /GP21))
    (pad 23 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /GN21))
    (pad 22 thru_hole oval (at 2.54 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 /GND22))
    (pad 21 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 /GND21))
    (pad 20 thru_hole oval (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /3VP20))
    (pad 19 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 /3VP19))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /GP20))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /GN20))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /GP19))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /GN19))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /GP18))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /GN18))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /GP17))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /GN17))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /GP16))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 /GN16))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /GP15))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 /GN15))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 /GP14))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 /GN14))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 /GND4))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 /GND3))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /3VP2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /3VP1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Horizontal (layer F.Cu) (tedit 5C9FB8EA)
    (at 119.38 132.08 180)
    (descr "Through hole angled pin header, 2x20, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x20 2.54mm double row")
    (fp_text reference J1 (at 1.27 21.59 180) (layer F.SilkS))
    (fp_text value "ULX3S HEADER" (at 1.27 52.07 180) (layer F.Fab))
    (fp_text user %R (at 5.31 24.13 270) (layer F.Fab))
    (pad 40 thru_hole oval (at 2.54 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /OUT5V))
    (pad 39 thru_hole oval (at 0 48.26 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /IN5V))
    (pad 38 thru_hole oval (at 2.54 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 /GND38))
    (pad 37 thru_hole oval (at 0 45.72 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /GND37))
    (pad 36 thru_hole oval (at 2.54 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /GP27))
    (pad 35 thru_hole oval (at 0 43.18 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /GN27))
    (pad 34 thru_hole oval (at 2.54 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 /GP26))
    (pad 33 thru_hole oval (at 0 40.64 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /GN26))
    (pad 32 thru_hole oval (at 2.54 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /GP25))
    (pad 31 thru_hole oval (at 0 38.1 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /GN25))
    (pad 30 thru_hole oval (at 2.54 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /GP24))
    (pad 29 thru_hole oval (at 0 35.56 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /GN24))
    (pad 28 thru_hole oval (at 2.54 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /GP23))
    (pad 27 thru_hole oval (at 0 33.02 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /GN23))
    (pad 26 thru_hole oval (at 2.54 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /GP22))
    (pad 25 thru_hole oval (at 0 30.48 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /GN22))
    (pad 24 thru_hole oval (at 2.54 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /GP21))
    (pad 23 thru_hole oval (at 0 27.94 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 /GN21))
    (pad 22 thru_hole oval (at 2.54 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 /GND22))
    (pad 21 thru_hole oval (at 0 25.4 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 /GND21))
    (pad 20 thru_hole oval (at 2.54 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /3VP20))
    (pad 19 thru_hole oval (at 0 22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 /3VP19))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 /GP20))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 /GN20))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /GP19))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /GN19))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /GP18))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /GN18))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /GP17))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /GN17))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /GP16))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 /GN16))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /GP15))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 /GN15))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 /GP14))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 /GN14))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 /GND4))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 /GND3))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 /3VP2))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /3VP1))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module library:PinHeader_1x20_Dual_P2.54mm_Vertical_TestPoint (layer F.Cu) (tedit 5CA0F25D)
    (at 147.32 83.82)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J3 (at 0.635 1.27) (layer F.SilkS))
    (fp_text value Conn_Dual_01x20_Male_Testpoint (at 0 -7.62) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /OUT5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /VCC5))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /GP25))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /DADCLK))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /GN25))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /DADB7))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /GP24))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /DADB6))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /GN24))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /DADB5))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /GP23))
    (pad 12 thru_hole oval (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /DADB4))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /GN23))
    (pad 14 thru_hole oval (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /DADB3))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /GP22))
    (pad 16 thru_hole oval (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /DADB2))
    (pad 17 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /GN22))
    (pad 18 thru_hole oval (at 2.54 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /DADB1))
    (pad 19 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 /GP21))
    (pad 20 thru_hole oval (at 2.54 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /DADB0))
    (pad 21 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 /GP19))
    (pad 22 thru_hole oval (at 2.54 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /ADDB0))
    (pad 23 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 /GN19))
    (pad 24 thru_hole oval (at 2.54 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /ADDB1))
    (pad 25 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 /GP18))
    (pad 26 thru_hole oval (at 2.54 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /ADDB2))
    (pad 27 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 /GN18))
    (pad 28 thru_hole oval (at 2.54 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /ADDB3))
    (pad 29 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 /GP17))
    (pad 30 thru_hole oval (at 2.54 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /ADDB4))
    (pad 31 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 /GN17))
    (pad 32 thru_hole oval (at 2.54 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /ADDB5))
    (pad 33 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 /GP16))
    (pad 34 thru_hole oval (at 2.54 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /ADDB6))
    (pad 35 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 /GN16))
    (pad 36 thru_hole oval (at 2.54 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /ADDB7))
    (pad 37 thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 /GP15))
    (pad 38 thru_hole oval (at 2.54 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /ADCLK))
    (pad 39 thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 /GND3))
    (pad 40 thru_hole oval (at 2.54 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /DCOM))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 5CA125EE)
    (at 124.46 86.36)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference MH1 (at 0 0) (layer F.SilkS))
    (fp_text value MountingHole (at 0 -5.08) (layer F.Fab))
    (fp_text user %R (at 0 -1.905) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 5CA125FA)
    (at 124.46 129.54)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference MH4 (at 0 0) (layer F.SilkS))
    (fp_text value MountingHole (at 0 6.35) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 5CA12605)
    (at 172.72 129.54)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference MH3 (at 0 0) (layer F.SilkS))
    (fp_text value MountingHole (at -1.27 7.62) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 3 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad (layer F.Cu) (tedit 5CA125E5)
    (at 172.72 86.36)
    (descr "Mounting Hole 3.2mm, M3, ISO14580")
    (tags "mounting hole 3.2mm m3 iso14580")
    (attr virtual)
    (fp_text reference MH2 (at 0 0) (layer F.SilkS))
    (fp_text value MountingHole (at 0 -6.35) (layer F.Fab))
    (fp_text user %R (at 0 -1.905) (layer F.Fab))
    (pad 4 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask))
  )
  (target plus (at 115.57 84.455) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 115.57 131.445) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 182.245 131.445) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 182.245 84.455) (size 5) (width 0.15) (layer Edge.Cuts))
  (gr_text 3V3 (at 123.19 132.08) (layer F.SilkS))
  (gr_text "- 27 +\n- 26 +\n- 25 +\n- 24 +\n- 23 +\n- 22 +" (at 125.095 95.25) (layer F.SilkS))
  (gr_text "- 20 +\n- 19 +\n- 18 +\n- 17 +\n- 16 +\n- 15 +\n- 14 +" (at 125.095 119.38) (layer F.SilkS))
  (gr_text GN (at 122.555 104.14) (layer F.SilkS))
  (gr_text GP (at 128.905 104.14) (layer F.SilkS))
  (gr_text D/A (at 172.72 97.79 90) (layer F.SilkS))
  (gr_text A/D (at 172.72 118.11 90) (layer F.SilkS))
  (gr_text "V\n\n7\n5\n3\n1\n\n\n\n\n1\n3\n5\n7" (at 182.88 105.41) (layer F.SilkS))
  (gr_text "V\n\n7\n5\n3\n1\n\n\n\n\n1\n3\n5\n7" (at 168.275 105.41) (layer F.SilkS))
  (gr_text "G\n\nK\n6\n4\n2\n0\n\n\n\n0\n2\n4\n6\nK" (at 177.8 106.68) (layer F.SilkS))
  (gr_text "G\n\nK\n6\n4\n2\n0\n\n\n\n0\n2\n4\n6\nK" (at 162.56 106.68) (layer F.SilkS))
  (gr_text "GND\n3V3" (at 124.46 107.95) (layer F.SilkS))
  (gr_text "GND\n3V3" (at 137.16 130.81) (layer F.SilkS))
  (gr_text "GND\n3V3" (at 137.16 107.95) (layer F.SilkS))
  (gr_text "20\n19\n18\n17\n16\n15\n14" (at 136.525 119.38) (layer F.SilkS))
  (gr_text "27\n26\n25\n24\n23\n22\n21" (at 136.525 96.52) (layer F.SilkS))
  (gr_line (start 113.03 81.915) (end 113.03 133.985) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.785 81.915) (end 113.03 81.915) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.785 133.985) (end 184.785 81.915) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113.03 133.985) (end 184.785 133.985) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 143.51 132.08) (layer F.SilkS))
  (gr_text "GN19\nGP18\nGN18\nGP17\nGN17\nGP16\nGN16\nGP15" (at 146.05 120.65) (layer F.SilkS))
  (gr_text "GP21\nGP19" (at 146.05 107.95) (layer F.SilkS))
  (gr_text GN22 (at 146.05 104.14) (layer F.SilkS))
  (gr_text GP22 (at 146.05 101.6) (layer F.SilkS))
  (gr_text GN23 (at 146.05 99.06) (layer F.SilkS))
  (gr_text GP23 (at 146.05 96.52) (layer F.SilkS))
  (gr_text GN24 (at 146.05 93.98) (layer F.SilkS))
  (gr_text GP24 (at 146.05 91.44) (layer F.SilkS))
  (gr_text GN25 (at 146.05 88.9) (layer F.SilkS))
  (gr_text GP25 (at 146.05 86.36) (layer F.SilkS))
  (gr_text OUT5V (at 142.24 83.82) (layer F.SilkS))
  (gr_text DCOM (at 151.13 132.08) (layer F.SilkS))
  (gr_text ADCLK (at 154.94 129.54) (layer F.SilkS))
  (gr_text ADDB7 (at 154.94 127) (layer F.SilkS))
  (gr_text ADDB6 (at 154.94 124.46) (layer F.SilkS))
  (gr_text ADDB5 (at 154.94 121.92) (layer F.SilkS))
  (gr_text ADDB4 (at 154.94 119.38) (layer F.SilkS))
  (gr_text ADDB3 (at 154.94 116.84) (layer F.SilkS))
  (gr_text ADDB2 (at 154.94 114.3) (layer F.SilkS))
  (gr_text ADDB1 (at 154.94 111.76) (layer F.SilkS))
  (gr_text ADDB0 (at 154.94 109.22) (layer F.SilkS))
  (gr_text DADB2 (at 151.13 101.6) (layer F.SilkS))
  (gr_text DADB3 (at 154.94 99.06) (layer F.SilkS))
  (gr_text DADB4 (at 154.94 96.52) (layer F.SilkS))
  (gr_text DADB6 (at 154.94 93.98) (layer F.SilkS))
  (gr_text DADB6 (at 151.13 91.44) (layer F.SilkS))
  (gr_text DADB7 (at 154.94 88.9) (layer F.SilkS))
  (gr_text DADCLK (at 151.13 86.36) (layer F.SilkS))
  (gr_text VCC5 (at 154.94 83.82) (layer F.SilkS))
  (gr_text DADB0 (at 154.94 106.68) (layer F.SilkS))
  (gr_text DADB1 (at 154.94 104.14) (layer F.SilkS))
)
