(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad13)")
  (net 2 "+5V")
  (net 3 "GND")
  (net 4 "+12V")
  (net 5 "Net-(D1-Pad12)")
  (net 6 "Net-(D1-Pad11)")
  (net 7 "unconnected-(D1-Pad10)")
  (net 8 "Net-(D2-Pad1)")
  (net 9 "Net-(D3-Pad1)")
  (net 10 "unconnected-(UNO1-Pad3V3)")
  (net 11 "unconnected-(UNO1-Pad5V2)")
  (net 12 "unconnected-(UNO1-PadA0)")
  (net 13 "unconnected-(UNO1-PadA1)")
  (net 14 "unconnected-(UNO1-PadA2)")
  (net 15 "unconnected-(UNO1-PadA3)")
  (net 16 "unconnected-(UNO1-PadA4)")
  (net 17 "unconnected-(UNO1-PadA5)")
  (net 18 "unconnected-(UNO1-PadAREF)")
  (net 19 "unconnected-(UNO1-PadD0)")
  (net 20 "unconnected-(UNO1-PadD1)")
  (net 21 "Net-(D1-Pad4)")
  (net 22 "Net-(D1-Pad7)")
  (net 23 "Net-(D1-Pad8)")
  (net 24 "Net-(D1-Pad3)")
  (net 25 "unconnected-(UNO1-PadGND4)")
  (net 26 "unconnected-(UNO1-PadMISO)")
  (net 27 "unconnected-(UNO1-PadMOSI)")
  (net 28 "unconnected-(UNO1-PadRST1)")
  (net 29 "unconnected-(UNO1-PadRST2)")
  (net 30 "unconnected-(UNO1-PadSCK)")
  (net 31 "Net-(D1-Pad2)")
  (net 32 "Net-(D1-Pad1)")
  (net 33 "unconnected-(UNO1-PadD6)")
  (net 34 "unconnected-(UNO1-PadD7)")
  (net 35 "Net-(D1-Pad14)")
  (net 36 "Net-(D4-Pad1)")
  (net 37 "Net-(D5-Pad1)")
  (footprint "Barrel Power Jack Adapter:PJ-102AH" (layer "F.Cu")
    (tedit 0)
    (at 172.240925 128.27 -90)
    (descr "PJ-102AH")
    (tags "Connector")
    (property "Description" "DC POWER JACK")
    (property "Height" "")
    (property "Manufacturer_Name" "CUI Devices")
    (property "Manufacturer_Part_Number" "PJ-102AH")
    (property "Mouser Part Number" "490-PJ-102AH")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CUI-Devices/PJ-102AH?qs=WyjlAZoYn50Yq4CrVLCXLw%3D%3D")
    (property "Sheetfile" "File: OPT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at 4.035 -6.411 -90) (layer "F.SilkS"))
    (fp_text value "PJ-102AH" (at 4.035 -6.411 -90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.035 -6.411 -90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 4.3 3 270) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 4 "+12V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 4.3 -3 270) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -0.4 0 270) (size 3 3) (drill 1.9) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "3") (pintype "passive"))
    (model "PJ-102AH.stp"
      (offset (xyz 4.309999878 -2.78999992 6.579999825))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "BNC 031-70578:0317057812G" (layer "F.Cu")
    (tedit 0)
    (at 106.68 81.28)
    (descr "031-70578-12G-2")
    (tags "Connector")
    (property "Description" "RF Connectors / Coaxial Connectors RF CONNECTOR BNC RIGHT ANGLE PCB")
    (property "Height" "11.18")
    (property "Manufacturer_Name" "Amphenol")
    (property "Manufacturer_Part_Number" "031-70578-12G")
    (property "Mouser Part Number" "523-0317057812G")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Amphenol-RF/031-70578-12G?qs=DRkmTr78QATSDA%2FxzBZ%252BjQ%3D%3D")
    (property "Sheetfile" "File: OPT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D2" (at -10.75 0) (layer "F.SilkS"))
    (fp_text value "031-70578-12G" (at -10.75 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -10.75 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.012 1.012) (drill 0.45) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 3.225 3.225) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 3.225 -3.225) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -3.225 -3.225) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at -3.225 3.225) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "5") (pintype "passive"))
  )
  (footprint "Arduino:Arduino_Uno_R2_Shield" (layer "F.Cu")
    (tedit 5A8605EC)
    (at 106.384 126.444237)
    (descr "https://startingelectronics.org/articles/arduino/uno-r3-r2-differences/")
    (property "Sheetfile" "File: OPT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "UNO1" (at 2.54 -54.356) (layer "B.SilkS"))
    (fp_text value "Arduino_Uno_R2_Shield" (at 27.305 -54.356) (layer "B.Fab"))
    (fp_text user "." (at 62.484 -32.004) (layer "B.SilkS"))
    (fp_text user "D0" (at 63.5 -48.895 unlocked) (layer "B.SilkS"))
    (fp_text user "." (at 62.484 -32.004) (layer "F.SilkS"))
    (fp_text user "D0" (at 63.5 -48.895 unlocked) (layer "F.SilkS"))
    (fp_text user "USB" (at 1.535 -38.0986) (layer "B.Fab"))
    (fp_text user "Barrel Jack" (at 5.065 -7.7981) (layer "B.Fab"))
    (pad "" np_thru_hole circle (at 15.24 -50.8) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 66.04 -35.56) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 13.97 -2.54) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 66.04 -7.62) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
    (pad "3V3" thru_hole oval (at 35.56 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 "unconnected-(UNO1-Pad3V3)") (pinfunction "3.3V") (pintype "power_out+no_connect"))
    (pad "5V1" thru_hole oval (at 38.1 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 "+5V") (pinfunction "5V") (pintype "power_in"))
    (pad "5V2" thru_hole oval (at 66.167 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 "unconnected-(UNO1-Pad5V2)") (pinfunction "SPI_5V") (pintype "power_in+no_connect"))
    (pad "A0" thru_hole oval (at 50.8 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 "unconnected-(UNO1-PadA0)") (pinfunction "A0") (pintype "bidirectional+no_connect"))
    (pad "A1" thru_hole oval (at 53.34 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 "unconnected-(UNO1-PadA1)") (pinfunction "A1") (pintype "bidirectional+no_connect"))
    (pad "A2" thru_hole oval (at 55.88 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 "unconnected-(UNO1-PadA2)") (pinfunction "A2") (pintype "bidirectional+no_connect"))
    (pad "A3" thru_hole oval (at 58.42 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 "unconnected-(UNO1-PadA3)") (pinfunction "A3") (pintype "bidirectional+no_connect"))
    (pad "A4" thru_hole oval (at 60.96 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 "unconnected-(UNO1-PadA4)") (pinfunction "A4/SDA") (pintype "bidirectional+no_connect"))
    (pad "A5" thru_hole oval (at 63.5 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 "unconnected-(UNO1-PadA5)") (pinfunction "A5/SCL") (pintype "bidirectional+no_connect"))
    (pad "AREF" thru_hole oval (at 23.876 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 "unconnected-(UNO1-PadAREF)") (pinfunction "AREF") (pintype "input+no_connect"))
    (pad "D0" thru_hole oval (at 63.5 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 "unconnected-(UNO1-PadD0)") (pinfunction "D0/RX") (pintype "bidirectional+no_connect"))
    (pad "D1" thru_hole oval (at 60.96 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "unconnected-(UNO1-PadD1)") (pinfunction "D1/TX") (pintype "bidirectional+no_connect"))
    (pad "D2" thru_hole oval (at 58.42 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 "Net-(D2-Pad1)") (pinfunction "D2_INT0") (pintype "bidirectional"))
    (pad "D3" thru_hole oval (at 55.88 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad1)") (pinfunction "D3_INT1") (pintype "bidirectional"))
    (pad "D4" thru_hole oval (at 53.34 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 "Net-(D4-Pad1)") (pinfunction "D4") (pintype "bidirectional"))
    (pad "D5" thru_hole oval (at 50.8 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "Net-(D5-Pad1)") (pinfunction "D5") (pintype "bidirectional"))
    (pad "D6" thru_hole oval (at 48.26 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 "unconnected-(UNO1-PadD6)") (pinfunction "D6") (pintype "bidirectional+no_connect"))
    (pad "D7" thru_hole oval (at 45.72 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 "unconnected-(UNO1-PadD7)") (pinfunction "D7") (pintype "bidirectional+no_connect"))
    (pad "D8" thru_hole oval (at 41.656 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 "Net-(D1-Pad1)") (pinfunction "D8") (pintype "bidirectional"))
    (pad "D9" thru_hole oval (at 39.116 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 "Net-(D1-Pad2)") (pinfunction "D9") (pintype "bidirectional"))
    (pad "D10" thru_hole oval (at 36.576 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(D1-Pad3)") (pinfunction "D10_CS") (pintype "bidirectional"))
    (pad "D11" thru_hole oval (at 34.036 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(D1-Pad4)") (pinfunction "D11") (pintype "bidirectional"))
    (pad "D12" thru_hole oval (at 31.496 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 "Net-(D1-Pad7)") (pinfunction "D12") (pintype "bidirectional"))
    (pad "D13" thru_hole oval (at 28.956 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(D1-Pad8)") (pinfunction "D13") (pintype "bidirectional"))
    (pad "GND1" thru_hole rect (at 26.416 -50.8) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "GND2" thru_hole rect (at 40.64 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "GND3" thru_hole rect (at 43.18 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "GND4" thru_hole rect (at 66.167 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "unconnected-(UNO1-PadGND4)") (pinfunction "SPI_GND") (pintype "power_in+no_connect"))
    (pad "MISO" thru_hole oval (at 63.627 -30.48) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "unconnected-(UNO1-PadMISO)") (pinfunction "SPI_MISO") (pintype "input+no_connect"))
    (pad "MOSI" thru_hole oval (at 66.167 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "unconnected-(UNO1-PadMOSI)") (pinfunction "SPI_MOSI") (pintype "output+no_connect"))
    (pad "RST1" thru_hole oval (at 33.02 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "unconnected-(UNO1-PadRST1)") (pinfunction "RESET") (pintype "open_collector+no_connect"))
    (pad "RST2" thru_hole oval (at 63.627 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "unconnected-(UNO1-PadRST2)") (pinfunction "SPI_RESET") (pintype "open_collector+no_connect"))
    (pad "SCK" thru_hole oval (at 63.627 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 "unconnected-(UNO1-PadSCK)") (pinfunction "SPI_SCK") (pintype "output+no_connect"))
    (pad "VIN" thru_hole oval (at 45.72 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 4 "+12V") (pinfunction "VIN") (pintype "power_in"))
  )
  (footprint "DRV8825 Stepper Motor:IC_DRV8825_STEPPER_MOTOR_DRIVER_CARRIER" (layer "F.Cu")
    (tedit 64DC31A3)
    (at 135.89 87.63 -90)
    (property "AVAILABILITY" "Unavailable")
    (property "Availability" "Not in stock")
    (property "Check_prices" "https://www.snapeda.com/parts/DRV8825%20STEPPER%20MOTOR%20DRIVER%20CARRIER/Pololu/view-part/?ref=eda")
    (property "DESCRIPTION" "Stepper motor controler; IC: DRV8825; 1.5A; Uin mot: 8.2÷45V")
    (property "Description" "\nStepper, Bipolar 8.2 ~ 45VDC Supply 1.5A 8.2 ~ 45V Load\n")
    (property "MF" "Pololu")
    (property "MP" "DRV8825 STEPPER MOTOR DRIVER CARRIER")
    (property "PACKAGE" "None")
    (property "PRICE" "None")
    (property "Package" "None")
    (property "Price" "None")
    (property "Sheetfile" "File: OPT.kicad_sch")
    (property "Sheetname" "")
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/DRV8825%20STEPPER%20MOTOR%20DRIVER%20CARRIER/Pololu/view-part/?ref=snap")
    (attr through_hole)
    (fp_text reference "D1" (at -4.445 -12.065 -90) (layer "F.SilkS"))
    (fp_text value "DRV8825_STEPPER_MOTOR_DRIVER_CARRIER" (at 17.145 12.065 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at -6.35 -8.89 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(D1-Pad1)") (pinfunction "~{EN}") (pintype "input"))
    (pad "2" thru_hole circle locked (at -6.35 -6.35 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 "Net-(D1-Pad2)") (pinfunction "M0") (pintype "input"))
    (pad "3" thru_hole circle locked (at -6.35 -3.81 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(D1-Pad3)") (pinfunction "M1") (pintype "input"))
    (pad "4" thru_hole circle locked (at -6.35 -1.27 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 "Net-(D1-Pad4)") (pinfunction "M2") (pintype "input"))
    (pad "5" thru_hole circle locked (at -6.35 1.27 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "+5V") (pinfunction "~{RST}") (pintype "input"))
    (pad "6" thru_hole circle locked (at -6.35 3.81 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "+5V") (pinfunction "~{SLP}") (pintype "input"))
    (pad "7" thru_hole circle locked (at -6.35 6.35 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 22 "Net-(D1-Pad7)") (pinfunction "STEP") (pintype "input"))
    (pad "8" thru_hole circle locked (at -6.35 8.89 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 23 "Net-(D1-Pad8)") (pinfunction "DIR") (pintype "input"))
    (pad "9" thru_hole circle locked (at 6.35 8.89 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "10" thru_hole circle locked (at 6.35 6.35 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "unconnected-(D1-Pad10)") (pinfunction "~{FLT}") (pintype "output+no_connect"))
    (pad "11" thru_hole circle locked (at 6.35 3.81 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad11)") (pinfunction "A2") (pintype "output"))
    (pad "12" thru_hole circle locked (at 6.35 1.27 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad12)") (pinfunction "A1") (pintype "output"))
    (pad "13" thru_hole circle locked (at 6.35 -1.27 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad13)") (pinfunction "B1") (pintype "output"))
    (pad "14" thru_hole circle locked (at 6.35 -3.81 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 "Net-(D1-Pad14)") (pinfunction "B2") (pintype "output"))
    (pad "15" thru_hole circle locked (at 6.35 -6.35 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "GND_MOT") (pintype "power_in"))
    (pad "16" thru_hole circle locked (at 6.35 -8.89 270) (size 1.65 1.65) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "+12V") (pinfunction "VMOT") (pintype "power_in"))
  )
  (footprint "BNC 031-70578:0317057812G" (layer "F.Cu")
    (tedit 0)
    (at 106.68 104.14)
    (descr "031-70578-12G-2")
    (tags "Connector")
    (property "Description" "RF Connectors / Coaxial Connectors RF CONNECTOR BNC RIGHT ANGLE PCB")
    (property "Height" "11.18")
    (property "Manufacturer_Name" "Amphenol")
    (property "Manufacturer_Part_Number" "031-70578-12G")
    (property "Mouser Part Number" "523-0317057812G")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Amphenol-RF/031-70578-12G?qs=DRkmTr78QATSDA%2FxzBZ%252BjQ%3D%3D")
    (property "Sheetfile" "File: OPT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D3" (at -10.75 0) (layer "F.SilkS"))
    (fp_text value "031-70578-12G" (at -10.75 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -10.75 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.012 1.012) (drill 0.45) (layers *.Cu *.Mask)
      (net 9 "Net-(D3-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 3.225 3.225) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 3.225 -3.225) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -3.225 -3.225) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at -3.225 3.225) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "5") (pintype "passive"))
  )
  (footprint "BNC 031-70578:0317057812G" (layer "F.Cu")
    (tedit 0)
    (at 177.718 109.22 180)
    (descr "031-70578-12G-2")
    (tags "Connector")
    (property "Description" "RF Connectors / Coaxial Connectors RF CONNECTOR BNC RIGHT ANGLE PCB")
    (property "Height" "11.18")
    (property "Manufacturer_Name" "Amphenol")
    (property "Manufacturer_Part_Number" "031-70578-12G")
    (property "Mouser Part Number" "523-0317057812G")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Amphenol-RF/031-70578-12G?qs=DRkmTr78QATSDA%2FxzBZ%252BjQ%3D%3D")
    (property "Sheetfile" "File: OPT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D5" (at -10.75 0 180) (layer "F.SilkS"))
    (fp_text value "031-70578-12G" (at -10.75 0 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -10.75 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.012 1.012) (drill 0.45) (layers *.Cu *.Mask)
      (net 37 "Net-(D5-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 3.225 3.225 180) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 3.225 -3.225 180) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -3.225 -3.225 180) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at -3.225 3.225 180) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "5") (pintype "passive"))
  )
  (footprint "BNC 031-70578:0317057812G" (layer "F.Cu")
    (tedit 0)
    (at 177.718 81.661 180)
    (descr "031-70578-12G-2")
    (tags "Connector")
    (property "Description" "RF Connectors / Coaxial Connectors RF CONNECTOR BNC RIGHT ANGLE PCB")
    (property "Height" "11.18")
    (property "Manufacturer_Name" "Amphenol")
    (property "Manufacturer_Part_Number" "031-70578-12G")
    (property "Mouser Part Number" "523-0317057812G")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Amphenol-RF/031-70578-12G?qs=DRkmTr78QATSDA%2FxzBZ%252BjQ%3D%3D")
    (property "Sheetfile" "File: OPT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D4" (at -10.75 0 180) (layer "F.SilkS"))
    (fp_text value "031-70578-12G" (at -10.75 0 180) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at -10.75 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.012 1.012) (drill 0.45) (layers *.Cu *.Mask)
      (net 36 "Net-(D4-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 3.225 3.225 180) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 3.225 -3.225 180) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at -3.225 -3.225 180) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at -3.225 3.225 180) (size 2.28 2.28) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "5") (pintype "passive"))
  )
  (footprint "SS-90000-014:SS90000014" (layer "F.Cu")
    (tedit 0)
    (at 110.97 125.095 -90)
    (descr "SS-90000-014-2")
    (tags "Connector")
    (property "Description" "Modular Connectors / Ethernet Connectors RJ45 1x1 Jack, 8p8v, 30u gold plating on contacts, unshielded")
    (property "Height" "16.53")
    (property "Manufacturer_Name" "BelFuse")
    (property "Manufacturer_Part_Number" "SS-90000-014")
    (property "Mouser Part Number" "530-SS-90000-014")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Stewart-Connector-Bel/SS-90000-014?qs=T%252BzbugeAwjghcmHx82uQzQ%3D%3D")
    (property "Sheetfile" "File: OPT.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 3.302 -5.489 90) (layer "F.SilkS"))
    (fp_text value "SS-90000-014" (at 4.445 4.29 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.445 4.29 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -1.27 6.35 270) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 10.16 6.35 270) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad12)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 1.27 -2.54 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 2.54 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(D1-Pad11)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 3.81 -2.54 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 5.08 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad13)") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 6.35 -2.54 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 7.62 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(D1-Pad14)") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 8.89 -2.54 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "GND") (pinfunction "8") (pintype "passive"))
    (model "SS-90000-014.stp"
      (offset (xyz 12.14999944 3.930000008 17.04000066))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 -180))
    )
  )
  (footprint "EMK325ABJ107MM:CAPC3225X270N" (layer "B.Cu")
    (tedit 0)
    (at 152.527 96.266 -90)
    (descr "1210")
    (tags "Capacitor")
    (property "Description" "Taiyo Yuden 1210 (3225M) 100uF MLCC 16V dc +/-20% SMD EMK325ABJ107MM-P")
    (property "Height" "2.7")
    (property "Manufacturer_Name" "TAIYO YUDEN")
    (property "Manufacturer_Part_Number" "EMK325ABJ107MM-P")
    (property "Mouser Part Number" "963-EMK325ABJ107MM-P")
    (property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/TAIYO-YUDEN/EMK325ABJ107MM-P?qs=Zy5V7Kj3rCUP4LQ55a4G6A%3D%3D")
    (property "Sheetfile" "File: OPT.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at -3.937 0 180) (layer "B.SilkS"))
    (fp_text value "EMK325ABJ107MM-P" (at 0 0 90) (layer "B.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.35 0 270) (size 1.22 2.72) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "+12V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.35 0 270) (size 1.22 2.72) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 3 "GND") (pintype "passive"))
    (model "EMK325ABJ107MM-P.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 182.88 71.12) (end 101.6 138.43) (layer "Edge.Cuts") (width 0.1) (fill none))
  (zone (net 3) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 182.88 138.43)
        (xy 101.6 138.303)
        (xy 101.727 71.12)
        (xy 182.88 71.12)
      )
    )
  )
)
