(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 149)
    (no_connects 0)
    (area 100.429287 77.056 176.118163 139.761)
    (thickness 1.6)
    (drawings 53)
    (tracks 597)
    (zones 0)
    (modules 65)
    (nets 48)
  )
  (page A4)
  (title_block
    (title "Nursery Pager Hardware")
    (date 2017-04-04)
    (rev A)
    (company Petezah)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.4 1.4)
    (pad_drill 0.95)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ./NurseryPager-Hardware-gerbers/))
  )
  (net 0 "")
  (net 1 VBUS)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C6-Pad1)")
  (net 6 "Net-(C7-Pad1)")
  (net 7 "Net-(C7-Pad2)")
  (net 8 "Net-(C8-Pad1)")
  (net 9 "Net-(C8-Pad2)")
  (net 10 "Net-(C9-Pad1)")
  (net 11 VBAT)
  (net 12 "Net-(C12-Pad1)")
  (net 13 "Net-(D2-Pad1)")
  (net 14 "Net-(D3-Pad2)")
  (net 15 "Net-(D4-Pad1)")
  (net 16 "Net-(IC1-Pad1)")
  (net 17 "Net-(IC1-Pad5)")
  (net 18 SCL)
  (net 19 SDA)
  (net 20 "Net-(IC2-Pad4)")
  (net 21 "Net-(IC3-Pad4)")
  (net 22 "Net-(IC4-Pad1)")
  (net 23 "Net-(IC4-Pad2)")
  (net 24 "Net-(IC4-Pad3)")
  (net 25 "Net-(IC4-Pad7)")
  (net 26 "Net-(P1-Pad2)")
  (net 27 "Net-(P1-Pad3)")
  (net 28 "Net-(P1-Pad4)")
  (net 29 "Net-(R10-Pad2)")
  (net 30 "Net-(J1-Pad7)")
  (net 31 "Net-(J1-Pad14)")
  (net 32 "Net-(J1-Pad26)")
  (net 33 /MOTOR-)
  (net 34 /MOTOR+)
  (net 35 /LDO_EN)
  (net 36 /TXD)
  (net 37 /RXD)
  (net 38 /ESP_EN)
  (net 39 /GPIO2)
  (net 40 /ADC)
  (net 41 /GPIO0)
  (net 42 /RESET)
  (net 43 /BTN1)
  (net 44 /BTN2)
  (net 45 /BTN3)
  (net 46 /BTN4)
  (net 47 /AUTORST)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /ADC)
    (add_net /AUTORST)
    (add_net /BTN1)
    (add_net /BTN2)
    (add_net /BTN3)
    (add_net /BTN4)
    (add_net /ESP_EN)
    (add_net /GPIO0)
    (add_net /GPIO2)
    (add_net /LDO_EN)
    (add_net /MOTOR+)
    (add_net /MOTOR-)
    (add_net /RESET)
    (add_net /RXD)
    (add_net /TXD)
    (add_net GND)
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC2-Pad4)")
    (add_net "Net-(IC3-Pad4)")
    (add_net "Net-(IC4-Pad1)")
    (add_net "Net-(IC4-Pad2)")
    (add_net "Net-(IC4-Pad3)")
    (add_net "Net-(IC4-Pad7)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(R10-Pad2)")
    (add_net SCL)
    (add_net SDA)
  )
  (net_class 3vPower ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
  )
  (net_class Motor ""
    (clearance 0.1524)
    (trace_width 0.3048)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
  )
  (net_class Power ""
    (clearance 0.1524)
    (trace_width 0.6096)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net VBAT)
    (add_net VBUS)
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0D44)
    (at 126.238 134.559 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K (at -0.061 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 /BTN2))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP7A placed (layer F.Cu) (tedit 587247C4)
    (at 158.7246 135.4836)
    (descr "Light Touch Switch,https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE20.pdf")
    (attr smd)
    (fp_text reference SW2 (at 0.0635 0 90) (layer F.SilkS))
    (fp_text value BTN1 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 1.8 -0.72) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.8 -0.72) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.8 0.72) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 43 /BTN1))
    (pad 2 smd rect (at -1.8 0.72) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 43 /BTN1))
  )
  (module kicad-libs:petezah-logo-tiny (layer B.Cu) (tedit 58DB1107)
    (at 122.6312 95.6056)
    (fp_text reference G2 (at -4.572 -2.54) (layer B.Fab) hide)
    (fp_text value LOGO (at -1.651 0.254) (layer B.Fab) hide)
  )
  (module LEDs:LED_0805 placed (layer F.Cu) (tedit 58D192C4)
    (at 159.809 87.5665)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 0 90) (layer F.SilkS))
    (fp_text value ORANGE (at 0 1.55) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 VBUS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0EE0)
    (at 150.368 96.155 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.238 1.651 90) (layer F.SilkS))
    (fp_text value 10pF (at 0.016 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0ED4)
    (at 147.082 95.25)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.524 -1.651 90) (layer F.SilkS))
    (fp_text value 10pF (at -0.016 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VBUS))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0DB8)
    (at 148.717 124.063 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -2.429 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.016 0.127 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0D7F)
    (at 137.922 124.063 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 2.397 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0DA3)
    (at 146.05 124.063 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -2.397 0 360) (layer F.SilkS))
    (fp_text value 1uF (at 0 0 360) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0DE2)
    (at 154.051 124.063 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -2.429 0 180) (layer F.SilkS))
    (fp_text value 4.7uF (at -0.016 0.127 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0D6B)
    (at 132.588 124.095 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 2.429 0 180) (layer F.SilkS))
    (fp_text value 1uF (at 0.016 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0D74)
    (at 135.255 124.063 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 2.397 0 180) (layer F.SilkS))
    (fp_text value 1uF (at -0.016 0.127 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0DF0)
    (at 156.718 124.095 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -2.397 0 180) (layer F.SilkS))
    (fp_text value 2.2uF (at 0.016 0.127 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0D5D)
    (at 160.401 126.603 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 2.683 0 360) (layer F.SilkS))
    (fp_text value 1uF (at 0.016 -0.127 360) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0F7E)
    (at 164.846 93.234 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 -1.778 450) (layer F.SilkS))
    (fp_text value 10uF (at 0 0 360) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 VBAT))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0DFE)
    (at 148.717 116.856 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 1uF (at -0.111 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 placed (layer F.Cu) (tedit 58DB0E44)
    (at 151.527 109.601)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 1uF (at 0.111 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123F placed (layer F.Cu) (tedit 587F7769)
    (at 156.334 96.774)
    (descr D_SOD-123F)
    (tags D_SOD-123F)
    (attr smd)
    (fp_text reference D1 (at 0.003 1.778) (layer F.SilkS))
    (fp_text value MBR120 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.4 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 1 VBUS))
    (pad 2 smd rect (at 1.4 0) (size 1.1 1.1) (layers F.Cu F.Paste F.Mask)
      (net 11 VBAT))
  )
  (module LEDs:LED_0805 placed (layer F.Cu) (tedit 58D192D3)
    (at 164.168 87.5665 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -0.127 270) (layer F.SilkS))
    (fp_text value GREEN (at 0 1.55 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 placed (layer F.Cu) (tedit 58D19A9A)
    (at 151.8588 87.5792 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 0 270) (layer F.SilkS))
    (fp_text value RED (at 0 1.55 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 placed (layer F.Cu) (tedit 5883B1A6)
    (at 161.587 93.134 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference IC1 (at 0.084 -0.188 180) (layer F.SilkS))
    (fp_text value MCP73831 (at 0 2.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 VBAT))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VBUS))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad5)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 placed (layer F.Cu) (tedit 5883B1A6)
    (at 147.15 98.232)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference IC3 (at 0.127 0 90) (layer F.SilkS))
    (fp_text value AP2112K-3.3 (at 0 2.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VBUS))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 35 /LDO_EN))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC3-Pad4)"))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm placed (layer F.Cu) (tedit 54130A77)
    (at 164.973 125.857 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC4 (at 0 0 90) (layer F.SilkS))
    (fp_text value ATECC508A (at 0 3.5 90) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC4-Pad1)"))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC4-Pad2)"))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC4-Pad3)"))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 SDA))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 SCL))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC4-Pad7)"))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-libs:Z4FC1B1301781 placed (layer F.Cu) (tedit 58C1771D)
    (at 162.433 111.655 180)
    (descr http://www.vibration-motor.com/products/download/Z4FC1B1301781.pdf)
    (tags "haptic motor erm")
    (fp_text reference M1 (at 0 -5.08 180) (layer F.SilkS))
    (fp_text value Motor_DC_Haptic (at 0 -8.89 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 2.825 180) (size 1.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /MOTOR+))
    (pad 2 smd rect (at 1.35 2.825 180) (size 1.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /MOTOR-))
    (pad "" smd rect (at 0 -1.375 180) (size 4.5 4.5) (layers F.Cu F.Paste F.Mask))
  )
  (module Connectors:USB_Micro-B_10103594-0001LF placed (layer F.Cu) (tedit 58DA845F)
    (at 144.709 90.774 180)
    (descr "Micro USB Type B 10103594-0001LF")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P1 (at -2.611 -0.158 180) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 6.17 180) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 VBUS))
    (pad 2 smd rect (at -0.65 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at 0 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 0.65 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(P1-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.5 270) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.42 -1.62 270) (size 1.4 1.4) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.42 -1.62 270) (size 1.4 1.4) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.73 1.38 270) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.73 1.38 270) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -0.96 1.62 270) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.96 1.62 270) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Connectors_JST:JST_PH_S2B-PH-SM4-TB_02x2.00mm_Angled placed (layer F.Cu) (tedit 58C50E40)
    (at 166.543 100.632 90)
    (descr "JST PH series connector, S2B-PH-SM4-TB, side entry type, surface mount, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (attr smd)
    (fp_text reference P2 (at 0 0.335 90) (layer F.SilkS))
    (fp_text value JSTPH (at 0 5.375 90) (layer F.Fab))
    (fp_text user %R (at 0 1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 -2.875 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 -2.875 90) (size 1 3.5) (layers F.Cu F.Paste F.Mask)
      (net 11 VBAT))
    (pad "" smd rect (at -3.35 2.875 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.35 2.875 90) (size 1.5 3.4) (layers F.Cu F.Paste F.Mask))
    (model Connectors_JST.3dshapes/JST_PH_S2B-PH-SM4-TB_02x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm placed (layer F.Cu) (tedit 58DB0BF4)
    (at 152.654 100.076)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P3 (at -2.54 0) (layer F.SilkS))
    (fp_text value VIN (at 0 2.39) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VBUS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm placed (layer F.Cu) (tedit 5862ED52)
    (at 138.303 89.535)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P4 (at 0 -2.39) (layer F.SilkS))
    (fp_text value UART (at 0 7.47) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /TXD))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /RXD))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0D93)
    (at 140.589 124.267 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.601 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0DD3)
    (at 151.384 124.267 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -2.225 0 180) (layer F.SilkS))
    (fp_text value 390K (at -0.066 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J1-Pad26)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0DA8)
    (at 143.256 124.267 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 2.601 0 180) (layer F.SilkS))
    (fp_text value 10K (at -0.066 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J1-Pad14)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0E8F)
    (at 143.891 95.951 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -0.066 1.905 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 360) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VBUS))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /LDO_EN))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0F18)
    (at 159.827 89.662)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.22 -0.127 90) (layer F.SilkS))
    (fp_text value 470 (at 0.066 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0F0D)
    (at 158.496 93.279 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -0.066 1.651 450) (layer F.SilkS))
    (fp_text value 10K (at 0.066 0 360) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad5)"))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0E52)
    (at 117.094 97.475 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -2.352 0 360) (layer F.SilkS))
    (fp_text value 10K (at 0 0 360) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 /ESP_EN))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0F23)
    (at 164.145 89.662)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 2.479 -0.127 90) (layer F.SilkS))
    (fp_text value 470 (at 0 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0E8A)
    (at 139.192 98.105 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -0.193 2.032 180) (layer F.SilkS))
    (fp_text value 10K (at 0 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 SCL))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0F8D)
    (at 138.811 108.905 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at -0.061 -1.651 90) (layer F.SilkS))
    (fp_text value 10K (at 0 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R10-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0E6A)
    (at 139.192 102.047 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at -0.955 -2.413 360) (layer F.SilkS))
    (fp_text value 10K (at 0.061 0 360) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 SDA))
    (pad 2 smd rect (at 0.95 0 270) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0E5B)
    (at 139.131 105.41)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 3.236 0.127 180) (layer F.SilkS))
    (fp_text value 10K (at 0.061 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 /GPIO2))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0F4B)
    (at 157.038 100.693271)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 2.474 -0.363271 270) (layer F.SilkS))
    (fp_text value 1220K (at 0 2.430729 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 /ADC))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 VBAT))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0F65)
    (at 157.033 103.251 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at -0.066 -1.905 360) (layer F.SilkS))
    (fp_text value 220K (at 0 2.667 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 /ADC))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0FAA)
    (at 151.958 89.789)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 2.474 0.127 270) (layer F.SilkS))
    (fp_text value 1K (at 0 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 /GPIO0))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0E30)
    (at 126.238 114.239 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at -2.474 0 180) (layer F.SilkS))
    (fp_text value 10K (at -0.061 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 42 /RESET))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0D4F)
    (at 164.0586 134.554 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10K (at 0 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /BTN1))
    (pad 2 smd rect (at 0.95 0 90) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0E18)
    (at 170.373 116.586 180)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 -1.65 180) (layer F.SilkS))
    (fp_text value 10K (at 0.066 0 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 /BTN3))
    (pad 2 smd rect (at 0.95 0 180) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 placed (layer F.Cu) (tedit 58DB0E0E)
    (at 117.033 117.348)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 0 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.65) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 /BTN4))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module kicad-libs:SJ placed (layer F.Cu) (tedit 58DA774F)
    (at 122.189 123.444 180)
    (tags "solder jumper open")
    (fp_text reference SJ1 (at 0 1.8 180) (layer F.Fab))
    (fp_text value WAKE (at 0.015 2.032 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.65 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 42 /RESET))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 47 /AUTORST))
  )
  (module kicad-libs:SJ_C placed (layer F.Cu) (tedit 58DA7745)
    (at 122.159 126.746)
    (tags "solder jumper closed")
    (fp_text reference SJ2 (at 0 1.8) (layer F.Fab))
    (fp_text value BTN4 (at 0.015 2.286) (layer F.SilkS))
    (pad 1 smd rect (at -0.65 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 46 /BTN4))
    (pad 2 smd rect (at 0.65 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 47 /AUTORST))
    (pad "" smd rect (at 0 0) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP7A placed (layer F.Cu) (tedit 58CC56AA)
    (at 130.832 135.4748)
    (descr "Light Touch Switch,https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE20.pdf")
    (attr smd)
    (fp_text reference SW3 (at 0.0635 0 90) (layer F.SilkS))
    (fp_text value BTN2 (at 0 3.25) (layer F.Fab))
    (fp_text user %R (at 0 -2.5) (layer F.Fab))
    (pad 1 smd rect (at 1.8 -0.72) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.8 -0.72) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.8 0.72) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 44 /BTN2))
    (pad 2 smd rect (at -1.8 0.72) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 44 /BTN2))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP7A placed (layer F.Cu) (tedit 587247C4)
    (at 171.0524 121.9166 90)
    (descr "Light Touch Switch,https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE20.pdf")
    (attr smd)
    (fp_text reference SW4 (at 0 -0.042 180) (layer F.SilkS))
    (fp_text value BTN3 (at 0 3.25 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 90) (layer F.Fab))
    (pad 1 smd rect (at 1.8 -0.72 90) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.8 -0.72 90) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.8 0.72 90) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 45 /BTN3))
    (pad 2 smd rect (at -1.8 0.72 90) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 45 /BTN3))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQP7A placed (layer F.Cu) (tedit 587247C4)
    (at 115.9852 121.9166 270)
    (descr "Light Touch Switch,https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE20.pdf")
    (attr smd)
    (fp_text reference SW5 (at 0 -0.254 360) (layer F.SilkS))
    (fp_text value BTN4 (at 0 3.25 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.5 270) (layer F.Fab))
    (pad 1 smd rect (at 1.8 -0.72 270) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.8 -0.72 270) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.8 0.72 270) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 46 /BTN4))
    (pad 2 smd rect (at -1.8 0.72 270) (size 1.4 1.05) (layers F.Cu F.Paste F.Mask)
      (net 46 /BTN4))
  )
  (module kicad-libs:ESP-12S placed (layer F.Cu) (tedit 58B999EA)
    (at 127.800757 99.598439)
    (attr smd)
    (fp_text reference X1 (at 0 3.81) (layer F.SilkS))
    (fp_text value ESP-12S (at 0 6.35) (layer F.SilkS))
    (pad 1 smd rect (at -7.49808 -4.49834) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 42 /RESET))
    (pad 2 smd rect (at -7.49808 -2.49936) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 40 /ADC))
    (pad 3 smd rect (at -7.49808 -0.49784) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 38 /ESP_EN))
    (pad 4 smd rect (at -7.49808 1.4986) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 47 /AUTORST))
    (pad 5 smd rect (at -7.49808 3.49758) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 45 /BTN3))
    (pad 6 smd rect (at -7.49808 5.4991) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 44 /BTN2))
    (pad 7 smd rect (at -7.49808 7.49808) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 43 /BTN1))
    (pad 8 smd rect (at -7.49808 9.4996) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 9 smd rect (at 7.49808 9.4996) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 7.49808 7.49808) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R10-Pad2)"))
    (pad 11 smd rect (at 7.49808 5.4991) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 39 /GPIO2))
    (pad 12 smd rect (at 7.49808 3.49758) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 41 /GPIO0))
    (pad 13 smd rect (at 7.49808 1.4986) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 19 SDA))
    (pad 14 smd rect (at 7.49808 -0.49784) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 18 SCL))
    (pad 15 smd rect (at 7.49808 -2.49936) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 37 /RXD))
    (pad 16 smd rect (at 7.49808 -4.49834) (size 1.99898 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 36 /TXD))
    (pad 17 smd rect (at 0 0) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module kicad-libs:FPC_30-ER-CON30HB-1 (layer F.Cu) (tedit 0)
    (at 144.78 128.27)
    (fp_text reference J1 (at 0 1.775) (layer F.SilkS))
    (fp_text value OLED-0.96W (at 0 3.125) (layer F.Fab))
    (pad 1 smd rect (at -7.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -6.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C7-Pad1)"))
    (pad 3 smd rect (at -6.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C7-Pad2)"))
    (pad 4 smd rect (at -5.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C8-Pad1)"))
    (pad 5 smd rect (at -5.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad2)"))
    (pad 6 smd rect (at -4.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 7 smd rect (at -4.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at -3.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at -3.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 10 smd rect (at -2.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 11 smd rect (at -2.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 12 smd rect (at -1.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at -1.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 14 smd rect (at -0.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J1-Pad14)"))
    (pad 15 smd rect (at -0.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd rect (at 0.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 0.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 18 smd rect (at 1.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 SCL))
    (pad 19 smd rect (at 1.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 SDA))
    (pad 20 smd rect (at 2.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 SDA))
    (pad 21 smd rect (at 2.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 3.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 23 smd rect (at 3.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 24 smd rect (at 4.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 25 smd rect (at 4.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 26 smd rect (at 5.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J1-Pad26)"))
    (pad 27 smd rect (at 5.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C6-Pad1)"))
    (pad 28 smd rect (at 6.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad1)"))
    (pad 29 smd rect (at 6.75 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 30 smd rect (at 7.25 0) (size 0.3 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 0 smd rect (at -8.79 2.325) (size 2 3) (layers F.Cu F.Paste F.Mask))
    (pad 0 smd rect (at 8.79 2.325) (size 2 3) (layers F.Cu F.Paste F.Mask))
  )
  (module kicad-libs:VSSOP-10 (layer F.Cu) (tedit 0)
    (at 152.908 115.783)
    (fp_text reference IC2 (at -0.016 -0.041 180) (layer F.SilkS))
    (fp_text value DRV2605L (at 0 0) (layer F.Fab))
    (pad 10 smd rect (at -1 -2.2) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -1 2.2) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C12-Pad1)"))
    (pad 9 smd rect (at -0.5 -2.2) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 33 /MOTOR-))
    (pad 2 smd rect (at -0.5 2.2) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 18 SCL))
    (pad 8 smd rect (at 0 -2.2) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 2.2) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 19 SDA))
    (pad 7 smd rect (at 0.5 -2.2) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 34 /MOTOR+))
    (pad 4 smd rect (at 0.5 2.2) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC2-Pad4)"))
    (pad 6 smd rect (at 1 -2.2) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at 1 2.2) (size 0.3 1.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58CFDADE)
    (at 122.424007 115.856573 90)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE7.pdf")
    (attr smd)
    (fp_text reference SW1 (at 0 0 90) (layer F.SilkS))
    (fp_text value RESET (at 0 3 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.65 90) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /RESET))
    (pad 1 smd rect (at -2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58CFDADB)
    (at 129.917007 115.795573 90)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE7.pdf")
    (attr smd)
    (fp_text reference SW6 (at 0 0 90) (layer F.SilkS))
    (fp_text value GPIO0 (at 0 3 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.65 90) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /GPIO0))
    (pad 1 smd rect (at -2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58CFDAD8)
    (at 134.870007 115.795573 90)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE7.pdf")
    (attr smd)
    (fp_text reference SW7 (at 0 0 90) (layer F.SilkS))
    (fp_text value GPIO2 (at 0 3 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.65 90) (layer F.Fab))
    (pad 2 smd rect (at 2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /GPIO2))
    (pad 1 smd rect (at -2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380 (layer F.Cu) (tedit 58DB084F)
    (at 170.434 88.646)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (fp_text reference MK1 (at 0.127 3.048) (layer F.Fab))
    (fp_text value Mounting_Hole (at 0 2.75) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380 (layer F.Cu) (tedit 58DB0849)
    (at 170.561 135.001)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (fp_text reference MK2 (at 0 -2.75) (layer F.Fab))
    (fp_text value Mounting_Hole (at 0 2.75) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380 (layer F.Cu) (tedit 58DB0844)
    (at 116.459 135.001)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (fp_text reference MK3 (at 0 -2.75) (layer F.Fab))
    (fp_text value Mounting_Hole (at 0 2.75) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO7380 (layer F.Cu) (tedit 58DB083E)
    (at 116.586 88.646)
    (descr "Mounting Hole 2.2mm, no annular, M2, ISO7380")
    (tags "mounting hole 2.2mm no annular m2 iso7380")
    (fp_text reference MK4 (at 0 3.048) (layer F.Fab))
    (fp_text value Mounting_Hole (at 0 2.75) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 58DB0BE8)
    (at 152.908 93.218)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P5 (at -2.54 -1.27) (layer F.SilkS))
    (fp_text value 3V3 (at 2.413 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module kicad-libs:petezah-logo-tiny (layer F.Cu) (tedit 58DB1107)
    (at 145.669 111.125)
    (fp_text reference G1 (at -4.572 2.54) (layer F.Fab) hide)
    (fp_text value LOGO (at -1.651 -0.254) (layer F.Fab) hide)
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 56C35ED0)
    (at 160.02 103.1748)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP1 (at 0.0508 2.3876 90) (layer F.SilkS))
    (fp_text value VBAT (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers F.Cu F.Mask)
      (net 11 VBAT))
  )
  (gr_text B3 (at 171.958 121.92 90) (layer B.SilkS))
  (gr_text B4 (at 115.189 121.793 270) (layer B.SilkS))
  (gr_text B2 (at 130.8862 136.3726) (layer B.SilkS))
  (gr_text B1 (at 158.7246 136.3726) (layer B.SilkS))
  (gr_text IO2 (at 138.303 119.253) (layer F.SilkS))
  (gr_text IO0 (at 126.619 119.253) (layer F.SilkS))
  (gr_text RST (at 118.745 112.522) (layer F.SilkS))
  (gr_text B3 (at 171.196 125.73) (layer F.SilkS))
  (gr_text B4 (at 116.078 125.73) (layer F.SilkS))
  (gr_text B1 (at 160.1216 132.9944) (layer F.SilkS))
  (gr_text B2 (at 129.159 132.969) (layer F.SilkS))
  (gr_text ESP-ID (at 158.242 101.092 180) (layer B.SilkS))
  (gr_text "Contains FCC ID: 2AHMR-ESP12S" (at 117.094 113.284 270) (layer B.SilkS))
  (gr_text "Nursery Pager, rev. A\n(C) Copyright 2017 Peter Dunshee" (at 168.275 100.965 90) (layer B.SilkS))
  (gr_text "Petezah\n@petezah" (at 127.6096 90.1192 180) (layer B.SilkS))
  (dimension 58.42 (width 0.3) (layer Dwgs.User)
    (gr_text "2.3000 in" (at 143.51 78.406) (layer Dwgs.User))
    (feature1 (pts (xy 172.72 85.09) (xy 172.72 77.056)))
    (feature2 (pts (xy 114.3 85.09) (xy 114.3 77.056)))
    (crossbar (pts (xy 114.3 79.756) (xy 172.72 79.756)))
    (arrow1a (pts (xy 172.72 79.756) (xy 171.593496 80.342421)))
    (arrow1b (pts (xy 172.72 79.756) (xy 171.593496 79.169579)))
    (arrow2a (pts (xy 114.3 79.756) (xy 115.426504 80.342421)))
    (arrow2b (pts (xy 114.3 79.756) (xy 115.426504 79.169579)))
  )
  (dimension 50.8 (width 0.3) (layer Dwgs.User)
    (gr_text "2.0000 in" (at 105.965 111.76 270) (layer Dwgs.User))
    (feature1 (pts (xy 111.76 137.16) (xy 104.615 137.16)))
    (feature2 (pts (xy 111.76 86.36) (xy 104.615 86.36)))
    (crossbar (pts (xy 107.315 86.36) (xy 107.315 137.16)))
    (arrow1a (pts (xy 107.315 137.16) (xy 106.728579 136.033496)))
    (arrow1b (pts (xy 107.315 137.16) (xy 107.901421 136.033496)))
    (arrow2a (pts (xy 107.315 86.36) (xy 106.728579 87.486504)))
    (arrow2b (pts (xy 107.315 86.36) (xy 107.901421 87.486504)))
  )
  (gr_line (start 118.11 137.16) (end 116.713 137.16) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3 125.984) (end 114.3 134.874) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.434 137.16) (end 168.91 137.16) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 172.72 107.442) (end 172.72 106.172) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 172.72 134.62) (end 172.72 134.747) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.307 86.36) (end 168.91 86.36) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 172.72 94.996) (end 172.72 88.646) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 170.307 88.773) (end 170.307 86.36) (angle 86.9872125) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 170.307 134.747) (end 172.72 134.747) (angle 86.9872125) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 116.713 134.747) (end 116.713 137.16) (angle 86.9872125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.3 88.773) (end 114.3 125.984) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.11 86.36) (end 116.586 86.36) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 116.712824 88.769665) (end 114.299824 88.769665) (angle 86.9872125) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.46 137.16) (end 118.11 137.16) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.589 86.36) (end 118.11 86.36) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 172.72 107.442) (end 172.72 134.62) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.704 105.156) (end 172.72 106.172) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.704 97.79) (end 171.704 105.156) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 171.704 96.012) (end 171.704 97.79) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 172.72 94.996) (end 171.704 96.012) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.971 86.36) (end 168.91 86.36) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 141.478 87.249) (end 148.082 87.249) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.589 86.36) (end 141.478 87.249) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 148.971 86.36) (end 148.082 87.249) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.83 137.16) (end 168.91 137.16) (layer Edge.Cuts) (width 0.1))
  (dimension 6.35 (width 0.127) (layer Dwgs.User)
    (gr_text "0.2500 in" (at 138.377471 132.678976 270) (layer Dwgs.User))
    (feature1 (pts (xy 142.267471 135.853976) (xy 137.027471 135.853976)))
    (feature2 (pts (xy 142.267471 129.503976) (xy 137.027471 129.503976)))
    (crossbar (pts (xy 139.727471 129.503976) (xy 139.727471 135.853976)))
    (arrow1a (pts (xy 139.727471 135.853976) (xy 139.14105 134.727472)))
    (arrow1b (pts (xy 139.727471 135.853976) (xy 140.313892 134.727472)))
    (arrow2a (pts (xy 139.727471 129.503976) (xy 139.14105 130.63048)))
    (arrow2b (pts (xy 139.727471 129.503976) (xy 140.313892 130.63048)))
  )
  (gr_line (start 127 137.16) (end 124.46 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 160.02 137.16) (end 163.83 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 130.81 137.16) (end 127 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.16 137.16) (end 130.81 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152.4 137.16) (end 160.02 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 138.43 137.16) (end 137.16 137.16) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 151.13 137.16) (end 151.13 135.89) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.43 135.89) (end 151.43 135.89) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3 86.36) (xy 114.3 137.16) (xy 172.72 137.16) (xy 172.72 86.36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.144 86.36) (xy 136.144 93.726) (xy 114.3 93.726) (xy 114.3 86.36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3 86.36) (xy 114.3 93.726) (xy 136.144 93.726) (xy 136.144 86.36)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer B.Cu) (hatch full 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3 86.36) (xy 172.72 86.36) (xy 172.72 137.16) (xy 114.3 137.16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.SilkS) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.223023 100.33) (xy 156.223023 91.44) (xy 171.463023 91.44) (xy 171.463023 100.33)
      )
    )
  )
)
