(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 55)
    (tracks 460)
    (zones 0)
    (modules 47)
    (nets 33)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.25)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6.4 6.4)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 "Net-(C7-Pad1)")
  (net 9 "Net-(C8-Pad1)")
  (net 10 "Net-(C9-Pad1)")
  (net 11 +3.3V)
  (net 12 "Net-(J1-Pad3)")
  (net 13 "Net-(J1-Pad4)")
  (net 14 VC_INTR)
  (net 15 SSEN_CLKIN)
  (net 16 OEB)
  (net 17 "Net-(J2-Pad1)")
  (net 18 "Net-(J4-Pad2)")
  (net 19 +3.3VREG)
  (net 20 CLK3)
  (net 21 CLK4)
  (net 22 CLK5)
  (net 23 CLK6)
  (net 24 CLK7)
  (net 25 CLK0)
  (net 26 CLK1)
  (net 27 CLK2)
  (net 28 "Net-(Q1-Pad1)")
  (net 29 "Net-(Q2-Pad1)")
  (net 30 "Net-(R3-Pad2)")
  (net 31 "Net-(R7-Pad1)")
  (net 32 "Net-(R7-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net +3.3VREG)
    (add_net +5V)
    (add_net CLK0)
    (add_net CLK1)
    (add_net CLK2)
    (add_net CLK3)
    (add_net CLK4)
    (add_net CLK5)
    (add_net CLK6)
    (add_net CLK7)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R7-Pad2)")
    (add_net OEB)
    (add_net SSEN_CLKIN)
    (add_net VC_INTR)
  )
  (net_class "50 Ohm" ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C312995)
    (at 123.6 84.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -3.1 0) (layer F.SilkS))
    (fp_text value 10 (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3.3VREG))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C313A7A)
    (at 114.4 77.4)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at -2.7 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 "Net-(Q2-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3.3VREG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 5C311B0D)
    (at 104 106)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad_Via (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 5C311B0D)
    (at 138 106)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad_Via (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 5C311B0D)
    (at 138 54)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad_Via (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C31240A)
    (at 119.9 65.4 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.3 0) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 +5V))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C312441)
    (at 112 65.4 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.3 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C312488)
    (at 120 70.4 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -2.3 0) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C312C23)
    (at 109.7 80.9 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.3 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C31282B)
    (at 111.7 83.9 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.3 0 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C313B6B)
    (at 123 93.5 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -0.8 1.9) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C6-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C3128CF)
    (at 120.8 83.9 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 1.1 1.9 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C3129A0)
    (at 123.6 86.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 2.6 -0.6 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5C312A78)
    (at 129.7 93.5 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -1 -1.9) (layer F.SilkS))
    (fp_text value 100n (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C9-Pad1)"))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 5C311BFD)
    (at 102 60)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Power/IO (at 0 20.11) (layer F.Fab) hide)
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +3.3V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 VC_INTR))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 SSEN_CLKIN))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 OEB))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:SMA-ENDLAUNCH (layer F.Cu) (tedit 5C3167CE)
    (at 100.1 97 270)
    (fp_text reference J2 (at -4.8 -1.9) (layer F.SilkS))
    (fp_text value VC/CLKIN (at 4.9 -3.7) (layer F.SilkS))
    (pad 1 smd rect (at 0 -2.54 270) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 17 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 3 -2.54 270) (size 1.8 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3 -2.54 270) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3 -0.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -4.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 2.5 -3.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 -3.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -2.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 2.5 -1.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 -1.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -0.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -4.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3.5 -3.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -2.5 -3.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -2.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3.5 -1.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -2.5 -1.5 270) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 smd rect (at 3 -2.54 270) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3 -2.54 270) (size 1.8 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5C3167C3)
    (at 108.7 94.4)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value VC/CLKIN (at 0 7.41) (layer F.SilkS) hide)
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 SSEN_CLKIN))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 VC_INTR))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5C3167AB)
    (at 102 83.2)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value "PS Sel" (at 0.7 7.2) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 +3.3VREG))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer F.Cu) (tedit 5C311D6D)
    (at 118.2 60.1 270)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J5 (at 0 7.8) (layer F.SilkS))
    (fp_text value "3.3V Sel" (at 0 -4.7) (layer F.SilkS))
    (fp_text user %R (at 0 2.54) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 +3.3V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 +3.3VREG))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 5C311E29)
    (at 109.5 108 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J6 (at -1.1 -2.4 180) (layer F.SilkS))
    (fp_text value CLK3-CLK7 (at 2.1 19.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 CLK1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 CLK3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 CLK5))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 CLK6))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 CLK7))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:SMA-ENDLAUNCH (layer F.Cu) (tedit 5C326D05)
    (at 142 64 90)
    (fp_text reference J10 (at -4.7 -1.3 180) (layer F.SilkS))
    (fp_text value CLK4 (at 4.8 -3.5 180) (layer F.SilkS))
    (pad 1 smd rect (at 0 -2.54 90) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 21 CLK4))
    (pad 2 smd rect (at 3 -2.54 90) (size 1.8 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3 -2.54 90) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 3 -0.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -4.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 2.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -2.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 2.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -0.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -4.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -2.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -2.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -2.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 smd rect (at 3 -2.54 90) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3 -2.54 90) (size 1.8 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
  )
  (module EtherkitKicadLibrary:SMA-ENDLAUNCH (layer F.Cu) (tedit 5C311F8F)
    (at 142 80 90)
    (fp_text reference J11 (at -4.7 -1.3 180) (layer F.SilkS))
    (fp_text value CLK0 (at 4.8 -3.5) (layer F.SilkS))
    (pad 2 smd rect (at -3 -2.54 90) (size 1.8 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3 -2.54 90) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -2.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -2.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -4.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -0.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 2.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -2.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 2.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -4.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -0.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 smd rect (at -3 -2.54 90) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3 -2.54 90) (size 1.8 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -2.54 90) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 25 CLK0))
  )
  (module EtherkitKicadLibrary:SMA-ENDLAUNCH (layer F.Cu) (tedit 5C311FEF)
    (at 142 96 90)
    (fp_text reference J12 (at -4.7 -1.3 180) (layer F.SilkS))
    (fp_text value CLK2 (at 4.8 -3.5 180) (layer F.SilkS))
    (pad 2 smd rect (at -3 -2.54 90) (size 1.8 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3 -2.54 90) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -2.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -2.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -2.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -4.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at -3 -0.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 2.5 -1.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -2.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 2.5 -3.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -4.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 thru_hole circle (at 3 -0.5 90) (size 0.3 0.3) (drill 0.2) (layers *.Cu *.Mask)
      (net 2 GND) (zone_connect 2))
    (pad 2 smd rect (at -3 -2.54 90) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 3 -2.54 90) (size 1.8 5.08) (layers B.Cu B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at 0 -2.54 90) (size 1.8 5.08) (layers F.Cu F.Mask)
      (net 27 CLK2))
  )
  (module EtherkitKicadLibrary:SOT23-2N7002 (layer F.Cu) (tedit 562D55A3)
    (at 118.2 74.5 180)
    (descr SOT23)
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q1 (at -1.7 1.1 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.889 -1.016 180) (size 0.9144 0.9144) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.889 -1.016 180) (size 0.9144 0.9144) (layers F.Cu F.Paste F.Mask)
      (net 19 +3.3VREG))
    (pad 3 smd rect (at 0 1.016 180) (size 0.9144 0.9144) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad3)"))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:SOT23-2N7002 (layer F.Cu) (tedit 562D55A3)
    (at 114.4 74.5 180)
    (descr SOT23)
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference Q2 (at 1.7 1.1 180) (layer F.SilkS))
    (fp_text value 2N7002 (at 0 0 180) (layer F.SilkS) hide)
    (pad 3 smd rect (at 0 1.016 180) (size 0.9144 0.9144) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad4)"))
    (pad 2 smd rect (at 0.889 -1.016 180) (size 0.9144 0.9144) (layers F.Cu F.Paste F.Mask)
      (net 19 +3.3VREG))
    (pad 1 smd rect (at -0.889 -1.016 180) (size 0.9144 0.9144) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q2-Pad1)"))
    (model smd/cms_sot23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.13 0.15 0.15))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C313084)
    (at 117.2 70.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2.3 0.2 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J4-Pad2)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C3138D6)
    (at 114.8 70.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.3 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 18 "Net-(J4-Pad2)"))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C312C7C)
    (at 108.4 84.8 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 1.5 180) (layer F.SilkS))
    (fp_text value 0 (at 0 1.65 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 180) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C312C11)
    (at 107.5 80.9 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at -2.3 0) (layer F.SilkS))
    (fp_text value 10 (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C4-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3.3VREG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C313A51)
    (at 118.2 77.4)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 2.6 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3.3VREG))
    (pad 2 smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:PAT1220 (layer F.Cu) (tedit 5A24BA83)
    (at 112.9 88.9)
    (fp_text reference R7 (at 0 -1.6) (layer F.SilkS))
    (fp_text value PAT1220-C-10dB (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 -0.6) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.75 -0.6) (size 0.8 0.7) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R7-Pad2)"))
    (pad 3 smd rect (at 0 0.6) (size 2.4 0.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C312810)
    (at 113.7 83.9 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at -2.3 0) (layer F.SilkS))
    (fp_text value 10 (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 "Net-(C5-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3.3VREG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C3128B8)
    (at 118.7 83.9 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 2.2 1) (layer F.SilkS))
    (fp_text value 10 (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3.3VREG))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C313B2B)
    (at 125.2 93.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 2.3 -0.4 180) (layer F.SilkS))
    (fp_text value 10 (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C6-Pad1)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3.3VREG))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C312A4C)
    (at 127.5 93.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 2.3 0.8 180) (layer F.SilkS))
    (fp_text value 10 (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3.3VREG))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:SOT23-5 (layer F.Cu) (tedit 562D732E)
    (at 116 65.7 180)
    (attr smd)
    (fp_text reference U1 (at 0 2.6) (layer F.SilkS))
    (fp_text value LP2985-3.3 (at 0 0 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.27 180) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at 0.9525 1.27 180) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -0.9525 -1.27 180) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 0 1.27 180) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.9525 -1.27 180) (size 0.508 0.762) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model smd/SOT23_5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.1 0.1 0.1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:ASTX-H11-25.000MHZ-T (layer F.Cu) (tedit 5C31255D)
    (at 109.5 89.1 270)
    (fp_text reference U2 (at -2.6 0) (layer F.SilkS))
    (fp_text value ASTX-H11-25.000MHZ-T (at 0 -2.35 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.15 0.95 270) (size 1.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 1.15 0.95 270) (size 1.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.15 -0.95 270) (size 1.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(R7-Pad1)"))
    (pad 4 smd rect (at -1.15 -0.95 270) (size 1.3 1.1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
  )
  (module EtherkitKicadLibrary:QFN-20-1EP_4x4mm_Pitch0.5mm (layer F.Cu) (tedit 5680A209)
    (at 118.7 89.3)
    (descr "20-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U3 (at -3.7 -3) (layer F.SilkS))
    (fp_text value Si5351B/C (at 0 -3.3) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.965 -1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R7-Pad2)"))
    (pad 2 smd rect (at -1.965 -0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(R3-Pad2)"))
    (pad 3 smd rect (at -1.965 0) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 VC_INTR))
    (pad 4 smd rect (at -1.965 0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(Q1-Pad1)"))
    (pad 5 smd rect (at -1.965 1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q2-Pad1)"))
    (pad 6 smd rect (at -1 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 15 SSEN_CLKIN))
    (pad 7 smd rect (at -0.5 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 OEB))
    (pad 8 smd rect (at 0 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 CLK3))
    (pad 9 smd rect (at 0.5 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 CLK2))
    (pad 10 smd rect (at 1 1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 11 smd rect (at 1.965 1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C9-Pad1)"))
    (pad 12 smd rect (at 1.965 0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 CLK1))
    (pad 13 smd rect (at 1.965 0) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 CLK0))
    (pad 14 smd rect (at 1.965 -0.5) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C8-Pad1)"))
    (pad 15 smd rect (at 1.965 -1) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 CLK7))
    (pad 16 smd rect (at 1 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 CLK6))
    (pad 17 smd rect (at 0.5 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 CLK5))
    (pad 18 smd rect (at 0 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 19 smd rect (at -0.5 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 CLK4))
    (pad 20 smd rect (at -1 -1.965 90) (size 0.73 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 21 smd rect (at 0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at 0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at -0.625 0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 21 smd rect (at -0.625 -0.625) (size 1.25 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_paste_margin_ratio -0.2))
    (pad 21 thru_hole circle (at 0.6 -0.6) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 21 thru_hole circle (at -0.6 -0.6) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 21 thru_hole circle (at -0.6 0.6) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 21 thru_hole circle (at 0.6 0.6) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C31201C)
    (at 133.5 64)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CLK4 (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 CLK4))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C312203)
    (at 133.5 80)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CLK0 (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 CLK0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 5C312231)
    (at 133.5 96)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J9 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CLK2 (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 CLK2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_Pad_Via (layer F.Cu) (tedit 5C311B0D)
    (at 104 54)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad_Via (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 -2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 -1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 2.4) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 1.697056 1.697056) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 2.4 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C313E3B)
    (at 109.3 65.4 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 2.3 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 +3.3VREG))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 VC_INTR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C313E6E)
    (at 109.3 70.1 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -2.3 -0.1) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 SSEN_CLKIN))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5C313EBE)
    (at 109.3 74.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 2.3 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.65 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GND))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 OEB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module EtherkitKicadLibrary:OSHWLogo4mm (layer F.Cu) (tedit 0)
    (at 133.2 72.7)
    (fp_text reference G*** (at 0 2.35966) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0 -2.35966) (layer F.SilkS) hide)
  )
  (module EtherkitKicadLibrary:EtherkitLogoSmall (layer F.Cu) (tedit 0)
    (at 132.6 56.8)
    (fp_text reference Ref** (at 0 3.25) (layer F.SilkS) hide)
    (fp_text value Val** (at 0 -2.95) (layer F.SilkS) hide)
  )
  (gr_text CLKIN (at 111 98.4) (layer F.SilkS))
  (gr_text VC (at 111 95.5) (layer F.SilkS))
  (gr_text CLK7 (at 129.9 106) (layer F.SilkS))
  (gr_text CLK6 (at 124.8 106) (layer F.SilkS))
  (gr_text CLK5 (at 119.6 106) (layer F.SilkS))
  (gr_text CLK3 (at 114.6 106) (layer F.SilkS))
  (gr_text GND (at 132.4 106) (layer F.SilkS))
  (gr_text GND (at 127.3 106) (layer F.SilkS))
  (gr_text GND (at 122.2 106) (layer F.SilkS))
  (gr_text GND (at 117.1 106) (layer F.SilkS))
  (gr_text GND (at 112.1 106) (layer F.SilkS))
  (gr_text CLK1 (at 109.5 106) (layer F.SilkS))
  (gr_text 3.3V (at 104.2 87.2) (layer F.SilkS))
  (gr_text 5V (at 104.2 84.4) (layer F.SilkS))
  (gr_text EXT (at 116.1 57.2) (layer F.SilkS))
  (gr_text VREG (at 112.8 57.2) (layer F.SilkS))
  (gr_text GND (at 103.5 77.8) (layer F.SilkS))
  (gr_text OEB (at 103.5 75.2) (layer F.SilkS))
  (gr_text "SSEN/\nCLKIN" (at 103.5 72.7) (layer F.SilkS))
  (gr_text VC/INT (at 103.5 70.1) (layer F.SilkS))
  (gr_text SDA (at 103.5 67.6) (layer F.SilkS))
  (gr_text SCL (at 103.5 65.1) (layer F.SilkS))
  (gr_text +3.3V (at 103.5 62.6) (layer F.SilkS))
  (gr_text +5V (at 103.5 60) (layer F.SilkS))
  (gr_text Correction (at 133.9 60) (layer B.SilkS))
  (gr_text "Creative Commons\nLicense 4.0 CC-BY-SA" (at 133.8 102.3) (layer F.SilkS))
  (gr_text "etherkit.com 2019" (at 107.9 54.8) (layer F.SilkS))
  (gr_text "Si5351B/C Breakout Board" (at 107.8 52.1) (layer F.SilkS))
  (gr_arc (start 140 108) (end 140 110) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102 108) (end 100 108) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102 52) (end 102 50) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 140 52) (end 142 52) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142 108) (end 142 52) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 52) (end 100 108) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102 110) (end 140 110) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102 50) (end 140 50) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 121.8 88.6) (xy 126.2 88.6) (xy 128.8 86) (xy 128.8 80.8) (xy 130.4 79.2)
        (xy 132.2 79.2) (xy 132.2 78.8) (xy 134.7 78.8) (xy 134.7 79.2) (xy 136.9 79.2)
        (xy 136.9 80.7) (xy 134.7 80.7) (xy 134.7 81.1) (xy 132.3 81.1) (xy 132.3 80.7)
        (xy 130.9 80.7) (xy 130.2 81.4) (xy 130.2 86.6) (xy 126.9 90) (xy 121.8 90)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 119.9 92.5) (xy 119.9 93.9) (xy 122.1 96.1) (xy 122.3 96.2) (xy 131.3 96.2)
        (xy 132.2 95.3) (xy 132.2 94.8) (xy 134.7 94.8) (xy 134.7 95.3) (xy 136.9 95.3)
        (xy 136.9 96.7) (xy 134.7 96.7) (xy 134.7 97.1) (xy 132.3 97.1) (xy 131.8 97.6)
        (xy 121.6 97.6) (xy 118.5 94.4) (xy 118.5 92.5)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 100.7 50.7) (xy 141.3 50.7) (xy 141.3 109.3) (xy 100.7 109.3)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 100.7 50.7) (xy 141.3 50.7) (xy 141.3 109.3) (xy 100.7 109.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25)
    (fill yes (arc_segments 32) (thermal_gap 0.25) (thermal_bridge_width 0.3) (smoothing chamfer) (radius 0.2))
    (polygon
      (pts
        (xy 115.7 85.3) (xy 115.7 80.6) (xy 116.7 79.6) (xy 124.2 79.6) (xy 125.6 78.2)
        (xy 125.6 67.5) (xy 129.7 63.4) (xy 132.2 63.4) (xy 132.2 62.8) (xy 134.7 62.8)
        (xy 134.7 63.4) (xy 136.9 63.4) (xy 136.9 64.6) (xy 134.7 64.6) (xy 134.7 65.1)
        (xy 132.4 65.1) (xy 132.4 64.7) (xy 130.3 64.7) (xy 126.9 68.1) (xy 126.9 78.8)
        (xy 124.8 80.9) (xy 117.3 80.9) (xy 117 81.2) (xy 117 85.3)
      )
    )
  )
)
