(kicad_pcb (version 4) (host pcbnew 4.0.7-e2-6376~58~ubuntu14.04.1)
  (general
    (links 99)
    (no_connects 0)
    (area 54.65 31.79 142.2 156.17)
    (thickness 1.6)
    (drawings 4)
    (tracks 402)
    (zones 0)
    (modules 37)
    (nets 44)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 1.7)
    (via_drill 1)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.75 1.75)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x200a0_00000000)
      (usegerberextensions false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 2)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 2)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory output/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(C3-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(CON1-Pad1)")
  (net 6 /In1)
  (net 7 "Net-(CON2-Pad1)")
  (net 8 /In2)
  (net 9 "Net-(CON3-Pad1)")
  (net 10 /In3)
  (net 11 "Net-(CON4-Pad1)")
  (net 12 /In4)
  (net 13 "Net-(CON5-Pad1)")
  (net 14 /In5)
  (net 15 "Net-(CON6-Pad1)")
  (net 16 /In6)
  (net 17 "Net-(CON7-Pad1)")
  (net 18 /In7)
  (net 19 "Net-(CON8-Pad1)")
  (net 20 /In8)
  (net 21 /Out1)
  (net 22 /Out2)
  (net 23 /Out3)
  (net 24 /Out4)
  (net 25 "Net-(IC1-Pad6)")
  (net 26 "Net-(IC1-Pad9)")
  (net 27 "Net-(IC1-Pad10)")
  (net 28 /Out5)
  (net 29 /Out6)
  (net 30 /Out7)
  (net 31 /Out8)
  (net 32 "Net-(IC1-Pad19)")
  (net 33 "Net-(IC1-Pad2)")
  (net 34 "Net-(IC1-Pad3)")
  (net 35 "Net-(Q1-PadE)")
  (net 36 "Net-(Q2-PadE)")
  (net 37 "Net-(Q3-PadE)")
  (net 38 "Net-(Q4-PadE)")
  (net 39 "Net-(Q5-PadE)")
  (net 40 "Net-(Q6-PadE)")
  (net 41 "Net-(Q7-PadE)")
  (net 42 "Net-(Q8-PadE)")
  (net 43 "Net-(IC1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 1.7)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /In1)
    (add_net /In2)
    (add_net /In3)
    (add_net /In4)
    (add_net /In5)
    (add_net /In6)
    (add_net /In7)
    (add_net /In8)
    (add_net /Out1)
    (add_net /Out2)
    (add_net /Out3)
    (add_net /Out4)
    (add_net /Out5)
    (add_net /Out6)
    (add_net /Out7)
    (add_net /Out8)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad9)")
  )
  (net_class 5v ""
    (clearance 0.2)
    (trace_width 2)
    (via_dia 1.7)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class thick ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1.7)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON2-Pad1)")
    (add_net "Net-(CON3-Pad1)")
    (add_net "Net-(CON4-Pad1)")
    (add_net "Net-(CON5-Pad1)")
    (add_net "Net-(CON6-Pad1)")
    (add_net "Net-(CON7-Pad1)")
    (add_net "Net-(CON8-Pad1)")
    (add_net "Net-(Q1-PadE)")
    (add_net "Net-(Q2-PadE)")
    (add_net "Net-(Q3-PadE)")
    (add_net "Net-(Q4-PadE)")
    (add_net "Net-(Q5-PadE)")
    (add_net "Net-(Q6-PadE)")
    (add_net "Net-(Q7-PadE)")
    (add_net "Net-(Q8-PadE)")
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 56686DA7)
    (at 92.71 104.14)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -4.318 -0.508) (layer B.SilkS))
    (fp_text value 100U (at -1.524 1.778) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 56686D9E)
    (at 93.98 101.6)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.556 -0.762) (layer B.SilkS))
    (fp_text value 10U (at -3.81 0.508) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 56686E14)
    (at 97.79 86.36 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -3.302 1.016 180) (layer B.SilkS))
    (fp_text value 100n (at -4.064 -0.508 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 56686E1D)
    (at 97.79 88.9)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 3.302 -0.762) (layer B.SilkS))
    (fp_text value 0 (at 3.048 0.762) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 56686E0A)
    (at 96.52 83.82 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at -3.81 1.27 180) (layer B.SilkS))
    (fp_text value 100 (at -3.81 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module smd_parts:Resistor_Array_SIP8 (layer F.Cu) (tedit 56686E80)
    (at 73.66 95.25 90)
    (descr "8 R pack")
    (tags R)
    (fp_text reference RR1 (at -9.652 -2.54 90) (layer F.SilkS))
    (fp_text value PD_RR8_10k (at -9.144 2.032 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -10.16 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at -7.62 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 21 /Out1))
    (pad 3 thru_hole circle (at -5.08 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 22 /Out2))
    (pad 4 thru_hole circle (at -2.54 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 23 /Out3))
    (pad 5 thru_hole circle (at 0 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 24 /Out4))
    (pad 6 thru_hole circle (at 2.54 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 28 /Out5))
    (pad 7 thru_hole circle (at 5.08 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 29 /Out6))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 30 /Out7))
    (pad 9 thru_hole circle (at 10.16 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 31 /Out8))
    (model Resistors_ThroughHole.3dshapes/Resistor_Array_SIP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module smd_parts:Resistor_Array_SIP8 (layer F.Cu) (tedit 56686E7A)
    (at 118.11 95.25 90)
    (descr "8 R pack")
    (tags R)
    (fp_text reference RR2 (at -7.874 -2.286 90) (layer F.SilkS))
    (fp_text value PU_RR8_10k (at -7.366 2.286 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -10.16 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 2 thru_hole circle (at -7.62 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 6 /In1))
    (pad 3 thru_hole circle (at -5.08 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 /In2))
    (pad 4 thru_hole circle (at -2.54 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 10 /In3))
    (pad 5 thru_hole circle (at 0 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 12 /In4))
    (pad 6 thru_hole circle (at 2.54 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 20 /In8))
    (pad 7 thru_hole circle (at 5.08 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 18 /In7))
    (pad 8 thru_hole circle (at 7.62 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 16 /In6))
    (pad 9 thru_hole circle (at 10.16 0 90) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 14 /In5))
    (model Resistors_ThroughHole.3dshapes/Resistor_Array_SIP8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module smd_parts:Crystal_Vertical_3Pin (layer F.Cu) (tedit 56686DB9)
    (at 101.6 101.6 180)
    (descr "Crystal, Quarz, HC49/U, vertical, stehend, 3 Pin,")
    (tags "Crystal, Quarz, HC49/U, vertical, stehend, 3 Pin,")
    (fp_text reference X1 (at 1.27 -3.048 180) (layer F.SilkS))
    (fp_text value CRYSTAL_WITH_CAPS (at -3.048 -1.524 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.44094 0 180) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(IC1-Pad10)"))
    (pad 3 thru_hole circle (at 2.44094 0 180) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad9)"))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module smd_parts:DIP-28__300 (layer F.Cu) (tedit 5650F605)
    (at 95.25 95.25)
    (descr "28 pins DIL package, round pads, width 300mil")
    (tags DIL)
    (fp_text reference IC1 (at -11.43 0) (layer F.SilkS))
    (fp_text value ATMEGA328P-P (at 10.16 0) (layer F.Fab))
    (pad 2 thru_hole circle (at -13.97 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole circle (at -11.43 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole circle (at -8.89 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 22 /Out2))
    (pad 5 thru_hole circle (at -6.35 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 21 /Out1))
    (pad 6 thru_hole circle (at -3.81 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(IC1-Pad6)"))
    (pad 7 thru_hole circle (at -1.27 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 8 thru_hole circle (at 1.27 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole circle (at 3.81 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad9)"))
    (pad 10 thru_hole circle (at 6.35 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(IC1-Pad10)"))
    (pad 11 thru_hole circle (at 8.89 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 6 /In1))
    (pad 12 thru_hole circle (at 11.43 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 8 /In2))
    (pad 13 thru_hole circle (at 13.97 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 10 /In3))
    (pad 14 thru_hole circle (at 16.51 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 12 /In4))
    (pad 1 thru_hole rect (at -16.51 3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(IC1-Pad1)"))
    (pad 15 thru_hole circle (at 16.51 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 20 /In8))
    (pad 16 thru_hole circle (at 13.97 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 18 /In7))
    (pad 17 thru_hole circle (at 11.43 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 16 /In6))
    (pad 18 thru_hole circle (at 8.89 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 14 /In5))
    (pad 19 thru_hole circle (at 6.35 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(IC1-Pad19)"))
    (pad 20 thru_hole circle (at 3.81 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 1 +5V))
    (pad 21 thru_hole circle (at 1.27 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C3-Pad1)"))
    (pad 22 thru_hole circle (at -1.27 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 23 thru_hole circle (at -3.81 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 23 /Out3))
    (pad 24 thru_hole circle (at -6.35 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 24 /Out4))
    (pad 25 thru_hole circle (at -8.89 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 31 /Out8))
    (pad 26 thru_hole circle (at -11.43 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 30 /Out7))
    (pad 27 thru_hole circle (at -13.97 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 29 /Out6))
    (pad 28 thru_hole circle (at -16.51 -3.81) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 28 /Out5))
    (model Sockets_DIP.3dshapes/DIP-28__300.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module smd_parts:SOT-223-Transistor (layer F.Cu) (tedit 565DC192)
    (at 73.66 127 270)
    (fp_text reference Q1 (at 0.3 5.3 270) (layer F.SilkS))
    (fp_text value Darl_NPN_ps (at 0 -5.2 270) (layer F.Fab))
    (pad E smd rect (at 2.3 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-PadE)"))
    (pad C smd rect (at 0 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad B smd rect (at -2.3 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /Out1))
    (pad C smd rect (at 0 -3.2 270) (size 3.3 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module smd_parts:SOT-223-Transistor (layer F.Cu) (tedit 565DC192)
    (at 90.17 127 270)
    (fp_text reference Q2 (at 0.3 5.3 270) (layer F.SilkS))
    (fp_text value Darl_NPN_ps (at 0 -5.2 270) (layer F.Fab))
    (pad E smd rect (at 2.3 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q2-PadE)"))
    (pad C smd rect (at 0 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad B smd rect (at -2.3 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /Out2))
    (pad C smd rect (at 0 -3.2 270) (size 3.3 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module smd_parts:SOT-223-Transistor (layer F.Cu) (tedit 565DC192)
    (at 106.68 127 270)
    (fp_text reference Q3 (at 0.3 5.3 270) (layer F.SilkS))
    (fp_text value Darl_NPN_ps (at 0 -5.2 270) (layer F.Fab))
    (pad E smd rect (at 2.3 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Q3-PadE)"))
    (pad C smd rect (at 0 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad B smd rect (at -2.3 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /Out3))
    (pad C smd rect (at 0 -3.2 270) (size 3.3 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module smd_parts:SOT-223-Transistor (layer F.Cu) (tedit 565DC192)
    (at 123.19 127 270)
    (fp_text reference Q4 (at 0.3 5.3 270) (layer F.SilkS))
    (fp_text value Darl_NPN_ps (at 0 -5.2 270) (layer F.Fab))
    (pad E smd rect (at 2.3 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(Q4-PadE)"))
    (pad C smd rect (at 0 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad B smd rect (at -2.3 3.1 270) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /Out4))
    (pad C smd rect (at 0 -3.2 270) (size 3.3 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module smd_parts:SOT-223-Transistor (layer F.Cu) (tedit 565DC192)
    (at 123.19 60.96 90)
    (fp_text reference Q5 (at 0.3 5.3 90) (layer F.SilkS))
    (fp_text value Darl_NPN_ps (at 0 -5.2 90) (layer F.Fab))
    (pad E smd rect (at 2.3 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(Q5-PadE)"))
    (pad C smd rect (at 0 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad B smd rect (at -2.3 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /Out5))
    (pad C smd rect (at 0 -3.2 90) (size 3.3 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module smd_parts:SOT-223-Transistor (layer F.Cu) (tedit 565DC192)
    (at 106.68 60.96 90)
    (fp_text reference Q6 (at 0.3 5.3 90) (layer F.SilkS))
    (fp_text value Darl_NPN_ps (at 0 -5.2 90) (layer F.Fab))
    (pad E smd rect (at 2.3 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(Q6-PadE)"))
    (pad C smd rect (at 0 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad B smd rect (at -2.3 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /Out6))
    (pad C smd rect (at 0 -3.2 90) (size 3.3 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module smd_parts:SOT-223-Transistor (layer F.Cu) (tedit 565DC192)
    (at 90.17 60.96 90)
    (fp_text reference Q7 (at 0.3 5.3 90) (layer F.SilkS))
    (fp_text value Darl_NPN_ps (at 0 -5.2 90) (layer F.Fab))
    (pad E smd rect (at 2.3 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(Q7-PadE)"))
    (pad C smd rect (at 0 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad B smd rect (at -2.3 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /Out7))
    (pad C smd rect (at 0 -3.2 90) (size 3.3 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module smd_parts:SOT-223-Transistor (layer F.Cu) (tedit 56686E3E)
    (at 73.66 60.96 90)
    (fp_text reference Q8 (at 0.3 5.3 90) (layer F.SilkS))
    (fp_text value Darl_NPN_ps (at -1.27 -1.27 90) (layer F.Fab))
    (pad E smd rect (at 2.3 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(Q8-PadE)"))
    (pad C smd rect (at 0 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad B smd rect (at -2.3 3.1 90) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /Out8))
    (pad C smd rect (at 0 -3.2 90) (size 3.3 1.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 56686D7E)
    (at 85.09 102.87 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 10k (at 3.81 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module smd_parts:C_Radial_D5_L11_P2.5_bigpad (layer F.Cu) (tedit 56686E26)
    (at 86.36 77.47 90)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C4 (at 1.25 -3.8 90) (layer F.SilkS))
    (fp_text value 1u (at -1.524 -2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.75 1.75) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module wafer:Socket_VH-RM3-96mm_Lock_4pin_straight (layer B.Cu) (tedit 56686EA8)
    (at 109.22 111.76 180)
    (descr "Socket, VH Connector, RM 3.96mm, Lock, 4pin, straight,")
    (tags "Socket, VH Connector, RM 3.96mm, Lock, 4pin, straight,")
    (fp_text reference P1 (at -8.636 -3.302 180) (layer B.SilkS))
    (fp_text value CONN_4 (at 0.254 -6.096 180) (layer B.Fab))
    (pad 2 thru_hole oval (at -1.98 0 180) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask B.SilkS)
      (net 1 +5V))
    (pad 3 thru_hole oval (at 1.98 0 180) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at -5.94 0 180) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask B.SilkS)
      (net 1 +5V))
    (pad 4 thru_hole oval (at 5.94 0 180) (size 2.99974 5.00126) (drill 1.80086) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
  )
  (module smd_parts:TSOPxx (layer F.Cu) (tedit 56686E29)
    (at 92.71 74.93 270)
    (descr "TO-92 horizontal, leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U1 (at 0 -11 450) (layer F.SilkS))
    (fp_text value IR_RECEIVER (at 0 1.778 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(IC1-Pad19)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1.75 1.75) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C4-Pad1)"))
    (model Housings_TO-92.3dshapes/TO-92_Horizontal2_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56686E88)
    (at 73.66 132.08)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at -1.524 0.508) (layer F.SilkS))
    (fp_text value 0.27 (at 0.762 -0.508) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 35 "Net-(Q1-PadE)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 "Net-(CON1-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56686E66)
    (at 121.92 55.88 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R5 (at 1.524 -0.508 180) (layer F.SilkS))
    (fp_text value 0.27 (at -0.762 0.508 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 39 "Net-(Q5-PadE)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 "Net-(CON5-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56686E92)
    (at 90.17 132.08)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R2 (at -1.524 0.508) (layer F.SilkS))
    (fp_text value 0.27 (at 0.762 -0.508) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 36 "Net-(Q2-PadE)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(CON2-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56686E99)
    (at 106.68 132.08)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R3 (at -1.524 0.508) (layer F.SilkS))
    (fp_text value 0.27 (at 1.016 -0.508) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 37 "Net-(Q3-PadE)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(CON3-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56686EA1)
    (at 123.19 132.08)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R4 (at -1.524 0.508) (layer F.SilkS))
    (fp_text value 0.27 (at 0.762 -0.508) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 38 "Net-(Q4-PadE)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(CON4-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56686E5D)
    (at 106.68 55.88 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R6 (at 1.524 -0.508 180) (layer F.SilkS))
    (fp_text value 0.27 (at -0.762 0.508 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 40 "Net-(Q6-PadE)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 "Net-(CON6-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56686E4B)
    (at 90.17 55.88 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R7 (at 1.524 -0.508 180) (layer F.SilkS))
    (fp_text value 0.27 (at -0.762 0.508 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 41 "Net-(Q7-PadE)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 17 "Net-(CON7-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56686E39)
    (at 73.66 55.88 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R8 (at 1.524 -0.762 180) (layer F.SilkS))
    (fp_text value 0.27 (at -0.762 0.254 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 42 "Net-(Q8-PadE)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 19 "Net-(CON8-Pad1)"))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module smd_parts:KLDX-SMT (layer F.Cu) (tedit 5665B8A2)
    (at 73.66 142.24)
    (fp_text reference CON1 (at 0 0.5) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 -8.1) (size 3.4 3) (drill 1 (offset 0 0.8)) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(CON1-Pad1)"))
    (pad 2 thru_hole rect (at -4.9 -2.43) (size 2.6 3) (drill 1 (offset -0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 4.9 -2.43) (size 2.6 3) (drill 1 (offset 0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 6 /In1))
    (pad 4 thru_hole circle (at 0 3.8) (size 2 2) (drill 1.75) (layers *.Cu *.Mask F.SilkS))
  )
  (module smd_parts:KLDX-SMT (layer F.Cu) (tedit 5665B8A2)
    (at 90.17 142.24)
    (fp_text reference CON2 (at 0 0.5) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 -8.1) (size 3.4 3) (drill 1 (offset 0 0.8)) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(CON2-Pad1)"))
    (pad 2 thru_hole rect (at -4.9 -2.43) (size 2.6 3) (drill 1 (offset -0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 4.9 -2.43) (size 2.6 3) (drill 1 (offset 0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 8 /In2))
    (pad 4 thru_hole circle (at 0 3.8) (size 2 2) (drill 1.75) (layers *.Cu *.Mask F.SilkS))
  )
  (module smd_parts:KLDX-SMT (layer F.Cu) (tedit 5665B8A2)
    (at 106.68 142.24)
    (fp_text reference CON3 (at 0 0.5) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 -8.1) (size 3.4 3) (drill 1 (offset 0 0.8)) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(CON3-Pad1)"))
    (pad 2 thru_hole rect (at -4.9 -2.43) (size 2.6 3) (drill 1 (offset -0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 4.9 -2.43) (size 2.6 3) (drill 1 (offset 0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 10 /In3))
    (pad 4 thru_hole circle (at 0 3.8) (size 2 2) (drill 1.75) (layers *.Cu *.Mask F.SilkS))
  )
  (module smd_parts:KLDX-SMT (layer F.Cu) (tedit 5665B8A2)
    (at 123.19 142.24)
    (fp_text reference CON4 (at 0 0.5) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 -8.1) (size 3.4 3) (drill 1 (offset 0 0.8)) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(CON4-Pad1)"))
    (pad 2 thru_hole rect (at -4.9 -2.43) (size 2.6 3) (drill 1 (offset -0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 4.9 -2.43) (size 2.6 3) (drill 1 (offset 0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 12 /In4))
    (pad 4 thru_hole circle (at 0 3.8) (size 2 2) (drill 1.75) (layers *.Cu *.Mask F.SilkS))
  )
  (module smd_parts:KLDX-SMT (layer F.Cu) (tedit 5665B8A2)
    (at 123.19 45.72 180)
    (fp_text reference CON5 (at 0 0.5 180) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -0.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 -8.1 180) (size 3.4 3) (drill 1 (offset 0 0.8)) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(CON5-Pad1)"))
    (pad 2 thru_hole rect (at -4.9 -2.43 180) (size 2.6 3) (drill 1 (offset -0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 4.9 -2.43 180) (size 2.6 3) (drill 1 (offset 0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 14 /In5))
    (pad 4 thru_hole circle (at 0 3.8 180) (size 2 2) (drill 1.75) (layers *.Cu *.Mask F.SilkS))
  )
  (module smd_parts:KLDX-SMT (layer F.Cu) (tedit 5665B8A2)
    (at 106.68 45.72 180)
    (fp_text reference CON6 (at 0 0.5 180) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -0.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 -8.1 180) (size 3.4 3) (drill 1 (offset 0 0.8)) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(CON6-Pad1)"))
    (pad 2 thru_hole rect (at -4.9 -2.43 180) (size 2.6 3) (drill 1 (offset -0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 4.9 -2.43 180) (size 2.6 3) (drill 1 (offset 0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 16 /In6))
    (pad 4 thru_hole circle (at 0 3.8 180) (size 2 2) (drill 1.75) (layers *.Cu *.Mask F.SilkS))
  )
  (module smd_parts:KLDX-SMT (layer F.Cu) (tedit 5665B8A2)
    (at 90.17 45.72 180)
    (fp_text reference CON7 (at 0 0.5 180) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -0.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 -8.1 180) (size 3.4 3) (drill 1 (offset 0 0.8)) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(CON7-Pad1)"))
    (pad 2 thru_hole rect (at -4.9 -2.43 180) (size 2.6 3) (drill 1 (offset -0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 4.9 -2.43 180) (size 2.6 3) (drill 1 (offset 0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 18 /In7))
    (pad 4 thru_hole circle (at 0 3.8 180) (size 2 2) (drill 1.75) (layers *.Cu *.Mask F.SilkS))
  )
  (module smd_parts:KLDX-SMT (layer F.Cu) (tedit 5665B8A2)
    (at 73.66 45.72 180)
    (fp_text reference CON8 (at 0 0.5 180) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -0.5 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 -8.1 180) (size 3.4 3) (drill 1 (offset 0 0.8)) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(CON8-Pad1)"))
    (pad 2 thru_hole rect (at -4.9 -2.43 180) (size 2.6 3) (drill 1 (offset -0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole rect (at 4.9 -2.43 180) (size 2.6 3) (drill 1 (offset 0.5 -0.7)) (layers *.Cu *.Mask F.SilkS)
      (net 20 /In8))
    (pad 4 thru_hole circle (at 0 3.8 180) (size 2 2) (drill 1.75) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_line (start 63.5 40.64) (end 63.5 147.32) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.35 40.64) (end 63.5 40.64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 133.35 147.32) (end 133.35 40.64) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 63.5 147.32) (end 133.35 147.32) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.08 43.18) (xy 132.08 146.05) (xy 64.77 146.05) (xy 64.77 41.91) (xy 132.08 41.91)
      )
    )
  )
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.65 102.87) (xy 120.65 111.76) (xy 116.84 115.57) (xy 109.22 115.57) (xy 109.22 102.87)
        (xy 120.65 102.87)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 132.08 41.91) (xy 132.08 146.05) (xy 64.77 146.05) (xy 64.77 41.91) (xy 132.08 41.91)
      )
    )
    (polygon
      (pts        (xy 107.95 116.84) (xy 116.84 116.84) (xy 121.92 111.76) (xy 121.92 101.6) (xy 107.95 101.6)
        (xy 107.95 116.84)
      )
    )
  )
)
