(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 37)
    (tracks 312)
    (zones 0)
    (modules 79)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.127)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.3048)
    (user_via 0.6858 0.3302)
    (user_via 0.8128 0.4064)
    (user_via 1.2192 0.6096)
    (user_via 1.4224 0.8128)
    (blind_buried_vias_allowed yes)
    (uvia_size 0.3)
    (uvia_drill 0.1016)
    (uvias_allowed yes)
    (uvia_min_size 0.2032)
    (uvia_min_drill 0.1016)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1)
    (pad_drill 0.65)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7EFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /Qinj1)
  (net 3 /Vpls1)
  (net 4 /Qinj2)
  (net 5 /Vpls2)
  (net 6 /Qinj3)
  (net 7 /Vpls3)
  (net 8 /Qinj4)
  (net 9 /Vpls4)
  (net 10 /Qinj5)
  (net 11 /Vpls5)
  (net 12 /Qinj6)
  (net 13 /Vpls6)
  (net 14 /Qinj7)
  (net 15 /Vpls7)
  (net 16 /Qinj8)
  (net 17 /Vpls8)
  (net 18 /VdivA)
  (net 19 /VdivB)
  (net 20 /VinA)
  (net 21 /VinB)
  (net 22 /HV1)
  (net 23 /HV2)
  (net 24 /HV3)
  (net 25 /HV4)
  (net 26 /HV5)
  (net 27 /HV6)
  (net 28 /HV7)
  (net 29 /HV8)
  (net 30 /V1)
  (net 31 /V2)
  (net 32 /V3)
  (net 33 /V4)
  (net 34 /V5)
  (net 35 /V6)
  (net 36 /V7)
  (net 37 /V8)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1016)
    (add_net /HV1)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /Qinj1)
    (add_net /Qinj2)
    (add_net /Qinj3)
    (add_net /Qinj4)
    (add_net /Qinj5)
    (add_net /Qinj6)
    (add_net /Qinj7)
    (add_net /Qinj8)
    (add_net /V1)
    (add_net /V2)
    (add_net /V3)
    (add_net /V4)
    (add_net /V5)
    (add_net /V6)
    (add_net /V7)
    (add_net /V8)
    (add_net /VdivA)
    (add_net /VdivB)
    (add_net /VinA)
    (add_net /VinB)
    (add_net /Vpls1)
    (add_net /Vpls2)
    (add_net /Vpls3)
    (add_net /Vpls4)
    (add_net /Vpls5)
    (add_net /Vpls6)
    (add_net /Vpls7)
    (add_net /Vpls8)
    (add_net GND)
  )
  (module MSAG_Misc:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5C52EDE1)
    (at 10.78992 10.3886 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_02x03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /V3))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /VdivA))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /V3))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /VdivB))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /V3))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at -3.048 25.4)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JHV7 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /HV7))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:MountingHole_4.3mm_M4_ISO14580_Pad (layer F.Cu) (tedit 611D2A38)
    (at -34.29 -15.875)
    (descr "Mounting Hole 4.3mm, M4, ISO14580")
    (tags "mounting hole 4.3mm m4 iso14580")
    (attr virtual)
    (fp_text reference MH4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 1) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MSAG_Misc:MountingHole_4.3mm_M4_ISO14580_Pad (layer F.Cu) (tedit 611D2A38)
    (at -34.925 53.34)
    (descr "Mounting Hole 4.3mm, M4, ISO14580")
    (tags "mounting hole 4.3mm m4 iso14580")
    (attr virtual)
    (fp_text reference MH3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 1) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MSAG_Misc:MountingHole_4.3mm_M4_ISO14580_Pad (layer F.Cu) (tedit 611D2A38)
    (at 24.765 -15.24)
    (descr "Mounting Hole 4.3mm, M4, ISO14580")
    (tags "mounting hole 4.3mm m4 iso14580")
    (attr virtual)
    (fp_text reference MH2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 1) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MSAG_Misc:MountingHole_4.3mm_M4_ISO14580_Pad (layer F.Cu) (tedit 611D2A38)
    (at 24.765 53.34)
    (descr "Mounting Hole 4.3mm, M4, ISO14580")
    (tags "mounting hole 4.3mm m4 iso14580")
    (attr virtual)
    (fp_text reference MH1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 1) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 4.3) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module MSAG_Misc:goddard_rocket_0.4inA (layer F.Cu) (tedit 0)
    (at -5.3086 40.9448)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MSAG_Misc:msag_logo2_0.6in (layer F.Cu) (tedit 0)
    (at 2.794 33.0708)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MSAG_Misc:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5C52EDE1)
    (at 10.78992 2.4638 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J1 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_02x03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /V1))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /VdivA))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /V1))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /VdivB))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 /V1))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -28.956 38.147 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R32 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 10 (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 /Vpls8))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -34.925 38.1 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R31 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 49.9 (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 /V8))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 20.447 36.068)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R30 (at -0.127 -1.651) (layer B.SilkS))
    (fp_text value 10 (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 /Vpls7))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 24.638 37.846 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R29 (at 3.302 0 180) (layer B.SilkS))
    (fp_text value 49.9 (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 36 /V7))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -30.734 20.955 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R28 (at 0 1.7) (layer B.SilkS))
    (fp_text value 10 (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 /Vpls6))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -34.798 23.114 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R27 (at 3.302 -0.254) (layer B.SilkS))
    (fp_text value 49.9 (at 0 -0.35 270) (layer B.Fab))
    (fp_text user %R (at 0 0.2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 35 /V6))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -30.353 42.037)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R24 (at 0 1.7) (layer B.SilkS))
    (fp_text value 2.7k (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 /V8))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 /Vpls8))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 20.4 42.037 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R23 (at 1.35 -2.54 90) (layer B.SilkS))
    (fp_text value 2.7k (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 36 /V7))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 /Vpls7))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -30.607 27.178)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R22 (at 1.524 2.54 90) (layer B.SilkS))
    (fp_text value 2.7k (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 35 /V6))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 /Vpls6))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 20.701 20.955)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 0 -1.651) (layer B.SilkS))
    (fp_text value 10 (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 /Vpls5))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 24.765 23.241 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R20 (at 3.048 0) (layer B.SilkS))
    (fp_text value 49.9 (at 0 -0.35 270) (layer B.Fab))
    (fp_text user %R (at 0 0.2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /V5))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -28.956 7.493 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 3.175 -0.508 180) (layer B.SilkS))
    (fp_text value 10 (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 /Vpls4))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -34.798 7.493 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 3.048 -0.254 180) (layer B.SilkS))
    (fp_text value 49.9 (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 33 /V4))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 20.527 5.334)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at -0.08 -1.651) (layer B.SilkS))
    (fp_text value 10 (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 /Vpls3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 24.765 7.493 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 3.175 0 180) (layer B.SilkS))
    (fp_text value 49.9 (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 32 /V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -26.67 -5.334 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 3.175 0 180) (layer B.SilkS))
    (fp_text value 10 (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /Vpls2))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -34.671 -7.747 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 1.651 2.413 180) (layer B.SilkS))
    (fp_text value 49.9 (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 31 /V2))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 18.923 -7.493 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at -0.127 -1.778 90) (layer B.SilkS))
    (fp_text value 10 (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /Vpls1))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 24.892 -7.874 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 1.524 2.54) (layer B.SilkS))
    (fp_text value 49.9 (at 0 -0.35 270) (layer B.Fab))
    (fp_text user %R (at 0 0.2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 /V1))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 20.748 27.178 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 1.444 -2.667 90) (layer B.SilkS))
    (fp_text value 2.7k (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 34 /V5))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 /Vpls5))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -30.654 11.557)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 1.317 2.667 90) (layer B.SilkS))
    (fp_text value 2.7k (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 33 /V4))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 /Vpls4))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 20.574 11.557 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 1.397 -2.159 270) (layer B.SilkS))
    (fp_text value 2.7k (at 0 -0.35 180) (layer B.Fab))
    (fp_text user %R (at 0 0.2 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 32 /V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 /Vpls3))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -30.48 -3.937)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 1.778 2.667 90) (layer B.SilkS))
    (fp_text value 2.7k (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 31 /V2))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /Vpls2))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at 20.32 -3.937 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 1.27 -2.032 90) (layer B.SilkS))
    (fp_text value 2.7k (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 /V1))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /Vpls1))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at 24.765 11.5316)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JC3 (at -5.7404 -5.3594) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.55) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 32 /V3))
    (pad 2 thru_hole circle (at 3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/parts/BNC-Connector-Straight.step
      (offset (xyz 0 0 17.78))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at 24.638 42.0624)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JC7 (at -5.7404 -5.3594) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.55) (layer F.Fab))
    (pad 5 thru_hole circle (at 3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 36 /V7))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at 24.765 27.1526)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JC5 (at -5.7404 -5.3594) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.55) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 /V5))
    (pad 2 thru_hole circle (at 3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at 24.892 -3.9624)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JC1 (at -5.7404 -5.3594) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.55) (layer F.Fab))
    (pad 5 thru_hole circle (at 3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 30 /V1))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/parts/BNC-Connector-Straight.step
      (offset (xyz 0 0 17.78))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at -34.8996 42.0624 270)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JC8 (at -5.7404 4.8514 180) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.55 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 37 /V8))
    (pad 2 thru_hole circle (at 3.23 -3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3.23 -3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -3.23 3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 3.23 3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at -34.7726 27.1526 270)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JC6 (at -5.5626 4.9784 180) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.55 90) (layer F.Fab))
    (pad 5 thru_hole circle (at 3.23 3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -3.23 3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3.23 -3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.23 -3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 /V6))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at -34.7726 11.5316 270)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JC4 (at -5.5626 5.1054 180) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.55 90) (layer F.Fab))
    (pad 5 thru_hole circle (at 3.23 3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -3.23 3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3.23 -3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.23 -3.23 270) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 /V4))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at -34.6456 -3.9624)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JC2 (at -4.9784 -5.6896) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85) (layer F.Fab))
    (fp_text user %R (at 0 -1.55) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 /V2))
    (pad 2 thru_hole circle (at 3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3.23 -3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at 3.23 3.23) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:nasa_logo_0.4inA (layer F.Cu) (tedit 0)
    (at 12.065 -13.97)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at -7.62 25.4)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JHV8 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /HV8))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at -7.62 17.78)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JHV6 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /HV6))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at -3.048 17.78)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JHV5 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /HV5))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at -7.874 10.16)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JHV4 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /HV4))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at -3.302 10.16)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JHV3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /HV3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at -7.874 2.54)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JHV2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /HV2))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5C52ECC1)
    (at -3.302 2.54)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JHV1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /HV1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -1.0414 35.17392)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 1.7) (layer B.SilkS))
    (fp_text value 10 (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /VdivB))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -2.40284 38.51148 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 2.7k (at 0 -0.35 270) (layer B.Fab))
    (fp_text user %R (at 0 0.2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 /VinB))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /VdivB))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -2.40284 43.31208 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 49.9 (at 0 -0.35 270) (layer B.Fab))
    (fp_text user %R (at 0 0.2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 /VinB))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -7.81304 35.179 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.7) (layer B.SilkS))
    (fp_text value 10 (at 0 -0.35) (layer B.Fab))
    (fp_text user %R (at 0 0.2) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 /VdivA))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -6.4516 38.56228 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 2.7k (at 0 -0.35 270) (layer B.Fab))
    (fp_text user %R (at 0 0.2 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 /VinA))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 /VdivA))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:R_0805_HandSoldering (layer B.Cu) (tedit 5C5B175C)
    (at -6.44144 43.4086 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 49.9 (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 /VinA))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at 6.7564 41.9608 90)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JB1 (at 5.4864 5.1308 180) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.55 90) (layer F.Fab))
    (pad 5 thru_hole circle (at 3.23 3.23 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -3.23 3.23 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3.23 -3.23 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.23 -3.23 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 21 /VinB))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:BNC_TE-5-1634503-1 (layer F.Cu) (tedit 5C5B374F)
    (at -16.1036 42.0624 90)
    (descr "25-pin D-Sub connector, straight/vertical, THT-mount, female, pitch 2.77x2.84mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector straight vertical THT female pitch 2.77x2.84mm mounting holes distance 47.1mm")
    (fp_text reference JA1 (at 5.08 -6.6294 180) (layer F.SilkS))
    (fp_text value BNC (at 0 0.85 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.55 90) (layer F.Fab))
    (pad 5 thru_hole circle (at 3.23 3.23 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -3.23 3.23 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at -3.23 -3.23 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 3.23 -3.23 90) (size 2.2 2.2) (drill 1.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask)
      (net 20 /VinA))
    (model ${MSAG}/MSAG_KiCad3d/TE-5-1634503-1.stp
      (offset (xyz 0 0 13.33499979972839))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5C52EDE1)
    (at -21.8694 32.7406 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J8 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_02x03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /V8))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /VdivA))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /V8))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /VdivB))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 /V8))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5C52EDE1)
    (at 10.78992 26.2636 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J7 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_02x03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /V7))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /VdivA))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /V7))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /VdivB))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /V7))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5C52EDE1)
    (at -21.8694 24.8158 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J6 (at 1.27 -2.33) (layer F.SilkS))
    (fp_text value Conn_02x03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /V6))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /VdivA))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /V6))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /VdivB))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /V6))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5C52EDE1)
    (at 10.78992 18.3388 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J5 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_02x03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /V5))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /VdivA))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /V5))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /VdivB))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /V5))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5C52EDE1)
    (at -21.8694 16.891 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J4 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_02x03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /V4))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /VdivA))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /V4))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /VdivB))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /V4))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5C52EDE1)
    (at -21.8694 8.9408 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J2 (at 1.27 -2.33 180) (layer F.SilkS))
    (fp_text value Conn_02x03 (at 1.27 7.41 90) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /V2))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /VdivA))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /V2))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /VdivB))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /V2))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${MSAG3D}/Connector_PinHeader_2.54mm.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805_HandSoldering (layer B.Cu) (tedit 5C5B15B8)
    (at -14.61008 31.46044 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0.01524 -1.93548 90) (layer B.SilkS))
    (fp_text value 130pF (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0.15 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 /Qinj8))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 17 /Vpls8))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805_HandSoldering (layer B.Cu) (tedit 5C5B15B8)
    (at 3.52552 27.50312 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 130pF (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0.15 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /Qinj7))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 15 /Vpls7))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805_HandSoldering (layer B.Cu) (tedit 5C5B15B8)
    (at -14.61516 23.55088 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -0.02032 -1.73228 90) (layer B.SilkS))
    (fp_text value 130pF (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0.15 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 12 /Qinj6))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 13 /Vpls6))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805_HandSoldering (layer B.Cu) (tedit 5C5B15B8)
    (at 3.5306 19.6088 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 130pF (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0.15 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 /Qinj5))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 11 /Vpls5))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805_HandSoldering (layer B.Cu) (tedit 5C5B15B8)
    (at -14.61516 15.60576 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0.00508 -1.74244 90) (layer B.SilkS))
    (fp_text value 130pF (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0.15 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 /Qinj4))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /Vpls4))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805_HandSoldering (layer B.Cu) (tedit 5C5B15B8)
    (at 3.5306 11.64336 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 130pF (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0.15 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 /Qinj3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 /Vpls3))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805_HandSoldering (layer B.Cu) (tedit 5C5B15B8)
    (at -14.59992 7.67588 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -0.02032 -1.77292 90) (layer B.SilkS))
    (fp_text value 130pF (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0.15 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 /Qinj2))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 /Vpls2))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:C_0805_HandSoldering (layer B.Cu) (tedit 5C5B15B8)
    (at 3.5306 3.7084 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0.0127 1.8923 270) (layer B.SilkS))
    (fp_text value 130pF (at 0 -0.35 90) (layer B.Fab))
    (fp_text user %R (at 0.15 0.2 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 /Qinj1))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /Vpls1))
    (model ${MSAG3D}/Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:PinHeader_1x10_P1.27mm_Vertical_0.65mm_pin (layer B.Cu) (tedit 59FED6E3)
    (at -11.0744 19.8374 90)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference JSSD6 (at 1.89484 -0.21 180) (layer B.SilkS))
    (fp_text value Conn_01x10_MALE (at 0 -13.125 90) (layer B.Fab))
    (fp_text user %R (at 0 -5.715 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -11.43 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 -8.89 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -6.35 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 -3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 12 /Qinj6))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 27 /HV6))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:PinHeader_1x10_P1.27mm_Vertical_0.65mm_pin (layer B.Cu) (tedit 59FED6E3)
    (at -11.0744 3.9624 90)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference JSSD2 (at 1.89484 0.2794 180) (layer B.SilkS))
    (fp_text value Conn_01x10_MALE (at 0 -13.125 90) (layer B.Fab))
    (fp_text user %R (at 0 -5.715 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -11.43 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 -8.89 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -6.35 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 -3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 /Qinj2))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 23 /HV2))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/HERMES_MERiT_FEE_Qinjflex_rev0.step
      (offset (xyz -1.397 -5.6388 108.0262))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 -90 0))
    )
  )
  (module MSAG_Misc:PinHeader_1x10_P1.27mm_Vertical_0.65mm_pin (layer B.Cu) (tedit 59FED6E3)
    (at -11.0744 11.9126 90)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference JSSD4 (at 1.89484 0.508 180) (layer B.SilkS))
    (fp_text value Conn_01x10_MALE (at 0 -13.125 90) (layer B.Fab))
    (fp_text user %R (at 0 -5.715 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -11.43 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 -8.89 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -6.35 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 -3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 /Qinj4))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 25 /HV4))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:PinHeader_1x10_P1.27mm_Vertical_0.65mm_pin (layer B.Cu) (tedit 59FED6E3)
    (at -11.0744 27.7876 90)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference JSSD8 (at 1.89484 -0.21 180) (layer B.SilkS))
    (fp_text value Conn_01x10_MALE (at 0 -13.125 90) (layer B.Fab))
    (fp_text user %R (at 0 -5.715 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -11.43 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 -8.89 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -6.35 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 -3.81 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 16 /Qinj8))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 29 /HV8))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:PinHeader_1x10_P1.27mm_Vertical_0.65mm_pin (layer B.Cu) (tedit 59FED6E3)
    (at 0 23.8252 270)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference JSSD7 (at -1.8288 -0.18968 180) (layer B.SilkS))
    (fp_text value Conn_01x10_MALE (at 0 -13.125 90) (layer B.Fab))
    (fp_text user %R (at 0 -5.715 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -11.43 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 28 /HV7))
    (pad 8 thru_hole oval (at 0 -8.89 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -6.35 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 -3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 14 /Qinj7))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:PinHeader_1x10_P1.27mm_Vertical_0.65mm_pin (layer B.Cu) (tedit 59FED6E3)
    (at 0 15.875 270)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference JSSD5 (at -1.8288 -0.18968 180) (layer B.SilkS))
    (fp_text value Conn_01x10_MALE (at 0 -13.125 90) (layer B.Fab))
    (fp_text user %R (at 0 -5.715 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -11.43 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 26 /HV5))
    (pad 8 thru_hole oval (at 0 -8.89 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -6.35 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 -3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 10 /Qinj5))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:PinHeader_1x10_P1.27mm_Vertical_0.65mm_pin (layer B.Cu) (tedit 59FED6E3)
    (at 0 7.9502 270)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference JSSD3 (at -1.9558 -0.25908 180) (layer B.SilkS))
    (fp_text value Conn_01x10_MALE (at 0 -13.125 90) (layer B.Fab))
    (fp_text user %R (at 0 -5.715 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -11.43 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 24 /HV3))
    (pad 8 thru_hole oval (at 0 -8.89 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -6.35 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 -3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 /Qinj3))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MSAG_Misc:PinHeader_1x10_P1.27mm_Vertical_0.65mm_pin (layer B.Cu) (tedit 59FED6E3)
    (at 0 0 270)
    (descr "Through hole straight pin header, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference JSSD1 (at -1.87452 -0.03048 180) (layer B.SilkS))
    (fp_text value Conn_01x10_MALE (at 0 -13.125 90) (layer B.Fab))
    (fp_text user %R (at 0 -5.715 180) (layer B.Fab))
    (pad 10 thru_hole oval (at 0 -11.43 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 22 /HV1))
    (pad 8 thru_hole oval (at 0 -8.89 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 0 -6.35 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 -3.81 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /Qinj1))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -1.27 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x10_P1.27mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "SSD2\nFEE2-3" (at -12.5476 6.6294) (layer F.SilkS))
  (gr_text "SSD4\nFEE2-4" (at -12.5476 14.8844) (layer F.SilkS))
  (gr_text "SSD8\nFEE2-2" (at -12.5476 30.7594) (layer F.SilkS))
  (gr_text "SSD6\nFEE2-1" (at -12.5476 22.5044) (layer F.SilkS))
  (gr_text "SSD7\nFEE1-2" (at 1.27 26.67) (layer F.SilkS))
  (gr_text "SSD5\nFEE1-1" (at 1.27 18.415) (layer F.SilkS))
  (gr_text "SSD3\nFEE1-4" (at 1.27 10.795) (layer F.SilkS))
  (gr_text "SSD1\nFEE1-3" (at 1.27 2.54) (layer F.SilkS))
  (gr_text B (at 12.827 47.244) (layer F.SilkS))
  (gr_text A (at -23.368 47.117) (layer F.SilkS))
  (gr_text 02/2022 (at -6.985 -7.62) (layer F.SilkS))
  (gr_text "HERMES MERiT \nDIB Qinj\nRev1" (at -10.795 -14.605) (layer F.SilkS))
  (gr_text 2 (at 12.954 17.653 90) (layer F.SilkS))
  (gr_text 1 (at 13.0048 29.1338 90) (layer F.SilkS))
  (gr_text 2 (at 12.954 9.779 90) (layer F.SilkS))
  (gr_text 2 (at 12.954 25.527 90) (layer F.SilkS))
  (gr_text 1 (at 13.0048 13.335 90) (layer F.SilkS))
  (gr_text 2 (at 12.954 1.778 90) (layer F.SilkS))
  (gr_text 1 (at 12.9794 21.2598 90) (layer F.SilkS))
  (gr_text 1 (at 12.9032 5.334 90) (layer F.SilkS))
  (gr_text 2 (at -24.0538 29.9212 90) (layer F.SilkS))
  (gr_text 1 (at -24.003 33.528 90) (layer F.SilkS))
  (gr_text 2 (at -24.0792 21.9202 90) (layer F.SilkS))
  (gr_text 1 (at -24.003 25.654 90) (layer F.SilkS))
  (gr_text 2 (at -24.0792 13.9192 90) (layer F.SilkS))
  (gr_text 1 (at -24.003 17.78 90) (layer F.SilkS))
  (gr_text 2 (at -24.0792 5.842 90) (layer F.SilkS))
  (gr_text 1 (at -24.003 9.779 90) (layer F.SilkS))
  (gr_line (start -41.91 -20.32) (end 31.75 -20.32) (layer Edge.Cuts) (width 0.12))
  (gr_line (start -41.91 58.42) (end 31.75 58.42) (layer Edge.Cuts) (width 0.12))
  (gr_line (start -41.91 -20.32) (end -41.91 58.42) (layer Edge.Cuts) (width 0.12))
  (gr_line (start 31.75 58.42) (end 31.75 -20.32) (layer Edge.Cuts) (width 0.12))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31.496 58.42) (xy -41.91 58.42) (xy -41.91 -20.32) (xy 31.75 -20.32)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31.75 58.42) (xy -41.91 58.42) (xy -41.91 -20.32) (xy 31.75 -20.32)
      )
    )
  )
)
