(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 87)
    (no_connects 0)
    (area 127.8922 25.070999 189.665858 46.366501)
    (thickness 1.6)
    (drawings 20)
    (tracks 362)
    (zones 0)
    (modules 39)
    (nets 37)
  )
  (page A4)
  (title_block
    (title iMatrix)
    (date 2016-09-22)
    (rev 0.02)
    (company "1rel interactive")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.2)
    (zone_clearance 0.7)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory OUT/PCB/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(D3-Pad1)")
  (net 6 "Net-(D4-Pad1)")
  (net 7 "Net-(D5-Pad1)")
  (net 8 "Net-(D6-Pad1)")
  (net 9 "Net-(D7-Pad1)")
  (net 10 "Net-(D8-Pad1)")
  (net 11 BM_INT)
  (net 12 BM_SCL)
  (net 13 BM_SDA)
  (net 14 LM_SER)
  (net 15 LM_SRCLK)
  (net 16 LM_RCLK)
  (net 17 BM_ADDR0)
  (net 18 BM_ADDR1)
  (net 19 BM_ADDR2)
  (net 20 LM_L00)
  (net 21 LM_L10)
  (net 22 LM_L20)
  (net 23 LM_L30)
  (net 24 LM_L11)
  (net 25 BM_B00)
  (net 26 BM_B01)
  (net 27 BM_B10)
  (net 28 BM_B11)
  (net 29 BM_B20)
  (net 30 BM_B21)
  (net 31 BM_B30)
  (net 32 BM_B31)
  (net 33 LM_L01)
  (net 34 LM_L21)
  (net 35 LM_L31)
  (net 36 LM_OUT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net BM_ADDR0)
    (add_net BM_ADDR1)
    (add_net BM_ADDR2)
    (add_net BM_B00)
    (add_net BM_B01)
    (add_net BM_B10)
    (add_net BM_B11)
    (add_net BM_B20)
    (add_net BM_B21)
    (add_net BM_B30)
    (add_net BM_B31)
    (add_net BM_INT)
    (add_net BM_SCL)
    (add_net BM_SDA)
    (add_net GND)
    (add_net LM_L00)
    (add_net LM_L01)
    (add_net LM_L10)
    (add_net LM_L11)
    (add_net LM_L20)
    (add_net LM_L21)
    (add_net LM_L30)
    (add_net LM_L31)
    (add_net LM_OUT)
    (add_net LM_RCLK)
    (add_net LM_SER)
    (add_net LM_SRCLK)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net VCC)
  )
  (module w_switch:smd_push2 (layer F.Cu) (tedit 57C310C7)
    (at 158.877 32.512 180)
    (descr "SMD Pushbutton 2")
    (autoplace_cost180 10)
    (fp_text reference SW1 (at -2.286 -3.048 180) (layer F.SilkS))
    (fp_text value DPST_mod0 (at 0 3.59918 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 25 BM_B00))
    (pad 2 smd rect (at 2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 25 BM_B00))
    (model walter/switch/smd_push2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_2 (layer F.Cu) (tedit 57E44EFF)
    (at 133.731 44.577)
    (descr "Pin strip 2pin")
    (tags "CONN DEV")
    (fp_text reference P2 (at 0.254 -2.032) (layer F.SilkS) hide)
    (fp_text value CONN_2 (at 0.254 -3.556) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 12 BM_SCL))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 BM_SDA))
    (model walter/pin_strip/pin_strip_2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0805 (layer F.Cu) (tedit 57E45167)
    (at 134.9756 38.354 90)
    (descr "SMT capacitor, 0805")
    (fp_text reference C1 (at -0.7112 1.4732 270) (layer F.SilkS))
    (fp_text value 1u (at 0 0.9906 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.9525 0 90) (size 1.30048 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model walter/smd_cap/c_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 57C31095)
    (at 143.4465 36.703)
    (descr "SMT capacitor, 0402")
    (fp_text reference C2 (at 0.127 1.016) (layer F.SilkS))
    (fp_text value 100n (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_0402 (layer F.Cu) (tedit 57E4556D)
    (at 140.97 42.291 270)
    (descr "SMT capacitor, 0402")
    (fp_text reference C3 (at 0.762 0.889 270) (layer F.SilkS))
    (fp_text value 100n (at 0 0.4826 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.54864 0 270) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model walter/smd_cap/c_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_0402 (layer F.Cu) (tedit 57E45353)
    (at 158.877 28.829)
    (descr "SMD LED, 0402")
    (fp_text reference D1 (at 0 -0.89916) (layer F.SilkS))
    (fp_text value LED (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_leds/led_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_0402 (layer F.Cu) (tedit 57E45356)
    (at 167.386 28.829)
    (descr "SMD LED, 0402")
    (fp_text reference D2 (at 0 -0.89916) (layer F.SilkS))
    (fp_text value LED (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_leds/led_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_0402 (layer F.Cu) (tedit 57E4535C)
    (at 175.514 28.829)
    (descr "SMD LED, 0402")
    (fp_text reference D3 (at 0 -0.89916) (layer F.SilkS))
    (fp_text value LED (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_leds/led_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_0402 (layer F.Cu) (tedit 57E45360)
    (at 184.023 28.829)
    (descr "SMD LED, 0402")
    (fp_text reference D4 (at 0 -0.89916) (layer F.SilkS))
    (fp_text value LED (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_leds/led_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_0402 (layer F.Cu) (tedit 57E45376)
    (at 158.877 38.227)
    (descr "SMD LED, 0402")
    (fp_text reference D5 (at 0 -0.89916) (layer F.SilkS))
    (fp_text value LED (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_leds/led_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_0402 (layer F.Cu) (tedit 57E45371)
    (at 167.386 38.227)
    (descr "SMD LED, 0402")
    (fp_text reference D6 (at 0 -0.89916) (layer F.SilkS))
    (fp_text value LED (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D6-Pad1)"))
    (pad 2 smd rect (at 0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_leds/led_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_0402 (layer F.Cu) (tedit 57E4536B)
    (at 175.514 38.227)
    (descr "SMD LED, 0402")
    (fp_text reference D7 (at 0 -0.89916) (layer F.SilkS))
    (fp_text value LED (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D7-Pad1)"))
    (pad 2 smd rect (at 0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_leds/led_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_leds:Led_0402 (layer F.Cu) (tedit 57E45367)
    (at 184.023 38.227)
    (descr "SMD LED, 0402")
    (fp_text reference D8 (at 0 -0.89916) (layer F.SilkS))
    (fp_text value LED (at 0 1.00076) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D8-Pad1)"))
    (pad 2 smd rect (at 0.54864 0) (size 0.5969 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_leds/led_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.Cu) (tedit 57E44EFA)
    (at 132.461 42.037 270)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference P1 (at 0.127 2.032 270) (layer F.SilkS) hide)
    (fp_text value CONN_1 (at 0.254 -3.556 270) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 BM_INT))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_2 (layer F.Cu) (tedit 57C31B08)
    (at 132.461 38.227 90)
    (descr "Pin strip 2pin")
    (tags "CONN DEV")
    (fp_text reference P4 (at 3.302 0.127 180) (layer F.SilkS))
    (fp_text value CONN_2 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57C33745)
    (at 138.303 33.2105)
    (descr "SMT resistor, 0402")
    (fp_text reference R1 (at 0 -0.4826) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 17 BM_ADDR0))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57C3373B)
    (at 138.303 32.1945)
    (descr "SMT resistor, 0402")
    (fp_text reference R2 (at 0 -0.4826) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 17 BM_ADDR0))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57C3374A)
    (at 138.303 35.4965)
    (descr "SMT resistor, 0402")
    (fp_text reference R3 (at 0 -0.4826 90) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 BM_ADDR1))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57C33747)
    (at 138.303 34.3535)
    (descr "SMT resistor, 0402")
    (fp_text reference R4 (at 0 -0.4826) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 18 BM_ADDR1))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57C33752)
    (at 138.303 37.6555)
    (descr "SMT resistor, 0402")
    (fp_text reference R5 (at 0 -0.4826) (layer F.SilkS) hide)
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 BM_ADDR2))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57E45315)
    (at 153.035 29.845 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R7 (at 1.651 -0.127 180) (layer F.SilkS))
    (fp_text value 220R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 20 LM_L00))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57E45310)
    (at 153.035 28.702 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R8 (at 1.651 -0.127 180) (layer F.SilkS))
    (fp_text value 220R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 21 LM_L10))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57E4530E)
    (at 153.035 27.559 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R9 (at 1.651 -0.127 180) (layer F.SilkS))
    (fp_text value 220R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 22 LM_L20))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57E4530B)
    (at 153.035 26.416 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R10 (at 1.905 -0.127 180) (layer F.SilkS))
    (fp_text value 220R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 23 LM_L30))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57E4532A)
    (at 153.035 38.1 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R11 (at 1.905 0 180) (layer F.SilkS))
    (fp_text value 220R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 33 LM_L01))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D5-Pad1)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57E45321)
    (at 153.035 36.957 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R12 (at 1.905 0 180) (layer F.SilkS))
    (fp_text value 220R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 24 LM_L11))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D6-Pad1)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57E4531E)
    (at 153.035 35.814 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R13 (at 1.905 -0.127 180) (layer F.SilkS))
    (fp_text value 220R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 34 LM_L21))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D7-Pad1)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 57E4531D)
    (at 153.035 34.671 180)
    (descr "SMT resistor, 0402")
    (fp_text reference R14 (at 1.905 -0.127 180) (layer F.SilkS))
    (fp_text value 220R (at 0 0.4826 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 35 LM_L31))
    (pad 2 smd rect (at -0.54864 0 180) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D8-Pad1)"))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_switch:smd_push2 (layer F.Cu) (tedit 57C3155D)
    (at 158.877 41.91 180)
    (descr "SMD Pushbutton 2")
    (autoplace_cost180 10)
    (fp_text reference SW2 (at -2.286 -3.048 180) (layer F.SilkS))
    (fp_text value DPST_mod0 (at 0 3.59918 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 26 BM_B01))
    (pad 2 smd rect (at 2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 26 BM_B01))
    (model walter/switch/smd_push2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_switch:smd_push2 (layer F.Cu) (tedit 57C31543)
    (at 167.259 32.512 180)
    (descr "SMD Pushbutton 2")
    (autoplace_cost180 10)
    (fp_text reference SW3 (at -2.54 -3.048 180) (layer F.SilkS))
    (fp_text value DPST_mod0 (at 0 3.59918 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 27 BM_B10))
    (pad 2 smd rect (at 2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 27 BM_B10))
    (model walter/switch/smd_push2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_switch:smd_push2 (layer F.Cu) (tedit 57C31563)
    (at 167.259 41.91 180)
    (descr "SMD Pushbutton 2")
    (autoplace_cost180 10)
    (fp_text reference SW4 (at -2.413 -3.048 180) (layer F.SilkS))
    (fp_text value DPST_mod0 (at 0 3.59918 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 28 BM_B11))
    (pad 2 smd rect (at 2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 28 BM_B11))
    (model walter/switch/smd_push2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_switch:smd_push2 (layer F.Cu) (tedit 57C3154F)
    (at 175.641 32.512 180)
    (descr "SMD Pushbutton 2")
    (autoplace_cost180 10)
    (fp_text reference SW5 (at -2.54 -3.048 180) (layer F.SilkS))
    (fp_text value DPST_mod0 (at 0 3.59918 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 29 BM_B20))
    (pad 2 smd rect (at 2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 29 BM_B20))
    (model walter/switch/smd_push2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_switch:smd_push2 (layer F.Cu) (tedit 57C31569)
    (at 175.641 41.91 180)
    (descr "SMD Pushbutton 2")
    (autoplace_cost180 10)
    (fp_text reference SW6 (at -2.413 -3.048 180) (layer F.SilkS))
    (fp_text value DPST_mod0 (at 0 3.59918 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 30 BM_B21))
    (pad 2 smd rect (at 2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 30 BM_B21))
    (model walter/switch/smd_push2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_switch:smd_push2 (layer F.Cu) (tedit 57C31555)
    (at 184.023 32.512 180)
    (descr "SMD Pushbutton 2")
    (autoplace_cost180 10)
    (fp_text reference SW7 (at -2.413 -3.048 180) (layer F.SilkS))
    (fp_text value DPST_mod0 (at 0 3.59918 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 31 BM_B30))
    (pad 2 smd rect (at 2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 31 BM_B30))
    (model walter/switch/smd_push2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_switch:smd_push2 (layer F.Cu) (tedit 57C31570)
    (at 184.023 41.91 180)
    (descr "SMD Pushbutton 2")
    (autoplace_cost180 10)
    (fp_text reference SW8 (at -2.413 -3.048 180) (layer F.SilkS))
    (fp_text value DPST_mod0 (at 0 3.59918 180) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 32 BM_B31))
    (pad 2 smd rect (at 2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.99974 1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.99974 -1.84912 180) (size 1.00076 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 32 BM_B31))
    (model walter/switch/smd_push2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4 (layer F.Cu) (tedit 57E44EF5)
    (at 132.461 30.607 90)
    (descr "Pin strip 4pin")
    (tags "CONN DEV")
    (fp_text reference P3 (at 0 -2.159 90) (layer F.SilkS) hide)
    (fp_text value CONN_4 (at 0.254 -3.556 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 14 LM_SER))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 16 LM_RCLK))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 15 LM_SRCLK))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 36 LM_OUT))
    (model walter/pin_strip/pin_strip_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_dil:so-16 (layer F.Cu) (tedit 57E451F9)
    (at 145.161 30.988 90)
    (descr SO-16)
    (fp_text reference U2 (at 0.3048 -0.9906 90) (layer F.SilkS))
    (fp_text value 74HC595 (at 0 1.016 90) (layer F.SilkS))
    (pad 1 smd rect (at -4.445 2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 24 LM_L11))
    (pad 2 smd rect (at -3.175 2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 34 LM_L21))
    (pad 3 smd rect (at -1.905 2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 35 LM_L31))
    (pad 4 smd rect (at -0.635 2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 20 LM_L00))
    (pad 5 smd rect (at 0.635 2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 21 LM_L10))
    (pad 6 smd rect (at 1.905 2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 22 LM_L20))
    (pad 7 smd rect (at 3.175 2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 23 LM_L30))
    (pad 8 smd rect (at 4.445 2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at 4.445 -2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 36 LM_OUT))
    (pad 10 smd rect (at 3.175 -2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 11 smd rect (at 1.905 -2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 15 LM_SRCLK))
    (pad 12 smd rect (at 0.635 -2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 16 LM_RCLK))
    (pad 13 smd rect (at -0.635 -2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -1.905 -2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 14 LM_SER))
    (pad 15 smd rect (at -3.175 -2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 33 LM_L01))
    (pad 16 smd rect (at -4.445 -2.794 90) (size 0.59944 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (model walter/smd_dil/so-16.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_dil:tssop-20 (layer F.Cu) (tedit 57E451D4)
    (at 145.415 41.91 270)
    (descr TSSOP-20)
    (fp_text reference U1 (at 0 0.508 270) (layer F.SilkS))
    (fp_text value PCF8574TS_20pin (at 0 -1.143 270) (layer F.SilkS) hide)
    (pad 5 smd rect (at -0.32512 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 6 smd rect (at 0.32512 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 17 BM_ADDR0))
    (pad 7 smd rect (at 0.97536 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 18 BM_ADDR1))
    (pad 8 smd rect (at 1.6256 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at -2.26568 -2.794 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 27 BM_B10))
    (pad 2 smd rect (at -2.27584 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 12 BM_SCL))
    (pad 3 smd rect (at -1.6256 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -0.97536 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 13 BM_SDA))
    (pad 12 smd rect (at 2.27584 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 30 BM_B21))
    (pad 13 smd rect (at 1.6256 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 0.97536 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 32 BM_B31))
    (pad 15 smd rect (at 0.32512 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 16 smd rect (at -0.32512 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 31 BM_B30))
    (pad 17 smd rect (at -0.97536 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 29 BM_B20))
    (pad 9 smd rect (at 2.27584 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 19 BM_ADDR2))
    (pad 18 smd rect (at -1.6256 -2.794 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -2.92608 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 11 BM_INT))
    (pad 10 smd rect (at 2.92608 2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 26 BM_B01))
    (pad 11 smd rect (at 2.92608 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 28 BM_B11))
    (pad 20 smd rect (at -2.92608 -2.79908 270) (size 0.4191 1.47066) (layers F.Cu F.Paste F.Mask)
      (net 25 BM_B00))
    (model walter/smd_dil/tssop-20.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_resistors:r_0402 (layer F.Cu) (tedit 0)
    (at 138.3284 36.6268)
    (descr "SMT resistor, 0402")
    (fp_text reference R6 (at 0 -0.4826) (layer F.SilkS))
    (fp_text value 0R (at 0 0.4826) (layer F.SilkS) hide)
    (pad 1 smd rect (at 0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 19 BM_ADDR2))
    (pad 2 smd rect (at -0.54864 0) (size 0.8001 0.6985) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_resistors/r_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text PCF8574TS (at 145.9992 43.2816 90) (layer F.SilkS))
  (gr_text "I2C\nSCL-SDA" (at 136.652 45.212) (layer F.SilkS))
  (gr_text INT (at 134.366 41.9608 90) (layer F.SilkS))
  (gr_text VCC (at 134.9756 40.5892) (layer F.SilkS))
  (gr_text GND (at 134.874 36.2204) (layer F.SilkS))
  (gr_text SER (at 134.366 34.3408 90) (layer F.SilkS))
  (gr_text RCLK (at 134.366 32.004 90) (layer F.SilkS))
  (gr_text SRCLK (at 134.366 29.3624 90) (layer F.SilkS))
  (gr_text OUT (at 134.366 26.8224 90) (layer F.SilkS))
  (gr_line (start 187.833 25.146) (end 187.833 46.2915) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 25.146) (end 187.833 25.146) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 46.2915) (end 187.833 46.2915) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 46.2915) (end 130.81 25.146) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "iMatrix4x2 rev0.02\n1rel/2016-09" (at 187.452 26.289) (layer F.SilkS))
  (gr_text 1 (at 139.827 37.719) (layer F.SilkS))
  (gr_text 1 (at 139.827 35.687) (layer F.SilkS))
  (gr_text 1 (at 139.827 33.401) (layer F.SilkS))
  (gr_text 0 (at 139.827 36.703) (layer F.SilkS))
  (gr_text 0 (at 139.827 34.544) (layer F.SilkS))
  (gr_text 0 (at 139.827 32.258) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.7))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.833 46.2915) (xy 130.81 46.2915) (xy 130.81 25.146) (xy 187.833 25.146)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.7))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.4) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.833 46.2915) (xy 130.81 46.2915) (xy 130.81 25.146) (xy 187.833 25.146)
      )
    )
  )
)
