(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~65~ubuntu17.10.1)
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 6)
    (zones 0)
    (modules 4)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.508)
    (trace_clearance 0.508)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.508)
    (via_min_size 0.381)
    (via_min_drill 0.508)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 TXD)
  (net 2 EN)
  (net 3 RXD)
  (net 4 IO0)
  (net 5 GND)
  (net 6 "Net-(J2-Pad2)")
  (net 7 "Net-(J2-Pad3)")
  (net 8 "Net-(J2-Pad6)")
  (net 9 "Net-(Mode1-Pad1)")
  (net 10 "Net-(Reset1-Pad2)")
  (net 11 "Net-(Reset1-Pad4)")
  (net 12 "Net-(J1-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.508)
    (trace_width 0.508)
    (via_dia 0.8)
    (via_drill 0.508)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.254)
    (add_net EN)
    (add_net GND)
    (add_net IO0)
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(Mode1-Pad1)")
    (add_net "Net-(Reset1-Pad2)")
    (add_net "Net-(Reset1-Pad4)")
    (add_net RXD)
    (add_net TXD)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical (layer F.Cu) (tedit 5BB9A9DA)
    (at 141.224 78.486)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference J1 (at -1.016 7.366) (layer F.SilkS))
    (fp_text value "OHS18 Badge" (at 1.27 7.41) (layer F.Fab))
    (fp_text user %R (at 1.27 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 TXD))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 RXD))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 EN))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 IO0))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5BB9A6D9)
    (at 133.604 72.136 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J2 (at 2.794 -8.382 90) (layer F.SilkS) hide)
    (fp_text value "FTDI 3.3V USB to Serial" (at 0 15.03 90) (layer F.Fab))
    (fp_text user %R (at 0 6.35 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 TXD))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 RXD))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad6)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Switch_Slide_11.6x4mm_EG1218 (layer F.Cu) (tedit 5BB9A63F)
    (at 150.114 78.486 270)
    (descr http://spec_sheets.e-switch.com/specs/P040040.pdf)
    (fp_text reference Mode1 (at -0.254 -5.08 270) (layer F.SilkS) hide)
    (fp_text value EG1218 (at 2.11 3.14 270) (layer F.Fab))
    (fp_text user %R (at 2.5 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(Mode1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 IO0))
    (pad 3 thru_hole circle (at 5 0 270) (size 1.9 1.9) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module digikey-footprints:Switch_Tactile_THT_B3F-1xxx (layer F.Cu) (tedit 5BB9A6E5)
    (at 131.3794 83.5672 90)
    (descr http://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (fp_text reference Reset (at -2.5388 0.4466 180) (layer F.SilkS))
    (fp_text value B3F-1000 (at 3.2512 7.1006 90) (layer F.Fab))
    (fp_text user %R (at 3.2512 2.2606 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0.0012 0.0106 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 6.5012 0.0106 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(Reset1-Pad2)"))
    (pad 3 thru_hole circle (at 0.0012 4.5106 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 EN))
    (pad 4 thru_hole circle (at 6.5012 4.5106 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(Reset1-Pad4)"))
  )
  (gr_text "#ohsummit18" (at 138.938 86.36) (layer B.SilkS))
  (gr_text drew@oshpark.com (at 141.224 74.422) (layer B.SilkS))
  (gr_arc (start 130.810001 71.119999) (end 131.064 69.088) (angle -97.12501635) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.13 69.088) (end 130.81 69.088) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 146.812 83.566) (layer F.SilkS))
  (gr_text IO0 (at 146.558 81.026) (layer F.SilkS))
  (gr_text EN (at 138.684 81.026) (layer F.SilkS))
  (gr_text RXD (at 138.684 78.74) (layer F.SilkS))
  (gr_text TXD (at 146.558 78.74) (layer F.SilkS))
  (gr_text Prog (at 146.05 86.614) (layer F.SilkS))
  (gr_text "FTDI cable" (at 141.478 70.104) (layer F.SilkS))
  (gr_text "github.com/oshwabadge2018/\n    adapter-board" (at 141.224 75.184) (layer F.SilkS))
  (gr_line (start 128.778 70.866) (end 128.778 85.852) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 130.809999 85.836188) (end 128.778 85.582189) (angle -97.12501635) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.876 87.884) (end 130.556 87.884) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 151.114188 85.852001) (end 150.860189 87.884) (angle -97.12501635) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.162 71.374) (end 153.162 86.106) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 151.130001 71.135812) (end 153.162 71.389811) (angle -97.12501635) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 152.4 73.66) (xy 152.654 87.376) (xy 129.286 87.376) (xy 129.286 69.85) (xy 152.4 69.85)
      )
    )
  )
)
