(kicad_pcb (version 20171130) (host pcbnew 5.1.6-c6e7f7d~87~ubuntu20.04.1)
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 27)
    (zones 0)
    (modules 3)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.4064)
    (trace_clearance 0.1778)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1778)
    (via_size 0.4064)
    (via_drill 0.254)
    (via_min_size 0.4064)
    (via_min_drill 0.254)
    (user_via 0.4064 0.254)
    (uvia_size 0.4064)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.4064)
    (uvia_min_drill 0.254)
    (edge_width 0.0254)
    (segment_width 0.1778)
    (pcb_text_width 0.2032)
    (pcb_text_size 1.2192 1.2192)
    (mod_edge_width 0.127)
    (mod_text_size 0.7112 0.7112)
    (mod_text_width 0.1016)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 147.32 96.52)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /DTR)
  (net 2 /DCD)
  (net 3 GND)
  (net 4 /CTS)
  (net 5 /RTS)
  (net 6 /RX)
  (net 7 /TX)
  (net 8 /DSR)
  (net_class Default "This is the default net class."
    (clearance 0.1778)
    (trace_width 0.1778)
    (via_dia 0.4064)
    (via_drill 0.254)
    (uvia_dia 0.4064)
    (uvia_drill 0.254)
    (diff_pair_width 0.1778)
    (diff_pair_gap 0.1778)
    (add_net /CTS)
    (add_net /DCD)
    (add_net /DSR)
    (add_net /DTR)
    (add_net /RI)
    (add_net /RTS)
    (add_net /RX)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad6)")
  )
  (module 0_LOCAL:NetTie-2_SMD_10 (layer F.Cu) (tedit 5F3D08F8)
    (at 136.1186 97.5614 225)
    (descr "Net tie, 2 pin, 0.5mm square SMD pads")
    (tags "net tie")
    (attr virtual)
    (fp_text reference NT1 (at 0 -1.2 45) (layer F.SilkS) hide)
    (fp_text value Net-Tie_2 (at 0 1.2 45) (layer F.Fab) hide)
    (pad 2 smd circle (at 0.254 0 225) (size 0.254 0.254) (layers F.Cu)
      (net 8 /DSR))
    (pad 1 smd circle (at -0.254 0 225) (size 0.254 0.254) (layers F.Cu)
      (net 2 /DCD))
  )
  (module 0_LOCAL:DSUB-9_Male_Vertical_P2.77x2.84mm (layer B.Cu) (tedit 5F569F84)
    (at 137.16 96.52 180)
    (descr "9-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 25mm")
    (fp_text reference J2 (at 0 1.524) (layer B.SilkS))
    (fp_text value DE9_Male (at 5.54 -8.73) (layer B.Fab))
    (fp_text user %R (at 5.54 -1.42) (layer B.Fab))
    (pad 9 thru_hole circle (at 9.695 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 8 thru_hole circle (at 6.925 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 4 /CTS))
    (pad 7 thru_hole circle (at 4.155 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 5 /RTS))
    (pad 6 thru_hole circle (at 1.385 -2.84 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 8 /DSR))
    (pad 5 thru_hole circle (at 11.08 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 4 thru_hole circle (at 8.31 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 1 /DTR))
    (pad 3 thru_hole circle (at 5.54 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 7 /TX))
    (pad 2 thru_hole circle (at 2.77 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 6 /RX))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask) (roundrect_rratio 0.1)
      (net 2 /DCD))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/A_DS_9_PP_Z_cut.step
      (offset (xyz 5.54 -1.42 6.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 0_LOCAL:DSUB-9_Male_Vertical_P2.77x2.84mm (layer F.Cu) (tedit 5F569F84)
    (at 142.24 96.52)
    (descr "9-pin D-Sub connector, straight/vertical, THT-mount, male, pitch 2.77x2.84mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "9-pin D-Sub connector straight vertical THT male pitch 2.77x2.84mm mounting holes distance 25mm")
    (fp_text reference J1 (at 0 -1.524) (layer F.SilkS))
    (fp_text value DE9_Male (at 5.54 8.73) (layer F.Fab))
    (fp_text user %R (at 5.54 1.42) (layer F.Fab))
    (pad 9 thru_hole circle (at 9.695 2.84) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 1 /DTR))
    (pad 8 thru_hole circle (at 6.925 2.84) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 2 /DCD))
    (pad 7 thru_hole circle (at 4.155 2.84) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 6 thru_hole circle (at 1.385 2.84) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 11.08 0) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 4 /CTS))
    (pad 4 thru_hole circle (at 8.31 0) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 5 /RTS))
    (pad 3 thru_hole circle (at 5.54 0) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 6 /RX))
    (pad 2 thru_hole circle (at 2.77 0) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask)
      (net 7 /TX))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.27 1.27) (drill 0.8382) (layers *.Cu *.Mask) (roundrect_rratio 0.1))
    (model ${KIPRJMOD}/0_LOCAL.3dshapes/A_DS_9_PP_Z_cut.step
      (offset (xyz 5.54 -1.42 6.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 126.492 95.758) (end 126.492 93.98) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 126.492 100.076) (end 124.714 100.076) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 152.908 100.076) (end 152.908 101.854) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 152.908 95.758) (end 154.686 95.758) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_text "TO Z88 ->" (at 131.6736 94.8944) (layer F.SilkS))
  (gr_text "RS-232 ->" (at 147.7264 94.996) (layer B.SilkS))
  (gr_line (start 126.492 93.98) (end 152.908 93.98) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 124.714 100.076) (end 124.714 95.758) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 152.908 101.854) (end 126.492 101.854) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 154.686 95.758) (end 154.686 100.076) (layer Edge.Cuts) (width 0.0254))
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 154.686 101.854) (xy 124.714 101.854) (xy 124.714 93.98) (xy 154.686 93.98)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.0762))
    (polygon
      (pts
        (xy 154.686 101.854) (xy 124.714 101.854) (xy 124.714 93.98) (xy 154.686 93.98)
      )
    )
  )
)
