(kicad_pcb (version 20171130) (host pcbnew "(5.1.4)-1")
  (general
    (thickness 1.6)
    (drawings 9)
    (tracks 14)
    (zones 0)
    (modules 5)
    (nets 13)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 152.4 101.6)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(IR1-Pad1)")
  (net 2 "Net-(IR1-Pad2)")
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J1-Pad2)")
  (net 7 "Net-(J2-Pad1)")
  (net 8 "Net-(J2-Pad2)")
  (net 9 "Net-(J2-Pad3)")
  (net 10 "Net-(J2-Pad5)")
  (net 11 "Net-(J2-Pad6)")
  (net 12 "Net-(J2-Pad7)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(IR1-Pad1)")
    (add_net "Net-(IR1-Pad2)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
  )
  (module Gateron_Optical:DIO_VSMB10940 (layer F.Cu) (tedit 5F2E43FD)
    (at 152.4 101.6)
    (fp_text reference IR1 (at -3.25 -4) (layer F.SilkS))
    (fp_text value VSBM10940 (at -6 0 90) (layer F.SilkS))
    (fp_text user + (at -3.81 3.13) (layer F.SilkS))
    (pad S smd rect (at -4.15 0 270) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.5 1.75 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IR1-Pad2)"))
    (pad 1 smd rect (at -3.5 -1.75 270) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(IR1-Pad1)"))
  )
  (module Gateron_Optical:VEMD10940F (layer F.Cu) (tedit 5F2E43DB)
    (at 152.4 101.6)
    (fp_text reference PD1 (at 3.5 4 180) (layer F.SilkS))
    (fp_text value VEMD10940F (at 6 0 90) (layer F.SilkS))
    (fp_text user + (at 3.81 -3.37) (layer F.SilkS))
    (pad 2 smd rect (at 3.5 -1.75 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-Pad7)"))
    (pad S smd rect (at 4.15 0 180) (size 0.889 0.889) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at 3.5 1.75 180) (size 1.4986 1.4986) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J2-Pad1)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical (layer B.Cu) (tedit 5F2E442C)
    (at 143.51 109.22)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J1 (at 0 0) (layer F.Fab) hide)
    (fp_text value "IR Breakout" (at 0 -17.57) (layer B.Fab))
    (fp_text user %R (at 0 -7.62 -90) (layer B.Fab))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(IR1-Pad1)"))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(IR1-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical (layer B.Cu) (tedit 5F2E4433)
    (at 161.29 109.22)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at -2 0.25) (layer F.Fab) hide)
    (fp_text value "PD Breakout" (at 0 -17.57) (layer B.Fab))
    (fp_text user %R (at 0 -7.62 -90) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 5 thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad7)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Gateron_Optical:Gateron_Optical (layer F.Cu) (tedit 5F2E3F51)
    (at 152.4 101.6)
    (fp_text reference SW1 (at 0 -8) (layer F.SilkS))
    (fp_text value Gateron_KS15_Optical (at 0 -11) (layer F.Fab))
    (fp_arc (start 0 0) (end -1.529999 1.452999) (angle -93) (layer Edge.Cuts) (width 0.1))
    (fp_arc (start 0 0) (end 1.529999 -1.452999) (angle -93) (layer Edge.Cuts) (width 0.1))
    (fp_line (start 1.53 -1.453) (end 1.53 1.453) (layer Edge.Cuts) (width 0.1))
    (fp_line (start -1.53 1.453) (end -1.53 -1.453) (layer Edge.Cuts) (width 0.1))
  )
  (gr_text "Crane's\nKS15 Tester\nAugust 2020" (at 152.4 108.1) (layer F.SilkS))
  (gr_text - (at 158.75 109.47 180) (layer F.SilkS))
  (gr_text - (at 146.05 93.73) (layer F.SilkS))
  (gr_text + (at 158.75 93.73 180) (layer F.SilkS))
  (gr_text + (at 146.05 109.47) (layer F.SilkS))
  (gr_line (start 162.62 110.55) (end 142.18 110.55) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 162.62 92.65) (end 162.62 110.55) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.18 92.65) (end 162.62 92.65) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.18 110.55) (end 142.18 92.65) (layer Edge.Cuts) (width 0.05))
)
