(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 15)
    (no_connects 0)
    (area 152.989999 107.269999 176.003572 128.1905)
    (thickness 1.6)
    (drawings 18)
    (tracks 51)
    (zones 0)
    (modules 7)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.125)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.125)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.3)
    (via_drill 0.254)
    (via_min_size 0.3)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /1)
  (net 2 /2)
  (net 3 /3)
  (net 4 /4)
  (net 5 /5)
  (net 6 /6)
  (net 7 /7)
  (net 8 /8)
  (net 9 "Net-(D1-Pad1)")
  (net 10 "Net-(D2-Pad1)")
  (net_class Default "Esta é a classe de net default."
    (clearance 0.125)
    (trace_width 0.25)
    (via_dia 0.3)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /1)
    (add_net /2)
    (add_net /3)
    (add_net /4)
    (add_net /5)
    (add_net /6)
    (add_net /7)
    (add_net /8)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
  )
  (module Housings_DFN_QFN:DFN-8-1EP_2x2mm_Pitch0.5mm (layer F.Cu) (tedit 5AB94AEC)
    (at 158.75 113.03)
    (descr "DFN8 2x2, 0.5P; CASE 506CN (see ON Semiconductor 506CN.PDF)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 10.414 -4.064) (layer F.SilkS) hide)
    (fp_text value ATTINY10-S (at 12.7 6.35) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -0.75) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /1))
    (pad 2 smd rect (at -0.9 -0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 /2))
    (pad 3 smd rect (at -0.9 0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /3))
    (pad 4 smd rect (at -0.9 0.75) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /4))
    (pad 5 smd rect (at 0.9 0.75) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /5))
    (pad 6 smd rect (at 0.9 0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /6))
    (pad 7 smd rect (at 0.9 -0.25) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /7))
    (pad 8 smd rect (at 0.9 -0.75) (size 0.5 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /8))
    (pad 4 smd rect (at 0 0.44) (size 1.06 0.88) (layers F.Cu F.Paste F.Mask)
      (net 4 /4) (solder_paste_margin_ratio -0.2))
    (pad 9 smd rect (at 0 -0.44) (size 1.06 0.88) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-8-1EP_2x2mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5AB943BD)
    (at 158.75 112.395)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 7.935 6.1595) (layer B.SilkS) hide)
    (fp_text value R (at 8.8875 4.191) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 /4))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer B.Cu) (tedit 5AB94376)
    (at 158.75 114.3)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 5.715 5.715) (layer B.SilkS))
    (fp_text value R (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 11.43 -1.27) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 /4))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5AB93F9E)
    (at 158.75 115.57)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 10.795 0) (layer F.SilkS) hide)
    (fp_text value LED (at 4.445 4.445) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 /5))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5AB93E36)
    (at 158.75 110.49)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 9.055 3.048) (layer F.SilkS) hide)
    (fp_text value LED (at 12.7 6.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 /7))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5AB93421)
    (at 154.94 109.22)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 14.224 15.8115) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 5.334 17.5895) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /1))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /2))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /4))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 -0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5AB9342C)
    (at 162.56 116.84 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at -4.445 -10.3505 180) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 2.3495 -5.5245 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /5))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /6))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /7))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /8))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 -0.05))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (gr_text Attiny10 (at 158.75 108.458) (layer F.SilkS))
  (gr_line (start 153.416 117.094) (end 153.416 108.966) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 162.814 118.364) (end 154.686 118.364) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.084 108.966) (end 164.084 117.094) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.686 107.696) (end 162.8775 107.696) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 162.814 108.966) (end 162.814 107.696) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 154.686 108.966) (end 153.416 108.966) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 154.686 117.094) (end 154.686 118.364) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 162.814 117.094) (end 164.084 117.094) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "Miguel\nReis\n" (at 158.75 117.094) (layer B.SilkS))
  (gr_text 8 (at 161.036 109.22) (layer F.SilkS))
  (gr_text 7 (at 161.036 111.76) (layer F.SilkS))
  (gr_text 6 (at 161.036 114.3) (layer F.SilkS))
  (gr_text 5 (at 161.036 116.84) (layer F.SilkS))
  (gr_text "4\n" (at 156.464 116.84) (layer F.SilkS))
  (gr_text 3 (at 156.464 114.3) (layer F.SilkS))
  (gr_text 2 (at 156.464 111.76) (layer F.SilkS))
  (gr_text 1 (at 156.464 109.22) (layer F.SilkS))
)
