(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6)
    (drawings 40)
    (tracks 332)
    (zones 0)
    (modules 18)
    (nets 63)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.152)
    (user_trace_width 0.152)
    (user_trace_width 0.2)
    (user_trace_width 0.3)
    (user_trace_width 0.6)
    (trace_clearance 0.1)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1)
    (segment_width 0.01)
    (edge_width 0.05)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.2)
    (user_via 0.4 0.2)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.2 1.2)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x110f8_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber__fab"))
  )
  (net 0 "")
  (net 1 /VCLK)
  (net 2 /VSYNC)
  (net 3 /HSYNC)
  (net 4 /D0)
  (net 5 /D1)
  (net 6 /D2)
  (net 7 /D3)
  (net 8 /D4)
  (net 9 /D5)
  (net 10 /D6)
  (net 11 /D7)
  (net 12 /D8)
  (net 13 /D9)
  (net 14 /D10)
  (net 15 /D11)
  (net 16 /ABCK)
  (net 17 /ADAT)
  (net 18 /ALRK)
  (net 19 /+5)
  (net 20 /+3.3)
  (net 21 "Net-(J3-Pad1)")
  (net 22 "Net-(J3-Pad2)")
  (net 23 "Net-(J3-Pad4)")
  (net 24 "Net-(J3-Pad5)")
  (net 25 "Net-(J3-Pad6)")
  (net 26 "Net-(J3-Pad7)")
  (net 27 "Net-(J3-Pad8)")
  (net 28 "Net-(J3-Pad9)")
  (net 29 "Net-(J3-Pad10)")
  (net 30 "Net-(J3-Pad11)")
  (net 31 "Net-(J3-Pad12)")
  (net 32 "Net-(J3-Pad13)")
  (net 33 "Net-(J3-Pad14)")
  (net 34 "Net-(J3-Pad15)")
  (net 35 "Net-(J2-Pad1)")
  (net 36 "Net-(J2-Pad2)")
  (net 37 "Net-(J2-Pad4)")
  (net 38 "Net-(J2-Pad5)")
  (net 39 "Net-(J2-Pad6)")
  (net 40 "Net-(J2-Pad7)")
  (net 41 "Net-(J2-Pad8)")
  (net 42 "Net-(J2-Pad9)")
  (net 43 "Net-(J2-Pad10)")
  (net 44 "Net-(J2-Pad11)")
  (net 45 "Net-(J2-Pad12)")
  (net 46 "Net-(J2-Pad13)")
  (net 47 "Net-(J2-Pad14)")
  (net 48 "Net-(J2-Pad15)")
  (net 49 "Net-(J2-Pad17)")
  (net 50 "Net-(J2-Pad16)")
  (net 51 "Net-(J2-Pad18)")
  (net 52 "Net-(J2-Pad22)")
  (net 53 "Net-(J2-Pad21)")
  (net 54 "Net-(J2-Pad19)")
  (net 55 "Net-(RN1-Pad2)")
  (net 56 "Net-(RN1-Pad7)")
  (net 57 "Net-(RN2-Pad6)")
  (net 58 "Net-(RN2-Pad3)")
  (net 59 "Net-(C1-Pad1)")
  (net 60 GND)
  (net 61 "Net-(J1-Pad28)")
  (net 62 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1)
    (trace_width 0.152)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+3.3)
    (add_net /+5)
    (add_net /ABCK)
    (add_net /ADAT)
    (add_net /ALRK)
    (add_net /D0)
    (add_net /D1)
    (add_net /D10)
    (add_net /D11)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net /HSYNC)
    (add_net /VCLK)
    (add_net /VSYNC)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad28)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad12)")
    (add_net "Net-(J3-Pad13)")
    (add_net "Net-(J3-Pad14)")
    (add_net "Net-(J3-Pad15)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(RN1-Pad2)")
    (add_net "Net-(RN1-Pad7)")
    (add_net "Net-(RN2-Pad3)")
    (add_net "Net-(RN2-Pad6)")
  )
  (module pads:DC_FLEX_BACKING (layer F.Cu) (tedit 0)
    (at 143.8 84.24)
    (attr smd)
    (fp_text reference G*** (at -5.27 3.2) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.13 3.28) (layer B.SilkS) hide)
  )
  (module pads:DC_FLEX_FFC_CON (layer F.Cu) (tedit 5C2F8D21)
    (at 62.18 70.14)
    (attr smd)
    (fp_text reference J1 (at -4.5 -2) (layer F.SilkS))
    (fp_text value Conn_01x32_Male (at 0 -3.5) (layer F.Fab))
    (pad 32 smd rect (at 0 15.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 20 /+3.3))
    (pad 31 smd rect (at 0 15) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 20 /+3.3))
    (pad 30 smd rect (at 0 14.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 20 /+3.3))
    (pad 29 smd rect (at 0 14) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 19 /+5))
    (pad 28 smd rect (at 0 13.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 61 "Net-(J1-Pad28)"))
    (pad 27 smd rect (at 0 13) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 18 /ALRK))
    (pad 26 smd rect (at 0 12.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 60 GND))
    (pad 25 smd rect (at 0 12) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 17 /ADAT))
    (pad 24 smd rect (at 0 11.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 16 /ABCK))
    (pad 23 smd rect (at 0 11) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 60 GND))
    (pad 22 smd rect (at 0 10.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 15 /D11))
    (pad 21 smd rect (at 0 10) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 14 /D10))
    (pad 20 smd rect (at 0 9.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 60 GND))
    (pad 19 smd rect (at 0 9) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 13 /D9))
    (pad 18 smd rect (at 0 8.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 12 /D8))
    (pad 17 smd rect (at 0 8) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 60 GND))
    (pad 16 smd rect (at 0 7.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 11 /D7))
    (pad 15 smd rect (at 0 7) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 10 /D6))
    (pad 14 smd rect (at 0 6.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 60 GND))
    (pad 13 smd rect (at 0 6) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 9 /D5))
    (pad 12 smd rect (at 0 5.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 8 /D4))
    (pad 11 smd rect (at 0 5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 60 GND))
    (pad 10 smd rect (at 0 4.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 7 /D3))
    (pad 9 smd rect (at 0 4) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 6 /D2))
    (pad 8 smd rect (at 0 3.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 60 GND))
    (pad 7 smd rect (at 0 3) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 5 /D1))
    (pad 6 smd rect (at 0 2.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 4 /D0))
    (pad 5 smd rect (at 0 2) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 60 GND))
    (pad 4 smd rect (at 0 1.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 3 /HSYNC))
    (pad 3 smd rect (at 0 1) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 2 /VSYNC))
    (pad 2 smd rect (at 0 0.5) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 60 GND))
    (pad 1 smd rect (at 0 0) (size 3.5 0.3) (layers F.Cu F.Mask)
      (net 1 /VCLK))
  )
  (module pads:DC_FLEX_AUDIO_HOOKUP (layer F.Cu) (tedit 5C2F8848)
    (at 227.92 98.569)
    (fp_text reference J3 (at 3.83 -0.689 90) (layer F.SilkS))
    (fp_text value Conn_01x15_Male (at 2.05 -4.869 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad1)"))
    (pad 1 smd roundrect (at -0.3 0) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 21 "Net-(J3-Pad1)"))
    (pad 1 thru_hole circle (at -0.6 0) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad1)"))
    (pad 1 smd roundrect (at -0.3 0) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 21 "Net-(J3-Pad1)"))
    (pad 2 smd roundrect (at -0.3 -0.65) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 22 "Net-(J3-Pad2)"))
    (pad 3 smd roundrect (at -0.3 -1.3) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 60 GND))
    (pad 4 smd roundrect (at -0.3 -1.95) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 23 "Net-(J3-Pad4)"))
    (pad 5 smd roundrect (at -0.3 -2.6) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 24 "Net-(J3-Pad5)"))
    (pad 6 smd roundrect (at -0.3 -3.25) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 25 "Net-(J3-Pad6)"))
    (pad 7 smd roundrect (at -0.3 -3.9) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 26 "Net-(J3-Pad7)"))
    (pad 8 smd roundrect (at -0.3 -4.55) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 27 "Net-(J3-Pad8)"))
    (pad 9 smd roundrect (at -0.3 -5.2) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 28 "Net-(J3-Pad9)"))
    (pad 10 smd roundrect (at -0.3 -5.85) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 29 "Net-(J3-Pad10)"))
    (pad 11 smd roundrect (at -0.3 -6.5) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 30 "Net-(J3-Pad11)"))
    (pad 12 smd roundrect (at -0.3 -7.15) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 31 "Net-(J3-Pad12)"))
    (pad 13 smd roundrect (at -0.3 -7.8) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 32 "Net-(J3-Pad13)"))
    (pad 14 smd roundrect (at -0.3 -8.45) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 33 "Net-(J3-Pad14)"))
    (pad 15 smd roundrect (at -0.3 -9.1) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 34 "Net-(J3-Pad15)"))
    (pad 2 smd roundrect (at -0.3 -0.65) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 22 "Net-(J3-Pad2)"))
    (pad 3 smd roundrect (at -0.3 -1.3) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 60 GND))
    (pad 4 smd roundrect (at -0.3 -1.95) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 23 "Net-(J3-Pad4)"))
    (pad 5 smd roundrect (at -0.3 -2.6) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 24 "Net-(J3-Pad5)"))
    (pad 6 smd roundrect (at -0.3 -3.25) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 25 "Net-(J3-Pad6)"))
    (pad 7 smd roundrect (at -0.3 -3.9) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 26 "Net-(J3-Pad7)"))
    (pad 8 smd roundrect (at -0.3 -4.55) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 27 "Net-(J3-Pad8)"))
    (pad 9 smd roundrect (at -0.3 -5.2) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 28 "Net-(J3-Pad9)"))
    (pad 10 smd roundrect (at -0.3 -5.85) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 29 "Net-(J3-Pad10)"))
    (pad 11 smd roundrect (at -0.3 -6.5) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 30 "Net-(J3-Pad11)"))
    (pad 12 smd roundrect (at -0.3 -7.15) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 31 "Net-(J3-Pad12)"))
    (pad 13 smd roundrect (at -0.3 -7.8) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 32 "Net-(J3-Pad13)"))
    (pad 14 smd roundrect (at -0.3 -8.45) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 33 "Net-(J3-Pad14)"))
    (pad 15 smd roundrect (at -0.3 -9.1) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 34 "Net-(J3-Pad15)"))
    (pad 2 thru_hole circle (at -0.6 -0.65) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad2)"))
    (pad 3 thru_hole circle (at -0.6 -1.3) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 60 GND))
    (pad 4 thru_hole circle (at -0.6 -1.95) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad4)"))
    (pad 5 thru_hole circle (at -0.6 -2.6) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad5)"))
    (pad 6 thru_hole circle (at -0.6 -3.25) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad6)"))
    (pad 7 thru_hole circle (at -0.6 -3.9) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad7)"))
    (pad 8 thru_hole circle (at -0.6 -4.55) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad8)"))
    (pad 9 thru_hole circle (at -0.6 -5.2) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad9)"))
    (pad 10 thru_hole circle (at -0.6 -5.85) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad10)"))
    (pad 11 thru_hole circle (at -0.6 -6.5) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad11)"))
    (pad 12 thru_hole circle (at -0.6 -7.15) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad12)"))
    (pad 13 thru_hole circle (at -0.6 -7.8) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad13)"))
    (pad 14 thru_hole circle (at -0.6 -8.45) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad14)"))
    (pad 15 thru_hole circle (at -0.6 -9.1) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad15)"))
    (pad 2 thru_hole circle (at 0 -0.65) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 22 "Net-(J3-Pad2)"))
    (pad 3 thru_hole circle (at 0 -1.3) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 60 GND))
    (pad 4 thru_hole circle (at 0 -1.95) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 23 "Net-(J3-Pad4)"))
    (pad 5 thru_hole circle (at 0 -2.6) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 24 "Net-(J3-Pad5)"))
    (pad 6 thru_hole circle (at 0 -3.25) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 25 "Net-(J3-Pad6)"))
    (pad 7 thru_hole circle (at 0 -3.9) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 26 "Net-(J3-Pad7)"))
    (pad 8 thru_hole circle (at 0 -4.55) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 27 "Net-(J3-Pad8)"))
    (pad 9 thru_hole circle (at 0 -5.2) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad9)"))
    (pad 10 thru_hole circle (at 0 -5.85) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 29 "Net-(J3-Pad10)"))
    (pad 11 thru_hole circle (at 0 -6.5) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 30 "Net-(J3-Pad11)"))
    (pad 12 thru_hole circle (at 0 -7.15) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 31 "Net-(J3-Pad12)"))
    (pad 13 thru_hole circle (at 0 -7.8) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 32 "Net-(J3-Pad13)"))
    (pad 14 thru_hole circle (at 0 -8.45) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 33 "Net-(J3-Pad14)"))
    (pad 15 thru_hole circle (at 0 -9.1) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad15)"))
  )
  (module pads:DC_FLEX_VIDEO_HOOKUP (layer F.Cu) (tedit 5C2F8C0C)
    (at 186.776627 89.49)
    (fp_text reference J2 (at 15.373373 -1.65) (layer F.SilkS))
    (fp_text value Conn_01x22_Male (at 7.663373 -1.71) (layer F.Fab))
    (pad 1 thru_hole circle (at 9.438373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad1)"))
    (pad 1 smd roundrect (at 9.438373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 35 "Net-(J2-Pad1)"))
    (pad 1 thru_hole circle (at 9.438373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 35 "Net-(J2-Pad1)"))
    (pad 1 smd roundrect (at 9.438373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 35 "Net-(J2-Pad1)"))
    (pad 2 smd roundrect (at 8.788373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 36 "Net-(J2-Pad2)"))
    (pad 3 smd roundrect (at 8.138373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 60 GND))
    (pad 4 smd roundrect (at 7.488373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 37 "Net-(J2-Pad4)"))
    (pad 5 smd roundrect (at 6.838373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 38 "Net-(J2-Pad5)"))
    (pad 6 smd roundrect (at 6.188373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 39 "Net-(J2-Pad6)"))
    (pad 7 smd roundrect (at 5.538373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 40 "Net-(J2-Pad7)"))
    (pad 8 smd roundrect (at 4.888373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 41 "Net-(J2-Pad8)"))
    (pad 9 smd roundrect (at 4.238373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 42 "Net-(J2-Pad9)"))
    (pad 10 smd roundrect (at 3.588373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 43 "Net-(J2-Pad10)"))
    (pad 11 smd roundrect (at 2.938373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 44 "Net-(J2-Pad11)"))
    (pad 12 smd roundrect (at 2.288373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 45 "Net-(J2-Pad12)"))
    (pad 13 smd roundrect (at 1.638373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 46 "Net-(J2-Pad13)"))
    (pad 14 smd roundrect (at 0.988373 1.345307 90) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 47 "Net-(J2-Pad14)"))
    (pad 2 smd roundrect (at 8.788373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 36 "Net-(J2-Pad2)"))
    (pad 3 smd roundrect (at 8.138373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 60 GND))
    (pad 4 smd roundrect (at 7.488373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 37 "Net-(J2-Pad4)"))
    (pad 5 smd roundrect (at 6.838373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 38 "Net-(J2-Pad5)"))
    (pad 6 smd roundrect (at 6.188373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 39 "Net-(J2-Pad6)"))
    (pad 7 smd roundrect (at 5.538373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 40 "Net-(J2-Pad7)"))
    (pad 8 smd roundrect (at 4.888373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 41 "Net-(J2-Pad8)"))
    (pad 9 smd roundrect (at 4.238373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 42 "Net-(J2-Pad9)"))
    (pad 10 smd roundrect (at 3.588373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 43 "Net-(J2-Pad10)"))
    (pad 11 smd roundrect (at 2.938373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 44 "Net-(J2-Pad11)"))
    (pad 12 smd roundrect (at 2.288373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 45 "Net-(J2-Pad12)"))
    (pad 13 smd roundrect (at 1.638373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 46 "Net-(J2-Pad13)"))
    (pad 14 smd roundrect (at 0.988373 1.345307 90) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 47 "Net-(J2-Pad14)"))
    (pad 2 thru_hole circle (at 8.788373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 8.138373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 60 GND))
    (pad 4 thru_hole circle (at 7.488373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 6.838373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at 6.188373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad6)"))
    (pad 7 thru_hole circle (at 5.538373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad7)"))
    (pad 8 thru_hole circle (at 4.888373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad8)"))
    (pad 9 thru_hole circle (at 4.238373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 42 "Net-(J2-Pad9)"))
    (pad 10 thru_hole circle (at 3.588373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 43 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at 2.938373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 44 "Net-(J2-Pad11)"))
    (pad 12 thru_hole circle (at 2.288373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 45 "Net-(J2-Pad12)"))
    (pad 13 thru_hole circle (at 1.638373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 46 "Net-(J2-Pad13)"))
    (pad 14 thru_hole circle (at 0.988373 1.645307 90) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 47 "Net-(J2-Pad14)"))
    (pad 2 thru_hole circle (at 8.788373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 8.138373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 60 GND))
    (pad 4 thru_hole circle (at 7.488373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 37 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 6.838373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at 6.188373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad6)"))
    (pad 7 thru_hole circle (at 5.538373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad7)"))
    (pad 8 thru_hole circle (at 4.888373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 41 "Net-(J2-Pad8)"))
    (pad 9 thru_hole circle (at 4.238373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 42 "Net-(J2-Pad9)"))
    (pad 10 thru_hole circle (at 3.588373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 43 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at 2.938373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 44 "Net-(J2-Pad11)"))
    (pad 12 thru_hole circle (at 2.288373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 45 "Net-(J2-Pad12)"))
    (pad 13 thru_hole circle (at 1.638373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 46 "Net-(J2-Pad13)"))
    (pad 14 thru_hole circle (at 0.988373 1.045307 90) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 47 "Net-(J2-Pad14)"))
    (pad 15 smd roundrect (at -1.376627 -1.101697) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 48 "Net-(J2-Pad15)"))
    (pad 17 smd roundrect (at -1.376627 -2.401697) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 49 "Net-(J2-Pad17)"))
    (pad 20 smd roundrect (at -1.376627 -4.351697) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 60 GND))
    (pad 16 thru_hole circle (at -1.676627 -1.751697) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 50 "Net-(J2-Pad16)"))
    (pad 18 smd roundrect (at -1.376627 -3.051697) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 51 "Net-(J2-Pad18)"))
    (pad 17 thru_hole circle (at -1.676627 -2.401697) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 49 "Net-(J2-Pad17)"))
    (pad 18 thru_hole circle (at -1.676627 -3.051697) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 51 "Net-(J2-Pad18)"))
    (pad 20 thru_hole circle (at -1.676627 -4.351697) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 60 GND))
    (pad 22 smd roundrect (at -1.376627 -5.651697) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 52 "Net-(J2-Pad22)"))
    (pad 16 smd roundrect (at -1.376627 -1.751697) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 50 "Net-(J2-Pad16)"))
    (pad 17 smd roundrect (at -1.376627 -2.401697) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 49 "Net-(J2-Pad17)"))
    (pad 21 smd roundrect (at -1.376627 -5.001697) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 53 "Net-(J2-Pad21)"))
    (pad 21 smd roundrect (at -1.376627 -5.001697) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 53 "Net-(J2-Pad21)"))
    (pad 22 thru_hole circle (at -1.676627 -5.651697) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 52 "Net-(J2-Pad22)"))
    (pad 16 smd roundrect (at -1.376627 -1.751697) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 50 "Net-(J2-Pad16)"))
    (pad 18 smd roundrect (at -1.376627 -3.051697) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 51 "Net-(J2-Pad18)"))
    (pad 15 thru_hole circle (at -1.076627 -1.101697) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 48 "Net-(J2-Pad15)"))
    (pad 16 thru_hole circle (at -1.076627 -1.751697) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 50 "Net-(J2-Pad16)"))
    (pad 22 smd roundrect (at -1.376627 -5.651697) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 52 "Net-(J2-Pad22)"))
    (pad 17 thru_hole circle (at -1.076627 -2.401697) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 49 "Net-(J2-Pad17)"))
    (pad 19 smd roundrect (at -1.376627 -3.701697) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 54 "Net-(J2-Pad19)"))
    (pad 19 thru_hole circle (at -1.076627 -3.701697) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 54 "Net-(J2-Pad19)"))
    (pad 20 thru_hole circle (at -1.076627 -4.351697) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 60 GND))
    (pad 19 smd roundrect (at -1.376627 -3.701697) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 54 "Net-(J2-Pad19)"))
    (pad 15 smd roundrect (at -1.376627 -1.101697) (size 1.1 0.5) (layers F.Cu F.Mask) (roundrect_rratio 0.5)
      (net 48 "Net-(J2-Pad15)"))
    (pad 21 thru_hole circle (at -1.676627 -5.001697) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 53 "Net-(J2-Pad21)"))
    (pad 19 thru_hole circle (at -1.676627 -3.701697) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 54 "Net-(J2-Pad19)"))
    (pad 20 smd roundrect (at -1.376627 -4.351697) (size 1.1 0.5) (layers B.Cu B.Mask) (roundrect_rratio 0.5)
      (net 60 GND))
    (pad 18 thru_hole circle (at -1.076627 -3.051697) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 51 "Net-(J2-Pad18)"))
    (pad 15 thru_hole circle (at -1.676627 -1.101697) (size 0.4 0.4) (drill 0.2) (layers *.Cu *.Mask)
      (net 48 "Net-(J2-Pad15)"))
    (pad 21 thru_hole circle (at -1.076627 -5.001697) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 53 "Net-(J2-Pad21)"))
    (pad 22 thru_hole circle (at -1.076627 -5.651697) (size 0.5 0.5) (drill 0.3) (layers *.Cu *.Mask)
      (net 52 "Net-(J2-Pad22)"))
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer F.Cu) (tedit 5C2FBBD9)
    (at 223.63 92.17)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value R_Pack04 (at -0.55 1.42) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 17 /ADAT))
    (pad 3 smd rect (at -0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 16 /ABCK))
    (pad 2 smd rect (at -0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(RN1-Pad2)"))
    (pad 4 smd rect (at -0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 18 /ALRK))
    (pad 7 smd rect (at 0.5 -0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(RN1-Pad7)"))
    (pad 8 smd rect (at 0.5 -0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J3-Pad8)"))
    (pad 6 smd rect (at 0.5 0.25) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J3-Pad5)"))
    (pad 5 smd rect (at 0.5 0.75) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J3-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer F.Cu) (tedit 5C2FBBF2)
    (at 193.51 93.65 90)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 -2.1 90) (layer F.SilkS))
    (fp_text value R_Pack04 (at -0.16 1.53 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 5 smd rect (at 0.5 0.75 90) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J2-Pad4)"))
    (pad 6 smd rect (at 0.5 0.25 90) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(RN2-Pad6)"))
    (pad 8 smd rect (at 0.5 -0.75 90) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at 0.5 -0.25 90) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J2-Pad5)"))
    (pad 4 smd rect (at -0.5 0.75 90) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 15 /D11))
    (pad 2 smd rect (at -0.5 -0.25 90) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 14 /D10))
    (pad 3 smd rect (at -0.5 0.25 90) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(RN2-Pad3)"))
    (pad 1 smd rect (at -0.5 -0.75 90) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 13 /D9))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Convex_8x0602 (layer F.Cu) (tedit 5C2FBC25)
    (at 184.15 93.41)
    (descr "Chip Resistor Network, ROHM MNR18 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at 0.01 3.05) (layer F.SilkS))
    (fp_text value R_Pack08 (at 0 3) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.9 -1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /D1))
    (pad 16 smd rect (at 0.9 -1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J2-Pad14)"))
    (pad 8 smd rect (at -0.9 1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /D8))
    (pad 9 smd rect (at 0.9 1.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(J2-Pad7)"))
    (pad 2 smd rect (at -0.9 -1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /D2))
    (pad 3 smd rect (at -0.9 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /D3))
    (pad 4 smd rect (at -0.9 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /D4))
    (pad 5 smd rect (at -0.9 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /D5))
    (pad 6 smd rect (at -0.9 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /D6))
    (pad 7 smd rect (at -0.9 1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /D7))
    (pad 15 smd rect (at 0.9 -1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J2-Pad13)"))
    (pad 14 smd rect (at 0.9 -0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J2-Pad12)"))
    (pad 13 smd rect (at 0.9 -0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(J2-Pad11)"))
    (pad 11 smd rect (at 0.9 0.75) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(J2-Pad9)"))
    (pad 12 smd rect (at 0.9 0.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(J2-Pad10)"))
    (pad 10 smd rect (at 0.9 1.25) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(J2-Pad8)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Convex_8x0602.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_Array_Concave_4x0402 (layer F.Cu) (tedit 5C2FBC11)
    (at 182.87 89.75 225)
    (descr "Thick Film Chip Resistor Array, Wave soldering, Vishay CRA04P (see cra04p.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN4 (at 1.916259 0.176777 315) (layer F.SilkS))
    (fp_text value R_Pack04 (at 0.021213 1.435427 225) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 1 smd rect (at -0.499999 -0.75 225) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J2-Pad15)"))
    (pad 3 smd rect (at -0.5 0.25 225) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J2-Pad18)"))
    (pad 2 smd rect (at -0.5 -0.25 225) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J2-Pad17)"))
    (pad 4 smd rect (at -0.499999 0.75 225) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J2-Pad19)"))
    (pad 7 smd rect (at 0.5 -0.25 225) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 1 /VCLK))
    (pad 8 smd rect (at 0.499999 -0.75 225) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 4 /D0))
    (pad 6 smd rect (at 0.5 0.25 225) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 3 /HSYNC))
    (pad 5 smd rect (at 0.499999 0.75 225) (size 0.5 0.32) (layers F.Cu F.Paste F.Mask)
      (net 2 /VSYNC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_Array_Concave_4x0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 5C2FBB06)
    (at 206.25 95.98 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at -0.06 -1.42 270) (layer F.SilkS))
    (fp_text value .1u (at 0.01 0.01) (layer F.Fab))
    (fp_text user %R (at -0.08 -1.44 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 60 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:DC-PIN6-PIN7 (layer F.Cu) (tedit 5C2FBBCE)
    (at 216.85 90.39)
    (fp_text reference J4 (at 2.52 -0.39) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at 2.6 0.34) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0.714 0.225) (size 1.6 1.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 62 "Net-(D1-Pad2)"))
  )
  (module pads:DC-PIN6-PIN7 (layer F.Cu) (tedit 5C2FBBB4)
    (at 216.63 94.4)
    (fp_text reference J5 (at -0.51 3.38) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at -0.34 4.05) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0.934 2.096) (size 1.6 1.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 59 "Net-(C1-Pad1)"))
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5C2FBB5E)
    (at 214.31 93.83 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at -1.8 -0.08 180) (layer F.SilkS))
    (fp_text value 47K (at -0.03 -0.01 270) (layer F.Fab))
    (fp_text user %R (at -1.8 -0.07 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /+3.3))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5C2FBB46)
    (at 214.33 95.43 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R2 (at -1.81 -0.02 180) (layer F.SilkS))
    (fp_text value 47K (at 0.01 -0.01 270) (layer F.Fab))
    (fp_text user %R (at -1.8 -0.02 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /+3.3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5C2FBAF3)
    (at 204.04 95.39 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R4 (at 1.84 -0.06 180) (layer F.SilkS))
    (fp_text value 1K (at 0.01 0.04 270) (layer F.Fab))
    (fp_text user %R (at 1.82 -0.05 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(J1-Pad28)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-523 (layer F.Cu) (tedit 5C2FBB25)
    (at 211.91 93.83)
    (descr "http://www.diodes.com/datasheets/ap02001.pdf p.144")
    (tags "Diode SOD523")
    (attr smd)
    (fp_text reference D1 (at -0.56 -1.3) (layer F.SilkS))
    (fp_text value 1N4148WT (at -0.01 0.85) (layer F.Fab) hide)
    (fp_text user %R (at -0.56 -1.3) (layer F.Fab))
    (pad 2 smd rect (at 0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -0.7 0 180) (size 0.6 0.7) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-523.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module pads:DC-3v3_power (layer F.Cu) (tedit 5C2FBDFD)
    (at 220.25 95.46)
    (fp_text reference J6 (at 4.02 -0.64) (layer F.SilkS))
    (fp_text value Conn_01x02_Female (at 0.27 1.06) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.219 1.219) (drill 0.889) (layers *.Cu *.Mask)
      (net 20 /+3.3))
    (pad 2 thru_hole circle (at 2.506 0) (size 1.219 1.219) (drill 0.889) (layers *.Cu *.Mask)
      (net 20 /+3.3))
  )
  (module pads:DC-PIN6-PIN7 (layer F.Cu) (tedit 5C2FBF49)
    (at 213.64 87.47)
    (fp_text reference J7 (at -6.5 -2.25) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at 0 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 GND))
  )
  (module pads:DC-PIN6-PIN7 (layer F.Cu) (tedit 5C2FBF3F)
    (at 179.3 87.17)
    (fp_text reference J8 (at -6.5 -2.25) (layer F.SilkS))
    (fp_text value Conn_01x01_Female (at 0 -4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.2 1.2) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /+5))
  )
  (gr_text + (at 213.4 92.7) (layer F.SilkS))
  (gr_line (start 170.3 98.96) (end 157.44 86.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.1 69.64) (end 174.53 88.257) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 219.403 95.451) (end 219.653 95.451) (angle -270) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 226.052 95.451) (end 226.052 95.701) (angle -270) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 213.597 90.936) (end 213.347 90.936) (angle -270) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 185.708 90.533) (end 185.708 90.283) (angle -270) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 183.079 83.567) (end 185.708 83.567) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 181.835 88.257) (end 181.585 88.257) (angle -270) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 179.332 88.257) (end 179.332 88.007) (angle -270) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 177.41 88.257) (end 177.16 88.257) (angle -270) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.41 87.125) (end 177.41 88.007) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 60.36 86.14) (end 60.36 69.64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.44 86.14) (end 60.36 86.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 217.608 98.96) (end 170.3 98.96) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 219.403 97.39) (end 217.608 98.96) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 219.403 95.701) (end 219.403 97.39) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 225.802 95.451) (end 219.653 95.451) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 226.052 98.869) (end 226.052 95.701) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 227.921 98.869) (end 226.052 98.869) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 227.921 89.169) (end 227.921 98.869) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 215.372 89.169) (end 227.921 89.169) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 214.711 88.394) (end 215.372 89.169) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 214.711 87.008) (end 214.711 88.394) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 214.329 86.291) (end 214.711 87.008) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 213.597 86.291) (end 214.329 86.291) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 213.597 90.686) (end 213.597 86.291) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 205.678 90.936) (end 213.347 90.936) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 205.093 90.533) (end 205.678 90.936) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 185.958 90.533) (end 205.093 90.533) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 185.708 83.567) (end 185.708 90.283) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 181.835 85.133) (end 183.079 83.567) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 181.835 88.007) (end 181.835 85.133) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179.582 88.257) (end 181.585 88.257) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 179.332 86.39) (end 179.332 88.007) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 178.012 86.39) (end 179.332 86.39) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 177.41 87.125) (end 178.012 86.39) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 174.53 88.257) (end 177.16 88.257) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 60.36 69.64) (end 156.1 69.64) (layer Edge.Cuts) (width 0.05))
)
