(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 64)
    (no_connects 0)
    (area 135.674999 91.924999 170.575001 126.825001)
    (thickness 1.6)
    (drawings 5)
    (tracks 301)
    (zones 0)
    (modules 5)
    (nets 66)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 1)
  (net 2 2)
  (net 3 3)
  (net 4 4)
  (net 5 5)
  (net 6 6)
  (net 7 7)
  (net 8 8)
  (net 9 9)
  (net 10 10)
  (net 11 11)
  (net 12 12)
  (net 13 13)
  (net 14 14)
  (net 15 15)
  (net 16 16)
  (net 17 17)
  (net 18 18)
  (net 19 19)
  (net 20 20)
  (net 21 21)
  (net 22 22)
  (net 23 23)
  (net 24 24)
  (net 25 25)
  (net 26 26)
  (net 27 27)
  (net 28 28)
  (net 29 29)
  (net 30 30)
  (net 31 31)
  (net 32 32)
  (net 33 33)
  (net 34 34)
  (net 35 35)
  (net 36 36)
  (net 37 37)
  (net 38 38)
  (net 39 39)
  (net 40 40)
  (net 41 41)
  (net 42 42)
  (net 43 43)
  (net 44 44)
  (net 45 45)
  (net 46 46)
  (net 47 47)
  (net 48 48)
  (net 49 49)
  (net 50 50)
  (net 51 51)
  (net 52 52)
  (net 53 53)
  (net 54 54)
  (net 55 55)
  (net 56 56)
  (net 57 57)
  (net 58 58)
  (net 59 59)
  (net 60 60)
  (net 61 61)
  (net 62 62)
  (net 63 63)
  (net 64 64)
  (net 65 "Net-(U1-PadGND)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 1)
    (add_net 10)
    (add_net 11)
    (add_net 12)
    (add_net 13)
    (add_net 14)
    (add_net 15)
    (add_net 16)
    (add_net 17)
    (add_net 18)
    (add_net 19)
    (add_net 2)
    (add_net 20)
    (add_net 21)
    (add_net 22)
    (add_net 23)
    (add_net 24)
    (add_net 25)
    (add_net 26)
    (add_net 27)
    (add_net 28)
    (add_net 29)
    (add_net 3)
    (add_net 30)
    (add_net 31)
    (add_net 32)
    (add_net 33)
    (add_net 34)
    (add_net 35)
    (add_net 36)
    (add_net 37)
    (add_net 38)
    (add_net 39)
    (add_net 4)
    (add_net 40)
    (add_net 41)
    (add_net 42)
    (add_net 43)
    (add_net 44)
    (add_net 45)
    (add_net 46)
    (add_net 47)
    (add_net 48)
    (add_net 49)
    (add_net 5)
    (add_net 50)
    (add_net 51)
    (add_net 52)
    (add_net 53)
    (add_net 54)
    (add_net 55)
    (add_net 56)
    (add_net 57)
    (add_net 58)
    (add_net 59)
    (add_net 6)
    (add_net 60)
    (add_net 61)
    (add_net 62)
    (add_net 63)
    (add_net 64)
    (add_net 7)
    (add_net 8)
    (add_net 9)
    (add_net "Net-(U1-PadGND)")
  )
  (module Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm (layer F.Cu) (tedit 58CD5449)
    (at 140.25 100.5)
    (descr "Through hole straight socket strip, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x08 2.54mm double row")
    (fp_text reference J1 (at -1.27 -2.33) (layer F.SilkS))
    (fp_text value CONN_02X08 (at -1.27 20.11) (layer F.Fab))
    (fp_text user %R (at -1.27 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 1))
    (pad 2 thru_hole oval (at -2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 2))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 3))
    (pad 4 thru_hole oval (at -2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 4))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 5))
    (pad 6 thru_hole oval (at -2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 6))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 7))
    (pad 8 thru_hole oval (at -2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 8))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 9))
    (pad 10 thru_hole oval (at -2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 10))
    (pad 11 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 11))
    (pad 12 thru_hole oval (at -2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 12))
    (pad 13 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 13))
    (pad 14 thru_hole oval (at -2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 14))
    (pad 15 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 15))
    (pad 16 thru_hole oval (at -2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 16))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm (layer F.Cu) (tedit 58CD5449)
    (at 144 122.25 90)
    (descr "Through hole straight socket strip, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x08 2.54mm double row")
    (fp_text reference J2 (at -1.27 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_02X08 (at -1.27 20.11 90) (layer F.Fab))
    (fp_text user %R (at -1.27 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 17))
    (pad 2 thru_hole oval (at -2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 18))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 19))
    (pad 4 thru_hole oval (at -2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 20))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 21))
    (pad 6 thru_hole oval (at -2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 22))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 23))
    (pad 8 thru_hole oval (at -2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 24))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 25))
    (pad 10 thru_hole oval (at -2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 26))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 27))
    (pad 12 thru_hole oval (at -2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 28))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 29))
    (pad 14 thru_hole oval (at -2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 30))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 31))
    (pad 16 thru_hole oval (at -2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 32))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm (layer F.Cu) (tedit 58CD5449)
    (at 165.75 118.25 180)
    (descr "Through hole straight socket strip, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x08 2.54mm double row")
    (fp_text reference J3 (at -1.27 -2.33 180) (layer F.SilkS))
    (fp_text value CONN_02X08 (at -1.27 20.11 180) (layer F.Fab))
    (fp_text user %R (at -1.27 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 33))
    (pad 2 thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 34))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 35))
    (pad 4 thru_hole oval (at -2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 36))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 37))
    (pad 6 thru_hole oval (at -2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 38))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 39))
    (pad 8 thru_hole oval (at -2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 40))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 41))
    (pad 10 thru_hole oval (at -2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 42))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 43))
    (pad 12 thru_hole oval (at -2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 44))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 45))
    (pad 14 thru_hole oval (at -2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 46))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 47))
    (pad 16 thru_hole oval (at -2.54 17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 48))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x08_Pitch2.54mm (layer F.Cu) (tedit 58CD5449)
    (at 161.75 96.5 270)
    (descr "Through hole straight socket strip, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x08 2.54mm double row")
    (fp_text reference J4 (at -1.27 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_02X08 (at -1.27 20.11 270) (layer F.Fab))
    (fp_text user %R (at -1.27 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 49))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 50))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 51))
    (pad 4 thru_hole oval (at -2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 52))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 53))
    (pad 6 thru_hole oval (at -2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 54))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 55))
    (pad 8 thru_hole oval (at -2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 56))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 57))
    (pad 10 thru_hole oval (at -2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 58))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 59))
    (pad 12 thru_hole oval (at -2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 60))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 61))
    (pad 14 thru_hole oval (at -2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 62))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 63))
    (pad 16 thru_hole oval (at -2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 64))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x08_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Misc:HVQFN_64 (layer F.Cu) (tedit 59788C53)
    (at 148.5011 105.0036)
    (fp_text reference U1 (at 4.7 -1.15) (layer F.SilkS))
    (fp_text value TDA19988 (at 4.65 10.25) (layer F.Fab))
    (pad 24 smd rect (at 4.25 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 24 24))
    (pad 25 smd rect (at 4.75 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 25 25))
    (pad 23 smd rect (at 3.75 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 23 23))
    (pad 22 smd rect (at 3.25 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 22 22))
    (pad 21 smd rect (at 2.75 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 21 21))
    (pad 20 smd rect (at 2.25 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 20 20))
    (pad 19 smd rect (at 1.75 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 19 19))
    (pad 18 smd rect (at 1.25 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 18 18))
    (pad 17 smd rect (at 0.75 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 17 17))
    (pad 26 smd rect (at 5.25 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 26 26))
    (pad 27 smd rect (at 5.75 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 27 27))
    (pad 28 smd rect (at 6.25 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 28 28))
    (pad 29 smd rect (at 6.75 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 29 29))
    (pad 30 smd rect (at 7.25 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 30 30))
    (pad 31 smd rect (at 7.75 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 31 31))
    (pad 32 smd rect (at 8.25 9.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 32 32))
    (pad 57 smd rect (at 4.25 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 57 57))
    (pad 56 smd rect (at 4.75 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 56 56))
    (pad 58 smd rect (at 3.75 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 58 58))
    (pad 59 smd rect (at 3.25 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 59 59))
    (pad 60 smd rect (at 2.75 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 60 60))
    (pad 61 smd rect (at 2.25 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 61 61))
    (pad 62 smd rect (at 1.75 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 62 62))
    (pad 63 smd rect (at 1.25 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 63 63))
    (pad 64 smd rect (at 0.75 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 64 64))
    (pad 55 smd rect (at 5.25 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 55 55))
    (pad 54 smd rect (at 5.75 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 54 54))
    (pad 53 smd rect (at 6.25 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 53 53))
    (pad 52 smd rect (at 6.75 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 52 52))
    (pad 51 smd rect (at 7.25 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 51 51))
    (pad 50 smd rect (at 7.75 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 50 50))
    (pad 49 smd rect (at 8.25 0.25) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 49 49))
    (pad 41 smd rect (at 8.75 4.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 41 41))
    (pad 40 smd rect (at 8.75 4.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 40 40))
    (pad 42 smd rect (at 8.75 3.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 42 42))
    (pad 43 smd rect (at 8.75 3.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 43 43))
    (pad 44 smd rect (at 8.75 2.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 44 44))
    (pad 45 smd rect (at 8.75 2.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 45 45))
    (pad 46 smd rect (at 8.75 1.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 46 46))
    (pad 47 smd rect (at 8.75 1.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 47 47))
    (pad 48 smd rect (at 8.75 0.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 48 48))
    (pad 39 smd rect (at 8.75 5.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 39 39))
    (pad 38 smd rect (at 8.75 5.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 38 38))
    (pad 37 smd rect (at 8.75 6.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 37 37))
    (pad 36 smd rect (at 8.75 6.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 36 36))
    (pad 35 smd rect (at 8.75 7.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 35 35))
    (pad 34 smd rect (at 8.75 7.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 34 34))
    (pad 33 smd rect (at 8.75 8.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 33 33))
    (pad 16 smd rect (at -0.25 8.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 16 16))
    (pad 15 smd rect (at -0.25 7.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 15 15))
    (pad 14 smd rect (at -0.25 7.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 14 14))
    (pad 13 smd rect (at -0.25 6.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 13 13))
    (pad 12 smd rect (at -0.25 6.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 12 12))
    (pad 11 smd rect (at -0.25 5.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 11 11))
    (pad 10 smd rect (at -0.25 5.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 10 10))
    (pad 1 smd rect (at -0.25 0.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 1 1))
    (pad 2 smd rect (at -0.25 1.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 2 2))
    (pad 3 smd rect (at -0.25 1.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 3 3))
    (pad 4 smd rect (at -0.25 2.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 4 4))
    (pad 5 smd rect (at -0.25 2.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 5 5))
    (pad 6 smd rect (at -0.25 3.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 6 6))
    (pad 7 smd rect (at -0.25 3.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 7 7))
    (pad 9 smd rect (at -0.25 4.75 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 9 9))
    (pad 8 smd rect (at -0.25 4.25 270) (size 0.2 0.5) (drill (offset 0 -0.25)) (layers F.Cu F.Paste F.Mask)
      (net 8 8))
    (pad GND smd rect (at 4.5 4.5) (size 5.1 5.1) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(U1-PadGND)"))
  )
  (gr_text "HVQFN64\nNick Palmer\n2017" (at 153 117) (layer B.SilkS))
  (gr_line (start 135.75 126.75) (end 135.75 92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.5 126.75) (end 135.75 126.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.5 92) (end 170.5 126.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 135.75 92) (end 170.5 92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 65) (net_name "Net-(U1-PadGND)") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 151 109.5) (xy 151 107.5) (xy 155 107.5) (xy 155 111.5) (xy 151 111.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156 108) (xy 156 106.5) (xy 150 106.5) (xy 150 112.5) (xy 156 112.5)
      )
    )
  )
)
