<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>OUT1</text>
<text>D11</text>
<text>D9</text>
<text>OUT2</text>
<text>OUT3</text>
<text>OUT4</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>RS485</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>RST</text>
<text>SCL</text>
<text>SDA</text>
<text>+5V</text>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>3V3</text>
<wire x1="0" y1="50.8" x2="2.54" y2="53.34" width="0.1016" layer="20"/>
<wire x1="2.54" y1="53.34" x2="55.88" y2="53.34" width="0.1016" layer="20"/>
<wire x1="55.88" y1="53.34" x2="57.15" y2="52.07" width="0.1016" layer="20"/>
<wire x1="57.15" y1="52.07" x2="57.15" y2="40.64" width="0.1016" layer="20"/>
<wire x1="57.15" y1="40.64" x2="59.69" y2="38.1" width="0.1016" layer="20"/>
<wire x1="59.69" y1="38.1" x2="59.69" y2="5.08" width="0.1016" layer="20"/>
<wire x1="59.69" y1="5.08" x2="57.15" y2="2.54" width="0.1016" layer="20"/>
<wire x1="57.15" y1="2.54" x2="57.15" y2="0" width="0.1016" layer="20"/>
<wire x1="57.15" y1="0" x2="2.54" y2="0" width="0.1016" layer="20"/>
<wire x1="2.54" y1="0" x2="0" y2="2.54" width="0.1016" layer="20"/>
<wire x1="0" y1="2.54" x2="0" y2="50.8" width="0.1016" layer="20"/>
<text>A</text>
<text>B</text>
<text>+5V</text>
<text>DAC 0-10V / RS485 Shield V1.0 
(c) Charles-Henri Hallard
https://github.com/hallard
https://hallard.me</text>
<text>OUT1</text>
<text>OUT2</text>
<text>OUT3</text>
<text>OUT4</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>RS485</text>
<text>B</text>
<text>A</text>
<text>GND</text>
<text>RST</text>
<text>SCL</text>
<text>SDA</text>
<text>+5V</text>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>3V3</text>
<text>+5V</text>
<text>D11</text>
<text>GND</text>
<text>GND</text>
<text>D9</text>
<text>A0</text>
<text>A1</text>
<text>5V</text>
<text>VIN</text>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUEMILANOVE_SHIELD_NOHOLES">
</package>
</packages>
</library>
<library name="Texas Instruments_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:45:58</description>
<packages>
<package name="SOP65P640X120-16N">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt;</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
<library name="_c2h">
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
<package name="1X06_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="LowPowerLab">
<packages>
<package name="0805-RES">
</package>
<package name="0805-CAP">
</package>
</packages>
</library>
<library name="microbuilder">
<description>&lt;h2&gt;&lt;b&gt;microBuilder.eu&lt;/b&gt; Eagle Footprint Library&lt;/h2&gt;

&lt;p&gt;Footprints for common components used in our projects and products.  This is the same library that we use internally, and it is regularly updated.  The newest version can always be found at &lt;b&gt;www.microBuilder.eu&lt;/b&gt;.  If you find this library useful, please feel free to purchase something from our online store. Please also note that all holes are optimised for metric drill bits!&lt;/p&gt;

&lt;h3&gt;Obligatory Warning&lt;/h3&gt;
&lt;p&gt;While it probably goes without saying, there are no guarantees that the footprints or schematic symbols in this library are flawless, and we make no promises of fitness for production, prototyping or any other purpose. These libraries are provided for information puposes only, and are used at your own discretion.  While we make every effort to produce accurate footprints, and many of the items found in this library have be proven in production, we can't make any promises of suitability for a specific purpose. If you do find any errors, though, please feel free to contact us at www.microbuilder.eu to let us know about it so that we can update the library accordingly!&lt;/p&gt;

&lt;h3&gt;License&lt;/h3&gt;
&lt;p&gt;This work is placed in the public domain, and may be freely used for commercial and non-commercial work with the following conditions:&lt;/p&gt;
&lt;p&gt;THIS SOFTWARE IS PROVIDED ''AS IS'' AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED.  IN NO EVENT SHALL THE INSTITUTE OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,  BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
&lt;/p&gt;</description>
<packages>
<package name="_0603">
<description>&lt;b&gt;0603&lt;/b&gt;</description>
</package>
<package name="_0805">
<description>&lt;b&gt;0805&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Seeed-Discrete">
<packages>
<package name="5P-13.75X11.7X6.5H">
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; SOIC 150 mil</description>
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="SW_TACT_SMALL">
</package>
<package name="M1X2">
</package>
<package name="M1X3">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="WS2812B">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ARDUINO" library="SparkFun-Boards" package="DUEMILANOVE_SHIELD_NOHOLES" value="SHIELD"/>
<element name="U1" library="Texas Instruments_By_element14_Batch_1" package="SOP65P640X120-16N" value="DAC7565">
<attribute name="PACKAGE" value="TSSOP-16"/>
<attribute name="OC_NEWARK" value="94M6804"/>
<attribute name="MPN" value="DAC7565IAPW"/>
<attribute name="SUPPLIER" value="Texas Instruments"/>
<attribute name="OC_FARNELL" value="1604982"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear" package="SO14" value="TLV2374">
<attribute name="VALUE"/>
</element>
<element name="OUT1" library="_c2h" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="LowPowerLab" package="0805-RES" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="LowPowerLab" package="0805-RES" value="10K 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="LowPowerLab" package="0805-CAP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="LowPowerLab" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT2" library="_c2h" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="LowPowerLab" package="0805-RES" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="LowPowerLab" package="0805-RES" value="10K 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT3" library="_c2h" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="R5" library="LowPowerLab" package="0805-RES" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="LowPowerLab" package="0805-RES" value="10K 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT4" library="_c2h" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="R7" library="LowPowerLab" package="0805-RES" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="LowPowerLab" package="0805-RES" value="10K 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="LowPowerLab" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="LowPowerLab" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FERRITE" library="microbuilder" package="_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="microbuilder" package="_0805" value="10uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="LowPowerLab" package="0805-CAP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="LowPowerLab" package="0805-CAP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="LowPowerLab" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="microbuilder" package="_0805" value="10uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="linear" package="SO08" value="TL072">
<attribute name="VALUE"/>
</element>
<element name="R9" library="LowPowerLab" package="0805-RES" value="10K 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="LowPowerLab" package="0805-RES" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="LowPowerLab" package="0805-RES" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="LowPowerLab" package="0805-RES" value="12k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="LowPowerLab" package="0805-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="LowPowerLab" package="0805-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT5" library="_c2h" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="R13" library="LowPowerLab" package="0805-RES" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="LowPowerLab" package="0805-RES" value="10K 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT6" library="_c2h" package="W237-102" value="">
<attribute name="VALUE"/>
</element>
<element name="C10" library="LowPowerLab" package="0805-CAP" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="LowPowerLab" package="0805-RES" value="15K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="LowPowerLab" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ROTENCODER" library="Seeed-Discrete" package="5P-13.75X11.7X6.5H" value="">
<attribute name="VALUE"/>
</element>
<element name="IC3" library="maxim" package="SO08" value="MAX485">
<attribute name="OC_NEWARK" value="90C3817"/>
<attribute name="MPN" value="MAX481CSA"/>
<attribute name="MF" value="MAXIM"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="LowPowerLab" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="LowPowerLab" package="0805-RES" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RS485" library="_c2h" package="W237-102" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="RESET" library="dp_devices" package="SW_TACT_SMALL" value="">
<attribute name="NAME"/>
</element>
<element name="JRX" library="dp_devices" package="M1X2" value="CON_HEADER_1X02-PTH">
<attribute name="NAME"/>
</element>
<element name="JTX" library="dp_devices" package="M1X2" value="CON_HEADER_1X02-PTH">
<attribute name="NAME"/>
</element>
<element name="U$1" library="_c2h" package="1X06_LOCK" value="OLED_I2C_ADAFRUIT"/>
<element name="U$2" library="_c2h" package="1X04_LOCK" value="OLED_I2C_TINDIE"/>
<element name="TP1" library="testpad" package="P1-13" value="">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="P1-13" value="">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="P1-13" value="">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="P1-13" value="">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VIN" library="testpad" package="P1-13" value="">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TGND" library="testpad" package="P1-13" value="">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED" library="adafruit" package="WS2812B" value="WS2812B">
<attribute name="NAME"/>
</element>
<element name="5V" library="testpad" package="P1-13" value="">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="LowPowerLab" package="0805-CAP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="dp_devices" package="M1X3" value="CON_HEADER_1X03-PTH"/>
<element name="R17" library="LowPowerLab" package="0805-RES" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="LowPowerLab" package="0805-RES" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="LowPowerLab" package="0805-RES" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="LowPowerLab" package="0805-RES" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="LowPowerLab" package="0805-RES" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="LowPowerLab" package="0805-RES" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="OUT1">
<contactref element="IC1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="OUT1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="ARDUINO" pad="GND@0"/>
<contactref element="IC1" pad="11"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="OUT1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="OUT2" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="OUT3" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="OUT4" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="R10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="OUT5" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="OUT6" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="ROTENCODER" pad="2"/>
<contactref element="ROTENCODER" pad="4"/>
<contactref element="RESET" pad="2"/>
<contactref element="RESET" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="2"/>
<contactref element="TGND" pad="TP"/>
<contactref element="U1" pad="14"/>
<contactref element="LED" pad="3-GND"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC3" pad="5"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="D13/SCK">
<contactref element="ARDUINO" pad="D13"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="D12/DIN">
<contactref element="ARDUINO" pad="D12"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="OUT2">
<contactref element="U1" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="OUT3">
<contactref element="U1" pad="7"/>
<contactref element="IC1" pad="10"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="OUT4">
<contactref element="U1" pad="8"/>
<contactref element="IC1" pad="12"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="R4" pad="1"/>
<contactref element="OUT2" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="N$11">
<contactref element="R6" pad="1"/>
<contactref element="OUT3" pad="1"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="N$13">
<contactref element="R8" pad="1"/>
<contactref element="OUT4" pad="1"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="5V">
<contactref element="L1" pad="1"/>
<contactref element="U1" pad="12"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="FERRITE" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="IC3" pad="8"/>
<contactref element="5V" pad="TP"/>
<contactref element="LED" pad="1-VDD"/>
<contactref element="C13" pad="1"/>
<contactref element="U$2" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="3"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="ARDUINO" pad="RES"/>
<contactref element="U1" pad="13"/>
<contactref element="RESET" pad="3"/>
<contactref element="RESET" pad="4"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="D8">
<contactref element="ARDUINO" pad="D8"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="D7/ENABLE">
<contactref element="ARDUINO" pad="D7"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="D4/SYNC">
<contactref element="ARDUINO" pad="D4"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="AVDD">
<contactref element="U1" pad="4"/>
<contactref element="FERRITE" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="ARDUINO" pad="5V"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="ARDUINO" pad="VIN"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R9" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="OUT5" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R11" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="D11">
<contactref element="R12" pad="1"/>
<contactref element="ARDUINO" pad="D11"/>
</signal>
<signal name="N$7">
<contactref element="R13" pad="2"/>
<contactref element="IC2" pad="6"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R14" pad="1"/>
<contactref element="IC2" pad="7"/>
<contactref element="OUT6" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="IC2" pad="5"/>
<contactref element="R15" pad="2"/>
<contactref element="C10" pad="2"/>
</signal>
<signal name="D9">
<contactref element="R15" pad="1"/>
<contactref element="ARDUINO" pad="D9"/>
</signal>
<signal name="VIN1">
<contactref element="C11" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="L2" pad="1"/>
<contactref element="VIN" pad="TP"/>
</signal>
<signal name="N$24">
<contactref element="IC3" pad="7"/>
<contactref element="R16" pad="2"/>
<contactref element="RS485" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="IC3" pad="6"/>
<contactref element="R16" pad="1"/>
<contactref element="RS485" pad="2"/>
</signal>
<signal name="RX">
<contactref element="ARDUINO" pad="RX"/>
<contactref element="JRX" pad="2"/>
</signal>
<signal name="TX">
<contactref element="ARDUINO" pad="TX"/>
<contactref element="JTX" pad="1"/>
</signal>
<signal name="D2">
<contactref element="ARDUINO" pad="D2"/>
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="D3">
<contactref element="ARDUINO" pad="D3"/>
<contactref element="LED" pad="4-DIN"/>
</signal>
<signal name="A0">
<contactref element="ARDUINO" pad="A0"/>
<contactref element="R17" pad="1"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="D5">
<contactref element="ARDUINO" pad="D5"/>
<contactref element="ROTENCODER" pad="1"/>
</signal>
<signal name="D6">
<contactref element="ARDUINO" pad="D6"/>
<contactref element="ROTENCODER" pad="3"/>
</signal>
<signal name="A1">
<contactref element="ARDUINO" pad="A1"/>
<contactref element="R18" pad="1"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="D10">
<contactref element="ARDUINO" pad="D10"/>
<contactref element="ROTENCODER" pad="5"/>
</signal>
<signal name="RX-485">
<contactref element="IC3" pad="1"/>
<contactref element="JRX" pad="1"/>
</signal>
<signal name="TX-485">
<contactref element="IC3" pad="4"/>
<contactref element="JTX" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="U$1" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="5"/>
<contactref element="U$2" pad="4"/>
<contactref element="ARDUINO" pad="A5"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="6"/>
<contactref element="U$2" pad="3"/>
<contactref element="ARDUINO" pad="A4"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="ARDUINO" pad="3.3V"/>
</signal>
<signal name="A0IN">
<contactref element="J1" pad="3"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="A1IN">
<contactref element="J1" pad="2"/>
<contactref element="R18" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
