<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="51.74" y2="0" width="0" layer="20"/>
<wire x1="51.74" y1="0" x2="51.74" y2="40.63" width="0" layer="20"/>
<wire x1="51.74" y1="40.63" x2="0" y2="40.63" width="0" layer="20"/>
<wire x1="0" y1="40.63" x2="0" y2="0" width="0" layer="20"/>
<text>THAT'S WHAT SOUNDS LIKE JAZZ</text>
<text>(that's how you know
it's a good one)</text>
<text>yeah it's a rat but like,
it's your rat, ya know?</text>
</plain>
<libraries>
<library name="gm-caps-film-chicklet">
<description>&lt;b&gt;Capacitors, Film, Chicklet&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;100pF - 0.1uF (uF = µF = mF)
&lt;li&gt;popular nonpolarized capacitors
&lt;li&gt;available from smallbearelec.com as Panasonic ECQ-B capacitors
&lt;li&gt;these become quite large for values near 1uF
&lt;/ul&gt;</description>
<packages>
<package name="070X030_3">
<description>&lt;b&gt;7mm x 3mm, 0.3" pad spacing&lt;/b&gt;
&lt;p&gt;Panasonic ECQ-B</description>
</package>
</packages>
</library>
<library name="gm-caps-electro-pol">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
<package name="DO35-3">
<description>&lt;B&gt;DO-35 0.3" spacing&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="gm-pots">
<description>&lt;b&gt;Potentiometers&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;chassis-mount (e.g., Alpha 16mm) pots&lt;/li&gt;
&lt;li&gt;board-mount trim pots (1/4" and 3/8")&lt;/li&gt;
&lt;li&gt; all pot values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="POT">
<description>&lt;b&gt;Potentiometer&lt;/b&gt;
&lt;p&gt;3 terminals for circuit board for wires connecting to 3 lugs of pot off-board</description>
</package>
</packages>
</library>
<library name="gm-supply">
<description>&lt;b&gt;Supply&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;input, output, ground, and power supply.  
&lt;li&gt;these are used on a schematic for placeholders and on a board for pads for off-board components like jacks.
&lt;/ul&gt;</description>
<packages>
<package name="SQUARE">
<description>&lt;b&gt;Square Pad&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;drill diameter 0.7 mm&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="AB9V">
<description>&lt;B&gt;9-V BATTERY CLIP&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="gm-ics">
<description>&lt;b&gt;Integrated Circuits&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;mostly op amps (e.g., 4558, TL072)&lt;/li&gt;
&lt;li&gt;also CD4049 (for Anderton's Tube Sound Fuzz, the Red Llama, ...)
&lt;li&gt;generally gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="gm-trans">
<description>&lt;b&gt;Transistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;small signal amps (e.g., 2N508x)
&lt;li&gt;switching transistors (e.g., 2N2222, 2N390x)
&lt;li&gt;JFETs (e.g., J201, 2N3819, 2N5457)
&lt;li&gt;MOSFETs (e.g., BS170, BS250)
&lt;li&gt;mostly copied from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="TO92-">
</package>
</packages>
</library>
<library name="gm-resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/4">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 4 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="gm-caps-film-chicklet" package="070X030_3" value="30pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="gm-caps-electro-pol" package="050_020_1" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="gm-caps-film-chicklet" package="070X030_3" value=".001uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="gm-caps-film-chicklet" package="070X030_3" value=".022uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="gm-caps-electro-pol" package="050_020_1" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="gm-caps-film-chicklet" package="070X030_3" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="gm-caps-film-chicklet" package="070X030_3" value="100pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="gm-caps-electro-pol" package="050_020_1" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="gm-caps-electro-pol" package="050_020_1" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="gm-caps-electro-pol" package="050_020_1" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="gm-caps-electro-pol" package="050_020_1" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="gm-caps-film-chicklet" package="070X030_3" value=".001uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="gm-caps-film-chicklet" package="070X030_3" value=".022uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="gm-caps-film-chicklet" package="070X030_3" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="gm-diodes" package="DO41-3" value="1N4002">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="gm-diodes" package="DO35-3" value="1N914.3">
<attribute name="NAME"/>
</element>
<element name="D3" library="gm-diodes" package="DO35-3" value="1N914.3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FILTH" library="gm-pots" package="POT" value="100KA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND1" library="gm-supply" package="SQUARE" value="GND(T)">
<attribute name="NAME"/>
</element>
<element name="GND6" library="gm-supply" package="SQUARE" value="GND(T)">
<attribute name="NAME"/>
</element>
<element name="IC1" library="gm-ics" package="DIL08" value="LM308N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IN1" library="gm-supply" package="SQUARE" value="IN(T)">
<attribute name="NAME"/>
</element>
<element name="OUT1" library="gm-supply" package="SQUARE" value="OUT(T)">
<attribute name="NAME"/>
</element>
<element name="Q1" library="gm-trans" package="TO92-" value="2N5458">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="gm-resistors" package="R0207/4" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="gm-resistors" package="R0207/4" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="gm-resistors" package="R0207/4" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="gm-resistors" package="R0207/4" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="gm-resistors" package="R0207/4" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="gm-resistors" package="R0207/4" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="gm-resistors" package="R0207/4" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="gm-resistors" package="R0207/4" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="gm-resistors" package="R0207/4" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="gm-resistors" package="R0207/4" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="gm-resistors" package="R0207/4" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="gm-resistors" package="R0207/4" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TONE" library="gm-pots" package="POT" value="100KA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V3" library="gm-supply" package="AB9V" value="9VBATTERY"/>
<element name="VOL" library="gm-pots" package="POT" value="100KA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H2" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="4"/>
<contactref element="C3" pad="-"/>
<contactref element="C4" pad="-"/>
<contactref element="C7" pad="2"/>
<contactref element="GND6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="V3" pad="-"/>
<contactref element="D1" pad="A"/>
<contactref element="C5" pad="-"/>
<contactref element="C9" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C6" pad="-"/>
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="A"/>
<contactref element="C11" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="VOL" pad="3"/>
<contactref element="GND1" pad="1"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="+9V">
<contactref element="IC1" pad="7"/>
<contactref element="C14" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="C5" pad="+"/>
<contactref element="C9" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="IC1" pad="8"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="FILTH" pad="1"/>
<contactref element="C10" pad="+"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="FILTH" pad="3"/>
<contactref element="FILTH" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="N$6">
<contactref element="R2" pad="1"/>
<contactref element="C4" pad="+"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="3"/>
<contactref element="C7" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="VA">
<contactref element="R4" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="C6" pad="+"/>
</signal>
<signal name="IN">
<contactref element="C8" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="IN1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R6" pad="1"/>
<contactref element="V3" pad="+"/>
</signal>
<signal name="N$8">
<contactref element="R9" pad="1"/>
<contactref element="C10" pad="-"/>
</signal>
<signal name="N$10">
<contactref element="R9" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="D3" pad="A"/>
<contactref element="TONE" pad="3"/>
<contactref element="TONE" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="TONE" pad="1"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R10" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="C12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="Q1" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="C13" pad="+"/>
</signal>
<signal name="N$15">
<contactref element="C13" pad="-"/>
<contactref element="VOL" pad="1"/>
</signal>
<signal name="OUT">
<contactref element="OUT1" pad="1"/>
<contactref element="VOL" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
