(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "RTC8088 - Real Time Clock for PC/XT")
    (date "2024-04-26")
    (rev "3.0")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/AS1")
  (net 3 "/AS0")
  (net 4 "VCC")
  (net 5 "/~{IRQ}")
  (net 6 "unconnected-(U1-Pad1)")
  (net 7 "Net-(U1-Pad2)")
  (net 8 "Net-(U1-Pad3)")
  (net 9 "/D0")
  (net 10 "/D1")
  (net 11 "/D2")
  (net 12 "/D3")
  (net 13 "/D4")
  (net 14 "/D5")
  (net 15 "/D6")
  (net 16 "/D7")
  (net 17 "/RTCALE")
  (net 18 "/RTCWR")
  (net 19 "/RTCRD")
  (net 20 "Net-(BT1-Pad1)")
  (net 21 "Net-(JP1-Pad1)")
  (net 22 "unconnected-(U1-Pad22)")
  (net 23 "unconnected-(U1-Pad23)")
  (net 24 "/A0")
  (net 25 "/A3")
  (net 26 "/A4")
  (net 27 "/A5")
  (net 28 "/A6")
  (net 29 "/A7")
  (net 30 "/A8")
  (net 31 "/A9")
  (net 32 "/IOW")
  (net 33 "/IOR")
  (net 34 "/AEN")
  (net 35 "/A2")
  (net 36 "/AS2")
  (footprint "My_Components:IC_DIP24_600" (layer "F.Cu")
    (tedit 662AE498)
    (at 179.07 71.12)
    (descr "24 pins DIL package, round pads, width 600mil")
    (tags "DIP DIL DIP24 DIL24")
    (property "Sheetfile" "RTC8088.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -7.62 9.525) (layer "F.SilkS"))
    (fp_text value "DS12885" (at 9.8425 9.525) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 6 "unconnected-(U1-Pad1)") (pinfunction "MOT") (pintype "input+no_connect"))
    (pad "2" thru_hole circle (at -11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad2)") (pinfunction "X1") (pintype "input"))
    (pad "3" thru_hole circle (at -8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad3)") (pinfunction "X2") (pintype "input"))
    (pad "4" thru_hole circle (at -6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 "/D0") (pinfunction "AD0") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at -3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 "/D1") (pinfunction "AD1") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at -1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "/D2") (pinfunction "AD2") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at 1.27 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 "/D3") (pinfunction "AD3") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at 3.81 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 "/D4") (pinfunction "AD4") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at 6.35 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 "/D5") (pinfunction "AD5") (pintype "bidirectional"))
    (pad "10" thru_hole circle (at 8.89 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 "/D6") (pinfunction "AD6") (pintype "bidirectional"))
    (pad "11" thru_hole circle (at 11.43 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 "/D7") (pinfunction "AD7") (pintype "bidirectional"))
    (pad "12" thru_hole circle (at 13.97 7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "13" thru_hole circle (at 13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "~{CS}") (pintype "input"))
    (pad "14" thru_hole circle (at 11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 "/RTCALE") (pinfunction "AS") (pintype "input"))
    (pad "15" thru_hole circle (at 8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 "/RTCWR") (pinfunction "R/~{W}") (pintype "input"))
    (pad "16" thru_hole circle (at 6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "17" thru_hole circle (at 3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 "/RTCRD") (pinfunction "DS") (pintype "input"))
    (pad "18" thru_hole circle (at 1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "VCC") (pinfunction "~{RESET}") (pintype "input"))
    (pad "19" thru_hole circle (at -1.27 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "/~{IRQ}") (pinfunction "~{IRQ}") (pintype "output"))
    (pad "20" thru_hole circle (at -3.81 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 "Net-(BT1-Pad1)") (pinfunction "VBAT") (pintype "power_in"))
    (pad "21" thru_hole circle (at -6.35 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 "Net-(JP1-Pad1)") (pinfunction "~{RCLR}") (pintype "input"))
    (pad "22" thru_hole circle (at -8.89 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 "unconnected-(U1-Pad22)") (pinfunction "NC") (pintype "input+no_connect"))
    (pad "23" thru_hole circle (at -11.43 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 "unconnected-(U1-Pad23)") (pinfunction "SQW") (pintype "input+no_connect"))
    (pad "24" thru_hole circle (at -13.97 -7.62) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-24_W15.24mm.wrl"
      (offset (xyz -13.97 -7.62 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "My_Components:Conn_SIL5" (layer "F.Cu")
    (tedit 662B4670)
    (at 116.84 68.58)
    (descr "Footprint, SIL-5")
    (tags "CONN SIL-5")
    (property "Sheetfile" "RTC8088.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "RN1" (at -5.715 -2.8575 90) (layer "F.SilkS"))
    (fp_text value "10k" (at -5.715 -5.715 90) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "VCC") (pinfunction "common") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "/AS0") (pinfunction "R1") (pintype "passive"))
    (pad "3" thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "/AS1") (pinfunction "R2") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 36 "/AS2") (pinfunction "R3") (pintype "passive"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 5 "/~{IRQ}") (pinfunction "R4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP5.wrl"
      (offset (xyz -5.08 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_Pin_Header_2x1_2.54mm_NoKey" (layer "F.Cu")
    (tedit 662AE0E5)
    (at 179.07 58.42)
    (descr "Pin Header, 2x1, 2.54mm pitch, no key")
    (tags "CONN 2x1 NOKEY")
    (property "Sheetfile" "RTC8088.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "JP1" (at -4.445 0 180) (layer "F.SilkS"))
    (fp_text value "Clear CMOS" (at 0 2.2225) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 "Net-(JP1-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 1.27 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "My_Components:IC_DIP20_300" (layer "F.Cu")
    (tedit 662AE447)
    (at 123.19 74.93)
    (descr "20 pins DIL package, round pads")
    (tags "DIP DIL DIP20 DIL20")
    (property "Sheetfile" "RTC8088.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -10.16 5.715) (layer "F.SilkS"))
    (fp_text value "ATF16V8B" (at 8.255 5.715) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 "/A0") (pinfunction "I/CLK") (pintype "input"))
    (pad "2" thru_hole circle (at -8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 35 "/A2") (pinfunction "I1") (pintype "input"))
    (pad "3" thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 "/A3") (pinfunction "I2") (pintype "input"))
    (pad "4" thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 "/A4") (pinfunction "I3") (pintype "input"))
    (pad "5" thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 "/A5") (pinfunction "I4") (pintype "input"))
    (pad "6" thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 "/A6") (pinfunction "I5") (pintype "input"))
    (pad "7" thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 "/A7") (pinfunction "I6") (pintype "input"))
    (pad "8" thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 "/A8") (pinfunction "I7") (pintype "input"))
    (pad "9" thru_hole circle (at 8.89 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "/A9") (pinfunction "I8") (pintype "input"))
    (pad "10" thru_hole circle (at 11.43 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" thru_hole circle (at 11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 36 "/AS2") (pinfunction "I9/~{OE}") (pintype "input"))
    (pad "12" thru_hole circle (at 8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 "/IOW") (pinfunction "I/O8") (pintype "bidirectional"))
    (pad "13" thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 33 "/IOR") (pinfunction "I/O7") (pintype "bidirectional"))
    (pad "14" thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 "/RTCALE") (pinfunction "I/O6") (pintype "bidirectional"))
    (pad "15" thru_hole circle (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 "/RTCWR") (pinfunction "I/O5") (pintype "bidirectional"))
    (pad "16" thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 "/RTCRD") (pinfunction "I/O4") (pintype "bidirectional"))
    (pad "17" thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 34 "/AEN") (pinfunction "I/O3") (pintype "bidirectional"))
    (pad "18" thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "/AS1") (pinfunction "I/O2") (pintype "bidirectional"))
    (pad "19" thru_hole circle (at -8.89 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "/AS0") (pinfunction "I/O1") (pintype "bidirectional"))
    (pad "20" thru_hole circle (at -11.43 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
      (offset (xyz -11.43 -3.81 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "My_Components:Switch_DIP_3_Positions" (layer "F.Cu")
    (tedit 662B45EE)
    (at 116.84 62.23)
    (descr "DIP Switch, 3 Positions")
    (tags "SWITCH DIP 3POS")
    (property "Sheetfile" "RTC8088.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at -5.715 -3.175 90) (layer "F.SilkS"))
    (fp_text value "Address Select" (at 5.715 0 90) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 3 "/AS0") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 "/AS1") (pintype "passive"))
    (pad "3" thru_hole circle (at 2.54 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 36 "/AS2") (pintype "passive"))
    (pad "4" thru_hole circle (at 2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "5" thru_hole circle (at 0 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "6" thru_hole circle (at -2.54 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx03_Slide_6.7x9.18mm_W7.62mm_P2.54mm_LowProfile.wrl"
      (offset (xyz -2.54 -3.81 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_Edge_PCB_ISA8" (layer "F.Cu")
    (tedit 662BE786)
    (at 152.4 91.1225)
    (descr "Connector, PCB Edge, ISA8")
    (tags "CONN BUS ISA")
    (property "Sheetfile" "RTC8088.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BUS1" (at 0 5.3975) (layer "F.SilkS") hide)
    (fp_text value "BUSPC_DEV" (at 0.3175 6.985) (layer "F.SilkS") hide)
    (pad "1" connect roundrect (at 38.1 0) (size 1.778 8.128) (layers "B.Cu") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "3" connect roundrect (at 33.02 0) (size 1.778 8.128) (layers "B.Cu") (roundrect_rratio 0.25)
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_out"))
    (pad "10" connect roundrect (at 15.24 0) (size 1.778 8.128) (layers "B.Cu") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "13" connect roundrect (at 7.62 0) (size 1.778 8.128) (layers "B.Cu") (roundrect_rratio 0.25)
      (net 32 "/IOW") (pinfunction "IOW") (pintype "output"))
    (pad "14" connect roundrect (at 5.08 0) (size 1.778 8.128) (layers "B.Cu") (roundrect_rratio 0.25)
      (net 33 "/IOR") (pinfunction "IOR") (pintype "output"))
    (pad "29" connect roundrect (at -33.02 0) (size 1.778 8.128) (layers "B.Cu") (roundrect_rratio 0.25)
      (net 4 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "31" connect roundrect (at -38.1 0) (size 1.778 8.128) (layers "B.Cu") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "33" connect roundrect (at 35.56 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 16 "/D7") (pinfunction "SD7") (pintype "bidirectional"))
    (pad "34" connect roundrect (at 33.02 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 15 "/D6") (pinfunction "SD6") (pintype "bidirectional"))
    (pad "35" connect roundrect (at 30.48 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 14 "/D5") (pinfunction "SD5") (pintype "bidirectional"))
    (pad "36" connect roundrect (at 27.94 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 13 "/D4") (pinfunction "SD4") (pintype "bidirectional"))
    (pad "37" connect roundrect (at 25.4 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 12 "/D3") (pinfunction "SD3") (pintype "bidirectional"))
    (pad "38" connect roundrect (at 22.86 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 11 "/D2") (pinfunction "SD2") (pintype "bidirectional"))
    (pad "39" connect roundrect (at 20.32 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 10 "/D1") (pinfunction "SD1") (pintype "bidirectional"))
    (pad "40" connect roundrect (at 17.78 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 9 "/D0") (pinfunction "SD0") (pintype "bidirectional"))
    (pad "42" connect roundrect (at 12.7 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 34 "/AEN") (pinfunction "AEN") (pintype "output"))
    (pad "53" connect roundrect (at -15.24 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 31 "/A9") (pinfunction "SA9") (pintype "output"))
    (pad "54" connect roundrect (at -17.78 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 30 "/A8") (pinfunction "SA8") (pintype "output"))
    (pad "55" connect roundrect (at -20.32 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 29 "/A7") (pinfunction "SA7") (pintype "output"))
    (pad "56" connect roundrect (at -22.86 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 28 "/A6") (pinfunction "SA6") (pintype "output"))
    (pad "57" connect roundrect (at -25.4 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 27 "/A5") (pinfunction "SA5") (pintype "output"))
    (pad "58" connect roundrect (at -27.94 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 26 "/A4") (pinfunction "SA4") (pintype "output"))
    (pad "59" connect roundrect (at -30.48 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 25 "/A3") (pinfunction "SA3") (pintype "output"))
    (pad "60" connect roundrect (at -33.02 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 35 "/A2") (pinfunction "SA2") (pintype "output"))
    (pad "62" connect roundrect (at -38.1 0) (size 1.778 8.128) (layers "F.Cu") (roundrect_rratio 0.25)
      (net 24 "/A0") (pinfunction "SA0") (pintype "output"))
  )
  (footprint "My_Components:Crystal_32K_Horiz" (layer "F.Cu")
    (tedit 662AE50C)
    (at 168.998685 82.55 -90)
    (descr "crystal resonator for RTC, 32768 Hz")
    (tags "CRYSTAL RTC")
    (property "Sheetfile" "RTC8088.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y1" (at 2.54 12.788685) (layer "F.SilkS"))
    (fp_text value "32768Hz" (at 2.54 8.343685) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 "Net-(U1-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 "Net-(U1-Pad3)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 1.5875 5.08 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (pad "3" thru_hole circle (at -1.5875 5.08 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_C26-LF_D2.1mm_L6.5mm_Horizontal.wrl"
      (offset (xyz -1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Cap_Cer_508" (layer "F.Cu")
    (tedit 6596010D)
    (at 167.64 58.42)
    (descr "Ceramic Capacitor, 5.08mm lead spacing")
    (tags "Cap_Cer_508")
    (property "Sheetfile" "RTC8088.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at -1.905 1.905) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.905 1.905) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz -2.54 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Battery_Holder_CR2032_Universal" (layer "F.Cu")
    (tedit 662AE319)
    (at 149.86 73.69302 -90)
    (descr "Battery Holder, CR2032, Through Hole, Universal")
    (tags "BATT HOLDER CR2032 TH")
    (property "Sheetfile" "RTC8088.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "BT1" (at -14.95552 -9.2075 180) (layer "F.SilkS"))
    (fp_text value "CR2032" (at -13.36802 -9.2075) (layer "F.SilkS"))
    (fp_text user "-" (at 5.9436 1.9812) (layer "F.SilkS"))
    (fp_text user "+" (at -13.9954 2.0066 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -14.00048 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 "Net-(BT1-Pad1)") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.99948 0 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Battery.3dshapes/BatteryHolder_Keystone_103_1x20mm.wrl"
      (offset (xyz -14.25 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 193.04 86.36) (end 193.04 94.615) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 193.04 94.615) (mid 192.854013 95.064013) (end 192.405 95.25) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 195.58 85.725) (mid 195.394013 86.174013) (end 194.945 86.36) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 194.945 86.36) (end 193.04 86.36) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 109.855 57.15) (end 194.945 57.15) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 111.76 86.36) (end 111.76 94.615) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 194.945 57.15) (mid 195.394013 57.335987) (end 195.58 57.785) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 195.58 57.785) (end 195.58 85.725) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 109.22 57.785) (mid 109.405987 57.335987) (end 109.855 57.15) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 112.395 95.25) (mid 111.945987 95.064013) (end 111.76 94.615) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 109.22 85.725) (end 109.22 57.785) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 111.76 86.36) (end 109.855 86.36) (layer "Edge.Cuts") (width 0.05))
  (gr_arc (start 109.855 86.36) (mid 109.405987 86.174013) (end 109.22 85.725) (layer "Edge.Cuts") (width 0.05))
  (gr_line (start 192.405 95.25) (end 112.395 95.25) (layer "Edge.Cuts") (width 0.05))
  (gr_text "Based on the previous work:\nSergey Kiselev - Xi 8088\nAitor Gómez García - RTC8088\nDr. Scott M. Baker - 8-bit ISA DiskOnChip / RTC board" (at 194.6275 83.185) (layer "B.SilkS"))
  (gr_text "Copyright (C) 2024 Sergey Kiselev\nCopyright (C) 2019 - 2021 Aitor Gómez García\n\nDesign files and documentation:\nhttps://github.com/spark2k06/RTC8088\n\nLicensed under CERN-OHL-S:\nhttps://cern-ohl.web.cern.ch" (at 194.6275 71.12) (layer "B.SilkS"))
  (gr_text "RTC8088 - Version 3.0" (at 194.6275 61.595) (layer "B.SilkS"))
  (gr_text "www.malinov.com" (at 177.165 83.82) (layer "F.SilkS"))
  (gr_text "Computer\nRear Side" (at 188.595 59.69) (layer "F.SilkS"))
  (gr_text "0x70:\n0x240:\n0x2A0:\n0x2C0:\n0x340:\n0x3A0:\n0x3C0:\nUSER:" (at 123.825 63.8175) (layer "F.SilkS"))
  (gr_text "OFF\nON\nOFF\nON\nOFF\nON\nOFF\nON\n" (at 129.54 63.8175) (layer "F.SilkS"))
  (gr_text "SC200" (at 189.23 83.82) (layer "F.SilkS"))
  (gr_text "OFF\nOFF\nOFF\nOFF\nON\nON\nON\nON" (at 135.89 63.8175) (layer "F.SilkS"))
  (gr_text "RTC8088 - Version 3.0\nCopyright (C) 2024 Sergey Kiselev\nCopyright (C) 2019 - 2021 Aitor Gómez García\n" (at 128.27 83.82) (layer "F.SilkS"))
  (gr_text "OFF\nOFF\nON\nON\nOFF\nOFF\nON\nON\n" (at 132.715 63.8175) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195.2625 57.785)
        (xy 195.2625 85.09)
        (xy 194.945 85.4075)
        (xy 109.855 85.4075)
        (xy 109.5375 85.09)
        (xy 109.5375 57.785)
        (xy 109.855 57.4675)
        (xy 194.945 57.4675)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 195.2625 57.785)
        (xy 195.2625 85.09)
        (xy 194.945 85.4075)
        (xy 109.855 85.4075)
        (xy 109.5375 85.09)
        (xy 109.5375 57.785)
        (xy 109.855 57.4675)
        (xy 194.945 57.4675)
      )
    )
  )
)
