(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 18)
    (tracks 14)
    (zones 0)
    (modules 5)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad8)")
  (net 2 "Net-(J1-Pad7)")
  (net 3 "Net-(J1-Pad6)")
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad4)")
  (net 6 "Net-(J1-Pad3)")
  (net 7 "Net-(J1-Pad2)")
  (net 8 "Net-(J1-Pad1)")
  (net 9 "Net-(J4-Pad8)")
  (net 10 "Net-(J4-Pad7)")
  (net 11 "Net-(J4-Pad6)")
  (net 12 "Net-(J4-Pad5)")
  (net 13 "Net-(J4-Pad4)")
  (net 14 "Net-(J4-Pad3)")
  (net 15 "Net-(J4-Pad2)")
  (net 16 "Net-(J4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad8)")
  )
  (module zotbins:zotbins_icon (layer F.Cu) (tedit 0)
    (at 147.32 93.98)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 158.75 83.82)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x08_Male (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J4-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J4-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal (layer F.Cu) (tedit 5B294EE5)
    (at 128.27 85.09 270)
    (descr "Terminal Block Phoenix MKDS-1,5-2, 2 pins, pitch 5mm, size 10x9.8mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/100425.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
    (tags "THT Terminal Block Phoenix MKDS-1,5-2 pitch 5mm size 10x9.8mm^2 drill 1.3mm pad 2.6mm")
    (fp_text reference J3 (at 2.5 -6.26 90) (layer Dwgs.User))
    (fp_text value Screw_Terminal_01x02 (at 2.5 5.66 90) (layer F.Fab))
    (fp_text user %R (at 2.5 3.2 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 5 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.6 2.6) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2_1x02_P5.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 151.13 83.82 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x04_Male (at 0 9.95 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 135.89 83.82)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x08_Male (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 11.43 (width 0.15) (layer Dwgs.User)
    (gr_text "11.430 mm" (at 156.24 94.615 270) (layer Dwgs.User))
    (feature1 (pts (xy 147.32 100.33) (xy 155.526421 100.33)))
    (feature2 (pts (xy 147.32 88.9) (xy 155.526421 88.9)))
    (crossbar (pts (xy 154.94 88.9) (xy 154.94 100.33)))
    (arrow1a (pts (xy 154.94 100.33) (xy 154.353579 99.203496)))
    (arrow1b (pts (xy 154.94 100.33) (xy 155.526421 99.203496)))
    (arrow2a (pts (xy 154.94 88.9) (xy 154.353579 90.026504)))
    (arrow2b (pts (xy 154.94 88.9) (xy 155.526421 90.026504)))
  )
  (dimension 10.16 (width 0.15) (layer Dwgs.User)
    (gr_text "10.160 mm" (at 147.32 99.09) (layer Dwgs.User))
    (feature1 (pts (xy 152.4 95.25) (xy 152.4 98.376421)))
    (feature2 (pts (xy 142.24 95.25) (xy 142.24 98.376421)))
    (crossbar (pts (xy 142.24 97.79) (xy 152.4 97.79)))
    (arrow1a (pts (xy 152.4 97.79) (xy 151.273496 98.376421)))
    (arrow1b (pts (xy 152.4 97.79) (xy 151.273496 97.203579)))
    (arrow2a (pts (xy 142.24 97.79) (xy 143.366504 98.376421)))
    (arrow2b (pts (xy 142.24 97.79) (xy 143.366504 97.203579)))
  )
  (gr_text GND (at 127 93.98) (layer F.SilkS))
  (gr_text 5V (at 128.27 81.28) (layer F.SilkS))
  (dimension 35.56 (width 0.12) (layer Dwgs.User)
    (gr_text "35.560 mm" (at 143.51 110.49) (layer Dwgs.User))
    (feature1 (pts (xy 161.29 104.14) (xy 161.29 109.806421)))
    (feature2 (pts (xy 125.73 104.14) (xy 125.73 109.806421)))
    (crossbar (pts (xy 125.73 109.22) (xy 161.29 109.22)))
    (arrow1a (pts (xy 161.29 109.22) (xy 160.163496 109.806421)))
    (arrow1b (pts (xy 161.29 109.22) (xy 160.163496 108.633579)))
    (arrow2a (pts (xy 125.73 109.22) (xy 126.856504 109.806421)))
    (arrow2b (pts (xy 125.73 109.22) (xy 126.856504 108.633579)))
  )
  (dimension 24.13 (width 0.12) (layer Dwgs.User)
    (gr_text "24.130 mm" (at 171.45 92.075 -90) (layer Dwgs.User))
    (feature1 (pts (xy 161.29 104.14) (xy 170.766421 104.14)))
    (feature2 (pts (xy 161.29 80.01) (xy 170.766421 80.01)))
    (crossbar (pts (xy 170.18 80.01) (xy 170.18 104.14)))
    (arrow1a (pts (xy 170.18 104.14) (xy 169.593579 103.013496)))
    (arrow1b (pts (xy 170.18 104.14) (xy 170.766421 103.013496)))
    (arrow2a (pts (xy 170.18 80.01) (xy 169.593579 81.136504)))
    (arrow2b (pts (xy 170.18 80.01) (xy 170.766421 81.136504)))
  )
  (gr_text Gnd (at 143.51 85.09 270) (layer F.SilkS))
  (gr_text Echo (at 146.05 85.09 -90) (layer F.SilkS))
  (gr_text Trig (at 148.59 85.09 -90) (layer F.SilkS))
  (gr_text 5V (at 151.13 85.09 270) (layer F.SilkS))
  (gr_text "Waste Watcher" (at 147.32 101.6) (layer F.SilkS))
  (gr_line (start 125.73 104.14) (end 125.73 80.01) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 161.29 104.14) (end 125.73 104.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 161.29 80.01) (end 161.29 104.14) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 125.73 80.01) (end 161.29 80.01) (layer Edge.Cuts) (width 0.05))
  (dimension 7.62 (width 0.15) (layer Dwgs.User)
    (gr_text "7.620 mm" (at 139.7 72.36) (layer Dwgs.User))
    (feature1 (pts (xy 143.51 83.82) (xy 143.51 73.073579)))
    (feature2 (pts (xy 135.89 83.82) (xy 135.89 73.073579)))
    (crossbar (pts (xy 135.89 73.66) (xy 143.51 73.66)))
    (arrow1a (pts (xy 143.51 73.66) (xy 142.383496 74.246421)))
    (arrow1b (pts (xy 143.51 73.66) (xy 142.383496 73.073579)))
    (arrow2a (pts (xy 135.89 73.66) (xy 137.016504 74.246421)))
    (arrow2b (pts (xy 135.89 73.66) (xy 137.016504 73.073579)))
  )
  (dimension 7.62 (width 0.15) (layer Dwgs.User)
    (gr_text "7.620 mm" (at 154.94 72.36) (layer Dwgs.User))
    (feature1 (pts (xy 158.75 83.82) (xy 158.75 73.073579)))
    (feature2 (pts (xy 151.13 83.82) (xy 151.13 73.073579)))
    (crossbar (pts (xy 151.13 73.66) (xy 158.75 73.66)))
    (arrow1a (pts (xy 158.75 73.66) (xy 157.623496 74.246421)))
    (arrow1b (pts (xy 158.75 73.66) (xy 157.623496 73.073579)))
    (arrow2a (pts (xy 151.13 73.66) (xy 152.256504 74.246421)))
    (arrow2b (pts (xy 151.13 73.66) (xy 152.256504 73.073579)))
  )
  (dimension 22.86 (width 0.15) (layer Dwgs.User)
    (gr_text "22.860 mm" (at 147.32 106.709999) (layer Dwgs.User))
    (feature1 (pts (xy 158.75 101.6) (xy 158.75 105.99642)))
    (feature2 (pts (xy 135.89 101.6) (xy 135.89 105.99642)))
    (crossbar (pts (xy 135.89 105.409999) (xy 158.75 105.409999)))
    (arrow1a (pts (xy 158.75 105.409999) (xy 157.623496 105.99642)))
    (arrow1b (pts (xy 158.75 105.409999) (xy 157.623496 104.823578)))
    (arrow2a (pts (xy 135.89 105.409999) (xy 137.016504 105.99642)))
    (arrow2b (pts (xy 135.89 105.409999) (xy 137.016504 104.823578)))
  )
)
