(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 43)
    (no_connects 0)
    (area 131.852099 83.453599 165.150101 126.552601)
    (thickness 1.6)
    (drawings 53)
    (tracks 133)
    (zones 0)
    (modules 16)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.27)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(1.5µF1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(1µF1-Pad1)")
  (net 4 "Net-(1µF1-Pad2)")
  (net 5 VDD)
  (net 6 "Net-(10KOhm1-Pad2)")
  (net 7 INT)
  (net 8 SCL)
  (net 9 SDA)
  (net 10 "Net-(>470OHM1-Pad2)")
  (net 11 "Net-(J1-Pad1)")
  (net 12 INT_B)
  (net 13 "Net-(J1-Pad3)")
  (net 14 "Net-(J1-Pad6)")
  (net 15 "Net-(J1-Pad7)")
  (net 16 "Net-(J1-Pad8)")
  (net 17 "Net-(J2-Pad3)")
  (net 18 "Net-(J2-Pad4)")
  (net 19 "Net-(J2-Pad5)")
  (net 20 AD_SELECT)
  (net 21 "Net-(U1-Pad1)")
  (net 22 "Net-(U1-Pad7)")
  (net 23 "Net-(U1-Pad8)")
  (net 24 "Net-(U1-Pad11)")
  (net 25 "Net-(U1-Pad14)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net AD_SELECT)
    (add_net GND)
    (add_net INT)
    (add_net INT_B)
    (add_net "Net-(1.5µF1-Pad1)")
    (add_net "Net-(10KOhm1-Pad2)")
    (add_net "Net-(1µF1-Pad1)")
    (add_net "Net-(1µF1-Pad2)")
    (add_net "Net-(>470OHM1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net SCL)
    (add_net SDA)
    (add_net VDD)
  )
  (module LOGO (layer F.Cu) (tedit 0)
    (at 148.59 115.57)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x07_Pitch2.54mm (layer F.Cu) (tedit 59119E4E)
    (at 159.893 100.711 168.9)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 168.9) (layer F.SilkS) hide)
    (fp_text value CONN_01X07 (at 0 17.57 168.9) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 168.9) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 168.9) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SCL))
    (pad 2 thru_hole oval (at 0 2.54 168.9) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SDA))
    (pad 3 thru_hole oval (at 0 5.08 168.9) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 168.9) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 168.9) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 168.9) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VDD))
    (pad 7 thru_hole oval (at 0 15.24 168.9) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59119E49)
    (at 156.718 90.805)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference 1.5µF1 (at 0 -1.5) (layer F.SilkS) hide)
    (fp_text value C_Small (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1.5µF1-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59119E24)
    (at 156.591 94.107 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference 1µF1 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value C_Small (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(1µF1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(1µF1-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59119E18)
    (at 149.86 99.568 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 10KOhm1 (at 0 -1.397 180) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.143 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(10KOhm1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59119E13)
    (at 142.875 99.06 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 10KOhm2 (at 0 -1.45 90) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.016 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 INT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59119E09)
    (at 140.208 89.027 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 10KOhm3 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59119E27)
    (at 143.383 88.773 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 10KOhm4 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value R (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59119E37)
    (at 154.813 88.773 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference 10µ11 (at 0 -1.5 90) (layer F.SilkS) hide)
    (fp_text value C_Small (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59119E3F)
    (at 156.591 96.901 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference 20Ohm1 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value R_Small (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.016 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(1µF1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 59119E0F)
    (at 141.351 99.06 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference >470OHM1 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value R_Small (at -0.127 1.27 270) (layer F.Fab))
    (fp_text user %R (at -0.127 -1.143 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 INT))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(>470OHM1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x10_Pitch2.54mm (layer F.Cu) (tedit 59119E44)
    (at 138.557 108.204 191.1)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 191.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X10 (at 0 25.19 191.1) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 191.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 191.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 191.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 INT_B))
    (pad 3 thru_hole oval (at 0 5.08 191.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 191.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SCL))
    (pad 5 thru_hole oval (at 0 10.16 191.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SDA))
    (pad 6 thru_hole oval (at 0 12.7 192.2) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 191.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 191.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 191.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 VDD))
    (pad 10 thru_hole oval (at 0 22.86 191.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x10_Pitch2.54mm.wrl
      (at (xyz 0 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 141.732 105.029 191.1)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP2 (at 0 -2.33 191.1) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87 191.1) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 191.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 191.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 INT_B))
    (pad 2 thru_hole oval (at 0 2.54 191.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(>470OHM1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module PROC_Grid_Eye:GridEyeSensor (layer B.Cu) (tedit 59119E33)
    (at 153.416 86.614 180)
    (fp_text reference AMG (at 4.064 1.143 180) (layer F.SilkS))
    (fp_text value AMG8834 (at 3.937 -12.7 360) (layer B.Fab))
    (pad 1 smd rect (at 7.127 -0.357 180) (size 3.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at 7.127 -2.927 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 SDA))
    (pad 3 smd rect (at 7.127 -4.197 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL))
    (pad 4 smd rect (at 7.127 -5.467 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 INT))
    (pad 5 smd rect (at 7.127 -6.737 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 AD_SELECT))
    (pad 6 smd rect (at 7.127 -8.007 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 7.127 -11.157 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 1.077 -11.157 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at 1.077 -8.007 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
    (pad 10 smd rect (at 1.077 -6.737 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(1µF1-Pad2)"))
    (pad 11 smd rect (at 1.077 -5.467 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 1.077 -4.197 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1.5µF1-Pad1)"))
    (pad 14 smd rect (at 1.077 -0.357 180) (size 2.64 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad14)"))
    (pad 13 smd rect (at 1.077 -2.927 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
  )
  (module PROC_Grid_Eye:GridEyeSensor (layer B.Cu) (tedit 56C2248B)
    (at 153.416 86.614 180)
    (fp_text reference U1 (at 3.683 2.659 180) (layer F.SilkS))
    (fp_text value AMG8834 (at 3.937 -14.089 360) (layer B.Fab))
    (pad 1 smd rect (at 7.127 -0.357 180) (size 3.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at 7.127 -2.927 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 SDA))
    (pad 3 smd rect (at 7.127 -4.197 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 SCL))
    (pad 4 smd rect (at 7.127 -5.467 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 INT))
    (pad 5 smd rect (at 7.127 -6.737 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 AD_SELECT))
    (pad 6 smd rect (at 7.127 -8.007 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 7.127 -11.157 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at 1.077 -11.157 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad8)"))
    (pad 9 smd rect (at 1.077 -8.007 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
    (pad 10 smd rect (at 1.077 -6.737 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(1µF1-Pad2)"))
    (pad 11 smd rect (at 1.077 -5.467 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at 1.077 -4.197 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(1.5µF1-Pad1)"))
    (pad 14 smd rect (at 1.077 -0.357 180) (size 2.64 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad14)"))
    (pad 13 smd rect (at 1.077 -2.927 180) (size 2.6 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 VDD))
  )
  (module SOLDER_JUMPER_3:SOLDER_JUMPER_3 (layer F.Cu) (tedit 5914C05E)
    (at 147.828 101.6 180)
    (fp_text reference JP1 (at 1.016 1.651 180) (layer F.SilkS))
    (fp_text value "Adress select" (at 0 -2 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 180) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(10KOhm1-Pad2)"))
    (pad 2 smd rect (at 0 0 180) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 20 AD_SELECT))
    (pad 3 smd rect (at 1.5 0 180) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (gr_text "By JanHenrik\n" (at 141.859 85.09) (layer F.SilkS))
  (gr_line (start 164.6011 83.5036) (end 132.4011 83.5036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.6637 83.5076) (end 164.6011 83.5036) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.7254 83.5193) (end 164.6637 83.5076) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.7851 83.5387) (end 164.7254 83.5193) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.842 83.5655) (end 164.7851 83.5387) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.895 83.5991) (end 164.842 83.5655) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.9434 83.6391) (end 164.895 83.5991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.9863 83.6849) (end 164.9434 83.6391) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.0232 83.7357) (end 164.9863 83.6849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.0535 83.7907) (end 165.0232 83.7357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.0766 83.8491) (end 165.0535 83.7907) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.0922 83.9099) (end 165.0766 83.8491) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.1001 83.9722) (end 165.0922 83.9099) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.1001 84.035) (end 165.1001 83.9722) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.0922 84.0973) (end 165.1001 84.035) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.98538 126.1279) (end 165.0922 84.0973) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.96597 126.1877) (end 156.98538 126.1279) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.93924 126.2445) (end 156.96597 126.1877) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.9056 126.2975) (end 156.93924 126.2445) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.86557 126.3459) (end 156.9056 126.2975) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.81981 126.3889) (end 156.86557 126.3459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.769 126.4257) (end 156.81981 126.3889) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.71398 126.456) (end 156.769 126.4257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.6556 126.4791) (end 156.71398 126.456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.59479 126.4947) (end 156.6556 126.4791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.53249 126.5026) (end 156.59479 126.4947) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.46971 126.5026) (end 156.53249 126.5026) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.40741 126.4947) (end 140.46971 126.5026) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.3466 126.4791) (end 140.40741 126.4947) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.28822 126.456) (end 140.3466 126.4791) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.2332 126.4257) (end 140.28822 126.456) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.18239 126.3889) (end 140.2332 126.4257) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.13663 126.3459) (end 140.18239 126.3889) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.0966 126.2975) (end 140.13663 126.3459) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.06296 126.2445) (end 140.0966 126.2975) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.03623 126.1877) (end 140.06296 126.2445) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 140.01682 126.1279) (end 140.03623 126.1877) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.91 84.0973) (end 140.01682 126.1279) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.9021 84.035) (end 131.91 84.0973) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.9021 83.9722) (end 131.9021 84.035) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.91 83.9099) (end 131.9021 83.9722) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.9256 83.8491) (end 131.91 83.9099) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.9487 83.7907) (end 131.9256 83.8491) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.979 83.7357) (end 131.9487 83.7907) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.0159 83.6849) (end 131.979 83.7357) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.0588 83.6391) (end 132.0159 83.6849) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.1072 83.5991) (end 132.0588 83.6391) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.1602 83.5655) (end 132.1072 83.5991) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.2171 83.5387) (end 132.1602 83.5655) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.2768 83.5193) (end 132.2171 83.5387) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.3385 83.5076) (end 132.2768 83.5193) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.4011 83.5036) (end 132.3385 83.5076) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.845 126.492) (xy 140.081 126.492) (xy 131.953 83.566) (xy 165.1 83.439)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.845 126.492) (xy 140.081 126.492) (xy 131.953 83.566) (xy 165.1 83.439)
      )
    )
  )
)
