<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>IN</text>
<text>OUT</text>
<text>GB</text>
<text>shop.catskull.net</text>
<text>SYNCMAP</text>
<text>LSDJ MIDI OUT</text>
<text>TX</text>
<text>RX</text>
<text>Arduinoboy</text>
<text>Developed by trash80 in California.
PCB and manufacturing by catskull.</text>
<text>2.0.1</text>
<text>PS/2</text>
<text>MODE</text>
<text>QC</text>
</plain>
<libraries>
<library name="optocoupler">
<description>&lt;b&gt;Opto Couplers&lt;/b&gt;&lt;p&gt;
Siemens, Hewlett-Packard, Texas Instuments, Sharp, Motorola&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="gm-diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="adafruit_modif">
<packages>
<package name="ARDUINO">
<description>&lt;b&gt;Arduino Uno&lt;/b&gt;
&lt;p&gt;
Make a shield with ease, this package has all the named pins as well as the two mounting drill holes and an outline of the USB and DC power connector. The outline is on the DIMENSION layer, so if your board house uses it they will cut the outline to match.</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="MIDI by Jazz">
<packages>
<package name="MIDI-DIN-5">
</package>
</packages>
</library>
<library name="mini_din">
<packages>
<package name="M_DIN6">
</package>
</packages>
</library>
<library name="Catskulls_link_port">
<packages>
<package name="GBA-LINK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="OK1" library="optocoupler" package="DIL08" value="6N138">
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO35-7" value="1N4148DO35-7"/>
<element name="MGB" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
</element>
<element name="NL" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
</element>
<element name="KB" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
</element>
<element name="MASTER" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
</element>
<element name="SLAVE" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
</element>
<element name="STATUS" library="gm-diodes" package="LED3MM" value="LED3MM">
<attribute name="NAME"/>
</element>
<element name="U$3" library="adafruit_modif" package="ARDUINO" value="ARDUINOUNO"/>
<element name="R4" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="270">
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="AXIAL-0.3" value="220">
<attribute name="VALUE"/>
</element>
<element name="S2" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="R6" library="SparkFun-Resistors" package="AXIAL-0.3" value="4.7k">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="MIDI by Jazz" package="MIDI-DIN-5" value="MIDI-DIN-5"/>
<element name="U$6" library="MIDI by Jazz" package="MIDI-DIN-5" value="MIDI-DIN-5"/>
<element name="X1" library="mini_din" package="M_DIN6" value="">
<attribute name="VALUE"/>
</element>
<element name="U$4" library="Catskulls_link_port" package="GBA-LINK" value="GBA-LINK"/>
</elements>
<signals>
<signal name="N$3">
</signal>
<signal name="PE">
</signal>
<signal name="VCC">
<contactref element="U$3" pad="5V"/>
<contactref element="R4" pad="P$2"/>
<contactref element="X1" pad="4"/>
<contactref element="U$4" pad="VCC"/>
<contactref element="U$4" pad="SD"/>
</signal>
<signal name="GND">
<contactref element="OK1" pad="5"/>
<contactref element="U$3" pad="GND"/>
<contactref element="R5" pad="P$1"/>
<contactref element="U$3" pad="GND1"/>
<contactref element="U$3" pad="GND2"/>
<contactref element="R6" pad="P$1"/>
<contactref element="U$2" pad="2"/>
<contactref element="X1" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="U$4" pad="GND"/>
</signal>
<signal name="N$1">
<contactref element="OK1" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="OK1" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="U$6" pad="5"/>
</signal>
<signal name="N$7">
<contactref element="U$3" pad="D1"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="OK1" pad="8"/>
<contactref element="U$3" pad="D4"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="OK1" pad="6"/>
<contactref element="U$3" pad="D0"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="3V">
<contactref element="U$3" pad="3V"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="P$1"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="U$3" pad="D8"/>
<contactref element="MGB" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="U$3" pad="D9"/>
<contactref element="NL" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="U$3" pad="D10"/>
<contactref element="KB" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="U$3" pad="D11"/>
<contactref element="MASTER" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="U$3" pad="D12"/>
<contactref element="SLAVE" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="U$3" pad="D13"/>
<contactref element="STATUS" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="MGB" pad="K"/>
<contactref element="R5" pad="P$2"/>
<contactref element="NL" pad="K"/>
<contactref element="KB" pad="K"/>
<contactref element="MASTER" pad="K"/>
<contactref element="SLAVE" pad="K"/>
<contactref element="STATUS" pad="K"/>
</signal>
<signal name="N$16">
<contactref element="R6" pad="P$2"/>
<contactref element="OK1" pad="7"/>
</signal>
<signal name="N$19">
<contactref element="R1" pad="P$2"/>
<contactref element="U$6" pad="4"/>
</signal>
<signal name="N$17">
<contactref element="U$3" pad="A0"/>
<contactref element="U$4" pad="SC"/>
</signal>
<signal name="N$21">
<contactref element="U$3" pad="A1"/>
<contactref element="U$4" pad="SO"/>
</signal>
<signal name="PE1">
<contactref element="X1" pad="SH1"/>
</signal>
<signal name="PE3">
<contactref element="X1" pad="SH3"/>
</signal>
<signal name="PE2">
<contactref element="X1" pad="SH2"/>
</signal>
<signal name="N$22">
<contactref element="U$3" pad="A2"/>
<contactref element="U$4" pad="SI"/>
</signal>
<signal name="PS2_CLK">
<contactref element="X1" pad="5"/>
<contactref element="U$3" pad="D3"/>
</signal>
<signal name="N$20">
<contactref element="S2" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="U$3" pad="D2"/>
</signal>
<signal name="PS2_DATA">
<contactref element="X1" pad="1"/>
<contactref element="U$3" pad="D7"/>
</signal>
<signal name="VIN">
<contactref element="U$3" pad="VIN"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
