(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C2-Pad2)")
  (net 3 "Net-(C4-Pad1)")
  (net 4 "ETH_GND")
  (net 5 "Net-(C5-Pad2)")
  (net 6 "Net-(C6-Pad1)")
  (net 7 "Net-(F1-Pad1)")
  (net 8 "Net-(J1-Pad1)")
  (net 9 "Net-(J1-Pad2)")
  (net 10 "Net-(J2-Pad1)")
  (net 11 "Net-(J2-Pad2)")
  (net 12 "Net-(J3-Pad1)")
  (net 13 "Net-(J3-Pad2)")
  (net 14 "Net-(J4-Pad1)")
  (net 15 "Net-(J5-Pad1)")
  (net 16 "SPI_SCK")
  (net 17 "COPI")
  (net 18 "Net-(J8-Pad1)")
  (net 19 "ETH_T+")
  (net 20 "ETH_T-")
  (net 21 "ETH_R+")
  (net 22 "ETH_R-")
  (net 23 "unconnected-(J9-Pad7)")
  (net 24 "ETH_LED")
  (net 25 "unconnected-(J9-Pad11)")
  (net 26 "unconnected-(J9-Pad12)")
  (net 27 "Net-(J10-Pad1)")
  (net 28 "Net-(J11-Pad1)")
  (net 29 "CIPO")
  (net 30 "CS")
  (net 31 "Net-(J14-Pad1)")
  (net 32 "Net-(J14-Pad2)")
  (net 33 "Net-(J14-Pad3)")
  (net 34 "Net-(J14-Pad4)")
  (net 35 "Net-(J14-Pad5)")
  (net 36 "Net-(J14-Pad6)")
  (net 37 "Net-(J14-Pad7)")
  (net 38 "Net-(J14-Pad8)")
  (net 39 "Net-(J14-Pad9)")
  (net 40 "Net-(J14-Pad10)")
  (net 41 "Net-(J14-Pad11)")
  (net 42 "Net-(J14-Pad13)")
  (net 43 "Net-(J14-Pad15)")
  (net 44 "Net-(J14-Pad16)")
  (net 45 "Net-(J14-Pad17)")
  (net 46 "Net-(J14-Pad18)")
  (net 47 "Net-(J14-Pad19)")
  (net 48 "Net-(J14-Pad20)")
  (net 49 "Net-(J14-Pad21)")
  (net 50 "Net-(J14-Pad22)")
  (net 51 "Net-(J14-Pad23)")
  (net 52 "Net-(J14-Pad24)")
  (net 53 "+3V3")
  (net 54 "Net-(J15-Pad4)")
  (net 55 "Net-(J15-Pad5)")
  (net 56 "Net-(J15-Pad6)")
  (net 57 "Net-(J15-Pad7)")
  (net 58 "Net-(J15-Pad8)")
  (net 59 "Net-(J15-Pad9)")
  (net 60 "Net-(J15-Pad10)")
  (net 61 "Net-(J15-Pad11)")
  (net 62 "Net-(J15-Pad12)")
  (net 63 "Net-(J15-Pad13)")
  (net 64 "Net-(J15-Pad14)")
  (net 65 "Net-(J15-Pad15)")
  (net 66 "Net-(J15-Pad16)")
  (net 67 "Net-(J15-Pad17)")
  (net 68 "Net-(J15-Pad18)")
  (net 69 "Net-(J15-Pad19)")
  (net 70 "Net-(J15-Pad20)")
  (net 71 "Net-(J15-Pad21)")
  (net 72 "Net-(J15-Pad22)")
  (net 73 "Net-(J15-Pad23)")
  (net 74 "Net-(J15-Pad24)")
  (net 75 "unconnected-(J16-Pad2)")
  (net 76 "Net-(R2-Pad2)")
  (net 77 "Net-(R3-Pad2)")
  (net 78 "Net-(R4-Pad1)")
  (net 79 "Net-(J17-Pad3)")
  (net 80 "Net-(J17-Pad4)")
  (net 81 "Net-(J17-Pad5)")
  (net 82 "Net-(J17-Pad6)")
  (net 83 "Net-(J17-Pad7)")
  (net 84 "Net-(J20-Pad2)")
  (net 85 "Net-(J20-Pad3)")
  (footprint "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm" (layer "F.Cu")
    (tedit 5DC5F6A3)
    (at 158.115 84.455 90)
    (descr "QFN, 24 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=278), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -3.3 90) (layer "F.SilkS"))
    (fp_text value "PCap04" (at 0 3.3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.65 -0.65 90) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 0.65 90) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at 0.65 -0.65 90) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.238095))
    (pad "" smd roundrect (at -0.65 0.65 90) (size 1.05 1.05) (layers "F.Paste") (roundrect_rratio 0.238095))
    (pad "1" smd roundrect (at -1.9375 -1.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(J3-Pad1)") (pinfunction "PC3") (pintype "input"))
    (pad "2" smd roundrect (at -1.9375 -0.75 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "ETH_GND") (pinfunction "GND") (pintype "input"))
    (pad "3" smd roundrect (at -1.9375 -0.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C2-Pad2)") (pinfunction "VDD18") (pintype "input"))
    (pad "4" smd roundrect (at -1.9375 0.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "+3V3") (pinfunction "VDD33") (pintype "input"))
    (pad "5" smd roundrect (at -1.9375 0.75 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(R2-Pad2)") (pinfunction "PT1") (pintype "input"))
    (pad "6" smd roundrect (at -1.9375 1.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R3-Pad2)") (pinfunction "PT0REF") (pintype "input"))
    (pad "7" smd roundrect (at -1.25 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C5-Pad2)") (pinfunction "PTOUT") (pintype "output"))
    (pad "8" smd roundrect (at -0.75 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "ETH_GND") (pinfunction "GND") (pintype "input"))
    (pad "9" smd roundrect (at -0.25 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "CS") (pinfunction "SSN_PG0") (pintype "input"))
    (pad "10" smd roundrect (at 0.25 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(R4-Pad1)") (pinfunction "MISO_PG1") (pintype "input"))
    (pad "11" smd roundrect (at 0.75 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(J11-Pad1)") (pinfunction "PG5") (pintype "input"))
    (pad "12" smd roundrect (at 1.25 1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(J10-Pad1)") (pinfunction "PG2") (pintype "input"))
    (pad "13" smd roundrect (at 1.9375 1.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J8-Pad1)") (pinfunction "IIC_EN") (pintype "input"))
    (pad "14" smd roundrect (at 1.9375 0.75 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "+3V3") (pinfunction "VDD33") (pintype "input"))
    (pad "15" smd roundrect (at 1.9375 0.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "COPI") (pinfunction "MOSI_SDA") (pintype "input"))
    (pad "16" smd roundrect (at 1.9375 -0.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "SPI_SCK") (pinfunction "SCK_SCL") (pintype "input"))
    (pad "17" smd roundrect (at 1.9375 -0.75 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J5-Pad1)") (pinfunction "PG3") (pintype "input"))
    (pad "18" smd roundrect (at 1.9375 -1.25 90) (size 0.825 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(J4-Pad1)") (pinfunction "PG4") (pintype "input"))
    (pad "19" smd roundrect (at 1.25 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)") (pinfunction "PCAUX") (pintype "input"))
    (pad "20" smd roundrect (at 0.75 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J1-Pad2)") (pinfunction "PC4") (pintype "input"))
    (pad "21" smd roundrect (at 0.25 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J1-Pad1)") (pinfunction "PC5") (pintype "input"))
    (pad "22" smd roundrect (at -0.25 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J2-Pad2)") (pinfunction "PC0") (pintype "input"))
    (pad "23" smd roundrect (at -0.75 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J2-Pad1)") (pinfunction "PC1") (pintype "input"))
    (pad "24" smd roundrect (at -1.25 -1.9375 90) (size 0.25 0.825) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J3-Pad2)") (pinfunction "PC2") (pintype "input"))
    (pad "25" smd rect (at 0 0 90) (size 2.6 2.6) (layers "F.Cu" "F.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 164.6975 92.075)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Digikey" "1292-0805N103J500CT-ND")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "10nF C0G" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "ETH_GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 5 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 163.195 66.675)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J6" (at 0 -2.25) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 16 "SPI_SCK") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 218.44 76.2 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J22" (at 1.27 10.795 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(J20-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(J20-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3V3") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 218.44 80.01 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J20" (at 0.635 10.795 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(J20-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(J20-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3V3") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 217.17 89.535)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at -3.81 0 90) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 154.305 71.465)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J7" (at 0 -2.25) (layer "F.SilkS"))
    (fp_text value "con" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 17 "COPI") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Axial_L5.1mm_D3.1mm_P12.50mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 169.445 56.515 180)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=12.5mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 12.5mm  length 5.1mm diameter 3.1mm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 14.505 0) (layer "F.SilkS"))
    (fp_text value "0F" (at 6.25 2.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.25 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P12.50mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 217.17 59.055)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 163.195 71.465)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J11" (at 0 -2.25) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 28 "Net-(J11-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 147.32 111.125)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 197.485 55.88)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J15" (at 3.175 -0.635) (layer "F.SilkS"))
    (fp_text value "Conn_01x24" (at 0 60.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 29.21 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(F1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3V3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Net-(J15-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 55 "Net-(J15-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 56 "Net-(J15-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "Net-(J15-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 58 "Net-(J15-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "Net-(J15-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 60 "Net-(J15-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "Net-(J15-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 62 "Net-(J15-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 "Net-(J15-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "Net-(J15-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "Net-(J15-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 "Net-(J15-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(J15-Pad17)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J15-Pad18)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J15-Pad19)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J15-Pad20)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 71 "Net-(J15-Pad21)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 72 "Net-(J15-Pad22)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 73 "Net-(J15-Pad23)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at 0 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(J15-Pad24)") (pinfunction "Pin_24") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm" (layer "F.Cu")
    (tedit 5C745284)
    (at 161.29 78.12 90)
    (descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "net tie solder jumper bridged")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP1" (at 0.015 1.905 90) (layer "F.SilkS"))
    (fp_text value "SolderJumper_2_Bridged" (at 0 1.9 90) (layer "F.Fab"))
    (pad "1" smd custom (at -0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 18 "Net-(J8-Pad1)") (pinfunction "A") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0.5 0.75)
            (xy 0 0.75)
            (xy 0 -0.75)
            (xy 0.5 -0.75)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.65 0 90) (size 1 0.5) (layers "F.Cu" "F.Mask")
      (net 4 "ETH_GND") (pinfunction "B") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_circle (center 0 0.25) (end 0.5 0.25) (width 0) (fill yes))
        (gr_circle (center 0 -0.25) (end 0.5 -0.25) (width 0) (fill yes))
        (gr_poly (pts
            (xy 0 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0 -0.75)
          ) (width 0) (fill yes))
      ))
  )
  (footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 210.185 90.17 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 1.25 -2.05 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 1.25 2.05 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 169.545 86.36)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J12" (at 0 -2.25) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 29 "CIPO") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 154.305 66.675)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J4" (at 0 -2.25) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 14 "Net-(J4-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 207.645 73.66 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Digikey" "1276-3063-1-ND")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.905 90) (layer "F.SilkS"))
    (fp_text value "47uF" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 6 "Net-(C6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "ETH_GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 165.735 96.52 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=1.9mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 1.9mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Digikey" "TT-PT-1000A-2050-11-AUNI-ND")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 0.95 -1.92) (layer "F.SilkS"))
    (fp_text value "1k RTD" (at 0.95 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.95 -1.92) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.9 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 76 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P1.90mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_2-G-3.81_1x02_P3.81mm_Vertical" (layer "F.Cu")
    (tedit 5B784ED1)
    (at 148.59 90.17 90)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-3.81; number of pins: 02; pin pitch: 3.81mm; Vertical || order number: 1803426 8A 160V")
    (tags "phoenix_contact connector MCV_01x02_G_3.81mm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -1.905 4.445 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 1.9 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.9 -3.55 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 10 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 3.81 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_2-G-3.81_1x02_P3.81mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 169.545 102.235 90)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Digikey" "273-MOX70031001BZE-ND")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 8.255 -2.54 90) (layer "F.SilkS"))
    (fp_text value "1k" (at 9.525 2.72 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 9.525 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 171.45 106.045 -90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J17" (at -2.54 12.7 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x08" (at 0 20.11 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(J17-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J17-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(J17-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(J17-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(J17-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3V3") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 158.75 71.465)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J10" (at 0 -2.25) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 27 "Net-(J10-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 156.845 91.0375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Digikey" "399-C0805C475K4RAC7210CT-ND")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "ETH_GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 2 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 167.64 71.465)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J13" (at 0 -2.25) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 30 "CS") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 169.545 60.96 180)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 15.24 0) (layer "F.SilkS"))
    (fp_text value "1k" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Teensy:Teensy41" (layer "F.Cu")
    (tedit 5FD6DEAD)
    (at 185.9788 85.09 -90)
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0 -10.16 90) (layer "F.SilkS"))
    (fp_text value "Teensy4.1" (at 0 10.16 90) (layer "F.Fab"))
    (fp_text user "Ethernet" (at -12.065 -3.2766) (layer "F.SilkS"))
    (fp_text user "USB" (at -26.67 0) (layer "F.SilkS"))
    (fp_text user "Micro SD" (at 24.13 0 90) (layer "F.SilkS"))
    (pad "1" thru_hole rect (at -29.21 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 31 "Net-(J14-Pad1)") (pinfunction "GND") (pintype "power_in"))
    (pad "2" thru_hole circle (at -26.67 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 32 "Net-(J14-Pad2)") (pinfunction "0_RX1_CRX2_CS1") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at -24.13 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 "Net-(J14-Pad3)") (pinfunction "1_TX1_CTX2_MISO1") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at -21.59 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 34 "Net-(J14-Pad4)") (pinfunction "2_OUT2") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at -19.05 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 "Net-(J14-Pad5)") (pinfunction "3_LRCLK2") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at -16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 "Net-(J14-Pad6)") (pinfunction "4_BCLK2") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at -13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(J14-Pad7)") (pinfunction "5_IN2") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at -11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(J14-Pad8)") (pinfunction "6_OUT1D") (pintype "bidirectional"))
    (pad "9" thru_hole circle (at -8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 "Net-(J14-Pad9)") (pinfunction "7_RX2_OUT1A") (pintype "bidirectional"))
    (pad "10" thru_hole circle (at -6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 "Net-(J14-Pad10)") (pinfunction "8_TX2_IN1") (pintype "bidirectional"))
    (pad "11" thru_hole circle (at -3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 41 "Net-(J14-Pad11)") (pinfunction "9_OUT1C") (pintype "bidirectional"))
    (pad "12" thru_hole circle (at -1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 30 "CS") (pinfunction "10_CS_MQSR") (pintype "bidirectional"))
    (pad "13" thru_hole circle (at 1.27 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 42 "Net-(J14-Pad13)") (pinfunction "11_MOSI_CTX1") (pintype "bidirectional"))
    (pad "14" thru_hole circle (at 3.81 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 29 "CIPO") (pinfunction "12_MISO_MQSL") (pintype "bidirectional"))
    (pad "15" thru_hole circle (at 6.35 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 43 "Net-(J14-Pad15)") (pinfunction "3V3") (pintype "power_in"))
    (pad "16" thru_hole circle (at 8.89 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 44 "Net-(J14-Pad16)") (pinfunction "24_A10_TX6_SCL2") (pintype "bidirectional"))
    (pad "17" thru_hole circle (at 11.43 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 45 "Net-(J14-Pad17)") (pinfunction "25_A11_RX6_SDA2") (pintype "bidirectional"))
    (pad "18" thru_hole circle (at 13.97 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 46 "Net-(J14-Pad18)") (pinfunction "26_A12_MOSI1") (pintype "bidirectional"))
    (pad "19" thru_hole circle (at 16.51 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 47 "Net-(J14-Pad19)") (pinfunction "27_A13_SCK1") (pintype "bidirectional"))
    (pad "20" thru_hole circle (at 19.05 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 48 "Net-(J14-Pad20)") (pinfunction "28_RX7") (pintype "bidirectional"))
    (pad "21" thru_hole circle (at 21.59 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 49 "Net-(J14-Pad21)") (pinfunction "29_TX7") (pintype "bidirectional"))
    (pad "22" thru_hole circle (at 24.13 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 50 "Net-(J14-Pad22)") (pinfunction "30_CRX3") (pintype "bidirectional"))
    (pad "23" thru_hole circle (at 26.67 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "Net-(J14-Pad23)") (pinfunction "31_CTX3") (pintype "bidirectional"))
    (pad "24" thru_hole circle (at 29.21 7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 52 "Net-(J14-Pad24)") (pinfunction "32_OUT1B") (pintype "bidirectional"))
    (pad "25" thru_hole circle (at 29.21 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 "Net-(J15-Pad24)") (pinfunction "33_MCLK2") (pintype "bidirectional"))
    (pad "26" thru_hole circle (at 26.67 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 73 "Net-(J15-Pad23)") (pinfunction "34_RX8") (pintype "bidirectional"))
    (pad "27" thru_hole circle (at 24.13 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 72 "Net-(J15-Pad22)") (pinfunction "35_TX8") (pintype "bidirectional"))
    (pad "28" thru_hole circle (at 21.59 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 71 "Net-(J15-Pad21)") (pinfunction "36_CS") (pintype "bidirectional"))
    (pad "29" thru_hole circle (at 19.05 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 70 "Net-(J15-Pad20)") (pinfunction "37_CS") (pintype "bidirectional"))
    (pad "30" thru_hole circle (at 16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 69 "Net-(J15-Pad19)") (pinfunction "38_CS1_IN1") (pintype "bidirectional"))
    (pad "31" thru_hole circle (at 13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 68 "Net-(J15-Pad18)") (pinfunction "39_MISO1_OUT1A") (pintype "bidirectional"))
    (pad "32" thru_hole circle (at 11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 67 "Net-(J15-Pad17)") (pinfunction "40_A16") (pintype "bidirectional"))
    (pad "33" thru_hole circle (at 8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 "Net-(J15-Pad16)") (pinfunction "41_A17") (pintype "bidirectional"))
    (pad "34" thru_hole circle (at 6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 "Net-(J15-Pad15)") (pinfunction "GND") (pintype "power_in"))
    (pad "35" thru_hole circle (at 3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 64 "Net-(J15-Pad14)") (pinfunction "13_SCK_LED") (pintype "bidirectional"))
    (pad "36" thru_hole circle (at 1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 63 "Net-(J15-Pad13)") (pinfunction "14_A0_TX3_SPDIF_OUT") (pintype "bidirectional"))
    (pad "37" thru_hole circle (at -1.27 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 62 "Net-(J15-Pad12)") (pinfunction "15_A1_RX3_SPDIF_IN") (pintype "bidirectional"))
    (pad "38" thru_hole circle (at -3.81 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 61 "Net-(J15-Pad11)") (pinfunction "16_A2_RX4_SCL1") (pintype "bidirectional"))
    (pad "39" thru_hole circle (at -6.35 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 60 "Net-(J15-Pad10)") (pinfunction "17_A3_TX4_SDA1") (pintype "bidirectional"))
    (pad "40" thru_hole circle (at -8.89 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 59 "Net-(J15-Pad9)") (pinfunction "18_A4_SDA") (pintype "bidirectional"))
    (pad "41" thru_hole circle (at -11.43 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 58 "Net-(J15-Pad8)") (pinfunction "19_A5_SCL") (pintype "bidirectional"))
    (pad "42" thru_hole circle (at -13.97 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 57 "Net-(J15-Pad7)") (pinfunction "20_A6_TX5_LRCLK1") (pintype "bidirectional"))
    (pad "43" thru_hole circle (at -16.51 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 56 "Net-(J15-Pad6)") (pinfunction "21_A7_RX5_BCLK1") (pintype "bidirectional"))
    (pad "44" thru_hole circle (at -19.05 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 55 "Net-(J15-Pad5)") (pinfunction "22_A8_CTX1") (pintype "bidirectional"))
    (pad "45" thru_hole circle (at -21.59 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 54 "Net-(J15-Pad4)") (pinfunction "23_A9_CRX1_MCLK1") (pintype "bidirectional"))
    (pad "46" thru_hole circle (at -24.13 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 53 "+3V3") (pinfunction "3V3") (pintype "output"))
    (pad "47" thru_hole circle (at -26.67 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "GND") (pintype "output"))
    (pad "48" thru_hole circle (at -29.21 -7.62 270) (size 1.6 1.6) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 "Net-(F1-Pad1)") (pinfunction "VIN") (pintype "power_in"))
    (pad "60" thru_hole rect (at -16.24 -5.1816 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "ETH_R+") (pinfunction "R+") (pintype "bidirectional"))
    (pad "61" thru_hole circle (at -16.24 -3.1816 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "ETH_LED") (pinfunction "LED") (pintype "bidirectional"))
    (pad "62" thru_hole circle (at -16.24 -1.1816 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "ETH_T-") (pinfunction "T-") (pintype "bidirectional"))
    (pad "63" thru_hole circle (at -14.24 -1.1816 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "ETH_T+") (pinfunction "T+") (pintype "bidirectional"))
    (pad "64" thru_hole circle (at -14.24 -3.1816 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "GND") (pintype "power_in"))
    (pad "65" thru_hole circle (at -14.24 -5.1816 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "ETH_R-") (pinfunction "R-") (pintype "bidirectional"))
    (model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.1_Assembly.STEP"
      (offset (xyz 0 0 0.762))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 165.465 86.36)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "22" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 78 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 29 "CIPO") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 158.75 66.675)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J5" (at 0 -2.25) (layer "F.SilkS"))
    (fp_text value "con" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 15 "Net-(J5-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 189.5 88.9 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "22" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 64 "Net-(J15-Pad14)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 16 "SPI_SCK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_BarrelJack:BarrelJack_Horizontal" (layer "F.Cu")
    (tedit 5A1DBF6A)
    (at 208.28 67.945 -90)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (property "Digikey" "CP-002A-ND")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J16" (at -8.45 5.75 90) (layer "F.SilkS"))
    (fp_text value "Barrel_Jack_Switch_Pin3Ring" (at -6.2 -5.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3 -2.95 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3.5 3.5) (drill oval 1 3) (layers *.Cu *.Mask)
      (net 6 "Net-(C6-Pad1)") (pintype "passive"))
    (pad "2" thru_hole roundrect (at -6 0 270) (size 3 3.5) (drill oval 1 3) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 75 "unconnected-(J16-Pad2)") (pintype "passive"))
    (pad "3" thru_hole roundrect (at -3 4.7 270) (size 3.5 3.5) (drill oval 3 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 "ETH_GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 171.45 109.855 -90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J18" (at -6.35 9.525 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x08" (at 0 20.11 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(J17-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J17-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(J17-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(J17-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(J17-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3V3") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x24_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 174.625 55.88)
    (descr "Through hole straight pin header, 1x24, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x24 2.54mm single row")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J14" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x24" (at 0 60.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 29.21 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J14-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J14-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J14-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J14-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J14-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J14-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J14-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J14-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J14-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J14-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J14-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "CS") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J14-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "CIPO") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J14-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J14-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J14-Pad17)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J14-Pad18)") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 45.72) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J14-Pad19)") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at 0 48.26) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "Net-(J14-Pad20)") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 50.8) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J14-Pad21)") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at 0 53.34) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "Net-(J14-Pad22)") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 55.88) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "Net-(J14-Pad23)") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at 0 58.42) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "Net-(J14-Pad24)") (pinfunction "Pin_24") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x24_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_2-G-3.81_1x02_P3.81mm_Vertical" (layer "F.Cu")
    (tedit 5B784ED1)
    (at 148.59 100.965 90)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-3.81; number of pins: 02; pin pitch: 3.81mm; Vertical || order number: 1803426 8A 160V")
    (tags "phoenix_contact connector MCV_01x02_G_3.81mm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -1.905 4.445 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 1.9 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.9 -3.55 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 12 "Net-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 3.81 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_2-G-3.81_1x02_P3.81mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 147.32 59.055)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.115 77.2 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "22" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 17 "COPI") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333)
      (net 42 "Net-(J14-Pad13)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 218.44 83.82 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J21" (at 0.635 10.795 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x04" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "Net-(J20-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 85 "Net-(J20-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3V3") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 171.45 113.665 -90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J19" (at -10.16 6.35 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x08" (at 0 20.11 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 "Net-(J17-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 80 "Net-(J17-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(J17-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 82 "Net-(J17-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 83 "Net-(J17-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "+3V3") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_RJ:RJ45_Cetus_J1B1211CCD_Horizontal" (layer "F.Cu")
    (tedit 5BBCB15F)
    (at 205.74 98.325)
    (descr "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, Cetus, used and distributed by WIZnet (https://wizwiki.net/wiki/lib/exe/fetch.php?media=products:wiz550web:wiz550webds_kr:j1b1211ccd.pdf)")
    (tags "RJ45 Magjack")
    (property "Digikey" "1278-1052-ND")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 5 -5) (layer "F.SilkS"))
    (fp_text value "RJ45_LED" (at 4.445 18) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4 16) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 10.16 6.35) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -1.27 6.35) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad "1" thru_hole roundrect (at 0 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask) (roundrect_rratio 0.167)
      (net 19 "ETH_T+") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.27 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "3" thru_hole circle (at 2.54 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "ETH_T-") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.81 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 "ETH_R+") (pintype "passive"))
    (pad "5" thru_hole circle (at 5.08 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "6" thru_hole circle (at 6.35 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "ETH_R-") (pintype "passive"))
    (pad "7" thru_hole circle (at 7.62 0) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 "unconnected-(J9-Pad7)") (pintype "passive"))
    (pad "8" thru_hole circle (at 8.89 -2.54) (size 1.5 1.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pintype "passive"))
    (pad "9" thru_hole circle (at -1.88 11.43) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 4 "ETH_GND") (pintype "passive"))
    (pad "10" thru_hole circle (at 0.66 9.73) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 24 "ETH_LED") (pintype "passive"))
    (pad "11" thru_hole circle (at 8.23 11.43) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 25 "unconnected-(J9-Pad11)") (pintype "passive"))
    (pad "12" thru_hole circle (at 10.77 9.73) (size 1.5 1.5) (drill 1.02) (layers *.Cu *.Mask)
      (net 26 "unconnected-(J9-Pad12)") (pintype "passive"))
    (pad "13" thru_hole circle (at 12.32 3.3) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (pad "13" thru_hole circle (at -3.43 3.3) (size 2.5 2.5) (drill 1.6) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Cetus_J1B1211CCD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric_Pad1.42x1.75mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 202.565 73.735 -90)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse handsolder")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at -0.075 1.905 90) (layer "F.SilkS"))
    (fp_text value "Polyfuse 500mA" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 7 "Net-(F1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.175439)
      (net 6 "Net-(C6-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (tedit 5EB70B43)
    (at 167.64 66.675)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "J8" (at 0 -2.25) (layer "F.SilkS"))
    (fp_text value "Conn_01x01_Male" (at 0 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2.1 2.1) (drill 1.1) (layers *.Cu *.Mask) (roundrect_rratio 0.119048)
      (net 18 "Net-(J8-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Phoenix_MC:PhoenixContact_MCV_1,5_2-G-3.81_1x02_P3.81mm_Vertical" (layer "F.Cu")
    (tedit 5B784ED1)
    (at 148.6075 79.3825 90)
    (descr "Generic Phoenix Contact connector footprint for: MCV_1,5/2-G-3.81; number of pins: 02; pin pitch: 3.81mm; Vertical || order number: 1803426 8A 160V")
    (tags "phoenix_contact connector MCV_01x02_G_3.81mm")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -1.8975 4.4275 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x02" (at 1.9 4.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.9 -3.55 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask) (roundrect_rratio 0.138889)
      (net 8 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 3.81 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MCV_1,5_2-G-3.81_1x02_P3.81mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 165.1 81.0475 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Digikey" "1276-1764-1-ND")
    (property "Sheetfile" "TeensyPicoCap4.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 4 "ETH_GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.212766)
      (net 53 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 220.98 116.84) (end 143.51 116.84) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 143.51 53.34) (end 220.98 53.34) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 220.98 53.34) (end 220.98 116.84) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 143.51 116.84) (end 143.51 53.34) (layer "Edge.Cuts") (width 0.1))
  (gr_text "PC0/1" (at 153.035 87.63 90) (layer "F.SilkS"))
  (gr_text "PC4/5" (at 153.035 77.47 90) (layer "F.SilkS"))
  (gr_text "5V" (at 215.265 65.405) (layer "F.SilkS"))
  (gr_text "GND" (at 168.91 115.57) (layer "F.SilkS"))
  (gr_text "B" (at 215.9 73.66 90) (layer "F.SilkS"))
  (gr_text "GND" (at 218.44 73.025 90) (layer "F.SilkS"))
  (gr_text "PCAUX" (at 152.4 59.055 90) (layer "F.SilkS"))
  (gr_text "PC2/3" (at 153.035 99.06 90) (layer "F.SilkS"))
  (gr_text "A" (at 213.36 73.66 90) (layer "F.SilkS"))
  (gr_text "PicoCap4\nV1" (at 146.05 67.31 90) (layer "F.SilkS"))
  (gr_text "3V3" (at 153.67 116.205) (layer "F.SilkS"))
  (gr_text "3V3" (at 210.82 73.025 90) (layer "F.SilkS"))
  (gr_text "GND" (at 171.45 115.57) (layer "F.SilkS"))
  (zone (net 4) (net_name "ETH_GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 220.345 116.205)
        (xy 167.005 116.205)
        (xy 167.005 102.87)
        (xy 152.4 102.87)
        (xy 152.4 69.85)
        (xy 172.085 69.85)
        (xy 172.085 63.5)
        (xy 165.735 63.5)
        (xy 165.735 53.975)
        (xy 220.345 53.975)
      )
    )
  )
)
