(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 28)
    (zones 0)
    (modules 2)
    (nets 7)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 TCK)
  (net 3 GND)
  (net 4 TDI)
  (net 5 TDO)
  (net 6 TMS)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net TCK)
    (add_net TDI)
    (add_net TDO)
    (add_net TMS)
    (add_net VCC)
  )
  (module Connector_PinHeader_1.00mm:PinHeader_2x03_P1.00mm_Vertical_SMD (layer B.Cu) (tedit 5C590E0F)
    (at 176.022 84.575001)
    (descr "surface-mounted straight pin header, 2x03, 1.00mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 1.00mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 2.56) (layer B.SilkS) hide)
    (fp_text value Conn_02x03_Odd_Even (at 0 -2.56) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 1 smd rect (at -1.65 1) (size 2 0.5) (layers B.Cu B.Paste B.Mask)
      (net 5 TDO))
    (pad 2 smd rect (at 1.65 1) (size 2 0.5) (layers B.Cu B.Paste B.Mask)
      (net 6 TMS))
    (pad 3 smd rect (at -1.65 0) (size 2 0.5) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 1.65 0) (size 2 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 TDI))
    (pad 5 smd rect (at -1.65 -1) (size 2 0.5) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 6 smd rect (at 1.65 -1) (size 2 0.5) (layers B.Cu B.Paste B.Mask)
      (net 2 TCK))
    (model ${KISYS3DMOD}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_2x03_P1.00mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 5C590DF1)
    (at 176.022 84.582)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 -4.87) (layer F.SilkS) hide)
    (fp_text value Conn_02x03_Odd_Even (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 2.525 -2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 2 TCK))
    (pad 3 smd rect (at -2.525 0) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 2.525 0) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 4 TDI))
    (pad 5 smd rect (at -2.525 2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 5 TDO))
    (pad 6 smd rect (at 2.525 2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 6 TMS))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 168.91 89.662) (end 168.91 79.502) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.134 89.662) (end 168.91 89.662) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.134 79.502) (end 183.134 89.662) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.91 79.502) (end 183.134 79.502) (layer Edge.Cuts) (width 0.15))
  (gr_text SDCARD (at 176.022 89.027) (layer F.SilkS))
  (gr_text USB (at 176.022 80.264) (layer F.SilkS))
  (gr_text VCC (at 171.704 82.042) (layer F.SilkS))
  (gr_text GND (at 171.704 84.582) (layer F.SilkS))
  (gr_text TDO (at 171.704 87.122) (layer F.SilkS))
  (gr_text TMS (at 180.34 87.122) (layer F.SilkS))
  (gr_text TDI (at 180.34 84.582) (layer F.SilkS))
  (gr_text TCK (at 180.34 82.042) (layer F.SilkS))
)
