(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 6)
    (tracks 101)
    (zones 0)
    (modules 2)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.35)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(X1-Pad1)")
  (net 2 "Net-(X1-Pad2)")
  (net 3 "Net-(X1-Pad3)")
  (net 4 "Net-(X1-Pad4)")
  (net 5 "Net-(X1-Pad5)")
  (net 6 "Net-(X1-Pad6)")
  (net 7 "Net-(X1-Pad7)")
  (net 8 "Net-(X1-Pad8)")
  (net 9 "Net-(X1-Pad9)")
  (net 10 "Net-(X1-Pad10)")
  (net 11 "Net-(X1-Pad11)")
  (net 12 "Net-(X1-Pad12)")
  (net 13 "Net-(X1-Pad13)")
  (net 14 "Net-(X1-Pad14)")
  (net 15 "Net-(X1-Pad15)")
  (net 16 "Net-(X1-Pad16)")
  (net 17 "Net-(X1-Pad17)")
  (net 18 "Net-(X1-Pad18)")
  (net 19 "Net-(X1-Pad19)")
  (net 20 "Net-(X1-Pad20)")
  (net 21 "Net-(X1-Pad21)")
  (net 22 "Net-(X1-Pad22)")
  (net 23 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(X1-Pad1)")
    (add_net "Net-(X1-Pad10)")
    (add_net "Net-(X1-Pad11)")
    (add_net "Net-(X1-Pad12)")
    (add_net "Net-(X1-Pad13)")
    (add_net "Net-(X1-Pad14)")
    (add_net "Net-(X1-Pad15)")
    (add_net "Net-(X1-Pad16)")
    (add_net "Net-(X1-Pad17)")
    (add_net "Net-(X1-Pad18)")
    (add_net "Net-(X1-Pad19)")
    (add_net "Net-(X1-Pad2)")
    (add_net "Net-(X1-Pad20)")
    (add_net "Net-(X1-Pad21)")
    (add_net "Net-(X1-Pad22)")
    (add_net "Net-(X1-Pad3)")
    (add_net "Net-(X1-Pad4)")
    (add_net "Net-(X1-Pad5)")
    (add_net "Net-(X1-Pad6)")
    (add_net "Net-(X1-Pad7)")
    (add_net "Net-(X1-Pad8)")
    (add_net "Net-(X1-Pad9)")
  )
  (module Connector_FFC-FPC:TE_2-84953-2_1x22-1MP_P1.0mm_Horizontal (layer F.Cu) (tedit 5AEE14E3)
    (at 148.58243 99.862898)
    (descr "TE FPC connector, 22 top-side contacts, 1.0mm pitch, 1.0mm height, SMT, http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=84953&DocType=Customer+Drawing&DocLang=English&DocFormat=pdf&PartCntxt=84953-4")
    (tags "te fpc 84953")
    (attr smd)
    (fp_text reference X1 (at 0.00508 1.89738) (layer F.SilkS))
    (fp_text value "Molex 52207-2233" (at 0.42926 3.24866) (layer F.Fab))
    (fp_text user %R (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -10.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(X1-Pad1)"))
    (pad 2 smd rect (at -9.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(X1-Pad2)"))
    (pad 3 smd rect (at -8.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(X1-Pad3)"))
    (pad 4 smd rect (at -7.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(X1-Pad4)"))
    (pad 5 smd rect (at -6.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(X1-Pad5)"))
    (pad 6 smd rect (at -5.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(X1-Pad6)"))
    (pad 7 smd rect (at -4.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(X1-Pad7)"))
    (pad 8 smd rect (at -3.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(X1-Pad8)"))
    (pad 9 smd rect (at -2.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(X1-Pad9)"))
    (pad 10 smd rect (at -1.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(X1-Pad10)"))
    (pad 11 smd rect (at -0.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(X1-Pad11)"))
    (pad 12 smd rect (at 0.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(X1-Pad12)"))
    (pad 13 smd rect (at 1.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(X1-Pad13)"))
    (pad 14 smd rect (at 2.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(X1-Pad14)"))
    (pad 15 smd rect (at 3.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(X1-Pad15)"))
    (pad 16 smd rect (at 4.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(X1-Pad16)"))
    (pad 17 smd rect (at 5.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(X1-Pad17)"))
    (pad 18 smd rect (at 6.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(X1-Pad18)"))
    (pad 19 smd rect (at 7.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(X1-Pad19)"))
    (pad 20 smd rect (at 8.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(X1-Pad20)"))
    (pad 21 smd rect (at 9.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(X1-Pad21)"))
    (pad 22 smd rect (at 10.5 -1.8) (size 0.61 2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(X1-Pad22)"))
    (pad MP smd rect (at -13.49 1) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask)
      (net 23 GND))
    (pad MP smd rect (at 13.49 1) (size 2.68 3.6) (layers F.Cu F.Paste F.Mask)
      (net 23 GND))
    (model ${KISYS3DMOD}/Connector_FFC-FPC.3dshapes/TE_2-84953-2_1x22-1MP_P1.0mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x11_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 134.92231 94.693998 90)
    (descr "Through hole straight pin header, 2x11, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x11 2.54mm double row")
    (fp_text reference X2 (at -2.88798 -0.81534 90) (layer F.SilkS))
    (fp_text value Conn_01x22 (at 0.04318 28.23718 90) (layer F.Fab))
    (fp_text user %R (at -2.87782 -0.80772 -90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(X1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(X1-Pad2)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(X1-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(X1-Pad4)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(X1-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(X1-Pad6)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(X1-Pad7)"))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(X1-Pad8)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(X1-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(X1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(X1-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(X1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(X1-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(X1-Pad14)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(X1-Pad15)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(X1-Pad16)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(X1-Pad17)"))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(X1-Pad18)"))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(X1-Pad19)"))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(X1-Pad20)"))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(X1-Pad21)"))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(X1-Pad22)"))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x11_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text llg.cubic.org (at 149.21235 97.973138) (layer B.Mask))
  (gr_text "22pin FPC/FFC Adapter" (at 148.61037 101.424998) (layer B.Mask))
  (gr_line (start 164.04595 90.342978) (end 164.04595 104.635558) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.12145 90.342978) (end 164.04595 90.342978) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.12145 104.633018) (end 133.12145 90.342978) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.04595 104.633018) (end 133.12145 104.633018) (layer Edge.Cuts) (width 0.15))
  (zone (net 23) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163.97229 90.416638) (xy 163.97229 104.559358) (xy 133.19511 104.559358) (xy 133.19257 90.414098)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.19506 90.41638) (xy 163.97478 90.41384) (xy 163.97224 104.5591) (xy 133.19506 104.5591)
      )
    )
  )
)
