(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C-J1-Pad2)")
  (net 3 "Net-(C-J1-Pad4)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 "Net-(C-J1-Pad3)")
  (net 7 "Net-(C2-Pad2)")
  (net 8 "Net-(C3-Pad2)")
  (net 9 "Net-(C4-Pad2)")
  (net 10 "Net-(R5-Pad1)")
  (net 11 "Net-(R5-Pad2)")
  (net 12 "Net-(C-J1-Pad7)")
  (net 13 "Net-(C7-Pad2)")
  (net 14 "Net-(R4-Pad2)")
  (net 15 "unconnected-(U1-Pad6)")
  (net 16 "unconnected-(U1-Pad7)")
  (net 17 "unconnected-(U1-Pad8)")
  (net 18 "Net-(C-J1-Pad6)")
  (net 19 "unconnected-(U1-Pad9)")
  (net 20 "unconnected-(U1-Pad10)")
  (net 21 "unconnected-(U1-Pad11)")
  (net 22 "unconnected-(U1-Pad12)")
  (net 23 "unconnected-(U1-Pad15)")
  (net 24 "unconnected-(U1-Pad17)")
  (net 25 "unconnected-(U2-Pad1)")
  (net 26 "unconnected-(U2-Pad5)")
  (net 27 "unconnected-(U2-Pad8)")
  (net 28 "VOut")
  (net 29 "AOut")
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 37.385 50.165 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C4" (at 2.5 1.905) (layer "F.SilkS"))
    (fp_text value "10nF" (at 2.5 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C3-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 32.385 53.975)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 2.5 -1.905) (layer "F.SilkS"))
    (fp_text value "47pF" (at 2.5 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-18_W7.62mm_LongPads" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 32.355 43.83 90)
    (descr "18-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "LM1889N" (at 3.81 22.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 10.16 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C4-Pad2)") (pinfunction "LEAD") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(C-J1-Pad3)") (pinfunction "R-Y") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)") (pinfunction "CHROMA_BIAS") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(C-J1-Pad7)") (pinfunction "B-Y") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "GROUND") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "unconnected-(U1-Pad6)") (pinfunction "CHBTANK") (pintype "passive+no_connect"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "unconnected-(U1-Pad7)") (pinfunction "CHBTANK") (pintype "passive+no_connect"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "unconnected-(U1-Pad8)") (pinfunction "CHATANK") (pintype "passive+no_connect"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "unconnected-(U1-Pad9)") (pinfunction "CHATANK") (pintype "passive+no_connect"))
    (pad "10" thru_hole oval (at 7.62 20.32 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "unconnected-(U1-Pad10)") (pinfunction "CHBOUT") (pintype "passive+no_connect"))
    (pad "11" thru_hole oval (at 7.62 17.78 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "unconnected-(U1-Pad11)") (pinfunction "CHAOUT") (pintype "passive+no_connect"))
    (pad "12" thru_hole oval (at 7.62 15.24 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "unconnected-(U1-Pad12)") (pinfunction "SOUNDIN") (pintype "passive+no_connect"))
    (pad "13" thru_hole oval (at 7.62 12.7 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C-J1-Pad6)") (pinfunction "VIDEOIN") (pintype "passive"))
    (pad "14" thru_hole oval (at 7.62 10.16 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C-J1-Pad4)") (pinfunction "RFSUPPLY") (pintype "passive"))
    (pad "15" thru_hole oval (at 7.62 7.62 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "unconnected-(U1-Pad15)") (pinfunction "SOUNDTANK") (pintype "passive+no_connect"))
    (pad "16" thru_hole oval (at 7.62 5.08 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C-J1-Pad4)") (pinfunction "SUPPLY") (pintype "passive"))
    (pad "17" thru_hole oval (at 7.62 2.54 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "unconnected-(U1-Pad17)") (pinfunction "CHROMA_OSC") (pintype "passive+no_connect"))
    (pad "18" thru_hole oval (at 7.62 0 90) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad2)") (pinfunction "LAG") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-18_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 60.96 25.4)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C8" (at 1.27 -3.81 180) (layer "F.SilkS"))
    (fp_text value "10uF" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(C-J1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "AOut") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 57.15 40.005 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 5.08 2.54 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(C-J1-Pad6)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A420)
    (at 24.75 34.925)
    (descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x08 2.54mm single row")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "CN1" (at 0 -2.77) (layer "F.SilkS"))
    (fp_text value "1x8" (at 0 20.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(C-J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(C-J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(C-J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(C-J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(C-J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Audio:Jack_3.5mm_CUI_SJ1-3525N_Horizontal" (layer "F.Cu")
    (tedit 62084D76)
    (at 75.184 20.32 180)
    (descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
    (tags "TRS audio jack stereo horizontal")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole exclude_from_pos_files)
    (fp_text reference "CN2" (at 0 -8.8) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Female" (at 0 -10) (layer "F.Fab"))
    (fp_text user "PCB edge" (at 0 3.65 180 unlocked) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -5 2.5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu))
    (pad "" np_thru_hole circle (at 5 0 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu))
    (pad "" np_thru_hole circle (at 0 -5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu))
    (pad "" np_thru_hole circle (at 5 2.5 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu))
    (pad "" np_thru_hole circle (at -5 0 180) (size 1.2 1.2) (drill 1.2) (layers *.Cu))
    (pad "R" thru_hole oval (at -5 -5 180) (size 1.2 2.2) (drill oval 0.4 1.4) (layers *.Cu *.Mask)
      (net 28 "VOut"))
    (pad "RN" thru_hole oval (at -2.5 -5 180) (size 1.2 2.2) (drill oval 0.4 1.4) (layers *.Cu *.Mask))
    (pad "S" thru_hole oval (at 0 0 180) (size 2.2 1.2) (drill oval 1.4 0.4) (layers *.Cu *.Mask)
      (net 1 "GND"))
    (pad "T" thru_hole oval (at 5 -5) (size 1.2 2.2) (drill oval 0.4 1.4) (layers *.Cu *.Mask)
      (net 29 "AOut"))
    (pad "TN" thru_hole oval (at 2.5 -5) (size 1.2 2.2) (drill oval 0.4 1.4) (layers *.Cu *.Mask))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3525N_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 73.66 53.975 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C5" (at 4.98 -0.04 180) (layer "F.SilkS"))
    (fp_text value "10uF" (at 1.25 3.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C-J1-Pad4)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_A-405_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 55.205 23.495 180)
    (descr "Diode, A-405 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "Diode A-405 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "6.2V")
    (attr through_hole)
    (fp_text reference "ZR1" (at 6.35 2.54) (layer "F.SilkS"))
    (fp_text value "1N4735A-B" (at 6.35 2.47) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.74 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.9) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(C-J1-Pad4)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_A-405_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 68.644888 42.545)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C7" (at 1.205112 -3.81 180) (layer "F.SilkS"))
    (fp_text value "47uF" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R5-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 28.535 23.495)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Comment" "This is in the position of R62 on the RF board.  R62 is a duplicate label, and R52 is listed in the parts list with this value and no corresponding label.")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 5.12 -2.54) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 23.495 29.21 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 5.08 0 180) (layer "F.SilkS"))
    (fp_text value "10uF" (at 1.25 3.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C-J1-Pad4)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 38.735 29.845 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 5.08 2.54) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 61.555 43.815 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 5.08 -2.5 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 51.435 50.165 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 5.08 2.54) (layer "F.SilkS"))
    (fp_text value "1K" (at 5.08 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 66.635 38.695 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C6" (at 2.5 -2.2 90) (layer "F.SilkS"))
    (fp_text value "27pF" (at 2.5 2.2 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 75.565 40.64 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at 5.08 -2.5 90) (layer "F.SilkS"))
    (fp_text value "75" (at 5.08 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(C7-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "VOut") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 61.605 47.635)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS"))
    (fp_text value "LM318" (at 3.81 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "unconnected-(U2-Pad1)") (pinfunction "BAL1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R5-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(R4-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "unconnected-(U2-Pad5)") (pinfunction "BAL3") (pintype "passive"))
    (pad "6" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R5-Pad2)") (pintype "output"))
    (pad "7" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C-J1-Pad4)") (pinfunction "V+") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "unconnected-(U2-Pad8)") (pinfunction "BAL2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 51.395 29.845 180)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.3*1.9mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 4.3mm width 1.9mm Capacitor")
    (property "Sheetfile" "Comp.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 1.905) (layer "F.SilkS"))
    (fp_text value "47pF" (at 2.5 2.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "CustomFootprints:Basic Ass Solder Pad" (layer "B.Cu")
    (tedit 0)
    (at 64.77 62.23 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 5.08 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Basic Ass Solder Pad" (at 0 -5.08 unlocked) (layer "B.Fab"))
  )
  (footprint "CustomFootprints:Basic Ass Solder Pad" (layer "B.Cu")
    (tedit 0)
    (at 31.75 18.542 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 5.08 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Basic Ass Solder Pad" (at 0 -5.08 unlocked) (layer "B.Fab"))
  )
  (footprint "CustomFootprints:Basic Ass Solder Pad" (layer "B.Cu")
    (tedit 0)
    (at 31.75 62.23 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 5.08 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Basic Ass Solder Pad" (at 0 -5.08 unlocked) (layer "B.Fab"))
  )
  (footprint "CustomFootprints:Basic Ass Solder Pad" (layer "B.Cu")
    (tedit 0)
    (at 64.77 18.542 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 5.08 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Basic Ass Solder Pad" (at 0 -5.08 unlocked) (layer "B.Fab"))
  )
  (footprint "CustomFootprints:Basic Ass Solder Pad" (layer "B.Cu")
    (tedit 0)
    (at 16.51 40.64 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 5.08 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Basic Ass Solder Pad" (at 0 -5.08 unlocked) (layer "B.Fab"))
  )
  (footprint "CustomFootprints:Basic Ass Solder Pad" (layer "B.Cu")
    (tedit 0)
    (at 80.518 40.64 180)
    (attr smd)
    (fp_text reference "REF**" (at 0 5.08 unlocked) (layer "B.SilkS") hide)
    (fp_text value "Basic Ass Solder Pad" (at 0 -5.08 unlocked) (layer "B.Fab"))
  )
  (gr_line (start 13.295 17.78) (end 15.24 15.405) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 15.24 15.405) (end 81.28 15.405) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 81.28 65.405) (end 83.295 63.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 13.295 63.5) (end 13.295 17.78) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 81.28 65.405) (end 15.24 65.405) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 83.295 45.72) (end 83.295 63.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 85.09 35.56) (end 83.295 35.56) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 15.24 65.405) (end 13.295 63.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 83.295 45.72) (end 85.09 45.72) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 83.295 17.78) (end 83.295 35.56) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 85.09 45.72) (end 85.09 35.56) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 83.295 17.78) (end 81.28 15.405) (layer "Edge.Cuts") (width 0.1))
  (gr_text "This Side Up" (at 48.26 18.415) (layer "B.SilkS"))
  (gr_text "Colecovision RF Replacement\nComposite Board - Rev 2\n\nAzura Bayta, 2024" (at 48.26 60.96) (layer "B.SilkS"))
  (gr_text "R1 1K\nR2 1K\nR3 1K\nR4 10K\nR5 10K\nR6 75\n\nC1 10uF\nC2 47pF\nC3 47pF\nC4 10nF\nC5 10uF\nC6 27pF\nC7 47uF\nC8 10uF\n\nZR1 1N4735\n\nU1 LM1889N\nU2 LM318" (at 15.24 46.99) (layer "F.SilkS"))
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87.63 44.45)
        (xy 83.82 66.04)
        (xy 12.7 66.04)
        (xy 12.7 15.24)
        (xy 83.82 15.24)
      )
    )
  )
)
