<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="11.43" y1="21.59" x2="41.91" y2="21.59" width="0.1524" layer="20"/>
<wire x1="41.91" y1="21.59" x2="41.91" y2="-3.81" width="0.1524" layer="20"/>
<wire x1="41.91" y1="-3.81" x2="11.43" y2="-3.81" width="0.1524" layer="20"/>
<wire x1="11.43" y1="-3.81" x2="11.43" y2="21.59" width="0.1524" layer="20"/>
<text>GND</text>
<text>Vout</text>
<text>PGD</text>
<text>SHDN</text>
<text>LTC3105
BOARD</text>
<text>UHMC
MICROCLIMATE
PROJECT</text>
<text>version 2</text>
<text>19 Oct 2017</text>
<text>GND</text>
<text>GND</text>
<text>UHMC
MICROCLIMATE
PROJECT</text>
<text>LDO</text>
</plain>
<libraries>
<library name="KEMET">
<packages>
<package name="1206_A">
</package>
<package name="0805_C">
</package>
</packages>
</library>
<library name="Stackpole">
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="LINEAR">
<packages>
<package name="MS12">
<description>12-Lead Plastic MSOP
paste 75% of pad</description>
</package>
</packages>
</library>
<library name="OST">
<packages>
<package name="OSTVN02">
</package>
<package name="OSTVN05">
<description>http://www.on-shore.com/wp-content/uploads/2015/09/ostvnxxa150.pdf</description>
</package>
</packages>
</library>
<library name="MURATA">
<packages>
<package name="LQH3">
<description>SMT Inductors&lt;br&gt;
http://search.murata.co.jp/Ceramy/image/img/P02/JELF243A-0114.pdf</description>
</package>
</packages>
</library>
<library name="3M">
<packages>
<package name="SJ5302">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0411V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0411, grid 3.81 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CIN" library="KEMET" package="1206_A" value="10u">
<attribute name="VALUE"/>
</element>
<element name="CAUX" library="KEMET" package="0805_C" value="1u"/>
<element name="R1" library="Stackpole" package="0805" value="1M"/>
<element name="R2" library="Stackpole" package="0805" value="301k"/>
<element name="RPU" library="Stackpole" package="0805" value="470K"/>
<element name="U$1" library="LINEAR" package="MS12" value="LTC3105"/>
<element name="SOLAR" library="OST" package="OSTVN02" value="M02"/>
<element name="L1" library="MURATA" package="LQH3" value="10u"/>
<element name="U$7" library="3M" package="SJ5302" value=""/>
<element name="U$8" library="3M" package="SJ5302" value=""/>
<element name="U$9" library="3M" package="SJ5302" value=""/>
<element name="U$10" library="3M" package="SJ5302" value=""/>
<element name="COUT" library="KEMET" package="1206_A" value="10u"/>
<element name="J1" library="OST" package="OSTVN05" value="M05OSTVN05"/>
<element name="CLDO" library="KEMET" package="1206_A" value="10u"/>
<element name="MPPC" library="adafruit" package="0411V" value="180K"/>
</elements>
<signals>
<signal name="SW">
<contactref element="U$1" pad="9"/>
<contactref element="L1" pad="B"/>
</signal>
<signal name="VIN">
<contactref element="U$1" pad="8"/>
<contactref element="CIN" pad="2"/>
<contactref element="SOLAR" pad="1"/>
<contactref element="L1" pad="A"/>
</signal>
<signal name="GND">
<contactref element="CIN" pad="1"/>
<contactref element="CAUX" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="7"/>
<contactref element="U$1" pad="3"/>
<contactref element="SOLAR" pad="2"/>
<contactref element="COUT" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="CLDO" pad="1"/>
<contactref element="MPPC" pad="1"/>
</signal>
<signal name="AUX">
<contactref element="U$1" pad="12"/>
<contactref element="CAUX" pad="2"/>
</signal>
<signal name="FB">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="U$1" pad="11"/>
<contactref element="R1" pad="2"/>
<contactref element="RPU" pad="2"/>
<contactref element="COUT" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="PGOOD">
<contactref element="U$1" pad="10"/>
<contactref element="RPU" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="MPCC">
<contactref element="U$1" pad="5"/>
<contactref element="MPPC" pad="2"/>
</signal>
<signal name="LDO">
<contactref element="U$1" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="CLDO" pad="2"/>
</signal>
<signal name="SHDN">
<contactref element="J1" pad="5"/>
<contactref element="U$1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
