<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.2">
<drawing>
<board>
<plain>
<wire x1="27.559" y1="27.813" x2="65.258" y2="27.813" width="0" layer="20"/>
<wire x1="65.258" y1="27.813" x2="65.258" y2="58.471" width="0" layer="20"/>
<wire x1="65.258" y1="58.471" x2="27.559" y2="58.598" width="0" layer="20"/>
<wire x1="27.559" y1="58.598" x2="27.559" y2="27.813" width="0" layer="20"/>
<text>VIN</text>
<text>GND</text>
<text>GND</text>
<text>Down</text>
<text>Up</text>
<text>RST</text>
<text>ADC</text>
<text>EN</text>
<text>GPIO16</text>
<text>GPIO14</text>
<text>GPIO12</text>
<text>GPIO13</text>
<text>3.3V</text>
<text>GPIO15</text>
<text>GPIO2</text>
<text>GPIO0</text>
<text>GPIO5</text>
<text>GPIO4</text>
<text>RX</text>
<text>TX</text>
<text>O</text>
<text>OLED INPUT</text>
<text>Avi's ESP Prototype
Rev 2.0</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="lm1117">
<description>&lt;b&gt;LM1117 Voltage Regulator&lt;/b&gt;
&lt;p&gt;800mA LDO Regulator, available in 1.8V, 2.5V, 2.85V, 3.3V, 5V, and adjustable versions.&lt;/p&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223 Small-Outline Transistor Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X08">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Res">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="ESP-12">
<packages>
<package name="ESP8266-ESP12">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="C2" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0805" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="lm1117" package="SOT223" value="LM1117"/>
<element name="J1" library="pinhead" package="1X03" value="">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="pinhead" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Res" package="0805" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R2" library="SparkFun-Res" package="0805" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R3" library="SparkFun-Res" package="0805" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R4" library="SparkFun-Res" package="0805" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R5" library="SparkFun-Res" package="0805" value=" ">
<attribute name="PROD_ID" value=" "/>
</element>
<element name="U$1" library="ESP-12" package="ESP8266-ESP12" value="ESP8266_ESP-12"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="JP1" pad="8"/>
<contactref element="JP7" pad="4"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="IC1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="JP2" pad="8"/>
<contactref element="U$1" pad="16"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="JP7" pad="3"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="PULL_UP">
<contactref element="J1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="PULL_DOWN">
<contactref element="J1" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="RST">
<contactref element="JP2" pad="1"/>
<contactref element="U$1" pad="9"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="ADC">
<contactref element="JP2" pad="2"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="CH_PD">
<contactref element="JP2" pad="3"/>
<contactref element="U$1" pad="11"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="GPIO14">
<contactref element="JP2" pad="5"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="GPIO12">
<contactref element="JP2" pad="6"/>
<contactref element="U$1" pad="14"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="GPIO13">
<contactref element="JP2" pad="7"/>
<contactref element="U$1" pad="15"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="TX">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="RX">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="GPIO4">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="GPIO5">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="GPIO0">
<contactref element="JP1" pad="5"/>
<contactref element="J1" pad="2"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="GPIO2">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="GPIO15">
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="GPIO16">
<contactref element="JP2" pad="4"/>
<contactref element="U$1" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
