(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-3-g5ebb6b6)")
  (general
    (thickness 1.6)
    (drawings 146)
    (tracks 2847)
    (zones 0)
    (modules 92)
    (nets 77)
  )
  (page A4)
  (title_block
    (title Crkbd)
    (date 2018/05/15)
    (rev 1.1)
    (company foostan)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 2.1)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4 4)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 194.8 63.4)
    (visible_elements FFFFF77F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 row0)
  (net 2 "Net-(D1-Pad2)")
  (net 3 row1)
  (net 4 "Net-(D2-Pad2)")
  (net 5 row2)
  (net 6 "Net-(D3-Pad2)")
  (net 7 row3)
  (net 8 "Net-(D4-Pad2)")
  (net 9 "Net-(D5-Pad2)")
  (net 10 "Net-(D6-Pad2)")
  (net 11 "Net-(D7-Pad2)")
  (net 12 "Net-(D8-Pad2)")
  (net 13 "Net-(D9-Pad2)")
  (net 14 "Net-(D10-Pad2)")
  (net 15 "Net-(D11-Pad2)")
  (net 16 "Net-(D12-Pad2)")
  (net 17 "Net-(D13-Pad2)")
  (net 18 "Net-(D14-Pad2)")
  (net 19 "Net-(D15-Pad2)")
  (net 20 "Net-(D16-Pad2)")
  (net 21 "Net-(D17-Pad2)")
  (net 22 "Net-(D18-Pad2)")
  (net 23 "Net-(D19-Pad2)")
  (net 24 "Net-(D20-Pad2)")
  (net 25 "Net-(D21-Pad2)")
  (net 26 GND)
  (net 27 VCC)
  (net 28 col0)
  (net 29 col1)
  (net 30 col2)
  (net 31 col3)
  (net 32 col4)
  (net 33 col5)
  (net 34 LED)
  (net 35 data)
  (net 36 "Net-(L1-Pad3)")
  (net 37 "Net-(L1-Pad1)")
  (net 38 "Net-(L3-Pad3)")
  (net 39 "Net-(L10-Pad1)")
  (net 40 "Net-(L11-Pad1)")
  (net 41 "Net-(L13-Pad1)")
  (net 42 "Net-(L14-Pad3)")
  (net 43 "Net-(L10-Pad3)")
  (net 44 "Net-(L12-Pad1)")
  (net 45 "Net-(L13-Pad3)")
  (net 46 "Net-(L15-Pad3)")
  (net 47 "Net-(L16-Pad3)")
  (net 48 reset)
  (net 49 SCL)
  (net 50 SDA)
  (net 51 "Net-(L5-Pad3)")
  (net 52 "Net-(U1-Pad14)")
  (net 53 "Net-(U1-Pad13)")
  (net 54 "Net-(U1-Pad12)")
  (net 55 "Net-(U1-Pad11)")
  (net 56 "Net-(J2-Pad1)")
  (net 57 "Net-(J2-Pad2)")
  (net 58 "Net-(J2-Pad3)")
  (net 59 "Net-(J2-Pad4)")
  (net 60 "Net-(L2-Pad3)")
  (net 61 "Net-(L3-Pad1)")
  (net 62 "Net-(L11-Pad3)")
  (net 63 "Net-(L14-Pad1)")
  (net 64 "Net-(L12-Pad3)")
  (net 65 "Net-(L17-Pad1)")
  (net 66 "Net-(L18-Pad3)")
  (net 67 "Net-(L19-Pad3)")
  (net 68 "Net-(J1-PadA)")
  (net 69 "Net-(J1-PadB)")
  (net 70 "Net-(U1-Pad24)")
  (net 71 "Net-(L21-Pad3)")
  (net 72 "Net-(L22-Pad3)")
  (net 73 "Net-(L22-Pad1)")
  (net 74 "Net-(L23-Pad3)")
  (net 75 "Net-(L25-Pad1)")
  (net 76 "Net-(L26-Pad1)")
  (net_class Default "これは標準のネット クラスです。"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net LED)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D15-Pad2)")
    (add_net "Net-(D16-Pad2)")
    (add_net "Net-(D17-Pad2)")
    (add_net "Net-(D18-Pad2)")
    (add_net "Net-(D19-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D20-Pad2)")
    (add_net "Net-(D21-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(J1-PadA)")
    (add_net "Net-(J1-PadB)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(L1-Pad3)")
    (add_net "Net-(L10-Pad1)")
    (add_net "Net-(L10-Pad3)")
    (add_net "Net-(L11-Pad1)")
    (add_net "Net-(L11-Pad3)")
    (add_net "Net-(L12-Pad1)")
    (add_net "Net-(L12-Pad3)")
    (add_net "Net-(L13-Pad1)")
    (add_net "Net-(L13-Pad3)")
    (add_net "Net-(L14-Pad1)")
    (add_net "Net-(L14-Pad3)")
    (add_net "Net-(L15-Pad3)")
    (add_net "Net-(L16-Pad3)")
    (add_net "Net-(L17-Pad1)")
    (add_net "Net-(L18-Pad3)")
    (add_net "Net-(L19-Pad3)")
    (add_net "Net-(L2-Pad3)")
    (add_net "Net-(L21-Pad3)")
    (add_net "Net-(L22-Pad1)")
    (add_net "Net-(L22-Pad3)")
    (add_net "Net-(L23-Pad3)")
    (add_net "Net-(L25-Pad1)")
    (add_net "Net-(L26-Pad1)")
    (add_net "Net-(L3-Pad1)")
    (add_net "Net-(L3-Pad3)")
    (add_net "Net-(L5-Pad3)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad24)")
    (add_net SCL)
    (add_net SDA)
    (add_net VCC)
    (add_net col0)
    (add_net col1)
    (add_net col2)
    (add_net col3)
    (add_net col4)
    (add_net col5)
    (add_net data)
    (add_net reset)
    (add_net row0)
    (add_net row1)
    (add_net row2)
    (add_net row3)
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 91 123.2 180)
    (fp_text reference SW14 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D14-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D14-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D14-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D14-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D14-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 109.5 110.375 180)
    (fp_text reference SW15 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D15-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D15-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D15-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D15-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D15-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 109.5 72.375 180)
    (fp_text reference SW3 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5BBACA09)
    (at 155.2448 82.3468)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF01 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at -3.048 -5.588) (layer F.Fab) hide)
    (fp_text user %R (at 0.254 2.54) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5BBACA09)
    (at 118.6942 99.6188)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF01 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at -3.048 -5.588) (layer F.Fab) hide)
    (fp_text user %R (at 0.254 2.54) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module footprints:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 178.75 133.25 165)
    (fp_text reference SW21 (at 4.600001 6 165) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 165) (layer F.Fab) hide)
    (pad 1 thru_hole oval (at 5.1 -3.9 115) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad "" np_thru_hole circle (at 0 0 255) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 255) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.5 0 255) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at -5.1 -3.9 215) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 2 thru_hole circle (at 0 -5.9 255) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(D21-Pad2)"))
    (pad 2 thru_hole circle (at 2.540001 -5.08 165) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(D21-Pad2)"))
    (pad 1 thru_hole oval (at -3.81 -2.54 215) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 1 thru_hole circle (at -2.54 -5.08 165) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 2 thru_hole oval (at 3.81 -2.54 115) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(D21-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 165) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(D21-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4 165) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(D21-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -4 165) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 1 thru_hole circle (at -2.54 -4.5 165) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad "" np_thru_hole circle (at 5.08 0 165) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 165) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 165) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.22 4.2 165) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module kbd:SK6812MINI_underglow_rev (layer F.Cu) (tedit 5B480106)
    (at 165 121.5 180)
    (fp_text reference L27 (at 0 -2.5 180) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7 180) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 -0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(L21-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 -0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(L26-Pad1)"))
    (pad 2 smd rect (at -2.4 0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(L21-Pad3)"))
    (pad 3 smd rect (at 2.4 0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(L26-Pad1)"))
    (pad 4 smd rect (at 2.4 -0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_underglow_rev (layer F.Cu) (tedit 5B480106)
    (at 165 83.5)
    (fp_text reference L24 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(L23-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 34 LED))
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(L23-Pad3)"))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 34 LED))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_underglow_rev (layer F.Cu) (tedit 5B480106)
    (at 127 78.8)
    (fp_text reference L23 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(L22-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 74 "Net-(L23-Pad3)"))
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(L22-Pad3)"))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(L23-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_underglow_rev (layer F.Cu) (tedit 5B480106)
    (at 81.1784 92.1512)
    (fp_text reference L22 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(L22-Pad1)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 72 "Net-(L22-Pad3)"))
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(L22-Pad1)"))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(L22-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_underglow_rev (layer F.Cu) (tedit 5B480106)
    (at 82.2706 112.2426 180)
    (fp_text reference L25 (at 0 -2.5 180) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7 180) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 -0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(L25-Pad1)"))
    (pad 4 smd rect (at 2.4 0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 -0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 73 "Net-(L22-Pad1)"))
    (pad 2 smd rect (at -2.4 0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(L25-Pad1)"))
    (pad 3 smd rect (at 2.4 0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(L22-Pad1)"))
    (pad 4 smd rect (at 2.4 -0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_underglow_rev (layer F.Cu) (tedit 5B480106)
    (at 122.047 117.9322 180)
    (fp_text reference L26 (at 0 -2.5 180) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7 180) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 -0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 76 "Net-(L26-Pad1)"))
    (pad 4 smd rect (at 2.4 0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 -0.875 180) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 75 "Net-(L25-Pad1)"))
    (pad 2 smd rect (at -2.4 0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(L26-Pad1)"))
    (pad 3 smd rect (at 2.4 0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(L25-Pad1)"))
    (pad 4 smd rect (at 2.4 -0.875 180) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:ProMicro_v2 (layer F.Cu) (tedit 5B7FE439)
    (at 185.75 86.25)
    (fp_text reference U1 (at -1.27 2.762 270) (layer F.SilkS) hide)
    (fp_text value ProMicro (at -1.27 14.732) (layer F.Fab) hide)
    (fp_text user "" (at -0.5 -17.25) (layer F.SilkS))
    (fp_text user "" (at -1.2065 -16.256) (layer B.SilkS))
    (fp_text user RAW (at -9.7155 -14.478) (layer F.SilkS))
    (fp_text user LED (at 5.5 -14.478) (layer F.SilkS))
    (fp_text user GND (at -9.7155 -11.938) (layer F.SilkS))
    (fp_text user DATA (at 5.35 -11.95) (layer F.SilkS))
    (fp_text user RST (at -9.7155 -9.3345) (layer F.SilkS))
    (fp_text user GND (at 5.5245 -9.3345) (layer F.SilkS))
    (fp_text user VCC (at -9.7155 -6.858) (layer F.SilkS))
    (fp_text user GND (at 5.461 -6.7945) (layer F.SilkS))
    (fp_text user COL3 (at -10 3.35) (layer F.SilkS))
    (fp_text user ROW0 (at 5.2 0.8) (layer F.SilkS))
    (fp_text user COL2 (at -9.9 0.762) (layer F.SilkS))
    (fp_text user SCL (at 5.461 -1.778) (layer F.SilkS))
    (fp_text user COL1 (at -9.85 -1.778) (layer F.SilkS))
    (fp_text user SDA (at 5.461 -4.318) (layer F.SilkS))
    (fp_text user COL0 (at -9.9 -4.3) (layer F.SilkS))
    (fp_text user B6 (at -10.05 13.5) (layer F.SilkS))
    (fp_text user B5 (at 5.2 13.5255) (layer F.SilkS))
    (fp_text user B4 (at 5.2 10.922) (layer F.SilkS))
    (fp_text user B2 (at -9.95 10.95) (layer F.SilkS))
    (fp_text user ROW3 (at 5.2 8.4455) (layer F.SilkS))
    (fp_text user COL5 (at -9.95 8.4455) (layer F.SilkS))
    (fp_text user ROW2 (at 5.2 5.85) (layer F.SilkS))
    (fp_text user COL4 (at -9.95 5.85) (layer F.SilkS))
    (fp_text user ROW1 (at 5.25 3.302) (layer F.SilkS))
    (fp_text user ROW1 (at -11.3 4.6355) (layer B.SilkS))
    (fp_text user COL4 (at 3.95 7.112) (layer B.SilkS))
    (fp_text user ROW2 (at -11.3 7.239) (layer B.SilkS))
    (fp_text user COL5 (at 4 9.75) (layer B.SilkS))
    (fp_text user ROW3 (at -11.3 9.75) (layer B.SilkS))
    (fp_text user B2 (at 4.5085 12.1285) (layer B.SilkS))
    (fp_text user B4 (at -11.049 12.2555) (layer B.SilkS))
    (fp_text user B5 (at -11.049 14.7955) (layer B.SilkS))
    (fp_text user B6 (at 4.445 14.732) (layer B.SilkS))
    (fp_text user COL0 (at 4 -2.95) (layer B.SilkS))
    (fp_text user SDA (at -11.049 -2.9845) (layer B.SilkS))
    (fp_text user COL1 (at 4 -0.4445) (layer B.SilkS))
    (fp_text user SCL (at -11.049 -0.4445) (layer B.SilkS))
    (fp_text user COL2 (at 4 2.1) (layer B.SilkS))
    (fp_text user ROW0 (at -11.3 2.032) (layer B.SilkS))
    (fp_text user COL3 (at 4 4.6) (layer B.SilkS))
    (fp_text user GND (at -11.049 -5.5245) (layer B.SilkS))
    (fp_text user VCC (at 4.1275 -5.5245) (layer B.SilkS))
    (fp_text user GND (at -11.049 -8.0645) (layer B.SilkS))
    (fp_text user RST (at 4.191 -8.0645) (layer B.SilkS))
    (fp_text user DATA (at -11.2 -10.5) (layer B.SilkS))
    (fp_text user GND (at 4.1275 -10.668) (layer B.SilkS))
    (fp_text user LED (at -11.049 -13.1445) (layer B.SilkS))
    (fp_text user RAW (at 4.191 -13.1445) (layer B.SilkS))
    (pad 24 thru_hole circle (at 6.35 -13.208) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(U1-Pad24)"))
    (pad 23 thru_hole circle (at 6.35 -10.668) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 GND))
    (pad 22 thru_hole circle (at 6.35 -8.128) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 reset))
    (pad 21 thru_hole circle (at 6.35 -5.588) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 VCC))
    (pad 20 thru_hole circle (at 6.35 -3.048) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 19 thru_hole circle (at 6.35 -0.508) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 18 thru_hole circle (at 6.35 2.032) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 17 thru_hole circle (at 6.35 4.572) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 16 thru_hole circle (at 6.35 7.112) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 15 thru_hole circle (at 6.35 9.652) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 14 thru_hole circle (at 6.35 12.192) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U1-Pad14)"))
    (pad 13 thru_hole circle (at 6.35 14.732) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(U1-Pad13)"))
    (pad 12 thru_hole circle (at -8.89 14.732) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(U1-Pad12)"))
    (pad 11 thru_hole circle (at -8.89 12.192) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(U1-Pad11)"))
    (pad 10 thru_hole circle (at -8.89 9.652) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 row3))
    (pad 9 thru_hole circle (at -8.89 7.112) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 row2))
    (pad 8 thru_hole circle (at -8.89 4.572) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 row1))
    (pad 7 thru_hole circle (at -8.89 2.032) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 row0))
    (pad 6 thru_hole circle (at -8.89 -0.508) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 SCL))
    (pad 5 thru_hole circle (at -8.89 -3.048) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 SDA))
    (pad 4 thru_hole circle (at -8.89 -5.588) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 GND))
    (pad 3 thru_hole circle (at -8.89 -8.128) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 GND))
    (pad 2 thru_hole circle (at -8.89 -10.668) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 data))
    (pad 1 thru_hole circle (at -8.89 -13.208) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 LED))
    (pad 1 thru_hole circle (at 7.6564 -14.478) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 LED))
    (pad 2 thru_hole circle (at 7.6564 -11.938) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 data))
    (pad 3 thru_hole circle (at 7.6564 -9.398) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 GND))
    (pad 4 thru_hole circle (at 7.6564 -6.858) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 GND))
    (pad 5 thru_hole circle (at 7.6564 -4.318) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 SDA))
    (pad 6 thru_hole circle (at 7.6564 -1.778) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 SCL))
    (pad 7 thru_hole circle (at 7.6564 0.762) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 row0))
    (pad 8 thru_hole circle (at 7.6564 3.302) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 row1))
    (pad 9 thru_hole circle (at 7.6564 5.842) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 row2))
    (pad 10 thru_hole circle (at 7.6564 8.382) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 row3))
    (pad 11 thru_hole circle (at 7.6564 10.922) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at 7.6564 13.462) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at -7.5636 13.462) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at -7.5636 10.922) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at -7.5636 8.382) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 16 thru_hole circle (at -7.5636 5.842) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 17 thru_hole circle (at -7.5636 3.302) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 18 thru_hole circle (at -7.5636 0.762) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 19 thru_hole circle (at -7.5636 -1.778) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 20 thru_hole circle (at -7.5636 -4.318) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 21 thru_hole circle (at -7.5636 -6.858) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 VCC))
    (pad 22 thru_hole circle (at -7.5636 -9.398) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 reset))
    (pad 23 thru_hole circle (at -7.5636 -11.938) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 GND))
    (pad 24 thru_hole circle (at -7.5636 -14.478) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(U1-Pad24)"))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 72.5 79.7)
    (fp_text reference L1 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(L1-Pad1)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(L1-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(L1-Pad1)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(L1-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 91 79.7)
    (fp_text reference L2 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(L1-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(L2-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(L1-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(L2-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 109.5 66.875)
    (fp_text reference L3 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(L3-Pad1)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(L3-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(L3-Pad1)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(L3-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 128 64.5)
    (fp_text reference L4 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 38 "Net-(L3-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(L10-Pad1)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(L3-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(L10-Pad1)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 146.5 66.875)
    (fp_text reference L5 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(L11-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(L5-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(L11-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(L5-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 165 69.25)
    (fp_text reference L6 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(L5-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(L12-Pad1)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(L5-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(L12-Pad1)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 72.5 98.7)
    (fp_text reference L7 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(L13-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(L13-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(L1-Pad1)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 91 98.7)
    (fp_text reference L8 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 60 "Net-(L2-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(L14-Pad1)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(L2-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(L14-Pad1)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 109.5 85.875)
    (fp_text reference L9 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(L15-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 61 "Net-(L3-Pad1)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(L15-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(L3-Pad1)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 128 83.5)
    (fp_text reference L10 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(L10-Pad1)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(L10-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(L10-Pad1)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(L10-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 146.5 85.875)
    (fp_text reference L11 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(L11-Pad1)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 62 "Net-(L11-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(L11-Pad1)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(L11-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 165 88.25)
    (fp_text reference L12 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 44 "Net-(L12-Pad1)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(L12-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(L12-Pad1)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(L12-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 72.5 117.7)
    (fp_text reference L13 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(L13-Pad1)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 45 "Net-(L13-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(L13-Pad1)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(L13-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 91 117.7)
    (fp_text reference L14 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 63 "Net-(L14-Pad1)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(L14-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(L14-Pad1)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(L14-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 109.5 104.875)
    (fp_text reference L15 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(L14-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 46 "Net-(L15-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(L14-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(L15-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 128 102.5)
    (fp_text reference L16 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(L10-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(L16-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(L10-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(L16-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 146.5 104.875)
    (fp_text reference L17 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(L17-Pad1)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(L11-Pad1)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(L17-Pad1)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(L11-Pad1)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 165 107.25)
    (fp_text reference L18 (at 0 -2.5) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 64 "Net-(L12-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(L18-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(L12-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(L18-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 135.3 128.05 15)
    (fp_text reference L19 (at 0 -2.5 15) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7 15) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875 15) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875 15) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(L16-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875 15) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875 15) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(L19-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875 15) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875 15) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(L16-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875 15) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(L19-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875 15) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 157.75 126.25)
    (fp_text reference L20 (at 0 -2.500001) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.7) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.399999 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 67 "Net-(L19-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.399999 0.875) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 65 "Net-(L17-Pad1)"))
    (pad 2 smd rect (at -2.399999 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(L19-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(L17-Pad1)"))
    (pad 4 smd rect (at 2.399999 0.875) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:SK6812MINI_rev (layer F.Cu) (tedit 5B46C121)
    (at 180.25 128 345)
    (fp_text reference L21 (at 0 -2.5 345) (layer F.SilkS) hide)
    (fp_text value SK6812MINI (at -0.3 2.700001 345) (layer F.Fab) hide)
    (pad 2 smd rect (at -2.4 0.875 345) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 -0.875 345) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 66 "Net-(L18-Pad3)"))
    (pad 4 smd rect (at 2.4 -0.875 345) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
    (pad 3 smd rect (at 2.4 0.875 345) (size 1.6 1) (layers B.Cu B.Paste B.Mask)
      (net 71 "Net-(L21-Pad3)"))
    (pad 2 smd rect (at -2.4 -0.875 345) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at -2.4 0.875 345) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(L18-Pad3)"))
    (pad 3 smd rect (at 2.4 -0.875 345) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(L21-Pad3)"))
    (pad 4 smd rect (at 2.4 0.875 345) (size 1.6 1) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 64.5 85.2 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D1 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 row0))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 1 row0))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 row0))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 99 85.2 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D2 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 row0))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 1 row0))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 row0))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 117.5 72.375 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D3 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 row0))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 1 row0))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 row0))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 136 70 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D4 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D4-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 row0))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 1 row0))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 row0))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 154.5 72.375 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D5 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D5-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D5-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 row0))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 1 row0))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D5-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 row0))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 157 72.375 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D6 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D6-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D6-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 row0))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 1 row0))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 row0))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 64.5 104.2 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D7 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D7-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D7-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 row1))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 3 row1))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 3 row1))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 99 104.2 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D8 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D8-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D8-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 row1))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 3 row1))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D8-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 3 row1))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 117.5 91.375 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D9 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D9-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D9-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 row1))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 3 row1))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D9-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 3 row1))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 136 89 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D10 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D10-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D10-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 row1))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 3 row1))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D10-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 3 row1))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 154.5 91.375 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D11 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D11-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D11-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 row1))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 3 row1))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D11-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 3 row1))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 157 91.375 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D12 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D12-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D12-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 row1))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 3 row1))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D12-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 3 row1))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 64.5 123.2 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D13 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D13-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D13-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 row2))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 5 row2))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D13-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 5 row2))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 99 123.2 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D14 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D14-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D14-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 row2))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 5 row2))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D14-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 5 row2))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 117.5 110.375 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D15 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D15-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D15-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 row2))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 5 row2))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D15-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 5 row2))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 136 108 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D16 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D16-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(D16-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 row2))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 5 row2))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(D16-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 5 row2))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 157 110.375 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D18 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D18-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D18-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 row2))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 5 row2))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(D18-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 5 row2))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 144.75 131.25 285)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D19 (at 0 1.75 285) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 285) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 285) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D19-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 -0.000001 285) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(D19-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0.000001 285) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 row3))
    (pad 1 smd rect (at -1.775 0 285) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 7 row3))
    (pad 2 smd rect (at 1.775 0 285) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(D19-Pad2)"))
    (pad 1 smd rect (at -1.775 0 285) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 7 row3))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 149.5 131.75 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D20 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(D20-Pad2)"))
    (pad 2 thru_hole circle (at 3.810001 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D20-Pad2)"))
    (pad 1 thru_hole rect (at -3.810001 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 row3))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 7 row3))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(D20-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 7 row3))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 170.75 131.75 255)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D21 (at 0 1.75 255) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 255) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 255) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(D21-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0.000001 255) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(D21-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 -0.000001 255) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 row3))
    (pad 1 smd rect (at -1.775 0 255) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 7 row3))
    (pad 2 smd rect (at 1.775 0 255) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(D21-Pad2)"))
    (pad 1 smd rect (at -1.775 0 255) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 7 row3))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:D3_TH_SMD (layer F.Cu) (tedit 5B7FD767)
    (at 154.5 110.375 270)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference D17 (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text value D (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D17-Pad2)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D17-Pad2)"))
    (pad 1 thru_hole rect (at -3.81 0 270) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 row2))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 5 row2))
    (pad 2 smd rect (at 1.775 0 270) (size 1.3 0.95) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D17-Pad2)"))
    (pad 1 smd rect (at -1.775 0 270) (size 1.3 0.95) (layers F.Cu F.Paste F.Mask)
      (net 5 row2))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.22 0.15 0.15))
      (rotate (xyz 0 0 180))
    )
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 72.5 85.2 180)
    (fp_text reference SW1 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 91 85.2 180)
    (fp_text reference SW2 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D2-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 128 70 180)
    (fp_text reference SW4 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D4-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D4-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D4-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D4-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D4-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 146.5 72.375 180)
    (fp_text reference SW5 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D5-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D5-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D5-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D5-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(D5-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 165 74.75 180)
    (fp_text reference SW6 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D6-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D6-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D6-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D6-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D6-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 72.5 104.2 180)
    (fp_text reference SW7 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D7-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D7-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D7-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D7-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(D7-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 91 104.2 180)
    (fp_text reference SW8 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D8-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D8-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D8-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D8-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D8-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 29 col1))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 109.5 91.375 180)
    (fp_text reference SW9 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D9-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D9-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D9-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D9-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D9-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 30 col2))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 128 89 180)
    (fp_text reference SW10 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D10-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D10-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D10-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D10-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D10-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 146.5 91.375 180)
    (fp_text reference SW11 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D11-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D11-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D11-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D11-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D11-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 165 93.75 180)
    (fp_text reference SW12 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D12-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D12-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D12-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D12-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D12-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 72.5 123.2 180)
    (fp_text reference SW13 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D13-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D13-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D13-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D13-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(D13-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 28 col0))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 146.5 110.375 180)
    (fp_text reference SW17 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D17-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D17-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D17-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D17-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(D17-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 165 112.75 180)
    (fp_text reference SW18 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D18-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D18-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D18-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D18-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(D18-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 33 col5))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 136.75 133.25 195)
    (fp_text reference SW19 (at 4.6 6 195) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 195) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 195) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 195) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 195) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 195) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 195) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 1 thru_hole circle (at -2.540001 -4 195) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 2 thru_hole circle (at 2.54 -4 195) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(D19-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 195) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(D19-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 145) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(D19-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 195) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 1 thru_hole oval (at -3.81 -2.54 245) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 2 thru_hole circle (at 2.54 -5.08 195) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(D19-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 285) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(D19-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 245) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad "" np_thru_hole circle (at 5.5 0 285) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 285) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 285) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 145) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 157.75 131.75 180)
    (fp_text reference SW20 (at 4.600001 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D20-Pad2)"))
    (pad 2 thru_hole circle (at 2.539999 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D20-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D20-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D20-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D20-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.099999 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 32 col4))
  )
  (module kbd:MX_ALPS_PG1350_noLed (layer F.Cu) (tedit 5B7FE0C4)
    (at 128 108 180)
    (fp_text reference SW16 (at 4.6 6 180) (layer F.Fab) hide)
    (fp_text value SW_PUSH (at 0.1 9.3 180) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.22 4.2 180) (size 1 1) (drill 1) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 5.08 0 180) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 1 thru_hole circle (at -2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 2 thru_hole circle (at 2.54 -4 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(D16-Pad2)"))
    (pad 2 thru_hole circle (at 2.54 -4.5 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(D16-Pad2)"))
    (pad 2 thru_hole oval (at 3.81 -2.54 130) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(D16-Pad2)"))
    (pad 1 thru_hole circle (at -2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 1 thru_hole oval (at -3.81 -2.54 230) (size 2.8 1.55) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad 2 thru_hole circle (at 2.54 -5.08 180) (size 2.4 2.4) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(D16-Pad2)"))
    (pad 2 thru_hole circle (at 0 -5.9 270) (size 2.2 2.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(D16-Pad2)"))
    (pad 1 thru_hole oval (at -5.1 -3.9 230) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
    (pad "" np_thru_hole circle (at 5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -5.5 0 270) (size 1.9 1.9) (drill 1.9) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 0 270) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole oval (at 5.1 -3.9 130) (size 2.2 1.25) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 31 col3))
  )
  (module kbd:R (layer F.Cu) (tedit 5AA93881)
    (at 187 108 180)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 0.05 -0.08 180) (layer F.SilkS))
    (fp_text value R (at 0 -1.6 180) (layer F.SilkS) hide)
    (fp_text user R1 (at 0 -0.0635 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 VCC))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 SDA))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.2 0.2 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:R (layer F.Cu) (tedit 5AA9387A)
    (at 187 110.3 180)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 0.05 -0.08 180) (layer F.SilkS))
    (fp_text value R (at 0 -1.6 180) (layer F.SilkS) hide)
    (fp_text user R2 (at 0 -0.0635 180) (layer B.SilkS))
    (pad 1 thru_hole circle (at -2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 VCC))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 SCL))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.2 0.2 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:Jumper (layer F.Cu) (tedit 5AA80FFE)
    (at 188.875 101.25 270)
    (attr smd)
    (fp_text reference JP2 (at -2.413 0.127 270) (layer F.SilkS) hide)
    (fp_text value " " (at -2.25 -0.125 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.50038 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 26 GND) (clearance 0.1905))
    (pad 2 smd rect (at 0.50038 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(J2-Pad4)") (clearance 0.1905))
    (model smd\resistors\R0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:Jumper (layer F.Cu) (tedit 5AA80FF1)
    (at 186.375 101.25 270)
    (attr smd)
    (fp_text reference JP3 (at -2.413 0.127 270) (layer F.SilkS) hide)
    (fp_text value " " (at -2.25 0.125 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.50038 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC) (clearance 0.1905))
    (pad 2 smd rect (at 0.50038 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(J2-Pad3)") (clearance 0.1905))
    (model smd\resistors\R0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:Jumper (layer F.Cu) (tedit 5AA80FE7)
    (at 183.875 101.25 270)
    (attr smd)
    (fp_text reference JP4 (at -2.413 0.127 270) (layer F.SilkS) hide)
    (fp_text value " " (at -2.5 -0.125 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.50038 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 49 SCL) (clearance 0.1905))
    (pad 2 smd rect (at 0.50038 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J2-Pad2)") (clearance 0.1905))
    (model smd\resistors\R0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:Jumper (layer F.Cu) (tedit 5AA80FDA)
    (at 181.375 101.25 270)
    (attr smd)
    (fp_text reference JP5 (at -2.413 0.127 270) (layer F.SilkS) hide)
    (fp_text value " " (at -2.25 -0.125 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.50038 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 50 SDA) (clearance 0.1905))
    (pad 2 smd rect (at 0.50038 0 270) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J2-Pad1)") (clearance 0.1905))
    (model smd\resistors\R0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:Jumper (layer B.Cu) (tedit 5AA81026)
    (at 188.875 101.25 270)
    (attr smd)
    (fp_text reference JP6 (at -2.413 -0.127 270) (layer B.SilkS) hide)
    (fp_text value " " (at -2.794 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.50038 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 50 SDA) (clearance 0.1905))
    (pad 2 smd rect (at 0.50038 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 59 "Net-(J2-Pad4)") (clearance 0.1905))
    (model smd\resistors\R0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:Jumper (layer B.Cu) (tedit 5AA8101B)
    (at 186.375 101.25 270)
    (attr smd)
    (fp_text reference JP7 (at -2.413 -0.127 270) (layer B.SilkS) hide)
    (fp_text value " " (at -2.794 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.50038 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 49 SCL) (clearance 0.1905))
    (pad 2 smd rect (at 0.50038 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 58 "Net-(J2-Pad3)") (clearance 0.1905))
    (model smd\resistors\R0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:Jumper (layer B.Cu) (tedit 5AA8100B)
    (at 183.875 101.25 270)
    (attr smd)
    (fp_text reference JP8 (at -2.413 -0.127 270) (layer B.SilkS) hide)
    (fp_text value " " (at -2.794 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.50038 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC) (clearance 0.1905))
    (pad 2 smd rect (at 0.50038 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 57 "Net-(J2-Pad2)") (clearance 0.1905))
    (model smd\resistors\R0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:Jumper (layer B.Cu) (tedit 5AA809C7)
    (at 181.375 101.25 270)
    (attr smd)
    (fp_text reference JP9 (at -2.413 -0.127 270) (layer B.SilkS) hide)
    (fp_text value " " (at -2.794 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.50038 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 26 GND) (clearance 0.1905))
    (pad 2 smd rect (at 0.50038 0 270) (size 0.635 1.143) (layers B.Cu B.Paste B.Mask)
      (net 56 "Net-(J2-Pad1)") (clearance 0.1905))
    (model smd\resistors\R0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:StripLED_rev (layer F.Cu) (tedit 5A0FFE9D)
    (at 174 107.9 180)
    (fp_text reference J3 (at 0 -2.54 180) (layer F.SilkS) hide)
    (fp_text value LED (at 0 7.62 180) (layer F.Fab) hide)
    (pad 3 smd rect (at 0 5.08 180) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 27 VCC))
    (pad 2 smd rect (at 0 2.54 180) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 34 LED))
    (pad 1 smd rect (at 0 0 180) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 26 GND))
    (pad 1 smd rect (at 0 5.08 180) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 26 GND))
    (pad 2 smd rect (at 0 2.54 180) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 34 LED))
    (pad 3 smd rect (at 0 0 180) (size 1.524 1.524) (layers B.Cu B.Paste B.Mask)
      (net 27 VCC))
  )
  (module kbd:JPC2 (layer F.Cu) (tedit 5AD20B15)
    (at 181.1 112.8)
    (attr smd)
    (fp_text reference data (at -0.1 2.3 270) (layer F.SilkS))
    (fp_text value " " (at 0 1.524) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.50038 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 35 data) (clearance 0.1905))
    (pad 2 smd rect (at 0.50038 0) (size 0.635 1.143) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(J1-PadB)") (clearance 0.1905))
    (pad "" smd rect (at 0 0 90) (size 0.381 0.381) (layers F.Cu F.Paste F.Mask)
      (clearance 0.00254))
    (model smd\resistors\R0603.wrl
      (offset (xyz 0 0 0.02539999961853028))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:OLED (layer F.Cu) (tedit 5AD20961)
    (at 181.3 105.3)
    (descr "Connecteur 6 pins")
    (tags "CONN DEV")
    (fp_text reference OLED (at 3.7 -2 180) (layer F.SilkS))
    (fp_text value OLED (at 3.81 1.27) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(J2-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(J2-Pad4)"))
  )
  (module kbd:1pin_conn (layer F.Cu) (tedit 5AD20A86)
    (at 181 108)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference P1 (at 1.9 0.1) (layer F.SilkS))
    (fp_text value i2c-pin (at 0 -1.4605) (layer F.SilkS) hide)
    (fp_text user P1 (at 1.8 0.1) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(J1-PadA)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.2 0.2 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:1pin_conn (layer F.Cu) (tedit 5AD20A9B)
    (at 181 110.3)
    (descr "Resitance 3 pas")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference P2 (at 1.8 0) (layer F.SilkS))
    (fp_text value i2c-pin (at 0 -1.4605) (layer F.SilkS) hide)
    (fp_text user P2 (at 1.8 0) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(J1-PadB)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.2 0.2 0.2))
      (rotate (xyz 0 0 0))
    )
  )
  (module kbd:ResetSW (layer F.Cu) (tedit 5AD77D8C)
    (at 192.9 107 90)
    (fp_text reference RSW1 (at 0.265 0.73 90) (layer F.SilkS) hide)
    (fp_text value Reset (at 0 0 270) (layer F.SilkS))
    (fp_text user Reset (at 0.127 0 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 3.25 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 48 reset))
    (pad 2 thru_hole circle (at -3.25 0 90) (size 2 2) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 26 GND))
  )
  (module kbd:MJ-4PP-9 (layer F.Cu) (tedit 5AD77DC2)
    (at 194.7 116.7 270)
    (fp_text reference TRRS (at -0.889 6.4135 270) (layer F.SilkS))
    (fp_text value MJ-4PP-9 (at 0 14 270) (layer F.Fab) hide)
    (fp_text user TRRS (at -0.8255 6.4135 270) (layer B.SilkS))
    (pad "" np_thru_hole circle (at -1.75 8.5 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -1.75 1.5 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad D thru_hole oval (at -3.85 10.3 270) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 27 VCC) (clearance 0.15))
    (pad A thru_hole oval (at 0.35 11.8 270) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(J1-PadA)") (clearance 0.15))
    (pad B thru_hole oval (at -3.85 3.3 270) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(J1-PadB)"))
    (pad C thru_hole oval (at -3.85 6.3 270) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 26 GND))
    (pad "" np_thru_hole circle (at 0 1.5 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 0 8.5 270) (size 1.2 1.2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad B thru_hole oval (at 2.1 3.3 270) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(J1-PadB)"))
    (pad C thru_hole oval (at 2.1 6.3 270) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 26 GND))
    (pad D thru_hole oval (at 2.1 10.3 270) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 27 VCC) (clearance 0.15))
    (pad A thru_hole oval (at -2.1 11.8 270) (size 1.7 2.5) (drill oval 1 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(J1-PadA)") (clearance 0.15))
    (model "../../../../../../Users/pluis/Documents/Magic Briefcase/Documents/KiCad/3d/AB2_TRS_3p5MM_PTH.wrl"
      (at (xyz 0 0 0))
      (scale (xyz 0.42 0.42 0.42))
      (rotate (xyz 0 0 90))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5BBACA09)
    (at 171.704 63.627)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF01 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at -3.048 -5.588) (layer F.Fab) hide)
    (fp_text user %R (at 0.254 2.54) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5BBACA0F)
    (at 81.7626 74.8538)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF02 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at -4.9784 -6.3119) (layer F.Fab) hide)
    (fp_text user %R (at -4.3053 -0.381) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5BBA82D9)
    (at 189.4078 137.4648)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF03 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value "" (at 11.43 6.35) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text "TinyPinky42 v0.1\nPCB design by ryo1kato@" (at 113.1316 122.6312) (layer B.Mask))
  (gr_text "TinyPinky42 v0.1\nPCB design by ryo1kato@" (at 113.3348 122.5804) (layer F.Mask))
  (gr_arc (start 89.130658 74.876679) (end 89.156058 76.197479) (angle 65.95690606) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 74.546942 74.851279) (end 74.521542 76.172079) (angle -65.95690606) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.9348 75.438) (end 86.743088 72.801471) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 75.7428 75.4126) (end 76.8858 72.7964) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 164.158142 64.437279) (end 164.132742 65.758079) (angle -65.95690606) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165.354 65.024) (end 166.878 61.6458) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.0192 67.2338) (end 176.692253 61.778721) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 2.230396 (width 0.3) (layer F.CrtYd)
    (gr_text "2.230 mm" (at 153.237799 59.572296 270) (layer F.CrtYd))
    (feature1 (pts (xy 171.009599 60.687494) (xy 154.751378 60.687494)))
    (feature2 (pts (xy 171.009599 58.457098) (xy 154.751378 58.457098)))
    (crossbar (pts (xy 155.337799 58.457098) (xy 155.337799 60.687494)))
    (arrow1a (pts (xy 155.337799 60.687494) (xy 154.751378 59.56099)))
    (arrow1b (pts (xy 155.337799 60.687494) (xy 155.92422 59.56099)))
    (arrow2a (pts (xy 155.337799 58.457098) (xy 154.751378 59.583602)))
    (arrow2b (pts (xy 155.337799 58.457098) (xy 155.92422 59.583602)))
  )
  (dimension 5.0038 (width 0.3) (layer F.CrtYd)
    (gr_text "clearance 5mm" (at 176.6697 52.459161) (layer F.CrtYd))
    (feature1 (pts (xy 179.1716 67.5132) (xy 179.1716 53.97274)))
    (feature2 (pts (xy 174.1678 67.5132) (xy 174.1678 53.97274)))
    (crossbar (pts (xy 174.1678 54.559161) (xy 179.1716 54.559161)))
    (arrow1a (pts (xy 179.1716 54.559161) (xy 178.045096 55.145582)))
    (arrow1b (pts (xy 179.1716 54.559161) (xy 178.045096 53.97274)))
    (arrow2a (pts (xy 174.1678 54.559161) (xy 175.294304 55.145582)))
    (arrow2b (pts (xy 174.1678 54.559161) (xy 175.294304 53.97274)))
  )
  (gr_arc (start 180.213 66.675) (end 180.2384 67.9958) (angle 65.95690606) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 171.765834 63.654793) (end 166.878 61.6458) (angle 136.8086076) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.0098 124.0518) (end 156.0098 128.498601) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.5098 124.0018) (end 156.0098 124.0018) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 192.3796 132.969) (end 192.9384 133.51764) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 193.492174 131.630677) (end 191.852553 131.039311) (angle -69.73198907) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 191.85128 131.04368) (end 194.75 120.091202) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.4107 125.4379) (end 137.5791 129.7686) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.0198 126.3396) (end 134.1882 130.6703) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.1882 130.683) (end 137.5791 129.7813) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.0325 126.3269) (end 136.4107 125.4252) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181.356 130.6195) (end 182.5244 126.2888) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.9651 129.7178) (end 179.1335 125.3871) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.9778 129.7305) (end 181.356 130.6195) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 81.8134 74.8284) (end 76.8858 72.7964) (angle 135.2392756) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 182.76824 142.6464) (end 189.402727 142.6464) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 189.410061 137.399788) (end 192.94075 133.518896) (angle 137.840902) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.39392 139.45108) (end 132.6642 142.58544) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 99.517204 131.648213) (end 100.017204 131.648213) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100.5252 126.9412) (end 100.0252 126.9412) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.0252 126.9492) (end 100.0252 131.6482) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125.811322 126.4412) (end 100.5332 126.4412) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.5236 76.1746) (end 63.9826 76.1746) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text OLED (at 185.1 103.3) (layer B.SilkS))
  (gr_text LED (at 171.9 106) (layer F.SilkS))
  (gr_text LED (at 172 106) (layer B.SilkS))
  (gr_text GND (at 172 108.5) (layer F.SilkS))
  (gr_text VCC (at 172 108.5) (layer B.SilkS))
  (gr_text GND (at 171.9 103.3) (layer B.SilkS))
  (gr_text VCC (at 171.9 103.3) (layer F.SilkS))
  (gr_text "Based on “Corne Classic” v2.0\nby foostan" (at 184.92724 95.92818 90) (layer F.Mask))
  (gr_line (start 194.25 68) (end 180.213 68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 132.207 140.95984) (end 132.6642 142.58544) (angle 92.94177375) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 125.809352 127.460039) (end 125.8062 126.4412) (angle 73.79876013) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.77648 127.14224) (end 130.556 141.33576) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 63.9873 131.648213) (end 63.9873 132.148213) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 63.9826 76.6746) (end 63.4826 76.6746) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 100.0078 75.692) (end 100.5078 75.692) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 101.0332 63.949814) (end 100.5078 63.975214) (angle 92.76775909) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.48592 62.9238) (end 118.98592 62.9238) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 119.499022 61.518746) (end 118.98592 61.518746) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 136.51268 61.50102) (end 136.51268 61.00102) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 137.5156 62.8984) (end 137.5156 63.3984) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 154.9908 63.89078) (end 154.9908 63.3984) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155.98539 65.243497) (end 155.97523 65.746037) (angle 86.46340276) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 194.25 68.5) (end 194.25 68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170.87088 139.45616) (end 182.76316 142.6464) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.3736 139.45616) (end 170.876042 139.45616) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 194.75 68.5) (end 194.75 120.091202) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.517204 132.148213) (end 63.9873 132.148213) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.1335 125.3744) (end 182.5244 126.2761) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.5098 128.498624) (end 159.5098 124.0018) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.0068 128.4986) (end 159.5068 128.4986) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.75 105) (end 163.25 105) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.75 109.5) (end 166.75 105) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.25 109.5) (end 166.75 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.25 105) (end 163.25 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.2453 102.6246) (end 144.7453 102.6246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.2453 107.1246) (end 148.2453 102.6246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.7453 107.1246) (end 148.2453 107.1246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.7453 102.6246) (end 144.7453 107.0746) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.7406 100.25) (end 126.2406 100.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.7406 104.75) (end 129.7406 100.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.2406 104.75) (end 129.7406 104.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.2406 100.3) (end 126.2406 104.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.2486 102.6246) (end 107.7486 102.6246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.2486 107.1246) (end 111.2486 102.6246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.7486 107.1246) (end 111.2486 107.1246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.7486 102.6246) (end 107.7486 107.0746) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.75 86) (end 163.25 86) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.75 90.5) (end 166.75 86) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.25 90.5) (end 166.75 90.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.25 86) (end 163.25 90.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.258 83.6246) (end 144.758 83.6246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.258 88.1246) (end 148.258 83.6246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.758 88.1246) (end 148.258 88.1246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.758 83.6246) (end 144.758 88.0746) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.7533 81.25) (end 126.2533 81.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.7533 85.75) (end 129.7533 81.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.2533 85.75) (end 129.7533 85.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.2533 81.3) (end 126.2533 85.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.2486 83.6246) (end 107.7486 83.6246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.2486 88.1246) (end 111.2486 83.6246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.7486 88.1246) (end 111.2486 88.1246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.7486 83.6246) (end 107.7486 88.0746) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.75 67) (end 163.25 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.75 71.5) (end 166.75 67) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.25 71.5) (end 166.75 71.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.25 67) (end 163.25 71.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.2453 64.6373) (end 144.7453 64.6373) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.2453 69.1373) (end 148.2453 64.6373) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.7453 69.1373) (end 148.2453 69.1373) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.7453 64.6373) (end 144.7453 69.0873) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.7533 62.25) (end 126.2533 62.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 129.7533 66.75) (end 129.7533 62.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.2533 66.75) (end 129.7533 66.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126.2533 62.25) (end 126.2533 66.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.2613 64.6246) (end 107.7613 64.6246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 111.2613 69.1246) (end 111.2613 64.6246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.7613 69.1246) (end 111.2613 69.1246) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107.7613 64.6246) (end 107.7613 69.0746) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.7566 115.4645) (end 89.2566 115.4645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.7566 119.9645) (end 92.7566 115.4645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.2566 119.9645) (end 92.7566 119.9645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.2566 115.4645) (end 89.2566 119.9645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.2519 115.4264) (end 70.7519 115.4264) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.2519 119.9264) (end 74.2519 115.4264) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.7519 119.9264) (end 74.2519 119.9264) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.7519 115.4264) (end 70.7519 119.9264) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.7566 96.4645) (end 89.2566 96.4645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.7566 100.9645) (end 92.7566 96.4645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.2566 100.9645) (end 92.7566 100.9645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.2566 96.4645) (end 89.2566 100.9645) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.2519 96.4264) (end 70.7519 96.4264) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.2519 100.9264) (end 74.2519 96.4264) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.7519 100.9264) (end 74.2519 100.9264) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.7519 96.4264) (end 70.7519 100.9264) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.7354 77.4446) (end 89.2354 77.4446) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.7354 81.9446) (end 92.7354 77.4446) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.2481 81.9531) (end 92.7481 81.9531) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.2429 77.4573) (end 89.2429 81.9573) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.2442 77.4319) (end 70.7442 77.4319) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.2442 81.9277) (end 74.2442 77.4277) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.7442 81.9404) (end 74.2442 81.9404) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.7517 77.4319) (end 70.7517 81.9319) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 63.4873 76.657186) (end 63.4873 131.648213) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 99.9998 76.19834) (end 89.154 76.19834) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100.5078 63.9572) (end 100.5078 75.6827) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.50881 63.4238) (end 101.058958 63.4238) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.98592 61.518746) (end 118.98592 62.9238) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.499603 61) (end 119.4816 61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.01268 62.890409) (end 137.01268 61.5134) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.973074 63.3984) (end 137.541 63.3984) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.48318 65.264356) (end 155.48318 63.89078) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.160213 65.75) (end 155.9814 65.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 26) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.7 67.9) (xy 179.4256 67.8942) (xy 174.0154 66.548) (xy 172.3136 67.2084) (xy 170.2562 67.0052)
        (xy 168.5544 65.6844) (xy 155.4988 65.7606) (xy 155.4861 63.2714) (xy 137.046711 63.2) (xy 137.062288 60.9)
        (xy 118.98492 60.9) (xy 118.9736 63.4492) (xy 100.5459 63.5381) (xy 100.457 76.2254) (xy 85.217 76.3016)
        (xy 83.9978 77.8256) (xy 81.8896 78.5876) (xy 79.8068 78.0288) (xy 78.2066 76.3016) (xy 63.5762 76.3016)
        (xy 63.5762 132.2578) (xy 100.0252 132.2324) (xy 100.025729 126.4539) (xy 126.619 126.3904) (xy 131.00304 142.96136)
        (xy 144.40408 139.35456) (xy 170.95724 139.36472) (xy 182.83428 142.56004) (xy 185.0136 142.5702) (xy 185.039 136.7282)
        (xy 187.1726 133.5532) (xy 191.389 132.5372) (xy 194.7418 120.2563) (xy 194.8 67.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.507 96.2152) (xy 120.7262 96.7232) (xy 121.4882 97.3328) (xy 122.0724 98.7552) (xy 122.0724 100.0506)
        (xy 121.5644 101.4984) (xy 120.7008 102.4128) (xy 119.2784 102.9462) (xy 117.729 102.9716) (xy 116.4336 102.3112)
        (xy 115.6208 101.3714) (xy 115.1636 100.2538) (xy 115.3414 98.7552) (xy 115.6716 97.8662) (xy 116.4082 96.9772)
        (xy 117.2464 96.4692) (xy 118.2624 96.1644)
      )
    )
  )
  (zone (net 26) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 194.7 67.9) (xy 179.4256 67.8942) (xy 174.0154 66.548) (xy 172.3136 67.2084) (xy 170.2562 67.0052)
        (xy 168.5544 65.6844) (xy 155.4988 65.7606) (xy 155.4861 63.2714) (xy 137.046711 63.2) (xy 137.062288 60.9)
        (xy 118.98492 60.9) (xy 118.9736 63.4492) (xy 100.5459 63.5381) (xy 100.457 76.2254) (xy 85.217 76.3016)
        (xy 83.9978 77.8256) (xy 81.8896 78.5876) (xy 79.8068 78.0288) (xy 78.2066 76.3016) (xy 63.5762 76.3016)
        (xy 63.5762 132.2578) (xy 100.0252 132.2324) (xy 100.025729 126.4539) (xy 126.619 126.3904) (xy 131.00304 142.96136)
        (xy 144.40408 139.35456) (xy 170.95724 139.36472) (xy 182.83428 142.56004) (xy 185.0136 142.5702) (xy 185.039 136.7282)
        (xy 187.1726 133.5532) (xy 191.389 132.5372) (xy 194.7418 120.2563) (xy 194.8 67.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 156.083 78.994) (xy 157.3022 79.502) (xy 158.0642 80.1116) (xy 158.6484 81.534) (xy 158.6484 82.8294)
        (xy 158.1404 84.2772) (xy 157.2768 85.1916) (xy 155.8544 85.725) (xy 154.305 85.7504) (xy 153.0096 85.09)
        (xy 152.1968 84.1502) (xy 151.7396 83.0326) (xy 151.9174 81.534) (xy 152.2476 80.645) (xy 152.9842 79.756)
        (xy 153.8224 79.248) (xy 154.8384 78.9432)
      )
    )
  )
)
