(kicad_pcb (version 20171130) (host pcbnew 5.1.7-a382d34a8~88~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 12)
    (tracks 26)
    (zones 0)
    (modules 3)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 38.675001 37.125001)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(J2-Pad7)")
  (net 2 "Net-(J2-Pad5)")
  (net 3 "Net-(J2-Pad8)")
  (net 4 "Net-(J2-Pad6)")
  (net 5 "Net-(J2-Pad4)")
  (net 6 "Net-(J2-Pad2)")
  (net 7 "Net-(J3-Pad1)")
  (net 8 "Net-(J3-Pad8)")
  (net 9 "Net-(J3-Pad4)")
  (net 10 "Net-(J3-Pad2)")
  (net 11 +5V)
  (net 12 /RX)
  (net 13 /TX)
  (net 14 /DTR)
  (net 15 /RTS)
  (net 16 GND)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /DTR)
    (add_net /RTS)
    (add_net /RX)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad8)")
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right (layer F.Cu) (tedit 5A19A424)
    (at 51.375001 37.125001)
    (descr "surface-mounted straight socket strip, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated")
    (tags "Surface mounted socket strip SMD 1x08 2.54mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference J3 (at 0 -11.76) (layer F.SilkS) hide)
    (fp_text value Conn_01x08_Female (at 0 11.76) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 7 smd rect (at 1.65 6.35) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 15 /RTS))
    (pad 5 smd rect (at 1.65 1.27) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /TX))
    (pad 3 smd rect (at 1.65 -3.81) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /DTR))
    (pad 1 smd rect (at 1.65 -8.89) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J3-Pad1)"))
    (pad 8 smd rect (at -1.65 8.89) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J3-Pad8)"))
    (pad 6 smd rect (at -1.65 3.81) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /RX))
    (pad 4 smd rect (at -1.65 -1.27) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J3-Pad4)"))
    (pad 2 smd rect (at -1.65 -6.35) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J3-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right (layer F.Cu) (tedit 5A19A424)
    (at 38.675001 37.125001)
    (descr "surface-mounted straight socket strip, 1x08, 2.54mm pitch, single row, style 2 (pin 1 right) (https://cdn.harwin.com/pdfs/M20-786.pdf), script generated")
    (tags "Surface mounted socket strip SMD 1x08 2.54mm single row style2 pin1 right")
    (attr smd)
    (fp_text reference J2 (at 0 -11.76) (layer F.SilkS) hide)
    (fp_text value Conn_01x08_Female (at 0 11.76) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 7 smd rect (at 1.65 6.35) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J2-Pad7)"))
    (pad 5 smd rect (at 1.65 1.27) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J2-Pad5)"))
    (pad 3 smd rect (at 1.65 -3.81) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad 1 smd rect (at 1.65 -8.89) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 11 +5V))
    (pad 8 smd rect (at -1.65 8.89) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J2-Pad8)"))
    (pad 6 smd rect (at -1.65 3.81) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J2-Pad6)"))
    (pad 4 smd rect (at -1.65 -1.27) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J2-Pad4)"))
    (pad 2 smd rect (at -1.65 -6.35) (size 1.9 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J2-Pad2)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical_SMD_Pin1Right.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "S6B-ZR-SM4A-TF(LF)(SN):JST_S6B-ZR-SM4A-TF(LF)(SN)" (layer F.Cu) (tedit 6015D2A5)
    (at 44.965001 51.035001)
    (fp_text reference J1 (at -2.826705 -2.336415) (layer F.SilkS) hide)
    (fp_text value "S6B-ZR-SM4A-TF(LF)(SN)" (at 10.51135 6.5658) (layer F.Fab))
    (pad 6 smd rect (at 3.75 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 +5V))
    (pad 5 smd rect (at 2.25 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /RX))
    (pad 4 smd rect (at 0.75 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /TX))
    (pad 3 smd rect (at -0.75 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /DTR))
    (pad 2 smd rect (at -2.25 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /RTS))
    (pad 1 smd rect (at -3.75 0) (size 0.7 2.5) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad SH2 smd rect (at 5.7 3.6) (size 1.1 1.9) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (pad SH1 smd rect (at -5.7 3.6) (size 1.1 1.9) (layers F.Cu F.Paste F.Mask)
      (net 16 GND))
    (model "/home/fgervais/personal/project-adafruit-3309-adapter/hardware/kicad-library/S6B-ZR-SM4A-TF(LF)(SN)/S6B-ZR-SM4A-TF_LF__SN_.step"
      (offset (xyz 0 0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (gr_text "François Gervais\n31 jan 2021\nv1.0.0" (at 53.675001 27.125001) (layer B.SilkS))
  (gr_arc (start 54.931001 55.921001) (end 54.931001 56.175001) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 35.119001 55.921001) (end 34.865001 55.921001) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 35.119001 23.409001) (end 35.119001 23.155001) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 54.931001 23.409001) (end 55.185001 23.409001) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 55.185001 25.695001) (end 55.185001 23.409001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 34.865001 25.695001) (end 34.865001 23.409001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 34.865001 55.921001) (end 34.865001 37.125001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 54.931001 56.175001) (end 35.119001 56.175001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 55.185001 25.695001) (end 55.185001 55.921001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 35.119001 23.155001) (end 54.931001 23.155001) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 34.865001 37.125001) (end 34.865001 25.695001) (layer Edge.Cuts) (width 0.05))
  (zone (net 11) (net_name +5V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.185001 56.175001) (xy 34.865001 56.175001) (xy 34.865001 23.155001) (xy 55.185001 23.155001)
      )
    )
  )
  (zone (net 16) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.185001 56.175001) (xy 34.865001 56.175001) (xy 34.865001 23.155001) (xy 55.185001 23.155001)
      )
    )
  )
)
