(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 93)
    (no_connects 0)
    (area 148.074999 79.167379 232.503321 133.152476)
    (thickness 1.6)
    (drawings 4)
    (tracks 563)
    (zones 0)
    (modules 37)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.6 5.6)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +5V)
  (net 4 "Net-(C6-Pad1)")
  (net 5 "Net-(C7-Pad1)")
  (net 6 /ETH_NETPWR)
  (net 7 /ETH_TX+)
  (net 8 /ETH_TX-)
  (net 9 /ETH_RX+)
  (net 10 /ETH_RX-)
  (net 11 "Net-(J3-Pad9)")
  (net 12 /Omega_RX)
  (net 13 /Omega_TX)
  (net 14 /TOUCH_RST)
  (net 15 /TOUCH_CHG)
  (net 16 /ETH_PWR+)
  (net 17 /ETH_PWR-)
  (net 18 "Net-(C12-Pad1)")
  (net 19 "Net-(C13-Pad1)")
  (net 20 "Net-(FB1-Pad1)")
  (net 21 "Net-(FB2-Pad1)")
  (net 22 /LEDCHAIN_DATA_5V)
  (net 23 /I2C_SCL_1)
  (net 24 /I2C_SDA_1)
  (net 25 /I2C_SCL_2)
  (net 26 /I2C_SDA_2)
  (net 27 /ETHLED_AMPEN)
  (net 28 /SD_MODE)
  (net 29 "Net-(R7-Pad2)")
  (net 30 /BITCLK)
  (net 31 /LRCLK_WS)
  (net 32 /LEDCHAIN_DATA_3V)
  (net 33 /I2S_DOUT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /BITCLK)
    (add_net /ETHLED_AMPEN)
    (add_net /ETH_NETPWR)
    (add_net /ETH_RX+)
    (add_net /ETH_RX-)
    (add_net /ETH_TX+)
    (add_net /ETH_TX-)
    (add_net /I2C_SCL_1)
    (add_net /I2C_SCL_2)
    (add_net /I2C_SDA_1)
    (add_net /I2C_SDA_2)
    (add_net /I2S_DOUT)
    (add_net /LEDCHAIN_DATA_3V)
    (add_net /LEDCHAIN_DATA_5V)
    (add_net /LRCLK_WS)
    (add_net /Omega_RX)
    (add_net /Omega_TX)
    (add_net /SD_MODE)
    (add_net /TOUCH_CHG)
    (add_net /TOUCH_RST)
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(FB1-Pad1)")
    (add_net "Net-(FB2-Pad1)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(R7-Pad2)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.75)
    (via_dia 1.2)
    (via_drill 0.6)
    (uvia_dia 1.2)
    (uvia_drill 0.6)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ETH_PWR+)
    (add_net /ETH_PWR-)
    (add_net GND)
  )
  (module plan44:plan44-HLJ-6115ANL (layer F.Cu) (tedit 581B6BD3)
    (at 209.042 90.678)
    (descr "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (tags "ETHERNET CONNECTOR (MAGJACK) FOR POE")
    (attr virtual)
    (fp_text reference J3 (at -1.27 -4.318 180) (layer F.SilkS))
    (fp_text value HLJ-6115ANL (at -1.90754 2.9591 180) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 4.45 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at 3.15468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 7 /ETH_TX+))
    (pad 2 thru_hole circle (at 1.88468 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 8 /ETH_TX-))
    (pad 3 thru_hole circle (at 0.61468 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 9 /ETH_RX+))
    (pad 4 thru_hole circle (at -0.65278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 6 /ETH_NETPWR))
    (pad 5 thru_hole circle (at -1.92278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 6 /ETH_NETPWR))
    (pad 6 thru_hole circle (at -3.19278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 10 /ETH_RX-))
    (pad 7 thru_hole circle (at -4.46278 5.8801) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 16 /ETH_PWR+))
    (pad 8 thru_hole circle (at -5.73278 8.4201) (size 1.4986 1.4986) (drill 0.89916) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 17 /ETH_PWR-))
    (pad 9 thru_hole circle (at 5.36956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 11 "Net-(J3-Pad9)"))
    (pad 10 thru_hole circle (at 2.82956 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad 11 thru_hole circle (at -5.32892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad 12 thru_hole circle (at -7.86892 -5.36956) (size 1.778 1.778) (drill 1.016) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad S1 thru_hole circle (at 6.477 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad S2 thru_hole circle (at -9.017 2.54) (size 3.048 3.048) (drill 1.59766) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad "" np_thru_hole circle (at -6.95 -0.5) (size 3.25 3.25) (drill 3.25) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 57FE2A1A)
    (at 160.02 87.63)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH1 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965_Pad (layer F.Cu) (tedit 57FE2A14)
    (at 202.438 126.492)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (fp_text reference MH2 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 3.8) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module TO_SOT_Packages_SMD:SOT-353 (layer F.Cu) (tedit 588C9996)
    (at 173.99 127.762 180)
    (descr SOT353)
    (attr smd)
    (fp_text reference U5 (at 0.1016 2.032 360) (layer F.SilkS))
    (fp_text value 74AHCT1G125 (at 0.09906 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.016 -0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.016 0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.016 -0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at -1.016 0 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 32 /LEDCHAIN_DATA_3V))
    (pad 4 smd rect (at 1.016 0.635 180) (size 0.508 0.3048) (layers F.Cu F.Paste F.Mask)
      (net 22 /LEDCHAIN_DATA_5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-353.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.07000000000000001 0.09 0.08))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 210 127.25 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C6634C)
    (at 209.75 115.25 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 4.35 0.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C6633D)
    (at 192.25 95.25 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -4.15 -0.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58AA84D1)
    (at 175.25 86.5)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 100nF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C66321)
    (at 180 109.75 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at -4.3 -0.05 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C6631A)
    (at 180 115.25 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at -4.4 -0.05 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C66357)
    (at 209.5 103.25)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C8 (at -2.7 2.25 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /ETH_NETPWR))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C469DB)
    (at 167.5 122.75 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at 0 1.75 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C46A16)
    (at 158.5 122.75 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 0 1.75 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C469B1)
    (at 167.5 115.75 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C12 (at -4 0 360) (layer F.SilkS))
    (fp_text value 220pF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C469BD)
    (at 158.5 115.75 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C13 (at -4 0.25 360) (layer F.SilkS))
    (fp_text value 220pF (at 0 2 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C469AE)
    (at 164.5 115.75 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference FB1 (at 4 0 180) (layer F.SilkS))
    (fp_text value Ferritebead (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(FB1-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C12-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58C469C9)
    (at 161.5 115.75 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference FB2 (at 4 0 180) (layer F.SilkS))
    (fp_text value Ferritebead (at 0 2 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(FB2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C13-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 159.766 128.016 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39 90) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 10.01 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /LEDCHAIN_DATA_5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 181.75 85.5 90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference P2 (at 0 -2.39 90) (layer F.SilkS))
    (fp_text value FDI_Cable (at 0 15.09 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /Omega_RX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /Omega_TX))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED53)
    (at 209.55 106.68)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (fp_text reference P3 (at 5.585 -2.27) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 5.585 7.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /I2C_SCL_1))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /TOUCH_RST))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /I2C_SDA_1))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /TOUCH_CHG))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED53)
    (at 209.55 118.618)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (fp_text reference P4 (at 5.585 -2.27) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 5.585 7.35) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /I2C_SCL_2))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /TOUCH_RST))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /I2C_SDA_2))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /TOUCH_CHG))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 158.5 108.5 180)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference P5 (at 4.315 -2.27 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 4.315 4.81 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(C13-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(C12-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 5862ED53)
    (at 201.168 106.172 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference P7 (at 1.27 -2.39 90) (layer F.SilkS))
    (fp_text value CONN_02X02 (at 1.27 4.93 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /ETH_PWR+))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /ETH_PWR-))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58C662DA)
    (at 188.75 111.25)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.45 -0.05) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /ETH_TX+))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58C662D4)
    (at 188.75 108.5)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.45 0) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /ETH_TX-))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58C662E6)
    (at 188.75 116.5)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.45 -0.1) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /ETH_RX+))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58C662E1)
    (at 188.75 114)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.45 0) (layer F.SilkS))
    (fp_text value 49.9_1% (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /ETH_RX-))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58C66347)
    (at 201.75 118)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 4.35 0.1) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9) (layer F.Fab))
    (fp_text user %R (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 /ETHLED_AMPEN))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J3-Pad9)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58C662F4)
    (at 188.75 123.25 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at -4.05 0.05 360) (layer F.SilkS))
    (fp_text value 1M (at 0 1.9 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 /SD_MODE))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58C66309)
    (at 174.75 121 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 4 0.05 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58C662EE)
    (at 186 123.25 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at 4.05 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58C66302)
    (at 180.5 126.5 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at 4 0 270) (layer F.SilkS))
    (fp_text value 1M (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 27 /ETHLED_AMPEN))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 28 /SD_MODE))
    (model Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module plan44:plan44-ONION-2MM-2X16 (layer F.Cu) (tedit 581313E0)
    (at 183.388 107.95)
    (descr "FOOTPRINT FÜR ONION OMEGA")
    (tags "FOOTPRINT FÜR ONION OMEGA")
    (attr virtual)
    (fp_text reference U1 (at 0 -19.812) (layer F.SilkS))
    (fp_text value ONION-OMEGA2 (at 0.20828 18.96364) (layer F.SilkS))
    (pad B1 thru_hole rect (at 12.39774 -13.99794) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad B2 thru_hole circle (at 12.39774 -11.99896) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 1 +3V3))
    (pad B3 thru_hole circle (at 12.39774 -9.99998) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad B4 thru_hole circle (at 12.39774 -7.99846) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad B5 thru_hole circle (at 12.39774 -5.99948) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 12 /Omega_RX))
    (pad B6 thru_hole circle (at 12.39774 -3.99796) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 13 /Omega_TX))
    (pad B7 thru_hole circle (at 12.39774 -1.99898) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad B8 thru_hole circle (at 12.39774 0) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 6 /ETH_NETPWR))
    (pad B9 thru_hole circle (at 12.39774 1.99898) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 8 /ETH_TX-))
    (pad B10 thru_hole circle (at 12.39774 3.99796) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 7 /ETH_TX+))
    (pad B11 thru_hole circle (at 12.39774 5.99948) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 10 /ETH_RX-))
    (pad B12 thru_hole circle (at 12.39774 7.99846) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 9 /ETH_RX+))
    (pad B13 thru_hole circle (at 12.39774 9.99998) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 27 /ETHLED_AMPEN))
    (pad B14 thru_hole circle (at 12.39774 11.99896) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 15 /TOUCH_CHG))
    (pad B15 thru_hole circle (at 12.39774 13.99794) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 23 /I2C_SCL_1))
    (pad B16 thru_hole circle (at 12.39774 15.99946) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 24 /I2C_SDA_1))
    (pad A1 thru_hole rect (at -11.99896 -13.99794) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 2 GND))
    (pad A2 thru_hole circle (at -11.99896 -11.99896) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A3 thru_hole circle (at -11.99896 -9.99998) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 30 /BITCLK))
    (pad A4 thru_hole circle (at -11.99896 -7.99846) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 31 /LRCLK_WS))
    (pad A5 thru_hole circle (at -11.99896 -5.99948) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 25 /I2C_SCL_2))
    (pad A6 thru_hole circle (at -11.99896 -3.99796) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 26 /I2C_SDA_2))
    (pad A7 thru_hole circle (at -11.99896 -1.99898) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 14 /TOUCH_RST))
    (pad A8 thru_hole circle (at -11.99896 0) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 32 /LEDCHAIN_DATA_3V))
    (pad A9 thru_hole circle (at -11.99896 1.99898) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A10 thru_hole circle (at -11.99896 3.99796) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A11 thru_hole circle (at -11.99896 5.99948) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A12 thru_hole circle (at -11.99896 7.99846) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A13 thru_hole circle (at -11.99896 9.99998) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A14 thru_hole circle (at -11.99896 11.99896) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS)
      (net 33 /I2S_DOUT))
    (pad A15 thru_hole circle (at -11.99896 13.99794) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
    (pad A16 thru_hole circle (at -11.99896 15.99946) (size 1.30556 1.30556) (drill 0.79756) (layers *.Cu *.Mask F.Paste F.SilkS))
  )
  (module Converters_DCDC_ACDC:DCDC-Conv_Recom_R-78HBxx-0.5 (layer F.Cu) (tedit 58C46976)
    (at 167.894 94.742 270)
    (descr "Recom R-78HBxx.0.5")
    (tags "Recom DCDC R-78")
    (fp_text reference U2 (at -2.242 7.644 270) (layer F.SilkS))
    (fp_text value Recom_R78Cxx (at 0 -3.85 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 1 thru_hole oval (at 0 0 270) (size 2.032 2.54) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 58C469FE)
    (at 163 122.5 90)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U3 (at -3 0 180) (layer F.SilkS))
    (fp_text value MAX98357A (at 0 2.85 90) (layer F.Fab))
    (pad 1 smd oval (at -1.475 -0.75 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /I2S_DOUT))
    (pad 2 smd oval (at -1.475 -0.25 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R7-Pad2)"))
    (pad 3 smd oval (at -1.475 0.25 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd oval (at -1.475 0.75 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 /SD_MODE))
    (pad 5 smd oval (at -0.75 1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd oval (at -0.25 1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd oval (at 0.25 1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 8 smd oval (at 0.75 1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 9 smd oval (at 1.475 0.75 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(FB1-Pad1)"))
    (pad 10 smd oval (at 1.475 0.25 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(FB2-Pad1)"))
    (pad 11 smd oval (at 1.475 -0.25 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd oval (at 1.475 -0.75 90) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd oval (at 0.75 -1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd oval (at 0.25 -1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /LRCLK_WS))
    (pad 15 smd oval (at -0.25 -1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 16 smd oval (at -0.75 -1.475 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /BITCLK))
    (pad 17 smd rect (at 0.45 0.45 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45 90) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 58C4696C)
    (at 167.75 87.5 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C4 (at 4 -3 180) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 4.21 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 58C46953)
    (at 167.75 107.25 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C9 (at 4 -3 180) (layer F.SilkS))
    (fp_text value 33uF (at 1.25 4.21 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 217.932 83.82) (end 156.464 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 156.464 130.302) (end 156.464 83.82) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.932 130.302) (end 156.464 130.302) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.932 83.82) (end 217.932 130.302) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157 84.5) (xy 217.5 84.5) (xy 217.5 129.75) (xy 156.75 129.75)
      )
    )
  )
  (zone (net 1) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 157 84.5) (xy 217.5 84.5) (xy 217.5 129.75) (xy 156.75 129.75)
      )
    )
  )
)
