(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 29)
    (no_connects 0)
    (area 76.124999 82.055 166.445001 154.635)
    (thickness 1.6)
    (drawings 42)
    (tracks 214)
    (zones 0)
    (modules 7)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 156.21 119.38)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(J1-Pad4)")
  (net 3 "Net-(J2-Pad2)")
  (net 4 "Net-(J1-Pad3)")
  (net 5 "Net-(J2-Pad4)")
  (net 6 "Net-(J1-Pad1)")
  (net 7 "Net-(J2-Pad6)")
  (net 8 "Net-(J1-Pad5)")
  (net 9 "Net-(J2-Pad8)")
  (net 10 "Net-(J2-Pad9)")
  (net 11 "Net-(J2-Pad10)")
  (net 12 "Net-(J2-Pad11)")
  (net 13 "Net-(J2-Pad12)")
  (net 14 "Net-(J2-Pad14)")
  (net 15 "Net-(J2-Pad15)")
  (net 16 "Net-(J2-Pad16)")
  (net 17 "Net-(J2-Pad17)")
  (net 18 "Net-(J2-Pad18)")
  (net 19 "Net-(J2-Pad19)")
  (net 20 "Net-(J2-Pad20)")
  (net 21 "Net-(J2-Pad21)")
  (net 22 "Net-(J2-Pad22)")
  (net 23 "Net-(J2-Pad23)")
  (net 24 "Net-(J2-Pad24)")
  (net 25 "Net-(J2-Pad26)")
  (net 26 "Net-(J1-Pad2)")
  (net 27 "Net-(J1-Pad6)")
  (net 28 "Net-(J3-Pad4)")
  (net 29 "Net-(J4-Pad2)")
  (net 30 "Net-(J4-Pad6)")
  (net 31 "Net-(J5-Pad1)")
  (net 32 "Net-(J5-Pad4)")
  (net 33 "Net-(J5-Pad6)")
  (net 34 "Net-(J5-Pad7)")
  (net 35 "Net-(J5-Pad8)")
  (net 36 "Net-(J5-Pad9)")
  (net 37 gnd)
  (net 38 "Net-(J2-Pad25)")
  (net 39 "Net-(J3-Pad11)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad18)")
    (add_net "Net-(J2-Pad19)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad20)")
    (add_net "Net-(J2-Pad21)")
    (add_net "Net-(J2-Pad22)")
    (add_net "Net-(J2-Pad23)")
    (add_net "Net-(J2-Pad24)")
    (add_net "Net-(J2-Pad25)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad6)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad11)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J5-Pad1)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J5-Pad7)")
    (add_net "Net-(J5-Pad8)")
    (add_net "Net-(J5-Pad9)")
    (add_net gnd)
  )
  (module Connectors_DSub:DSUB-9_Male_Horizontal_Pitch2.77x2.54mm_EdgePinOffset9.40mm (layer F.Cu) (tedit 59F2C3AC)
    (at 105.41 102.87 180)
    (descr "9-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, male, pitch 2.77x2.54mm, pin-PCB-offset 9.4mm, see http://docs-europe.electrocomponents.com/webdocs/1585/0900766b81585df2.pdf")
    (tags "9-pin D-Sub connector horizontal angled 90deg THT male pitch 2.77x2.54mm pin-PCB-offset 9.4mm")
    (fp_text reference J5 (at 5.54 -1.8 180) (layer F.SilkS))
    (fp_text value DB9_Male_MountingHoles (at 5.54 19.84 180) (layer F.Fab))
    (fp_text user %R (at 5.54 15.34 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J5-Pad1)"))
    (pad 2 thru_hole circle (at 2.77 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad12)"))
    (pad 3 thru_hole circle (at 5.54 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad10)"))
    (pad 4 thru_hole circle (at 8.31 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J5-Pad4)"))
    (pad 5 thru_hole circle (at 11.08 0 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 37 gnd))
    (pad 6 thru_hole circle (at 1.385 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J5-Pad6)"))
    (pad 7 thru_hole circle (at 4.155 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J5-Pad7)"))
    (pad 8 thru_hole circle (at 6.925 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J5-Pad8)"))
    (pad 9 thru_hole circle (at 9.695 2.54 180) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J5-Pad9)"))
    (model ${KISYS3DMOD}/Connectors_DSub.3dshapes/DSUB-9_Male_Horizontal_Pitch2.77x2.54mm_EdgePinOffset9.40mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_DSub:DSUB-15-HD_Female_Horizontal_Pitch2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm (layer F.Cu) (tedit 59F2C3AC)
    (at 149.86 133.35)
    (descr "15-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, female, pitch 2.29x1.98mm, pin-PCB-offset 8.35mm, distance of mounting holes 25mm, distance of mounting holes to PCB edge 10.889999999999999mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "15-pin D-Sub connector horizontal angled 90deg THT female pitch 2.29x1.98mm pin-PCB-offset 8.35mm mounting-holes-distance 25mm mounting-hole-offset 25mm")
    (fp_text reference J3 (at -4.315 -2.58) (layer F.SilkS))
    (fp_text value DB15_Female_HighDensity_MountingHoles (at -4.315 20.21) (layer F.Fab))
    (fp_text user %R (at -4.315 15.71) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad15)"))
    (pad 2 thru_hole circle (at -2.29 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad16)"))
    (pad 3 thru_hole circle (at -4.58 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad20)"))
    (pad 4 thru_hole circle (at -6.87 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad4)"))
    (pad 5 thru_hole circle (at -9.16 0) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad26)"))
    (pad 6 thru_hole circle (at 1.145 1.98) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad17)"))
    (pad 7 thru_hole circle (at -1.145 1.98) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad14)"))
    (pad 8 thru_hole circle (at -3.435 1.98) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad18)"))
    (pad 9 thru_hole circle (at -5.725 1.98) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad22)"))
    (pad 10 thru_hole circle (at -8.015 1.98) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad24)"))
    (pad 11 thru_hole circle (at 0 3.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J3-Pad11)"))
    (pad 12 thru_hole circle (at -2.29 3.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad19)"))
    (pad 13 thru_hole circle (at -4.58 3.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad21)"))
    (pad 14 thru_hole circle (at -6.87 3.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad23)"))
    (pad 15 thru_hole circle (at -9.16 3.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad25)"))
    (pad 0 thru_hole circle (at -16.815 1.42) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 37 gnd))
    (pad 0 thru_hole circle (at 8.185 1.42) (size 4 4) (drill 3.2) (layers *.Cu *.Mask)
      (net 37 gnd))
    (model ${KISYS3DMOD}/Connectors_DSub.3dshapes/DSUB-15-HD_Female_Horizontal_Pitch2.29x1.98mm_EdgePinOffset8.35mm_Housed_MountingHolesOffset10.89mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x13_Pitch2.54mm (layer B.Cu) (tedit 58CD5449)
    (at 114.3 109.22 270)
    (descr "Through hole straight socket strip, 2x13, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x13 2.54mm double row")
    (fp_text reference J2 (at -1.27 2.33 270) (layer B.SilkS))
    (fp_text value Conn_02x13_Odd_Even (at -1.27 -32.81 270) (layer B.Fab))
    (fp_text user %R (at -1.27 2.33 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad4)"))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad6)"))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad8)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad9)"))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad12)"))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 gnd))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad16)"))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J2-Pad17)"))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad18)"))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J2-Pad19)"))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J2-Pad20)"))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J2-Pad21)"))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad22)"))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J2-Pad23)"))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad24)"))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J2-Pad25)"))
    (pad 26 thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad26)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x13_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.6 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module custom_kicad_footprints:Connector_Mini-DIN_Female_6Pin_2rows (layer F.Cu) (tedit 58E946D2)
    (at 95.25 137.16)
    (descr "A footprint for the generic 6 pin Mini-DIN through hole connector with shell.")
    (tags "mini din 6pin connector socket")
    (fp_text reference J4 (at -1.27 -6.35) (layer F.SilkS))
    (fp_text value Mini-DIN-6 (at -0.03 10.15) (layer F.Fab))
    (fp_text user %R (at -1.27 -6.35) (layer F.Fab))
    (pad 7 thru_hole oval (at -8.15 2.85) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 5.55 2.85) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad6)"))
    (pad 2 thru_hole circle (at -2.6 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(J4-Pad2)"))
    (pad 3 thru_hole circle (at 2.1 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad4)"))
    (pad 4 thru_hole circle (at -4.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(J2-Pad2)"))
    (pad 5 thru_hole circle (at 2.1 -2.8) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad8)"))
    (pad 6 thru_hole circle (at -4.7 -2.8) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(J4-Pad6)"))
    (pad 7 thru_hole oval (at -1.3 3.65) (size 4 2) (drill oval 3 1) (layers *.Cu *.Mask))
  )
  (module LEDs:LED_D5.0mm_Horizontal_O6.35mm_Z15.0mm (layer F.Cu) (tedit 5880A863)
    (at 124.46 137.16)
    (descr "LED, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 3.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 9.0mm, 2 pins, diameter 5.0mm z-position of LED center 15.0mm, 2 pins, diameter 5.0mm z-position of LED center 15.0mm, 2 pins, diameter 5.0mm z-position of LED center 15.0mm, 2 pins")
    (tags "LED diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 3.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 9.0mm 2 pins diameter 5.0mm z-position of LED center 15.0mm 2 pins diameter 5.0mm z-position of LED center 15.0mm 2 pins diameter 5.0mm z-position of LED center 15.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -1.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 16.01) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 gnd))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm_Horizontal_O6.35mm_Z15.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 124.46 116.84 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 270) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad9)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom_kicad_footprints:Connector_Mini-DIN_Female_6Pin_2rows (layer F.Cu) (tedit 58E946D2)
    (at 113.03 137.16)
    (descr "A footprint for the generic 6 pin Mini-DIN through hole connector with shell.")
    (tags "mini din 6pin connector socket")
    (fp_text reference J1 (at -1.27 -6.35) (layer F.SilkS))
    (fp_text value Mini-DIN-6 (at -0.03 10.15) (layer F.Fab))
    (fp_text user %R (at -1.27 -6.35) (layer F.Fab))
    (pad 7 thru_hole oval (at -8.15 2.85) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 5.55 2.85) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -2.6 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 2.1 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -4.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at 2.1 -2.8) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -4.7 -2.8) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at -1.3 3.65) (size 4 2) (drill oval 3 1) (layers *.Cu *.Mask))
  )
  (gr_text "HP MEDIASMART SERVER DEBUG BOARD\n" (at 125.73 129.54) (layer F.SilkS))
  (gr_line (start 76.2 142.24) (end 76.2 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.01 146.05) (end 162.56 146.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 80.01 142.24) (end 80.01 146.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 80.01 91.44) (end 162.56 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 80.01 95.25) (end 76.2 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 95.25) (end 166.37 142.24) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 162.56 142.24) (end 166.37 142.24) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 162.56 95.25) (end 162.56 91.44) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "VGA-15_DDC-CLOCK  " (at 144.78 120.65 90) (layer B.SilkS))
  (gr_text "VGA-14_VSYNC     " (at 142.24 119.38 90) (layer B.SilkS))
  (gr_text "VGA-21_HSYNC    " (at 139.7 119.38 90) (layer B.SilkS))
  (gr_text "VGA-12_DDC-DATA   " (at 137.16 120.65 90) (layer B.SilkS))
  (gr_text "VGA-06_GND      " (at 134.62 119.38 90) (layer B.SilkS))
  (gr_text "VGA-01_RED      " (at 132.08 119.38 90) (layer B.SilkS))
  (gr_text VGA-05_GND-- (at 144.78 99.06 90) (layer B.SilkS))
  (gr_text VGA-10_GND-- (at 142.24 99.06 90) (layer B.SilkS))
  (gr_text VGA-09_5V--- (at 139.7 99.06 90) (layer B.SilkS))
  (gr_text VGA-03_BLUE- (at 137.16 99.06 90) (layer B.SilkS))
  (gr_text VGA-08_GND-- (at 134.62 99.06 90) (layer B.SilkS))
  (gr_text "VGA-02_GREEN " (at 132.08 99.06 90) (layer B.SilkS))
  (gr_text VGA-07_GND-- (at 129.54 99.06 90) (layer B.SilkS))
  (gr_text "VGA-07_GND  " (at 129.54 97.79 90) (layer F.SilkS))
  (gr_text VGA-02_GREEN (at 132.08 97.79 90) (layer F.SilkS))
  (gr_text "VGA-08_GND  " (at 134.62 97.79 90) (layer F.SilkS))
  (gr_text "VGA-03_BLUE " (at 137.16 97.79 90) (layer F.SilkS))
  (gr_text "VGA-09_5V   " (at 139.7 97.79 90) (layer F.SilkS))
  (gr_text "VGA-10_GND  " (at 142.24 97.79 90) (layer F.SilkS))
  (gr_text "VGA-05_GND  " (at 144.78 97.79 90) (layer F.SilkS))
  (gr_text VGA-15_DDC-CLOCK- (at 144.78 119.38 90) (layer F.SilkS))
  (gr_text "VGA-14_VSYNC---- " (at 142.24 119.38 90) (layer F.SilkS))
  (gr_text VGA-06_GND------ (at 134.62 119.38 90) (layer F.SilkS))
  (gr_text VGA-01_RED------ (at 132.08 119.38 90) (layer F.SilkS))
  (gr_text VGA-21_HSYNC---- (at 139.7 119.38 90) (layer F.SilkS))
  (gr_text VGA-12_DDC-DATA-- (at 137.16 119.38 90) (layer F.SilkS))
  (gr_circle (center 80.01 95.25) (end 81.28 93.98) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 80.01 142.24) (end 78.74 140.97) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 80.01 142.24) (end 78.74 140.97) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 80.01 142.24) (end 78.74 140.97) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 80.01 142.24) (end 78.74 140.97) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 162.56 142.24) (end 161.29 140.97) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 162.56 95.25) (end 161.29 93.98) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 146.05) (xy 76.2 146.05) (xy 76.2 91.44) (xy 166.37 91.44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 146.05) (xy 76.2 146.05) (xy 76.2 91.44) (xy 166.37 91.44)
      )
    )
  )
)
