(kicad_pcb (version 20171130) (host pcbnew 5.1.10)
  (general
    (thickness 1.6)
    (drawings 22)
    (tracks 211)
    (zones 0)
    (modules 26)
    (nets 45)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 8.6 8.6)
    (pad_drill 4.3)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad1)")
  (net 2 "Net-(A1-Pad2)")
  (net 3 "Net-(A1-Pad3)")
  (net 4 LCD_A0)
  (net 5 GND)
  (net 6 LCD_A1)
  (net 7 NANO_AUDIO_OUTPUT)
  (net 8 LCD_A2)
  (net 9 SDCARD_CD)
  (net 10 LCD_A3)
  (net 11 BUTTON_PLAY)
  (net 12 LCD_I2C_SDA)
  (net 13 BUTTON_STOP)
  (net 14 LCD_I2C_SCL)
  (net 15 BUTTON_PREV)
  (net 16 BUTTON_NEXT)
  (net 17 LCD_D8)
  (net 18 "Net-(A1-Pad27)")
  (net 19 LCD_D9)
  (net 20 SDCARD_CS)
  (net 21 SDCARD_DI)
  (net 22 SDCARD_DO)
  (net 23 SDCARD_CLK)
  (net 24 "Net-(C1-Pad1)")
  (net 25 +5V)
  (net 26 "Net-(C3-Pad1)")
  (net 27 AUDIO_OUT)
  (net 28 "Net-(J3-Pad2)")
  (net 29 "Net-(J4-PadTN)")
  (net 30 "Net-(U2-Pad7)")
  (net 31 "Net-(U2-Pad8)")
  (net 32 "Net-(U2-Pad9)")
  (net 33 "Net-(U2-Pad10)")
  (net 34 "Net-(RV1-Pad2)")
  (net 35 +3V3)
  (net 36 "Net-(A1-Pad18)")
  (net 37 "Net-(A1-Pad25)")
  (net 38 "Net-(A1-Pad26)")
  (net 39 "Net-(A1-Pad28)")
  (net 40 "Net-(A1-Pad30)")
  (net 41 PWR_IN)
  (net 42 "Net-(J8-Pad3)")
  (net 43 "Net-(J4-PadRN)")
  (net 44 "Net-(J4-PadR)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net AUDIO_OUT)
    (add_net BUTTON_NEXT)
    (add_net BUTTON_PLAY)
    (add_net BUTTON_PREV)
    (add_net BUTTON_STOP)
    (add_net GND)
    (add_net LCD_A0)
    (add_net LCD_A1)
    (add_net LCD_A2)
    (add_net LCD_A3)
    (add_net LCD_D8)
    (add_net LCD_D9)
    (add_net LCD_I2C_SCL)
    (add_net LCD_I2C_SDA)
    (add_net NANO_AUDIO_OUTPUT)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad27)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad30)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-PadR)")
    (add_net "Net-(J4-PadRN)")
    (add_net "Net-(J4-PadTN)")
    (add_net "Net-(J8-Pad3)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net PWR_IN)
    (add_net SDCARD_CD)
    (add_net SDCARD_CLK)
    (add_net SDCARD_CS)
    (add_net SDCARD_DI)
    (add_net SDCARD_DO)
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 6136BC26)
    (at 110.49 106.934)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS))
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 6136BC1E)
    (at 18.288 106.68)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS))
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 6136BC0B)
    (at 18.034 30.734)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS))
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module MountingHole:MountingHole_4.3mm_M4_Pad (layer F.Cu) (tedit 6136BC14)
    (at 110.744 30.988)
    (descr "Mounting Hole 4.3mm, M4")
    (tags "mounting hole 4.3mm m4")
    (attr virtual)
    (fp_text reference REF** (at 0 -5.3) (layer F.SilkS))
    (fp_text value MountingHole_4.3mm_M4_Pad (at 0 5.3) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 8.6 8.6) (drill 4.3) (layers *.Cu *.Mask)
      (net 5 GND))
  )
  (module Display:RC1602A (layer F.Cu) (tedit 5A02FE80)
    (at 63.407001 44.978001)
    (descr http://www.raystar-optronics.com/down.php?ProID=18)
    (tags "LCD 16x2 Alphanumeric 16pin")
    (fp_text reference U2 (at -38.53 -3.41 180) (layer F.SilkS))
    (fp_text value RC1602A (at -37.22 43.58 180) (layer F.Fab))
    (fp_text user %R (at 0.185 21.705) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 +5V))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 "Net-(RV1-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 19 LCD_D9))
    (pad 5 thru_hole oval (at 10.16 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 6 thru_hole oval (at 12.7 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 LCD_D8))
    (pad 7 thru_hole oval (at 15.24 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 30 "Net-(U2-Pad7)"))
    (pad 8 thru_hole oval (at 17.78 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad8)"))
    (pad 9 thru_hole oval (at 20.32 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 32 "Net-(U2-Pad9)"))
    (pad 10 thru_hole oval (at 22.86 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 "Net-(U2-Pad10)"))
    (pad 11 thru_hole oval (at 25.4 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 LCD_A0))
    (pad 12 thru_hole oval (at 27.94 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 LCD_A1))
    (pad 13 thru_hole oval (at 30.48508 0.00254 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 LCD_A2))
    (pad 14 thru_hole oval (at 33.02 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 10 LCD_A3))
    (pad 15 thru_hole oval (at -5.08 0 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 35 +3V3))
    (pad 16 thru_hole oval (at -2.53492 0.00254 180) (size 1.8 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad "" np_thru_hole circle (at 39.22 2 180) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 40.72 38 180) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -38.28 38 180) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -36.78 2 180) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
    (pad A1 thru_hole rect (at -39.28 26.68 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad A1 thru_hole rect (at -39.28 24.14 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad A1 thru_hole rect (at -36.74 24.14 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad K1 thru_hole rect (at -36.74 19.06 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad K1 thru_hole rect (at -39.28 19.06 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (pad K1 thru_hole rect (at -39.28 16.52 180) (size 2 2) (drill 1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Display.3dshapes/RC1602A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 86.106 89.916 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value LCD_I2C (at 0 9.95 90) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 LCD_I2C_SDA))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 LCD_I2C_SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 51.054 27.94 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 2.032 -0.254 180) (layer F.SilkS))
    (fp_text value POWER (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 PWR_IN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 86.36 57.658)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS))
    (fp_text value ADAFRUIT_SDCARD (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 8.89 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 SDCARD_CLK))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 SDCARD_DO))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 SDCARD_DI))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 SDCARD_CS))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SDCARD_CD))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 40.386 27.94 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J5 (at -2.54 3.048 180) (layer F.SilkS))
    (fp_text value AUDIO (at 0 4.87 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 AUDIO_OUT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 46.736 89.662 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value BUTTONS (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 BUTTON_PLAY))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 BUTTON_STOP))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 BUTTON_PREV))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 BUTTON_NEXT))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 48.26 34.036)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 1.27 -2.37) (layer F.SilkS))
    (fp_text value 3.9K (at -2.54 -0.254 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 NANO_AUDIO_OUTPUT))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical (layer F.Cu) (tedit 5AE5139B)
    (at 50.292 39.116 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 1.27 -2.37) (layer F.SilkS))
    (fp_text value 1K (at 4.572 0.254 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.37) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:KSA_Tactile_SPST (layer F.Cu) (tedit 5A02FE31)
    (at 23.622 94.234)
    (descr "KSA http://www.ckswitches.com/media/1457/ksa_ksl.pdf")
    (tags "SWITCH SMD KSA SW")
    (fp_text reference SW1 (at 2.54 -2) (layer F.SilkS))
    (fp_text value PLAY (at 2.54 10) (layer F.Fab))
    (fp_text user %R (at 2.54 4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 11 BUTTON_PLAY))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 5.08 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.54 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/KSA_Tactile_SPST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:KSA_Tactile_SPST (layer F.Cu) (tedit 5A02FE31)
    (at 49.276 94.234)
    (descr "KSA http://www.ckswitches.com/media/1457/ksa_ksl.pdf")
    (tags "SWITCH SMD KSA SW")
    (fp_text reference SW2 (at 2.54 -2) (layer F.SilkS))
    (fp_text value STOP (at 2.54 10) (layer F.Fab))
    (fp_text user %R (at 2.54 4) (layer F.Fab))
    (pad 5 thru_hole circle (at 0 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.54 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 13 BUTTON_STOP))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/KSA_Tactile_SPST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:KSA_Tactile_SPST (layer F.Cu) (tedit 5A02FE31)
    (at 74.93 94.234)
    (descr "KSA http://www.ckswitches.com/media/1457/ksa_ksl.pdf")
    (tags "SWITCH SMD KSA SW")
    (fp_text reference SW3 (at 2.54 -2) (layer F.SilkS))
    (fp_text value PREV (at 2.54 10) (layer F.Fab))
    (fp_text user %R (at 2.54 4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 15 BUTTON_PREV))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 5.08 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.54 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (pad 5 thru_hole circle (at 0 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/KSA_Tactile_SPST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:KSA_Tactile_SPST (layer F.Cu) (tedit 5A02FE31)
    (at 100.584 94.234)
    (descr "KSA http://www.ckswitches.com/media/1457/ksa_ksl.pdf")
    (tags "SWITCH SMD KSA SW")
    (fp_text reference SW4 (at 2.54 -2) (layer F.SilkS))
    (fp_text value NEXT (at 2.54 10) (layer F.Fab))
    (fp_text user %R (at 2.54 4) (layer F.Fab))
    (pad 5 thru_hole circle (at 0 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 2.54 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 5.08 7.62) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 5.08 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole circle (at 0 0) (size 1.778 1.778) (drill 1.143) (layers *.Cu *.Mask)
      (net 16 BUTTON_NEXT))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/KSA_Tactile_SPST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 94.234 29.464)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference U1 (at 9.144 -0.254) (layer F.SilkS))
    (fp_text value LM7805_TO220 (at 2.54 2.5) (layer F.Fab))
    (fp_text user %R (at 9.144 -0.254) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 24 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 25 +5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3266P_Horizontal (layer F.Cu) (tedit 5A3D4994)
    (at 66.294 36.068 90)
    (descr "Potentiometer, horizontal, Bourns 3266P, https://www.bourns.com/docs/Product-Datasheets/3266.pdf")
    (tags "Potentiometer horizontal Bourns 3266P")
    (fp_text reference RV1 (at 4.826 2.286 180) (layer F.SilkS))
    (fp_text value 10k (at -0.76 7.145 90) (layer F.Fab))
    (fp_text user %R (at 0 2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at -2.54 2.54 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(RV1-Pad2)"))
    (pad 3 thru_hole circle (at 0 5.08 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 +5V))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3266P_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 85.852 33.02 180)
    (descr "Diode, DO-15 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Horizontal pin pitch 10.16mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D1 (at 5.588 3.048) (layer F.SilkS))
    (fp_text value 1n4001 (at 5.334 1.016) (layer F.Fab))
    (fp_text user K (at 0 -2.2) (layer F.SilkS))
    (fp_text user K (at 0 -2.2) (layer F.Fab))
    (fp_text user %R (at 5.842 -0.508) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 41 PWR_IN))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 24 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-15_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 75.692 39.116)
    (descr "Diode, DO-15 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=7.6*3.6mm^2, , http://www.diodes.com/_files/packages/DO-15.pdf")
    (tags "Diode DO-15 series Axial Horizontal pin pitch 10.16mm  length 7.6mm diameter 3.6mm")
    (fp_text reference D2 (at 5.08 -3.048) (layer F.SilkS))
    (fp_text value 1n4001 (at 5.334 1.27) (layer F.Fab))
    (fp_text user %R (at 5.65 -0.762) (layer F.Fab))
    (fp_text user K (at 0 -2.2) (layer F.Fab))
    (fp_text user K (at 0 -2.2) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad27)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 25 +5V))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-15_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 90.932 37.592)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -4.4) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 4.4) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 101.854 37.592 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1.016 4.572) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 4.4) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 +5V))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D6.3mm_P2.50mm (layer F.Cu) (tedit 5AE50EF0)
    (at 42.672 36.83 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (fp_text reference C3 (at 1.25 -4.4) (layer F.SilkS))
    (fp_text value 1uF (at 1.25 4.4) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 AUDIO_OUT))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Module:Arduino_Nano (layer B.Cu) (tedit 58ACAF70)
    (at 64.77 74.676 90)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (fp_text reference A1 (at 7.62 5.08 270) (layer B.SilkS))
    (fp_text value Arduino_Nano_v2.x (at 8.89 -19.05) (layer B.Fab))
    (fp_text user %R (at 6.35 -19.05) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 17 thru_hole oval (at 15.24 -33.02 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 35 +3V3))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad2)"))
    (pad 18 thru_hole oval (at 15.24 -30.48 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(A1-Pad18)"))
    (pad 3 thru_hole oval (at 0 -5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad3)"))
    (pad 19 thru_hole oval (at 15.24 -27.94 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 4 LCD_A0))
    (pad 4 thru_hole oval (at 0 -7.62 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 20 thru_hole oval (at 15.24 -25.4 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 6 LCD_A1))
    (pad 5 thru_hole oval (at 0 -10.16 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 7 NANO_AUDIO_OUTPUT))
    (pad 21 thru_hole oval (at 15.24 -22.86 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 8 LCD_A2))
    (pad 6 thru_hole oval (at 0 -12.7 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 9 SDCARD_CD))
    (pad 22 thru_hole oval (at 15.24 -20.32 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 10 LCD_A3))
    (pad 7 thru_hole oval (at 0 -15.24 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 16 BUTTON_NEXT))
    (pad 23 thru_hole oval (at 15.24 -17.78 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 12 LCD_I2C_SDA))
    (pad 8 thru_hole oval (at 0 -17.78 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 15 BUTTON_PREV))
    (pad 24 thru_hole oval (at 15.24 -15.24 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 14 LCD_I2C_SCL))
    (pad 9 thru_hole oval (at 0 -20.32 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 13 BUTTON_STOP))
    (pad 25 thru_hole oval (at 15.24 -12.7 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(A1-Pad25)"))
    (pad 10 thru_hole oval (at 0 -22.86 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 11 BUTTON_PLAY))
    (pad 26 thru_hole oval (at 15.24 -10.16 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(A1-Pad26)"))
    (pad 11 thru_hole oval (at 0 -25.4 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 17 LCD_D8))
    (pad 27 thru_hole oval (at 15.24 -7.62 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad27)"))
    (pad 12 thru_hole oval (at 0 -27.94 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 19 LCD_D9))
    (pad 28 thru_hole oval (at 15.24 -5.08 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(A1-Pad28)"))
    (pad 13 thru_hole oval (at 0 -30.48 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 20 SDCARD_CS))
    (pad 29 thru_hole oval (at 15.24 -2.54 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 14 thru_hole oval (at 0 -33.02 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 21 SDCARD_DI))
    (pad 30 thru_hole oval (at 15.24 0 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(A1-Pad30)"))
    (pad 15 thru_hole oval (at 0 -35.56 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 22 SDCARD_DO))
    (pad 16 thru_hole oval (at 15.24 -35.56 90) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 23 SDCARD_CLK))
    (model ${KISYS3DMOD}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_BarrelJack:BarrelJack_CUI_PJ-102AH_Horizontal (layer F.Cu) (tedit 5A1DBF38)
    (at 59.182 39.624 180)
    (descr "Thin-pin DC Barrel Jack, https://cdn-shop.adafruit.com/datasheets/21mmdcjackDatasheet.pdf")
    (tags "Power Jack")
    (fp_text reference J8 (at 5.75 8.45 90) (layer F.SilkS))
    (fp_text value "DC Input" (at -5.5 6.2 90) (layer F.Fab))
    (fp_text user %R (at 0 6.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 41 PWR_IN))
    (pad 2 thru_hole circle (at 0 6 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 5 GND))
    (pad 3 thru_hole circle (at 4.7 3 180) (size 2.6 2.6) (drill 1.6) (layers *.Cu *.Mask)
      (net 42 "Net-(J8-Pad3)"))
    (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-102AH_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Audio:Jack_3.5mm_Ledino_KB3SPRS_Horizontal (layer F.Cu) (tedit 5BC12D58)
    (at 25.4 31.75 270)
    (descr https://www.reichelt.de/index.html?ACTION=7&LA=3&OPEN=0&INDEX=0&FILENAME=C160%252FKB3SPRS.pdf)
    (tags "jack stereo TRS")
    (fp_text reference J4 (at -3.5 2.3 90) (layer F.SilkS))
    (fp_text value AUDIO (at 2.3 -12.2 90) (layer F.Fab))
    (fp_text user %R (at 2.7 -4.6 90) (layer F.Fab))
    (pad T thru_hole rect (at 0 0 270) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 27 AUDIO_OUT))
    (pad TN thru_hole oval (at 7.3 -0.5) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 29 "Net-(J4-PadTN)"))
    (pad RN thru_hole oval (at 2.9 -7.1 270) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 43 "Net-(J4-PadRN)"))
    (pad R thru_hole oval (at 4.1 -9.8 270) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 44 "Net-(J4-PadR)"))
    (pad S thru_hole oval (at -3.9 -4.6 270) (size 2.2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_Ledino_KB3SPRS_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "9v DC input" (at 68.58 26.924) (layer F.SilkS))
  (gr_text "i2c LCD" (at 90.424 93.218) (layer F.SilkS))
  (gr_text GND (at 59.182 89.662 90) (layer F.SilkS))
  (gr_text +5v (at 86.106 91.948) (layer F.SilkS))
  (gr_text GND (at 93.98 91.948) (layer F.SilkS))
  (gr_text SCL (at 91.44 91.948) (layer F.SilkS))
  (gr_text "SDA\n" (at 88.646 91.948) (layer F.SilkS))
  (gr_text AUDIO (at 37.846 28.448 90) (layer F.SilkS))
  (gr_text +5v (at 53.086 27.94 90) (layer F.SilkS))
  (gr_text "Adafruit SD card shield\n" (at 89.408 66.802 90) (layer F.SilkS))
  (gr_text "Apple-ii cassette player - prototype 0.1\nSeptember 6, 2021\nAdrian Chadd <adrian@freebsd.org>" (at 65.278 108.204) (layer F.SilkS))
  (gr_text NEXT (at 103.124 104.14) (layer F.SilkS))
  (gr_text PREV (at 77.47 104.14) (layer F.SilkS))
  (gr_text STOP (at 51.816 104.14) (layer F.SilkS))
  (gr_text PLAY (at 26.162 104.14) (layer F.SilkS))
  (dimension 25.654 (width 0.15) (layer Dwgs.User)
    (gr_text "25.654 mm" (at 62.103 103.408) (layer Dwgs.User))
    (feature1 (pts (xy 74.93 102.108) (xy 74.93 102.694421)))
    (feature2 (pts (xy 49.276 102.108) (xy 49.276 102.694421)))
    (crossbar (pts (xy 49.276 102.108) (xy 74.93 102.108)))
    (arrow1a (pts (xy 74.93 102.108) (xy 73.803496 102.694421)))
    (arrow1b (pts (xy 74.93 102.108) (xy 73.803496 101.521579)))
    (arrow2a (pts (xy 49.276 102.108) (xy 50.402504 102.694421)))
    (arrow2b (pts (xy 49.276 102.108) (xy 50.402504 101.521579)))
  )
  (dimension 25.654 (width 0.15) (layer Dwgs.User)
    (gr_text "25.654 mm" (at 36.449 106.456) (layer Dwgs.User))
    (feature1 (pts (xy 49.276 102.108) (xy 49.276 105.742421)))
    (feature2 (pts (xy 23.622 102.108) (xy 23.622 105.742421)))
    (crossbar (pts (xy 23.622 105.156) (xy 49.276 105.156)))
    (arrow1a (pts (xy 49.276 105.156) (xy 48.149496 105.742421)))
    (arrow1b (pts (xy 49.276 105.156) (xy 48.149496 104.569579)))
    (arrow2a (pts (xy 23.622 105.156) (xy 24.748504 105.742421)))
    (arrow2b (pts (xy 23.622 105.156) (xy 24.748504 104.569579)))
  )
  (dimension 76.962 (width 0.15) (layer Dwgs.User)
    (gr_text "76.962 mm" (at 62.103 110.774) (layer Dwgs.User))
    (feature1 (pts (xy 23.622 101.854) (xy 23.622 110.060421)))
    (feature2 (pts (xy 100.584 101.854) (xy 100.584 110.060421)))
    (crossbar (pts (xy 100.584 109.474) (xy 23.622 109.474)))
    (arrow1a (pts (xy 23.622 109.474) (xy 24.748504 108.887579)))
    (arrow1b (pts (xy 23.622 109.474) (xy 24.748504 110.060421)))
    (arrow2a (pts (xy 100.584 109.474) (xy 99.457496 108.887579)))
    (arrow2b (pts (xy 100.584 109.474) (xy 99.457496 110.060421)))
  )
  (gr_line (start 116.586 25.4) (end 116.586 112.522) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 12.7 25.4) (end 116.586 25.4) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 12.7 112.522) (end 12.7 25.4) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.586 112.522) (end 12.7 112.522) (layer Edge.Cuts) (width 0.1))
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.332 25.4) (xy 116.332 112.268) (xy 12.192 112.268) (xy 12.7 25.146)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.586 112.522) (xy 12.7 112.522) (xy 12.7 25.4) (xy 116.586 25.4)
      )
    )
  )
)
