(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 37)
    (no_connects 0)
    (area 143.0302 102.4002 177.2548 137.3498)
    (thickness 1.6)
    (drawings 18)
    (tracks 110)
    (zones 0)
    (modules 17)
    (nets 18)
  )
  (page A4)
  (title_block
    (title "Roomba Christmas Tree Barrier")
    (date 2018-01-03)
    (rev B)
    (company Petezah)
    (comment 1 "(C) 2017 Peter Dunshee")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 5.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 VBUS)
  (net 2 GND)
  (net 3 +3V3)
  (net 4 /MISO/IR)
  (net 5 /SCK)
  (net 6 /MOSI/INDICATOR)
  (net 7 /RST)
  (net 8 "Net-(D1-Pad2)")
  (net 9 "Net-(D2-Pad1)")
  (net 10 "Net-(D2-Pad2)")
  (net 11 "Net-(IC1-Pad4)")
  (net 12 "Net-(J1-Pad2)")
  (net 13 "Net-(J1-Pad3)")
  (net 14 "Net-(J1-Pad4)")
  (net 15 "Net-(U1-Pad2)")
  (net 16 "Net-(U1-Pad3)")
  (net 17 "Net-(Q1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net /MISO/IR)
    (add_net /MOSI/INDICATOR)
    (add_net /RST)
    (add_net /SCK)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
  )
  (net_class 3V3 ""
    (clearance 0.3048)
    (trace_width 0.3048)
    (via_dia 1.3716)
    (via_drill 0.6604)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net +3V3)
    (add_net VBUS)
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5A1DE19F)
    (at 160.02 106.68)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.2) (layer F.Fab))
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module kicad-libs:petezah-logo-tiny (layer B.Cu) (tedit 0)
    (at 169.164 125.476 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module lib_fp:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 165.1 124.46)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 10uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VBUS))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:C_1206 (layer F.Cu) (tedit 58AA84B8)
    (at 165.1 114.3)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 10uF (at 0 2) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:Pin_Header_Straight_2x03_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 147.32 124.46)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference CON1 (at 1.27 2.33) (layer B.SilkS))
    (fp_text value AVR-ISP-6 (at 1.27 -7.41) (layer B.Fab))
    (fp_text user %R (at 1.27 -2.54 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /MISO/IR))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SCK))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /MOSI/INDICATOR))
    (pad 5 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /RST))
    (pad 6 thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:SOT-23-5_HandSoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 160.02 123.19 90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference IC1 (at 0 -2.9 90) (layer F.SilkS))
    (fp_text value MIC5225-3.3 (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VBUS))
    (pad 2 smd rect (at -1.35 0 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 VBUS))
    (pad 4 smd rect (at 1.35 0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad4)"))
    (pad 5 smd rect (at 1.35 -0.95 90) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:USB_Micro-B_10103594-0001LF placed (layer F.Cu) (tedit 58DA845F)
    (at 159.83 130)
    (descr "Micro USB Type B 10103594-0001LF")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference J1 (at -2.611 -0.158) (layer F.SilkS))
    (fp_text value USB_OTG (at 0 6.17) (layer F.Fab))
    (pad 1 smd rect (at -1.3 -1.5 90) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 VBUS))
    (pad 2 smd rect (at -0.65 -1.5 90) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at 0 -1.5 90) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad3)"))
    (pad 4 smd rect (at 0.65 -1.5 90) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at 1.3 -1.5 90) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.42 -1.62 90) (size 1.4 1.4) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.42 -1.62 90) (size 1.4 1.4) (drill 0.95) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at -2.73 1.38 90) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 thru_hole circle (at 2.73 1.38 90) (size 1.7 1.7) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -0.96 1.62 90) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.96 1.62 90) (size 2.5 1.43) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module lib_fp:JST_PH_B2B-PH-SM4-TB_02x2.00mm_Straight (layer B.Cu) (tedit 58D40574)
    (at 148.735 111.76 270)
    (descr "JST PH series connector, B2B-PH-SM4-TB, top entry type, surface mount, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (attr smd)
    (fp_text reference J2 (at 0 4.625 270) (layer B.SilkS))
    (fp_text value JSTPH (at 0 -4.875 270) (layer B.Fab))
    (fp_text user %R (at 0 2.625 270) (layer B.Fab))
    (pad 1 smd rect (at -1 -1.125 270) (size 1 5.5) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 -1.125 270) (size 1 5.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad "" smd rect (at -3.4 1.125 270) (size 1.6 3) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 3.4 1.125 270) (size 1.6 3) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B2B-PH-SM4-TB_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:JST_PH_B2B-PH-SM4-TB_02x2.00mm_Straight (layer B.Cu) (tedit 58D40574)
    (at 171.45 111.76 90)
    (descr "JST PH series connector, B2B-PH-SM4-TB, top entry type, surface mount, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (attr smd)
    (fp_text reference J3 (at 0 4.625 90) (layer B.SilkS))
    (fp_text value JSTPH (at 0 -4.875 90) (layer B.Fab))
    (fp_text user %R (at 0 2.625 90) (layer B.Fab))
    (pad 1 smd rect (at -1 -1.125 90) (size 1 5.5) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1 -1.125 90) (size 1 5.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad "" smd rect (at -3.4 1.125 90) (size 1.6 3) (layers B.Cu B.Paste B.Mask))
    (pad "" smd rect (at 3.4 1.125 90) (size 1.6 3) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_B2B-PH-SM4-TB_02x2.00mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:SOT-23_Handsoldering (layer F.Cu) (tedit 58CE4E7E)
    (at 172.72 121.69 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 152.4 130.81 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 560 (at 0 1.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 /MOSI/INDICATOR))
    (pad 2 smd rect (at 1.45 0 180) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 165.1 118.11)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85) (layer F.SilkS))
    (fp_text value 560 (at 0 1.95) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 /MISO/IR))
    (pad 2 smd rect (at 1.45 0) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:R_1206 (layer F.Cu) (tedit 58E0A804)
    (at 167.64 129.54 270)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85 270) (layer F.SilkS))
    (fp_text value 51 (at 0 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.45 0 270) (size 0.9 1.7) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module lib_fp:Resonator_SMD_muRata_CSTCE_G-3pin_3.0x0.7mm (layer F.Cu) (tedit 5A1DD9EF)
    (at 153.232 108.712 180)
    (fp_text reference Y1 (at 0 -2 180) (layer F.SilkS))
    (fp_text value 8Mhz (at 0 2 180) (layer F.Fab))
    (pad 1 smd rect (at 1.2 0 180) (size 0.4 2.1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad2)"))
    (pad 2 smd rect (at 0 0 180) (size 0.4 2.1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.2 0 180) (size 0.4 2.1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad3)"))
  )
  (module lib_fp:SOIC-8_5.35x5.40mm_Pitch1.27mm (layer F.Cu) (tedit 0)
    (at 157.48 115.57 270)
    (fp_text reference U1 (at -0.004224 -3.831624 270) (layer F.SilkS))
    (fp_text value ATTINY45-20SU (at -1.27 3.81 270) (layer F.Fab))
    (pad 8 smd rect (at 2.695776 -1.891624 180) (size 0.48 2.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -2.704224 -1.891624 180) (size 0.48 2.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /RST))
    (pad 7 smd rect (at 2.695776 -0.621624 180) (size 0.48 2.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCK))
    (pad 2 smd rect (at -2.704224 -0.621624 180) (size 0.48 2.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad2)"))
    (pad 6 smd rect (at 2.695776 0.648376 180) (size 0.48 2.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /MISO/IR))
    (pad 3 smd rect (at -2.704224 0.648376 180) (size 0.48 2.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad3)"))
    (pad 5 smd rect (at 2.695776 1.918376 180) (size 0.48 2.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /MOSI/INDICATOR))
    (pad 4 smd rect (at -2.704224 1.918376 180) (size 0.48 2.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module lib_fp:LED_1206 (layer F.Cu) (tedit 57FE943C)
    (at 147.32 129.54 270)
    (descr "LED 1206 smd package")
    (tags "LED led 1206 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.6 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.7 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.65 0 90) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module lib_fp:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 171.45 129.71 270)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45 270) (layer F.SilkS))
    (fp_text value IR_LED (at 0 1.55 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text "@Petezah\n" (at 163.068 126.492) (layer B.SilkS))
  (gr_text "Roomba Christmas Tree Barrier\n(C) Copyright 2017 Peter Dunshee\n@Petezah\n" (at 152.908 132.588 270) (layer B.SilkS))
  (gr_line (start 167.132 104.14) (end 154.94 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 147.32 106.68) (end 144.78 106.68) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 147.32 104.14) (end 154.94 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 115.824) (end 144.78 106.68) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.228 106.68) (end 173.228 104.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 147.32 132.08) (end 147.32 134.62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 173.228 132.08) (end 175.768 132.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.94 134.62) (end 147.32 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 115.824) (end 144.78 132.08) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.448 133.604) (end 154.94 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.084 133.604) (end 155.448 133.604) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173.228 104.14) (end 167.132 104.14) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.768 109.22) (end 175.768 106.68) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 175.768 132.08) (end 175.768 109.22) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.592 134.62) (end 173.228 134.62) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 164.084 133.604) (end 164.592 134.62) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.956 104.14) (xy 155.956 109.728) (xy 164.084 109.728) (xy 164.084 104.14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.956 104.14) (xy 155.956 109.728) (xy 164.084 109.728) (xy 164.084 104.14)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.78 104.14) (xy 144.78 134.62) (xy 175.768 134.62) (xy 175.768 104.14)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.78 104.14) (xy 144.78 134.62) (xy 175.768 134.62) (xy 175.768 104.14)
      )
    )
  )
)
