<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="38" y2="0" width="0" layer="20"/>
<wire x1="38" y1="0" x2="38" y2="15" width="0" layer="20"/>
<wire x1="38" y1="15" x2="0" y2="15" width="0" layer="20"/>
<wire x1="0" y1="15" x2="0" y2="0" width="0" layer="20"/>
<text>BT RC Car</text>
<text>Remote Rev 6</text>
<text>BT RC Car</text>
<text>Remote Rev 6</text>
<text>Designed by:</text>
<text>MrSwirlyEyes</text>
</plain>
<libraries>
<library name="PiB_ic_microcontrollers">
<packages>
<package name="SOIC127P798X216-8">
<description>8-SOIC, 1.27 mm pitch, 7.98 mm span, 5.24 X 5.29 X 2.16 mm body
&lt;p&gt;8-pin SOIC package with 1.27 mm pitch, 7.98 mm span with body size 5.24 X 5.29 X 2.16 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_capacitors">
<packages>
<package name="CAPC2012X95_SMD-0805">
<description>CHIP, 2 X 1.25 X 0.95 mm body
&lt;p&gt;CHIP package with body size 2 X 1.25 X 0.95 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB">
<packages>
<package name="HDRRAR5W60P254_1X5_1320X850X274B">
<description>Single-row, 5-pin Receptacle Header (Female) Right Angle, 2.54 mm (0.10 in) col pitch, 8.50 mm insulator length, 13.20 X 8.50 X 2.74 mm body
&lt;p&gt;Single-row (1X5), 5-pin Receptacle Header (Female) Right Angle package with 2.54 mm (0.10 in) col pitch, 0.60 mm lead width, 3.15 mm tail length and 8.50 mm insulator length with body size 13.20 X 8.50 X 2.74 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_switches">
<packages>
<package name="SW_SLIDE_SPDT_VERT_8.6L-4.3W">
</package>
</packages>
</library>
<library name="PiB_leds">
<packages>
<package name="LEDC2012X120_LED-0805">
<description>CHIP, 2 X 1.25 X 1.2 mm body
&lt;p&gt;CHIP package with body size 2 X 1.25 X 1.2 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_resistors">
<packages>
<package name="RESC2012X60_SMD-0805">
<description>CHIP, 2 X 1.25 X 0.6 mm body
&lt;p&gt;CHIP package with body size 2 X 1.25 X 0.6 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_ic_power">
<packages>
<package name="SOT95P280X145-5">
<description>5-SOT23, 0.95 mm pitch, 2.8 mm span, 2.9 X 1.6 X 1.45 mm body
&lt;p&gt;5-pin SOT23 package with 0.95 mm pitch, 2.8 mm span with body size 2.9 X 1.6 X 1.45 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_radio_frequency">
<packages>
<package name="HDRRAR6W60P254_1X6_1574X850X274B">
<description>Single-row, 6-pin Receptacle Header (Female) Right Angle, 2.54 mm (0.10 in) col pitch, 8.50 mm insulator length, 15.74 X 8.50 X 2.74 mm body
&lt;p&gt;Single-row (1X6), 6-pin Receptacle Header (Female) Right Angle package with 2.54 mm (0.10 in) col pitch, 0.60 mm lead width, 3.15 mm tail length and 8.50 mm insulator length with body size 15.74 X 8.50 X 2.74 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_connectors">
<packages>
<package name="HDRV6W64P254_2X3_762X483X838B_AVR-ISP">
<description>Double-row, 6-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 7.62 X 4.83 X 8.38 mm body
&lt;p&gt;Double-row (2X3), 6-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) row pitch, 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.05 mm tail length and 5.84 mm mating length with overall size 7.62 X 4.83 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="SMT-JUMPER_3_NO_SILK">
</package>
</packages>
</library>
<library name="PiB_logo">
<packages>
<package name="PIB-LOGO">
</package>
<package name="MRSWIRLYEYES-LOGO">
</package>
</packages>
</library>
<library name="PiB_batteries">
<packages>
<package name="DUAL_PTH_PADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MCU1" library="PiB_ic_microcontrollers" package="SOIC127P798X216-8" value="ATtiny85V">
<attribute name="DATASHEET" value="http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2586-AVR-8-bit-Microcontroller-ATtiny25-ATtiny45-ATtiny85_Datasheet-Summary.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=ATTINY85V-10SU-ND"/>
<attribute name="DISTPN" value="ATTINY85V-10SU-ND"/>
<attribute name="MFR" value="Microchip Technology"/>
<attribute name="MPN" value="ATTINY85V-10SU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="THUMBSTICK_L" library="PiB" package="HDRRAR5W60P254_1X5_1320X850X274B" value="Thumbstick">
<attribute name="DATASHEET_CONNECTOR" value="http://www.sullinscorp.com/drawings/78_P(N)PxCxx1LGBN-RC,_10493-G.pdf"/>
<attribute name="DIST" value="Amazon"/>
<attribute name="DISTLINK" value="https://www.amazon.com/WGCD-Joystick-Breakout-Controller-Arduino/dp/B01N59MK0U/ref=pd_lpo_vtph_107_bs_t_2?_encoding=UTF8&amp;psc=1&amp;refRID=MHMRTBXG0N745Z8HJ9AT"/>
<attribute name="DISTLINK_CONNECTOR" value="https://www.digikey.com/products/en?keywords=PPTC051LGBN-RC"/>
<attribute name="DISTPN" value="B01N59MK0U"/>
<attribute name="DIST_CONNECTOR" value="Digikey"/>
<attribute name="MFR" value="WGCD"/>
<attribute name="MFR_CONNECTOR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="N/A"/>
<attribute name="MPN_CONNECTOR" value="PPTC051LGBN-RC"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="Thumbstick"/>
</element>
<element name="THUMBSTICK_R" library="PiB" package="HDRRAR5W60P254_1X5_1320X850X274B" value="Thumbstick">
<attribute name="DATASHEET_CONNECTOR" value="http://www.sullinscorp.com/drawings/78_P(N)PxCxx1LGBN-RC,_10493-G.pdf"/>
<attribute name="DIST" value="Amazon"/>
<attribute name="DISTLINK" value="https://www.amazon.com/WGCD-Joystick-Breakout-Controller-Arduino/dp/B01N59MK0U/ref=pd_lpo_vtph_107_bs_t_2?_encoding=UTF8&amp;psc=1&amp;refRID=MHMRTBXG0N745Z8HJ9AT"/>
<attribute name="DISTLINK_CONNECTOR" value="https://www.digikey.com/products/en?keywords=PPTC051LGBN-RC"/>
<attribute name="DISTPN" value="B01N59MK0U"/>
<attribute name="DIST_CONNECTOR" value="Digikey"/>
<attribute name="MFR" value="WGCD"/>
<attribute name="MFR_CONNECTOR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="N/A"/>
<attribute name="MPN_CONNECTOR" value="PPTC051LGBN-RC"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="Thumbstick"/>
</element>
<element name="BT1" library="PiB_radio_frequency" package="HDRRAR6W60P254_1X6_1574X850X274B" value="HM-10">
<attribute name="DATASHEET" value="http://fab.cba.mit.edu/classes/863.15/doc/tutorials/programming/bluetooth/bluetooth40_en.pdf"/>
<attribute name="DATASHEET_CONNECTOR" value="http://www.sullinscorp.com/drawings/78_P(N)PxCxx1LGBN-RC,_10493-G.pdf"/>
<attribute name="DIST" value="Amazon"/>
<attribute name="DISTLINK" value="https://www.amazon.com/SunFounder-Bluetooth-Master-Module-Arduino/dp/B00V07U93U"/>
<attribute name="DISTLINK_CONNECTOR" value="https://www.digikey.com/products/en?keywords=PPTC061LGBN-RC"/>
<attribute name="DISTPN" value="B00V07U93U"/>
<attribute name="DISTPN_CONNECTOR" value="S5442-ND"/>
<attribute name="DIST_CONNECTOR" value="Digikey"/>
<attribute name="MFR" value="JNHuaMao Technology Company"/>
<attribute name="MFR_CONNECTOR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="HM-10"/>
<attribute name="MPN_CONNECTOR" value="PPTC061LGBN-RC"/>
<attribute name="NAME"/>
<attribute name="VALUE" value="HM-10"/>
</element>
<element name="AVR_ISP1" library="PiB_connectors" package="HDRV6W64P254_2X3_762X483X838B_AVR-ISP" value="PTH VERT MALE">
<attribute name="DATASHEET" value="https://cdn.amphenol-icc.com/media/wysiwyg/files/drawing/67996.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=609-3234-ND"/>
<attribute name="DISTPN" value="609-3234-ND"/>
<attribute name="MFR" value="Amphenol FCI"/>
<attribute name="MPN" value="67997-206HLF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE" value="PTH VERT MALE"/>
</element>
<element name="C3" library="PiB_capacitors" package="CAPC2012X95_SMD-0805" value="0.1uF/35V">
<attribute name="DATASHEET" value="http://ds.yuden.co.jp/TYCOMPAS/ut/detail.do?productNo=GMK212BJ104KGHT&amp;fileName=GMK212BJ104KGHT_SS&amp;mode=specSheetDownload"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=587-3364-1-ND"/>
<attribute name="DISTPN" value="587-3364-1-ND"/>
<attribute name="MFR" value="Taiyo Yuden"/>
<attribute name="MPN" value="GMK212BJ104KGHT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="PiB_resistors" package="RESC2012X60_SMD-0805" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-10KARCT-ND"/>
<attribute name="DISTPN" value="311-10KARCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0805JR-0710KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="PiB_capacitors" package="CAPC2012X95_SMD-0805" value="1uF/25V">
<attribute name="DATASHEET" value="https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM216R61E105KA12-01.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-1700-1-ND"/>
<attribute name="DISTPN" value="490-1700-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM216R61E105KA12D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="PiB_capacitors" package="CAPC2012X95_SMD-0805" value="1uF/25V">
<attribute name="DATASHEET" value="https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM216R61E105KA12-01.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=490-1700-1-ND"/>
<attribute name="DISTPN" value="490-1700-1-ND"/>
<attribute name="MFR" value="Murata Electronics North America"/>
<attribute name="MPN" value="GRM216R61E105KA12D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="PiB_leds" package="LEDC2012X120_LED-0805" value="BLUE">
<attribute name="DATASHEET" value="http://optoelectronics.liteon.com/upload/download/DS-22-99-0226/LTST-C170TBKT.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=160-1579-1-ND"/>
<attribute name="DISTPN" value="160-1579-1-ND"/>
<attribute name="MFR" value="Lite-On Inc."/>
<attribute name="MPN" value="LTST-C170TBKT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="PiB_resistors" package="RESC2012X60_SMD-0805" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KARCT-ND"/>
<attribute name="DISTPN" value="311-1.0KARCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0805JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="PiB_leds" package="LEDC2012X120_LED-0805" value="GREEN">
<attribute name="DATASHEET" value="http://optoelectronics.liteon.com/upload/download/DS22-2000-073/LTST-C170KGKT.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=160-1414-1-ND"/>
<attribute name="DISTPN" value="160-1414-1-ND"/>
<attribute name="MFR" value="Lite-On Inc."/>
<attribute name="MPN" value="LTST-C170KGKT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="PiB_resistors" package="RESC2012X60_SMD-0805" value="1K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-1.0KARCT-ND"/>
<attribute name="DISTPN" value="311-1.0KARCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0805JR-071KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="PiB_switches" package="SW_SLIDE_SPDT_VERT_8.6L-4.3W" value="300mA/30V">
<attribute name="DATASHEET" value="https://media.digikey.com/pdf/Data%20Sheets/C&amp;K/SS-12D07-VG_GA_PA.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=CKN10397-ND"/>
<attribute name="DISTPN" value="CKN10397-ND"/>
<attribute name="MFR" value="C&amp;K"/>
<attribute name="MPN" value="SS-12D07-VG 4 NS GA PA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VREG1" library="PiB_ic_power" package="SOT95P280X145-5" value="MCP1802 300mA/3.3V">
<attribute name="DATASHEET" value="http://ww1.microchip.com/downloads/en/DeviceDoc/22053C.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=MCP1802T-3302I%2FOTCT-ND"/>
<attribute name="DISTPN" value="MCP1802T-3302I/OTCT-ND"/>
<attribute name="MFR" value="Microchip Technology"/>
<attribute name="MPN" value="MCP1802T-3302I/OT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="PiB_logo" package="PIB-LOGO" value=""/>
<element name="U$1" library="PiB_logo" package="MRSWIRLYEYES-LOGO" value=""/>
<element name="LIPO1" library="PiB_batteries" package="DUAL_PTH_PADS" value="BATTERY_LIPO_2S">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP_R" library="PiB_connectors" package="SMT-JUMPER_3_NO_SILK" value="JUMPER_SMD_3-PAD_NO_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP_L" library="PiB_connectors" package="SMT-JUMPER_3_NO_SILK" value="JUMPER_SMD_3-PAD_NO_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="MCU1" pad="4"/>
<contactref element="THUMBSTICK_L" pad="GND"/>
<contactref element="THUMBSTICK_R" pad="GND"/>
<contactref element="BT1" pad="GND"/>
<contactref element="AVR_ISP1" pad="GND"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="VREG1" pad="2"/>
<contactref element="LIPO1" pad="-"/>
</signal>
<signal name="THUMBSTICK_L">
<contactref element="MCU1" pad="3"/>
<contactref element="JP_L" pad="2"/>
</signal>
<signal name="THUMBSTICK_R">
<contactref element="MCU1" pad="2"/>
<contactref element="JP_R" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="MCU1" pad="1"/>
<contactref element="AVR_ISP1" pad="RESET"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="RX">
<contactref element="MCU1" pad="7"/>
<contactref element="AVR_ISP1" pad="SCK"/>
<contactref element="BT1" pad="TX"/>
</signal>
<signal name="TX">
<contactref element="MCU1" pad="6"/>
<contactref element="AVR_ISP1" pad="MISO"/>
<contactref element="BT1" pad="RX"/>
</signal>
<signal name="MOSI">
<contactref element="MCU1" pad="5"/>
<contactref element="AVR_ISP1" pad="MOSI"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="VIN">
<contactref element="C1" pad="1"/>
<contactref element="SW1" pad="P"/>
<contactref element="VREG1" pad="1"/>
<contactref element="VREG1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="LED2" pad="K"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="LED1" pad="K"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="C2" pad="1"/>
<contactref element="VREG1" pad="5"/>
<contactref element="LED1" pad="A"/>
<contactref element="MCU1" pad="8"/>
<contactref element="C3" pad="1"/>
<contactref element="THUMBSTICK_L" pad="VCC"/>
<contactref element="THUMBSTICK_R" pad="VCC"/>
<contactref element="BT1" pad="VCC"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="+">
<contactref element="SW1" pad="S1"/>
<contactref element="LIPO1" pad="+"/>
</signal>
<signal name="N$2">
<contactref element="THUMBSTICK_L" pad="X"/>
<contactref element="JP_L" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="THUMBSTICK_L" pad="Y"/>
<contactref element="JP_L" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="THUMBSTICK_R" pad="X"/>
<contactref element="JP_R" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="JP_R" pad="3"/>
<contactref element="THUMBSTICK_R" pad="Y"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
