(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 51)
    (no_connects 0)
    (area 136.924999 103.924999 177.075001 124.075001)
    (thickness 1.6)
    (drawings 16)
    (tracks 267)
    (zones 0)
    (modules 19)
    (nets 26)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.1524)
    (user_trace_width 0.3048)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (user_via 0.508 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 2.5)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 137 104)
    (grid_origin 174.4 111.1)
    (visible_elements FFFEFF7F)
    (pcbplotparams
      (layerselection 0x010b0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 /RESET)
  (net 2 "Net-(U2-Pad2)")
  (net 3 +3V3)
  (net 4 "Net-(U2-Pad4)")
  (net 5 /SCL)
  (net 6 "Net-(U2-Pad6)")
  (net 7 "Net-(U2-Pad7)")
  (net 8 GND)
  (net 9 /SDA)
  (net 10 /BOOT)
  (net 11 /LED)
  (net 12 /RXD)
  (net 13 /TXD)
  (net 14 "Net-(U2-Pad17)")
  (net 15 "Net-(U2-Pad18)")
  (net 16 "Net-(U2-Pad19)")
  (net 17 "Net-(U2-Pad20)")
  (net 18 "Net-(U2-Pad21)")
  (net 19 "Net-(U2-Pad22)")
  (net 20 +5V)
  (net 21 "Net-(D1-Pad1)")
  (net 22 "Net-(U3-Pad3)")
  (net 23 "Net-(U3-Pad4)")
  (net 24 /DATA)
  (net 25 "Net-(R6-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /BOOT)
    (add_net /DATA)
    (add_net /LED)
    (add_net /RESET)
    (add_net /RXD)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TXD)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad4)")
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AA52EB3)
    (at 169.8 107.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.9 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 1 /RESET))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ESP8266:ESP-12E_SMD (layer F.Cu) (tedit 5AA5B1A6)
    (at 151.4 105.6)
    (descr "Module, ESP-8266, ESP-12, 16 pad, SMD")
    (tags "Module ESP-8266 ESP8266")
    (fp_text reference U2 (at 7 6.8) (layer F.SilkS))
    (fp_text value ESP-12F (at 5.08 6.35 90) (layer F.Fab) hide)
    (fp_text user "No Copper" (at 6.892 -5.4) (layer F.CrtYd))
    (pad 1 smd rect (at 0 0) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 1 /RESET))
    (pad 2 smd rect (at 0 2) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 2 "Net-(U2-Pad2)"))
    (pad 3 smd rect (at 0 4) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at 0 6) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 4 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at 0 8) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 5 /SCL))
    (pad 6 smd rect (at 0 10) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 6 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at 0 12) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 7 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at 0 14) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 9 smd rect (at 14 14) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad 10 smd rect (at 14 12) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Mask)
      (net 25 "Net-(R6-Pad2)"))
    (pad 11 smd rect (at 14 10) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Mask)
      (net 9 /SDA))
    (pad 12 smd rect (at 14 8) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Mask)
      (net 10 /BOOT))
    (pad 13 smd rect (at 14 6) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Mask)
      (net 11 /LED))
    (pad 14 smd rect (at 14 4) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Mask)
      (net 24 /DATA))
    (pad 15 smd rect (at 14 2) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Mask)
      (net 12 /RXD))
    (pad 16 smd rect (at 14 0) (size 2.5 1.1) (drill (offset 0.7 0)) (layers F.Cu F.Mask)
      (net 13 /TXD))
    (pad 17 smd rect (at 1.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 14 "Net-(U2-Pad17)"))
    (pad 18 smd rect (at 3.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 15 "Net-(U2-Pad18)"))
    (pad 19 smd rect (at 5.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 16 "Net-(U2-Pad19)"))
    (pad 20 smd rect (at 7.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 17 "Net-(U2-Pad20)"))
    (pad 21 smd rect (at 9.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 18 "Net-(U2-Pad21)"))
    (pad 22 smd rect (at 11.99 15 90) (size 2.5 1.1) (drill (offset -0.7 0)) (layers F.Cu F.Mask)
      (net 19 "Net-(U2-Pad22)"))
    (model ../../../../../Users/max/Documents/KiCad/Libraries/kicad-ESP8266-master/ESP8266.3dshapes/ESP-12-E-better.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MaxNil:BOSCH_BMP280 (layer F.Cu) (tedit 5AA51BE9)
    (at 174 107.9 270)
    (fp_text reference U4 (at 0.2 2 270) (layer F.SilkS) hide)
    (fp_text value BMP280 (at 0 -0.5 270) (layer F.Fab))
    (pad 1 smd rect (at -0.975 -0.8 270) (size 0.35 0.5) (layers F.Cu F.Mask)
      (net 8 GND) (solder_mask_margin 0.05))
    (pad 2 smd rect (at -0.325 -0.8 270) (size 0.35 0.5) (layers F.Cu F.Mask)
      (net 3 +3V3) (solder_mask_margin 0.05))
    (pad 3 smd rect (at 0.325 -0.8 270) (size 0.35 0.5) (layers F.Cu F.Mask)
      (net 9 /SDA) (solder_mask_margin 0.05))
    (pad 4 smd rect (at 0.975 -0.8 270) (size 0.35 0.5) (layers F.Cu F.Mask)
      (net 5 /SCL) (solder_mask_margin 0.05))
    (pad 8 smd rect (at -0.975 0.8 270) (size 0.35 0.5) (layers F.Cu F.Mask)
      (net 3 +3V3) (solder_mask_margin 0.05))
    (pad 7 smd rect (at -0.325 0.8 270) (size 0.35 0.5) (layers F.Cu F.Mask)
      (net 8 GND) (solder_mask_margin 0.05))
    (pad 6 smd rect (at 0.325 0.8 270) (size 0.35 0.5) (layers F.Cu F.Mask)
      (net 3 +3V3) (solder_mask_margin 0.05))
    (pad 5 smd rect (at 0.975 0.8 270) (size 0.35 0.5) (layers F.Cu F.Mask)
      (net 8 GND) (solder_mask_margin 0.05))
    (model ../../../../../Users/max/Documents/KiCad/Libraries/Module_LGA_2.0x2.5_Bosch-BMP280.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AA52E1F)
    (at 147.6 106.6 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -1.9 0 360) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 20 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AA52E25)
    (at 147.6 109.8 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2 0 360) (layer F.SilkS))
    (fp_text value 1u (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AA52E93)
    (at 174 105.5)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2 0) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AA52E96)
    (at 174 110.3)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2 0 180) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5AA52E9B)
    (at 174 122.1 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -2 0 360) (layer F.SilkS))
    (fp_text value 0.1u (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 5AA51C05)
    (at 169.8 121.6 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.25 180) (layer F.SilkS) hide)
    (fp_text value "White LED" (at 0 1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AA52EB0)
    (at 169.8 109.6 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.9 0 360) (layer F.SilkS))
    (fp_text value 4.7k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 24 /DATA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AA52EAD)
    (at 169.8 111.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.9 0 180) (layer F.SilkS))
    (fp_text value 82 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 11 /LED))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 21 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AA6F022)
    (at 169.8 115.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 1.9 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 9 /SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AA6F07D)
    (at 169.8 119.6 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -1.9 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 25 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 5AA52043)
    (at 142.2 108.2 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -4.5 180) (layer F.SilkS) hide)
    (fp_text value AZ1117-3.3 (at 0 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Mask))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Mask)
      (net 20 +5V))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-6-1EP_3x3mm_Pitch0.95mm (layer F.Cu) (tedit 5AA522A1)
    (at 174 119.6)
    (descr "DFN6 3*3 MM, 0.95 PITCH; CASE 506AH-01 (see ON Semiconductor 506AH.PDF)")
    (tags "DFN 0.95")
    (attr smd)
    (fp_text reference U3 (at -3 -2.2) (layer F.SilkS) hide)
    (fp_text value Si7021 (at 0 2.575) (layer F.Fab))
    (pad 1 smd rect (at -1.34 -0.95) (size 0.63 0.45) (layers F.Cu F.Mask)
      (net 9 /SDA))
    (pad 2 smd rect (at -1.34 0) (size 0.63 0.45) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad 3 smd rect (at -1.34 0.95) (size 0.63 0.45) (layers F.Cu F.Mask)
      (net 22 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at 1.34 0.95) (size 0.63 0.45) (layers F.Cu F.Mask)
      (net 23 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at 1.34 0) (size 0.63 0.45) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 6 smd rect (at 1.34 -0.95) (size 0.63 0.45) (layers F.Cu F.Mask)
      (net 5 /SCL))
    (pad 7 smd rect (at 0 0) (size 1.6 2.5) (layers F.Cu F.Mask)
      (solder_mask_margin 0.01) (solder_paste_margin_ratio -0.2) (clearance 0.01))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/DFN-6-1EP_3x3mm_Pitch0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04_Pitch2.54mm_SMD (layer F.Cu) (tedit 5AA57387)
    (at 143.6 117.8 180)
    (descr "surface-mounted straight pin header, 2x04, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x04 2.54mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 -6.14 180) (layer F.SilkS) hide)
    (fp_text value Con1 (at 0 6.14 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -3.81 180) (size 3.15 1) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad 2 smd rect (at 2.525 -3.81 180) (size 3.15 1) (layers F.Cu F.Mask)
      (net 1 /RESET))
    (pad 3 smd rect (at -2.525 -1.27 180) (size 3.15 1) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad 4 smd rect (at 2.525 -1.27 180) (size 3.15 1) (layers F.Cu F.Mask)
      (net 10 /BOOT))
    (pad 5 smd rect (at -2.525 1.27 180) (size 3.15 1) (layers F.Cu F.Mask)
      (net 12 /RXD))
    (pad 6 smd rect (at 2.525 1.27 180) (size 3.15 1) (layers F.Cu F.Mask)
      (net 13 /TXD))
    (pad 7 smd rect (at -2.525 3.81 180) (size 3.15 1) (layers F.Cu F.Mask)
      (net 8 GND))
    (pad 8 smd rect (at 2.525 3.81 180) (size 3.15 1) (layers F.Cu F.Mask)
      (net 20 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x04_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5AA51BEF)
    (at 174.9 115.8 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U5 (at 1.2 1.4 90) (layer F.SilkS) hide)
    (fp_text value DS1821C (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 24 /DATA))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 1 thru_hole rect (at 0 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AA52EAB)
    (at 169.8 113.6 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.9 0 360) (layer F.SilkS))
    (fp_text value 1k (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 10 /BOOT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5AA6F075)
    (at 169.8 117.6)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.9 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 5 /SCL))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "ESP8266\nTemperature\nHumidity\nPressure" (at 157 112.8) (layer B.SilkS))
  (gr_text "(c)2018 MaxNil" (at 157 121.7) (layer B.SilkS))
  (gr_text G (at 148.2 121.6) (layer F.SilkS))
  (gr_text G (at 148.2 119.1) (layer F.SilkS))
  (gr_text G (at 148.2 114) (layer F.SilkS))
  (gr_text TX (at 138 116.6) (layer F.SilkS))
  (gr_text RX (at 148.6 116.5) (layer F.SilkS))
  (gr_text +5V (at 138.1 114) (layer F.SilkS))
  (gr_text RST (at 138.3 121.6) (layer F.SilkS))
  (gr_text FLA (at 138.2 119.1) (layer F.SilkS))
  (gr_text MN016 (at 141.9 121.7) (layer B.Cu))
  (gr_line (start 137 124) (end 137 104) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177 124) (end 137 124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177 104) (end 177 124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137 104) (end 177 104) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 25 (width 0.3) (layer F.Fab)
    (gr_text "25.000 mm" (at 160.7 148.65) (layer F.Fab))
    (feature1 (pts (xy 173.2 145.1) (xy 173.2 150)))
    (feature2 (pts (xy 148.2 145.1) (xy 148.2 150)))
    (crossbar (pts (xy 148.2 147.3) (xy 173.2 147.3)))
    (arrow1a (pts (xy 173.2 147.3) (xy 172.073496 147.886421)))
    (arrow1b (pts (xy 173.2 147.3) (xy 172.073496 146.713579)))
    (arrow2a (pts (xy 148.2 147.3) (xy 149.326504 147.886421)))
    (arrow2b (pts (xy 148.2 147.3) (xy 149.326504 146.713579)))
  )
)
