(kicad_pcb (version 20171130) (host pcbnew "(6.0.0-rc1-dev-634-gb5e3f6406)")
  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 72)
    (zones 0)
    (modules 3)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.254)
    (trace_clearance 0.0508)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.508)
    (via_drill 0.254)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.254)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /+5V)
  (net 2 /CLR)
  (net 3 /GND)
  (net 4 /SEL)
  (net 5 /D2)
  (net 6 /D1)
  (net 7 /D0)
  (net 8 /D3)
  (net_class Default "This is the default net class."
    (clearance 0.0508)
    (trace_width 0.1524)
    (via_dia 0.508)
    (via_drill 0.254)
    (uvia_dia 0.508)
    (uvia_drill 0.254)
    (add_net /+5V)
    (add_net /CLR)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /GND)
    (add_net /SEL)
  )
  (module w_conn_av:minidin-8 (layer F.Cu) (tedit 5B96EBEC)
    (at 60.8395 43.024 270)
    (descr "MiniDin 8 (S-Video), Tyco P/N 1734096-1")
    (fp_text reference J3 (at 0 8.128 270) (layer F.SilkS))
    (fp_text value M-DIN-8 (at 0 -7.366 270) (layer F.SilkS))
    (pad SH thru_hole circle (at 0 2.6 270) (size 3.50012 3.50012) (drill 2.19964) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole circle (at 1.3 -1.2 270) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 1 /+5V))
    (pad 7 thru_hole circle (at -0.9 -3.8 270) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 /CLR))
    (pad 8 thru_hole circle (at -3.4 -3.8 270) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 3 /GND))
    (pad 6 thru_hole circle (at 3.4 -3.8 270) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 4 /SEL))
    (pad 4 thru_hole circle (at 1.3 -3.8 270) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 5 /D2))
    (pad 3 thru_hole circle (at 3.4 -1.2 270) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 6 /D1))
    (pad 2 thru_hole circle (at -1.3 -1.2 270) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 7 /D0))
    (pad 5 thru_hole circle (at -3.4 -1.2 270) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 8 /D3))
    (pad SH thru_hole circle (at 6.75 1.8 270) (size 3.50012 3.50012) (drill 2.19964) (layers *.Cu *.SilkS *.Mask))
    (pad SH thru_hole circle (at -6.75 1.8 270) (size 3.50012 3.50012) (drill 2.19964) (layers *.Cu *.SilkS *.Mask))
    (model walter/conn_av/minidin-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 61.214 54.737 90)
    (descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x09 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x09 (at 0 22.65 90) (layer F.Fab))
    (fp_text user %R (at 0 10.16 180) (layer F.Fab))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /+5V))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /CLR))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /SEL))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /D3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /D2))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /D1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D0))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_av:minidin-8 (layer F.Cu) (tedit 5B96EBEC)
    (at 83.947 42.926 90)
    (descr "MiniDin 8 (S-Video), Tyco P/N 1734096-1")
    (fp_text reference J1 (at 0 8.128 90) (layer F.SilkS))
    (fp_text value M-DIN-8 (at 0 -7.366 90) (layer F.SilkS))
    (pad SH thru_hole circle (at 0 2.6 90) (size 3.50012 3.50012) (drill 2.19964) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole circle (at 1.3 -1.2 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 1 /+5V))
    (pad 7 thru_hole circle (at -0.9 -3.8 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 2 /CLR))
    (pad 8 thru_hole circle (at -3.4 -3.8 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 3 /GND))
    (pad 6 thru_hole circle (at 3.4 -3.8 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 4 /SEL))
    (pad 4 thru_hole circle (at 1.3 -3.8 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 5 /D2))
    (pad 3 thru_hole circle (at 3.4 -1.2 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 6 /D1))
    (pad 2 thru_hole circle (at -1.3 -1.2 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 7 /D0))
    (pad 5 thru_hole circle (at -3.4 -1.2 90) (size 1.50114 1.50114) (drill 0.9) (layers *.Cu *.SilkS *.Mask)
      (net 8 /D3))
    (pad SH thru_hole circle (at 6.75 1.8 90) (size 3.50012 3.50012) (drill 2.19964) (layers *.Cu *.SilkS *.Mask))
    (pad SH thru_hole circle (at -6.75 1.8 90) (size 3.50012 3.50012) (drill 2.19964) (layers *.Cu *.SilkS *.Mask))
    (model walter/conn_av/minidin-8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 89.662 33.02) (end 55.118 33.02) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 89.662 57.404) (end 89.662 33.02) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 55.118 57.404) (end 89.662 57.404) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 55.118 33.02) (end 55.118 57.404) (layer Edge.Cuts) (width 0.05))
  (zone (net 3) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.118 32.766) (xy 55.118 57.658) (xy 89.662 57.658) (xy 89.662 32.766)
      )
    )
  )
  (zone (net 3) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55.118 32.766) (xy 55.118 57.658) (xy 89.662 57.658) (xy 89.662 32.766)
      )
    )
  )
)
