<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="-2" x2="90" y2="-2" width="0.05" layer="20"/>
<wire x1="90" y1="-2" x2="90" y2="31" width="0.05" layer="20"/>
<wire x1="90" y1="31" x2="65.5" y2="31" width="0.05" layer="20"/>
<wire x1="0" y1="8.5" x2="0" y2="-2" width="0.05" layer="20"/>
<wire x1="0" y1="8.5" x2="65.5" y2="8.5" width="0.05" layer="20"/>
<wire x1="65.5" y1="8.5" x2="65.5" y2="31" width="0.05" layer="20"/>
<hole x="8.5" y="1.8" drill="3.5"/>
<hole x="58" y="1.8" drill="3.5"/>
<text>J.Chong</text>
<text>RevB - Build 10/18</text>
<text>POWER</text>
<text>READY?</text>
<text>1.  This drawing is CAD generated. No manual changes authorized after release. 
2.  All printed wiring boards to be manufactured in accordance with IPC-610 Class 2. 
      In case of conflict this drawing governs all other specifications. 
3.  Material, copper sheet laminate, copper clad FR4 170Tg. Interior 
      layers (if applicable) to be 0.5oz copper. Exterior layers to be 1oz copper finished. 
      Final thickness to be 0.063" (1.6mm). 
4.  All holes are plated through holes unless noted otherwise. Minimum plated through holes 
      to have 25um thick walls. 
5.  All finished trace widths to be +/- 20% measured at the bottom, minimum finished 
      spacing to be 100um. 
6.  All exposed copper to be finished with ENIG Solder finish over clean bare copper. 
7.  Drill boards using drill data, drill patterns, and drill table provided. Hole locations 
      shall be 0.003" (0.075mm) about true position (radial error). All finished holes to be +/-0.003" (0.075mm) 
      diameter unless noted otherwise. All finished vias to be +/-0.003" (0.075mm) to closed diameter. 
8. Minimum annular ring to be 50um external layers and 25um internal layers (if applicable). 
9. Layer to layer misalignment shall not exceed 75um (radial error) about true position. 
10. Solder mask construction to be SMOBC using green LPI solder mask material. Solder mask 
      to be 18 ~ 50um thick after curing, both sides. 
11. Solder mask misalignment shall not exceed 0.003" (0.075mm). Solder mask may overlap through hole 
      solder pads by 0.001" (0.025mm) maximum, but shall not overlap SMT pads. 
12. Silkscreen should be applied over solder mask using a white epoxy-based ink. The silkscreen 
      should not overlap solder pads unless noted otherwise. 
13. Dimensions shown reflect the board size after plating. 
14. The circuit board manufacturer shall apply a name and date code on the bottom side 
      of the board in copper etch. </text>
<text>LAYER-STACK</text>
<text>01-16</text>
<text>01-20</text>
</plain>
<libraries>
<library name="Analog Devices iSensors">
<packages>
<package name="ADIS1647X">
</package>
</packages>
</library>
<library name="SSM-105-XXX-DV">
<packages>
<package name="SSM-105-XXX-DV">
<description>.100" DOUBLE ROW SOCKET ASAEMBLY.</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="drilegend">
<packages>
<package name="DRILEGEND">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Analog Devices iSensors" package="ADIS1647X" value="ADIS1647X">
<attribute name="NAME"/>
<attribute name="PARTNO" value="ADIS16470-ENG"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SSM-105-XXX-DV" package="SSM-105-XXX-DV" value="SSM-105-XXX-DV">
<attribute name="NAME"/>
<attribute name="PARTNO" value="SSM-105-S-DV"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
<attribute name="PARTNO" value="ERJ-3GEYJ331V"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="PARTNO" value="LTST-C191KGKT"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
<attribute name="PARTNO" value="ERJ-3GEYJ331V"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="adafruit" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="PARTNO" value="LTST-C191KGKT"/>
<attribute name="VALUE"/>
</element>
<element name="DRILEGEND" library="drilegend" package="DRILEGEND" value=""/>
</elements>
<signals>
<signal name="MISO">
<contactref element="U1" pad="H3"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="G6"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="SCLK">
<contactref element="U1" pad="H6"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="CS0">
<contactref element="U1" pad="G3"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="CS1/DR">
<contactref element="U1" pad="J6"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="A1"/>
<contactref element="U1" pad="K8"/>
<contactref element="U1" pad="K3"/>
<contactref element="U1" pad="K1"/>
<contactref element="U1" pad="J7"/>
<contactref element="U1" pad="J2"/>
<contactref element="U1" pad="H8"/>
<contactref element="U1" pad="G7"/>
<contactref element="U1" pad="G2"/>
<contactref element="U1" pad="F8"/>
<contactref element="U1" pad="F6"/>
<contactref element="U1" pad="F1"/>
<contactref element="U1" pad="E7"/>
<contactref element="U1" pad="E6"/>
<contactref element="U1" pad="E2"/>
<contactref element="U1" pad="D3"/>
<contactref element="U1" pad="C6"/>
<contactref element="U1" pad="C2"/>
<contactref element="U1" pad="B6"/>
<contactref element="U1" pad="B5"/>
<contactref element="U1" pad="B4"/>
<contactref element="U1" pad="B3"/>
<contactref element="U1" pad="A8"/>
<contactref element="U1" pad="A7"/>
<contactref element="U1" pad="A6"/>
<contactref element="U1" pad="A5"/>
<contactref element="U1" pad="A4"/>
<contactref element="U1" pad="A3"/>
<contactref element="U1" pad="A2"/>
<contactref element="J1" pad="10"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="H1"/>
<contactref element="U1" pad="J4"/>
<contactref element="U1" pad="J5"/>
<contactref element="U1" pad="K6"/>
<contactref element="U1" pad="E3"/>
<contactref element="U1" pad="D6"/>
<contactref element="U1" pad="C7"/>
<contactref element="U1" pad="C3"/>
<contactref element="J1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="CS2/RST">
<contactref element="U1" pad="F3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="CS3/SYNC">
<contactref element="U1" pad="J3"/>
<contactref element="J1" pad="1"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="D2" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
