(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 135)
    (no_connects 0)
    (area 109.424999 50.208999 141.575001 135.859008)
    (thickness 1.6)
    (drawings 64)
    (tracks 681)
    (zones 0)
    (modules 57)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 2)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 RST)
  (net 4 "Net-(C3-Pad1)")
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad1)")
  (net 8 "Net-(C7-Pad1)")
  (net 9 VCC)
  (net 10 "Net-(C11-Pad1)")
  (net 11 "Net-(C16-Pad1)")
  (net 12 "Net-(D2-Pad1)")
  (net 13 RS485_RX)
  (net 14 RS485_TX)
  (net 15 RS485_EN)
  (net 16 A2)
  (net 17 A0)
  (net 18 A1)
  (net 19 SDA)
  (net 20 "Net-(P2-Pad2)")
  (net 21 CT1-A0)
  (net 22 CE)
  (net 23 CSN)
  (net 24 MOSI)
  (net 25 MISO)
  (net 26 SCK)
  (net 27 A3)
  (net 28 IRQ)
  (net 29 RS485-A)
  (net 30 RS485-B)
  (net 31 RGB2)
  (net 32 RGB3)
  (net 33 BTN1)
  (net 34 BTN2)
  (net 35 RGB1)
  (net 36 SCL)
  (net 37 RXI)
  (net 38 TXO)
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net BTN1)
    (add_net BTN2)
    (add_net CE)
    (add_net CSN)
    (add_net CT1-A0)
    (add_net GND)
    (add_net IRQ)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net RGB1)
    (add_net RGB2)
    (add_net RGB3)
    (add_net RS485-A)
    (add_net RS485-B)
    (add_net RS485_EN)
    (add_net RS485_RX)
    (add_net RS485_TX)
    (add_net RST)
    (add_net RXI)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net TXO)
    (add_net VCC)
  )
  (module footprints:TerminalBlock_Multicomp-5-08-6pol (layer F.Cu) (tedit 58435A39)
    (at 112.8395 130.67624)
    (descr "6-way 5.08mm pitch terminal block, Multicomp MC000038")
    (fp_text reference P2 (at 12.5 5.9) (layer F.SilkS) hide)
    (fp_text value CONN4 (at 12.7 7.366) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 25.4 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 21 CT1-A0))
    (pad 5 thru_hole circle (at 20.32 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 27 A3))
    (pad 4 thru_hole circle (at 15.24 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 29 RS485-A))
    (pad 3 thru_hole circle (at 10.16 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 30 RS485-B))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 5.08 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 20 "Net-(P2-Pad2)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-6pol.wrl
      (at (xyz 0.4921 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58435A0C)
    (at 113.5 70)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at -6.312 -2.436) (layer F.SilkS) hide)
    (fp_text value "" (at -15.456 0.612) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 58447C58)
    (at 132.842 78.486)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference RADIO1 (at -0.772 6.474) (layer F.SilkS))
    (fp_text value CONN_NRF24L01 (at -8.382 7.112) (layer F.Fab) hide)
    (pad 7 thru_hole oval (at -9.144 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 MISO))
    (pad 8 thru_hole oval (at -9.144 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 IRQ))
    (pad 5 thru_hole oval (at -6.604 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 SCK))
    (pad 6 thru_hole oval (at -6.604 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 MOSI))
    (pad 3 thru_hole oval (at -4.064 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 CE))
    (pad 4 thru_hole oval (at -4.064 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 CSN))
    (pad 1 thru_hole rect (at -1.524 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at -1.524 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C11-Pad1)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58435A19)
    (at 113.5 110.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at -6.312 -1.788) (layer F.SilkS) hide)
    (fp_text value "" (at -13.932 1.26) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 584359F6)
    (at 137.5 110.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 9.312 1.26) (layer F.SilkS) hide)
    (fp_text value "" (at 17.44 3.292) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 58435A00)
    (at 137.5 70)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference "" (at 9.312 -1.928) (layer F.SilkS) hide)
    (fp_text value "" (at 16.424 0.104) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 584360AD)
    (at 119.126 122.428)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D2 (at -2.54 -1.524) (layer F.SilkS))
    (fp_text value TL431 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C16-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 125.222 93.218 135)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 -6.05 135) (layer F.SilkS))
    (fp_text value ATMEGA328-A (at 0 6.05 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 RS485_RX))
    (pad 2 smd rect (at -4.25 -2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 BTN1))
    (pad 3 smd rect (at -4.25 -1.2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 -0.4 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 5 smd rect (at -4.25 0.4 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 1.2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 7 smd rect (at -4.25 2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 8 smd rect (at -4.25 2.8 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 9 smd rect (at -2.8 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 RGB3))
    (pad 10 smd rect (at -2 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 BTN2))
    (pad 11 smd rect (at -1.2 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 RGB2))
    (pad 12 smd rect (at -0.4 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 RGB1))
    (pad 13 smd rect (at 0.4 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 CE))
    (pad 14 smd rect (at 1.2 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 CSN))
    (pad 15 smd rect (at 2 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 MOSI))
    (pad 16 smd rect (at 2.8 4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 MISO))
    (pad 17 smd rect (at 4.25 2.8 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 SCK))
    (pad 18 smd rect (at 4.25 2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 19 smd rect (at 4.25 1.2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 A0))
    (pad 20 smd rect (at 4.25 0.4 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 21 smd rect (at 4.25 -0.4 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 -1.2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 A1))
    (pad 23 smd rect (at 4.25 -2 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 A2))
    (pad 24 smd rect (at 4.25 -2.8 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 A3))
    (pad 25 smd rect (at 2.8 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 RS485_TX))
    (pad 26 smd rect (at 2 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 RS485_EN))
    (pad 27 smd rect (at 1.2 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 SDA))
    (pad 28 smd rect (at 0.4 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 SCL))
    (pad 29 smd rect (at -0.4 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 RST))
    (pad 30 smd rect (at -1.2 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 RXI))
    (pad 31 smd rect (at -2 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 TXO))
    (pad 32 smd rect (at -2.8 -4.25 225) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 IRQ))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 584360B5)
    (at 113.284 117.856)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.54 0) (layer F.SilkS))
    (fp_text value 2N2222 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P2-Pad2)"))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Power_Integrations:SO-8 (layer F.Cu) (tedit 0)
    (at 113.538 94.742)
    (descr "SO-8 Surface Mount Small Outline 150mil 8pin Package")
    (tags "Power Integrations D Package")
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value MAX485CSA (at 0 0) (layer F.Fab))
    (pad 1 smd oval (at -1.905 2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 14 RS485_TX))
    (pad 2 smd oval (at -0.635 2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 15 RS485_EN))
    (pad 3 smd oval (at 0.635 2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 15 RS485_EN))
    (pad 4 smd oval (at 1.905 2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 13 RS485_RX))
    (pad 5 smd oval (at 1.905 -2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd oval (at 0.635 -2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 29 RS485-A))
    (pad 7 smd oval (at -0.635 -2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 30 RS485-B))
    (pad 8 smd oval (at -1.905 -2.794) (size 0.6096 1.4732) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 5841A087)
    (at 121.412 71.628)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 4.318 -1.524 90) (layer F.SilkS))
    (fp_text value AMS1117-3.3V (at 0 0.762) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 584360FE)
    (at 133.35 99.568 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U3 (at 1.27 -1.524 180) (layer F.SilkS))
    (fp_text value ATSHA204A (at 0 3.81 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 19 SDA))
    (pad 2 smd rect (at 0.95 1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 3 smd rect (at 0 -1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5844270E)
    (at 119.38 86.614 135)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -0.004243 1.579677 135) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1 135) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 135) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 135) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5843E9E9)
    (at 130.302 106.172)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.556 0) (layer F.SilkS))
    (fp_text value 22pF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5841A0D5)
    (at 130.302 103.124)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 3.556 0) (layer F.SilkS))
    (fp_text value 22pF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5841A39D)
    (at 136.906 63.754 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5841A45D)
    (at 116.586 63.754 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5841A3E8)
    (at 126.746 63.754 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5841A05D)
    (at 128.778 70.612 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -3.81 -0.254 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5841A05B)
    (at 128.778 72.898)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 4.318 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58436084)
    (at 112.776 88.646)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 3.81 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58436059)
    (at 128.524 99.568 225)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0.179605 -1.616446 225) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 225) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 225) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.25 0 225) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 584360B0)
    (at 123.444 122.174 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -2.54 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5843609E)
    (at 119.126 115.316)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58436103)
    (at 134.874 95.504 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C18 (at 3.048 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58436110)
    (at 124.206 104.648 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.048 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 RST))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5841A395)
    (at 139.446 63.754 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.556 0 270) (layer F.SilkS))
    (fp_text value 33 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 A0))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5841A3A4)
    (at 131.826 63.754 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5841A3A2)
    (at 134.366 63.754 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5841A456)
    (at 111.506 63.754 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -3.556 0 270) (layer F.SilkS))
    (fp_text value 33 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 A2))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5841A458)
    (at 114.046 63.754 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5841A45A)
    (at 119.126 63.754 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5841A404)
    (at 121.666 63.754 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -3.556 0 270) (layer F.SilkS))
    (fp_text value 33 (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 A1))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5841A3D1)
    (at 124.206 63.754 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 3.556 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5841A3DC)
    (at 129.286 63.754 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 4.064 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58436053)
    (at 114.046 100.33)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 3.81 0.254) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 RS485_RX))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58436046)
    (at 117.094 105.156)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 3.81 0) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 RS485_EN))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58436049)
    (at 117.094 102.87)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 3.81 0) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 RS485_EN))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58436040)
    (at 112.522 103.886 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 -1.778 90) (layer F.SilkS))
    (fp_text value 10KR (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 RS485_TX))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58436005)
    (at 113.538 75.946)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 20K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 RS485-A))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5843600C)
    (at 113.538 79.502)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 20K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 RS485-B))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5843600E)
    (at 113.538 83.058)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R19 (at 0 -1.778) (layer F.SilkS))
    (fp_text value 120 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 RS485-B))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 RS485-A))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 584360B2)
    (at 113.284 122.682 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R24 (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value 1.5K (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(P2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 584360A5)
    (at 119.126 118.618)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R25 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 27.4K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C16-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5843609B)
    (at 123.444 116.84 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R26 (at 0 1.778 90) (layer F.SilkS))
    (fp_text value 27.4K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 584360C6)
    (at 133.8 122.6 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C20 (at -3.81 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 CT1-A0))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 58436156)
    (at 128.778 110.49)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 17.018 4.826) (layer F.SilkS) hide)
    (fp_text value CONN_ICSP (at -0.254 7.62) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 MISO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 SCK))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 MOSI))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 RST))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 584360CA)
    (at 136.2 122.6 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R28 (at 3.81 0 90) (layer F.SilkS))
    (fp_text value 33 (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 27 A3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 CT1-A0))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 584360CE)
    (at 138.6 122.6 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R29 (at -3.81 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 CT1-A0))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 584360C2)
    (at 131.4 122.6 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R30 (at -3.81 0 270) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 CT1-A0))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_obscurities:XTAL_3.2x1.5mm (layer F.Cu) (tedit 5843E9CF)
    (at 126.746 104.648 90)
    (descr "XTAL 3.2 x 1.5mm footprint")
    (tags Xtal)
    (fp_text reference Y1 (at 3.048 -0.508 360) (layer F.SilkS))
    (fp_text value Crystal (at 0 1.8 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 0 90) (size 1.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 1.5 0 90) (size 1.5 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_smd_5x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.64 0.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:TerminalBlock_Multicomp-5-08-6pol (layer F.Cu) (tedit 58435A40)
    (at 138.2268 55.364 180)
    (descr "6-way 5.08mm pitch terminal block, Multicomp MC000038")
    (fp_text reference P5 (at 12.5 5.9 180) (layer F.SilkS) hide)
    (fp_text value CONN6 (at 12.954 7.62 180) (layer F.Fab) hide)
    (pad 6 thru_hole circle (at 25.4 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 16 A2))
    (pad 5 thru_hole circle (at 20.32 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(C6-Pad1)"))
    (pad 4 thru_hole circle (at 15.24 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 A1))
    (pad 3 thru_hole circle (at 10.16 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(C7-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 17 A0))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-6pol.wrl
      (at (xyz 0.4921 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x12 (layer F.Cu) (tedit 58435A72)
    (at 139.192 104.648 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P1 (at 1.524 5.08 90) (layer F.SilkS) hide)
    (fp_text value CONN_02X06 (at 1.524 3.556 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 9 VCC))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 RXI))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 TXO))
    (pad 5 thru_hole oval (at 10.16 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 36 SCL))
    (pad 6 thru_hole oval (at 12.7 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 3 RST))
    (pad 7 thru_hole oval (at 15.24 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 SDA))
    (pad 8 thru_hole oval (at 17.78 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 BTN1))
    (pad 9 thru_hole oval (at 20.32 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 RGB3))
    (pad 10 thru_hole oval (at 22.86 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 BTN2))
    (pad 11 thru_hole oval (at 25.4 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 RGB2))
    (pad 12 thru_hole oval (at 27.94 0 90) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask)
      (net 35 RGB1))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0.55 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5841A067)
    (at 128.778 75.184)
    (attr smd)
    (fp_text reference C9 (at 3.81 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5841A06D)
    (at 128.524 68.326)
    (attr smd)
    (fp_text reference C10 (at 4.318 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5843607C)
    (at 113.03 86.36)
    (attr smd)
    (fp_text reference C13 (at 4.064 0) (layer F.SilkS))
    (fp_text value 10uF (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 9 VCC))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module libs:calaos_logo (layer B.Cu) (tedit 0)
    (at 119.92 93.32 270)
    (fp_text reference G*** (at 0 0 270) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer B.SilkS) hide)
  )
  (gr_text CE (at 128.76 77.62 90) (layer F.SilkS))
  (gr_text SCK (at 126.22 77.77 90) (layer F.SilkS))
  (gr_text MISO (at 120.38 80.1) (layer F.SilkS))
  (gr_text IRQ (at 123.67 85.1 90) (layer F.SilkS))
  (gr_text MOSI (at 126.25 85.59 90) (layer F.SilkS))
  (gr_text CSN (at 128.78 85.28 90) (layer F.SilkS))
  (gr_text +3.3V (at 134.53 82.53) (layer F.SilkS))
  (gr_text GND (at 134.53 79.96) (layer F.SilkS))
  (gr_text "Gateway v1.0" (at 115.46 118.97 90) (layer B.SilkS))
  (gr_text "CT Sensor 3" (at 115.28 58.23 180) (layer B.SilkS))
  (gr_text "CT Sensor 2" (at 125.59 58.2 180) (layer B.SilkS))
  (gr_text "CT Sensor 1" (at 135.9 58.22 180) (layer B.SilkS))
  (gr_text "CT Sensor 0" (at 135.84 128) (layer B.SilkS))
  (gr_text RS485 (at 125.53 128.13) (layer B.SilkS))
  (gr_text Power (at 115.53 128.02) (layer B.SilkS))
  (gr_text B (at 128.11 133.91) (layer B.SilkS))
  (gr_text A (at 123.04 133.91) (layer B.SilkS))
  (gr_text "+5V\n+24V" (at 117.96 133.89) (layer B.SilkS))
  (gr_text GND (at 112.82 133.87) (layer B.SilkS))
  (gr_text MISO (at 125 110.56) (layer B.SilkS))
  (gr_text SCK (at 125.48 113.07) (layer B.SilkS))
  (gr_text RST (at 125.67 115.53) (layer B.SilkS))
  (gr_text GND (at 134.61 115.67) (layer B.SilkS))
  (gr_text MOSI (at 135.01 113.44) (layer B.SilkS))
  (gr_text VCC (at 132.16 108.49) (layer B.SilkS))
  (gr_text VCC (at 135.4 104.61) (layer B.SilkS))
  (gr_text RXI (at 135.93 102.09) (layer B.SilkS))
  (gr_text GND (at 135.43 99.52) (layer B.SilkS))
  (gr_text TXO (at 135.51 96.95) (layer B.SilkS))
  (gr_text SCL (at 135.68 94.47) (layer B.SilkS))
  (gr_text RST (at 135.76 91.92) (layer B.SilkS))
  (gr_text SDA (at 135.68 89.32) (layer B.SilkS))
  (gr_text BTN1 (at 134.95 86.84) (layer B.SilkS))
  (gr_text RGB3 (at 134.84 84.29) (layer B.SilkS))
  (gr_text BTN2 (at 134.98 81.78) (layer B.SilkS))
  (gr_text RGB2 (at 134.84 79.22) (layer B.SilkS))
  (gr_text RGB1 (at 134.84 76.7) (layer B.SilkS))
  (gr_line (start 109.5 135.784007) (end 109.5 50.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.5 135.784007) (end 141.5 135.784007) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.5 50.284) (end 141.5 135.784007) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.5 50.284) (end 141.5 50.284) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141 135) (xy 110 135) (xy 110 51) (xy 141 51)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141 135) (xy 110 135) (xy 110 51) (xy 141 51)
      )
    )
  )
)
