<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="-11" y1="10" x2="27" y2="10" width="0" layer="20"/>
<wire x1="27" y1="10" x2="29" y2="8" width="0" layer="20" curve="-90"/>
<wire x1="29" y1="8" x2="29" y2="-6" width="0" layer="20"/>
<wire x1="29" y1="-6" x2="27" y2="-8" width="0" layer="20" curve="-90"/>
<wire x1="27" y1="-8" x2="-11" y2="-8" width="0" layer="20"/>
<wire x1="-11" y1="-8" x2="-13" y2="-6" width="0" layer="20" curve="-90"/>
<wire x1="-13" y1="-6" x2="-13" y2="8" width="0" layer="20"/>
<wire x1="-13" y1="8" x2="-11" y2="10" width="0" layer="20" curve="-90"/>
<text>5.00V</text>
<text>3.30V</text>
<text>1.15V</text>
<text>1.00V</text>
<text>+</text>
<text>-</text>
<text>1</text>
<text>3</text>
<text>4</text>
<text>2</text>
<text>PowerMii</text>
<text>Lite</text>
<text>(C) 2017 BitBuilt LLC</text>
</plain>
<libraries>
<library name="passives">
<description>&lt;b&gt;LAB11&lt;/b&gt; - Resistors, caps, etc.</description>
<packages>
<package name="0402_CAP">
</package>
<package name="0402_RES">
</package>
<package name="0805_CAP">
<description>Based on muRata GRM capacitor specifications</description>
</package>
<package name="0603_CAP">
</package>
<package name="IHL-1212BZ-11">
</package>
</packages>
</library>
<library name="chips">
<description>&lt;b&gt;LAB11&lt;/b&gt; - ICs and other digital/analog chips.</description>
<packages>
<package name="TQFN-16/3MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="chips" package="TQFN-16/3MM" value="TLV62130">
<attribute name="DIGIKEY" value="296-35978-1-ND"/>
</element>
<element name="C1" library="passives" package="0805_CAP" value="10 uF"/>
<element name="C2" library="passives" package="0402_CAP" value="0.1 uF"/>
<element name="C3" library="passives" package="0402_CAP" value="3.3 nF"/>
<element name="C4" library="passives" package="0603_CAP" value="22 uF"/>
<element name="R33" library="passives" package="0402_RES" value="680 kΩ"/>
<element name="R34" library="passives" package="0402_RES" value="130 kΩ"/>
<element name="R35" library="passives" package="0402_RES" value="100 kΩ"/>
<element name="L1" library="passives" package="IHL-1212BZ-11" value="2.2 uH">
<attribute name="DIGIKEY" value="541-1322-1-ND"/>
</element>
<element name="U2" library="chips" package="TQFN-16/3MM" value="TLV62130">
<attribute name="DIGIKEY" value="296-35978-1-ND"/>
</element>
<element name="C5" library="passives" package="0805_CAP" value="10 uF"/>
<element name="C6" library="passives" package="0402_CAP" value="0.1 uF"/>
<element name="C7" library="passives" package="0402_CAP" value="3.3 nF"/>
<element name="C8" library="passives" package="0603_CAP" value="22 uF"/>
<element name="R1" library="passives" package="0402_RES" value="680 kΩ"/>
<element name="R2" library="passives" package="0402_RES" value="130 kΩ"/>
<element name="R3" library="passives" package="0402_RES" value="100 kΩ"/>
<element name="L2" library="passives" package="IHL-1212BZ-11" value="2.2 uH">
<attribute name="DIGIKEY" value="541-1322-1-ND"/>
</element>
<element name="U3" library="chips" package="TQFN-16/3MM" value="TLV62130">
<attribute name="DIGIKEY" value="296-35978-1-ND"/>
</element>
<element name="C9" library="passives" package="0805_CAP" value="10 uF"/>
<element name="C10" library="passives" package="0402_CAP" value="0.1 uF"/>
<element name="C11" library="passives" package="0402_CAP" value="3.3 nF"/>
<element name="C12" library="passives" package="0603_CAP" value="22 uF"/>
<element name="R4" library="passives" package="0402_RES" value="680 kΩ"/>
<element name="R5" library="passives" package="0402_RES" value="130 kΩ"/>
<element name="R6" library="passives" package="0402_RES" value="100 kΩ"/>
<element name="L3" library="passives" package="IHL-1212BZ-11" value="2.2 uH">
<attribute name="DIGIKEY" value="541-1322-1-ND"/>
</element>
<element name="U4" library="chips" package="TQFN-16/3MM" value="TLV62130">
<attribute name="DIGIKEY" value="296-35978-1-ND"/>
</element>
<element name="C13" library="passives" package="0805_CAP" value="10 uF"/>
<element name="C14" library="passives" package="0402_CAP" value="0.1 uF"/>
<element name="C15" library="passives" package="0402_CAP" value="3.3 nF"/>
<element name="C16" library="passives" package="0603_CAP" value="22 uF"/>
<element name="R7" library="passives" package="0402_RES" value="680 kΩ"/>
<element name="R8" library="passives" package="0402_RES" value="130 kΩ"/>
<element name="R9" library="passives" package="0402_RES" value="100 kΩ"/>
<element name="L4" library="passives" package="IHL-1212BZ-11" value="2.2 uH">
<attribute name="DIGIKEY" value="541-1322-1-ND"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="7"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="P$2"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="16"/>
<contactref element="U1" pad="15"/>
<contactref element="R34" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="GND"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="7"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="C5" pad="P$2"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="16"/>
<contactref element="U2" pad="15"/>
<contactref element="R2" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U2" pad="GND"/>
<contactref element="U3" pad="8"/>
<contactref element="U3" pad="7"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="C9" pad="P$2"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="16"/>
<contactref element="U3" pad="15"/>
<contactref element="R5" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U3" pad="GND"/>
<contactref element="U4" pad="8"/>
<contactref element="U4" pad="7"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C13" pad="P$2"/>
<contactref element="U4" pad="6"/>
<contactref element="U4" pad="16"/>
<contactref element="U4" pad="15"/>
<contactref element="R8" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="U4" pad="GND"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="9"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="L1" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="R35" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="R34" pad="2"/>
<contactref element="R33" pad="1"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$14">
</signal>
<signal name="VIN">
<contactref element="C1" pad="P$1"/>
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="12"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="10"/>
<contactref element="U1" pad="13"/>
<contactref element="C5" pad="P$1"/>
<contactref element="U2" pad="11"/>
<contactref element="U2" pad="12"/>
<contactref element="C6" pad="1"/>
<contactref element="U2" pad="10"/>
<contactref element="U2" pad="13"/>
<contactref element="C9" pad="P$1"/>
<contactref element="U3" pad="11"/>
<contactref element="U3" pad="12"/>
<contactref element="C10" pad="1"/>
<contactref element="U3" pad="10"/>
<contactref element="U3" pad="13"/>
<contactref element="C13" pad="P$1"/>
<contactref element="U4" pad="11"/>
<contactref element="U4" pad="12"/>
<contactref element="C14" pad="1"/>
<contactref element="U4" pad="10"/>
<contactref element="U4" pad="13"/>
</signal>
<signal name="VOUT">
<contactref element="U1" pad="14"/>
<contactref element="L1" pad="P$2"/>
<contactref element="R35" pad="2"/>
<contactref element="R33" pad="2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="9"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="L2" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$8">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="VOUT1">
<contactref element="U2" pad="14"/>
<contactref element="L2" pad="P$2"/>
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U3" pad="9"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="L3" pad="P$1"/>
</signal>
<signal name="N$13">
<contactref element="R6" pad="1"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="R5" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="VOUT2">
<contactref element="U3" pad="14"/>
<contactref element="L3" pad="P$2"/>
<contactref element="R6" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="U4" pad="9"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="U4" pad="3"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="1"/>
<contactref element="L4" pad="P$1"/>
</signal>
<signal name="N$21">
<contactref element="R9" pad="1"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="N$22">
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="N$23">
</signal>
<signal name="N$24">
</signal>
<signal name="VOUT3">
<contactref element="U4" pad="14"/>
<contactref element="L4" pad="P$2"/>
<contactref element="R9" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="S$1">
</signal>
<signal name="S$2">
</signal>
<signal name="S$3">
</signal>
<signal name="S$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
