(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 22)
    (no_connects 0)
    (area 103.324999 81.645 138.305 119.930001)
    (thickness 1.6)
    (drawings 4)
    (tracks 85)
    (zones 0)
    (modules 9)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J2-Pad1)")
  (net 6 "Net-(J3-Pad2)")
  (net 7 "Net-(J3-Pad3)")
  (net 8 "Net-(J3-Pad4)")
  (net 9 "Net-(J3-Pad5)")
  (net 10 "Net-(J3-Pad6)")
  (net 11 "Net-(Q1-Pad2)")
  (net 12 +3V3)
  (net 13 VAC)
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad4)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(Q1-Pad2)")
  )
  (net_class AC ""
    (clearance 0.4)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net VAC)
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_MPT-2.54mm_2pol (layer F.Cu) (tedit 59FF0755)
    (at 132.715 116.205)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J1 (at 1.27 -4.50088) (layer F.SilkS))
    (fp_text value Out (at -3.175 1.905) (layer F.Fab))
    (fp_text user %R (at 1.27 1.045) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-2.54mm_2pol.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlocks_Phoenix:TerminalBlock_Phoenix_MPT-2.54mm_2pol (layer F.Cu) (tedit 59FF0755)
    (at 121.92 116.205)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J2 (at 1.27 -4.50088) (layer F.SilkS))
    (fp_text value AC (at 5.715 -1.27) (layer F.Fab))
    (fp_text user %R (at 1.27 1.045 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 13 VAC))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
    (pad "" np_thru_hole circle (at 0 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 2.54 2.54) (size 1.1 1.1) (drill 1.1) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MPT-2.54mm_2pol.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 121.92 97.79 180)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J3 (at 4.385 2.27 180) (layer B.SilkS))
    (fp_text value Debug (at 4.385 -14.97 180) (layer B.Fab))
    (fp_text user %R (at 2.77 -6.35 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad4)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad5)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Wide (layer F.Cu) (tedit 58CE52AF)
    (at 132.08 106.68 180)
    (descr "TO-92 leads molded, wide, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 2.54 -4.19 360) (layer F.SilkS))
    (fp_text value 2N3906 (at 6.985 -1.27 270) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.19 360) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.54 -2.54 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.52 1.52) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Wide.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 121.92 93.98 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 -2.31 180) (layer F.SilkS))
    (fp_text value R470 (at 5.08 2.31 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad5)"))
    (pad 2 thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module espRelayFootprint:G5V-1-DC (layer F.Cu) (tedit 5AC2FD3E)
    (at 129.54 99.06 90)
    (fp_text reference U1 (at 2.54 1.27 90) (layer F.SilkS))
    (fp_text value G5V-1-DC3 (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -3.81 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 10 thru_hole circle (at -3.81 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 9 thru_hole circle (at -1.27 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at -1.27 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 6 thru_hole circle (at 6.35 -2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 VAC))
    (pad 5 thru_hole circle (at 6.35 2.54 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 VAC))
  )
  (module espRelayFootprint:IRM-02 (layer B.Cu) (tedit 5AC2FDD2)
    (at 120.65 101.6)
    (fp_text reference U2 (at 0 -1.27) (layer B.SilkS))
    (fp_text value IRM-02-3.3 (at 0 0.5) (layer B.Fab))
    (pad 13 thru_hole circle (at -14 -7.6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole circle (at -14 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 +3V3))
    (pad 1 thru_hole circle (at 14 7.6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 13 VAC))
    (pad 24 thru_hole circle (at 14 -7.6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(J2-Pad1)"))
  )
  (module espRelayFootprint:ESP8266-01 (layer F.Cu) (tedit 5AC2FD8A)
    (at 111.76 105.41)
    (fp_text reference U3 (at 0 1.27) (layer F.SilkS))
    (fp_text value ESP8266 (at 0 -0.5) (layer F.Fab))
    (pad 1 thru_hole rect (at -3.81 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at -1.27 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 10 "Net-(J3-Pad6)"))
    (pad 5 thru_hole circle (at 1.27 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 "Net-(J3-Pad5)"))
    (pad 7 thru_hole circle (at 3.81 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at -3.81 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(J3-Pad2)"))
    (pad 4 thru_hole circle (at -1.27 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 +3V3))
    (pad 6 thru_hole circle (at 1.27 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad4)"))
    (pad 8 thru_hole circle (at 3.81 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 +3V3))
  )
  (module Diodes_THT:D_A-405_P10.16mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 134.62 106.68 90)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 5.08 -2.41 90) (layer F.SilkS))
    (fp_text value D (at 5.08 2.41 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 103.505 120.015) (end 103.505 90.17) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.795 120.015) (end 103.505 120.015) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.795 90.17) (end 137.795 120.015) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.505 90.17) (end 137.795 90.17) (layer Edge.Cuts) (width 0.15))
)
