<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="17.78" x2="0" y2="0" width="0.1524" layer="20"/>
<wire x1="0" y1="0" x2="34.29" y2="0" width="0.1524" layer="20"/>
<wire x1="34.29" y1="0" x2="34.29" y2="17.78" width="0.1524" layer="20"/>
<wire x1="34.29" y1="17.78" x2="0" y2="17.78" width="0.1524" layer="20"/>
<hole x="2.54" y="6.35" drill="3.048"/>
<hole x="31.75" y="6.35" drill="3.048"/>
<text>Blown TVS</text>
<text>BLUE</text>
<text>BLACK</text>
<text>RED</text>
<text>SIGNAL</text>
<text>GND</text>
<text>+12V</text>
<text>RV-Project.Com
TVS Adapter</text>
<text>5/6/2020</text>
<text>5A</text>
<text>LED GND</text>
</plain>
<libraries>
<library name="a-lib">
<description>&lt;b&gt;Al's Components.&lt;/b&gt;
&lt;p&gt;Including:
&lt;ul&gt;
&lt;li&gt;GPS Receivers
&lt;li&gt;ASK Transmitters and Receivers
&lt;li&gt;Specialtiy Switches
&lt;/ul&gt;</description>
<packages>
<package name="251SMALL">
<description>Pitch: 0.45"&lt;br&gt;
Drill: 0.027" dia</description>
</package>
<package name="LED-1206">
</package>
<package name="1206-RES">
</package>
<package name="SOD-123">
<description>Suitable for 4148
&lt;br&gt;Pad Size:  0.55"x0.8"</description>
</package>
<package name="MO1-18AWG">
</package>
</packages>
</library>
<library name="a-lib_Connectors">
<description>Thru-Hole Connectors (Connectors, Terminals)</description>
<packages>
<package name="WAFER3PINVERTICAL">
<description>Pitch: 0.15" (3.81mm)</description>
</package>
<package name="MO1-18AWG">
</package>
</packages>
</library>
<library name="a-lib_Asthetics">
<description>Miscellaneous Items (Hardware, Power Points, Logos, etc)</description>
<packages>
<package name="RVPROJECT_NEWLOGO_XSMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="F1" library="a-lib" package="251SMALL" value="2.5A"/>
<element name="LED1" library="a-lib" package="LED-1206" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="a-lib" package="1206-RES" value="1.5k"/>
<element name="TVS1" library="a-lib" package="SOD-123" value="TVS-SSOD123"/>
<element name="J1" library="a-lib_Connectors" package="WAFER3PINVERTICAL" value="M3VERTICAL"/>
<element name="SIGNAL" library="a-lib_Connectors" package="MO1-18AWG" value=""/>
<element name="GND" library="a-lib_Connectors" package="MO1-18AWG" value="GND"/>
<element name="VCC" library="a-lib_Connectors" package="MO1-18AWG" value="VCC"/>
<element name="U$1" library="a-lib_Asthetics" package="RVPROJECT_NEWLOGO_XSMALL" value=""/>
<element name="R2" library="a-lib" package="1206-RES" value="1.2K">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="a-lib" package="MO1-18AWG" value="">
<attribute name="AMPERAGE" value="10A"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="F1" pad="P$2"/>
<contactref element="TVS1" pad="A"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="GND">
<contactref element="F1" pad="P$1"/>
<contactref element="J1" pad="P$2"/>
<contactref element="GND" pad="P$1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="P$3"/>
<contactref element="SIGNAL" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="TVS1" pad="C"/>
<contactref element="J1" pad="P$1"/>
<contactref element="VCC" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="JP2" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
