(kicad_pcb (version 20171130) (host pcbnew 5.1.2-f72e74a~84~ubuntu19.04.1)
  (general
    (thickness 1.6)
    (drawings 20)
    (tracks 282)
    (zones 0)
    (modules 30)
    (nets 48)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.3)
    (via_drill 0.254)
    (via_min_size 0.3)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(U1-Pad32)")
  (net 3 "Net-(U1-Pad28)")
  (net 4 "Net-(U1-Pad27)")
  (net 5 "Net-(U1-Pad24)")
  (net 6 "Net-(U1-Pad17)")
  (net 7 "Net-(U1-Pad18)")
  (net 8 "Net-(U1-Pad19)")
  (net 9 "Net-(U1-Pad20)")
  (net 10 "Net-(U1-Pad21)")
  (net 11 "Net-(U1-Pad22)")
  (net 12 +3V3)
  (net 13 "Net-(U1-Pad9)")
  (net 14 "Net-(U1-Pad11)")
  (net 15 "Net-(J2-Pad3)")
  (net 16 "Net-(U1-Pad6)")
  (net 17 "Net-(U1-Pad5)")
  (net 18 "Net-(U1-Pad4)")
  (net 19 "Net-(U1-Pad7)")
  (net 20 "Net-(U1-Pad12)")
  (net 21 "Net-(J2-Pad4)")
  (net 22 "Net-(U3-Pad4)")
  (net 23 "Net-(C5-Pad1)")
  (net 24 "Net-(U2-Pad2)")
  (net 25 "Net-(U2-Pad3)")
  (net 26 "Net-(J1-Pad2)")
  (net 27 "Net-(J1-Pad3)")
  (net 28 "Net-(J1-Pad4)")
  (net 29 "Net-(Q1-Pad1)")
  (net 30 IO32)
  (net 31 IO21)
  (net 32 IO23)
  (net 33 IO22)
  (net 34 IO25)
  (net 35 RX)
  (net 36 TX)
  (net 37 EN)
  (net 38 IO0)
  (net 39 "Net-(TP4-Pad1)")
  (net 40 "Net-(TP5-Pad1)")
  (net 41 "Net-(U2-Pad11)")
  (net 42 "Net-(U2-Pad10)")
  (net 43 VUSB)
  (net 44 "Net-(U1-Pad29)")
  (net 45 "Net-(U1-Pad14)")
  (net 46 "Net-(U1-Pad31)")
  (net 47 "Net-(U1-Pad30)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.3)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net EN)
    (add_net GND)
    (add_net IO0)
    (add_net IO21)
    (add_net IO22)
    (add_net IO23)
    (add_net IO25)
    (add_net IO32)
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(TP4-Pad1)")
    (add_net "Net-(TP5-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad31)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U3-Pad4)")
    (add_net RX)
    (add_net TX)
    (add_net VUSB)
  )
  (net_class regular ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.3)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Package_LGA:LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y (layer F.Cu) (tedit 5AFC1041)
    (at 169 89.5 180)
    (descr "LGA, 14 Pin (http://www.st.com/resource/en/datasheet/lsm6ds3.pdf), generated with kicad-footprint-generator ipc_lga_layoutBorder_generator.py")
    (tags "LGA LGA")
    (attr smd)
    (fp_text reference U2 (at 0 -2.2) (layer F.SilkS))
    (fp_text value LSM6DS3 (at 0 2.2) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd custom (at -0.5 -0.8875 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 IO21)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.2 -0.3375) (xy 0.2 -0.3375) (xy 0.2 0.3375) (xy 0.05 0.3375) (xy -0.2 0.0875)
) (width 0))
      ))
    (pad 13 smd rect (at 0 -0.8875 180) (size 0.4 0.675) (layers F.Cu F.Paste F.Mask)
      (net 32 IO23))
    (pad 12 smd custom (at 0.5 -0.8875 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 34 IO25)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.2 -0.3375) (xy 0.2 -0.3375) (xy 0.2 0.0875) (xy -0.05 0.3375) (xy -0.2 0.3375)
) (width 0))
      ))
    (pad 11 smd custom (at 1.1375 -0.75 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U2-Pad11)")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.3375 0.05) (xy -0.0875 -0.2) (xy 0.3375 -0.2) (xy 0.3375 0.2) (xy -0.3375 0.2)
) (width 0))
      ))
    (pad 10 smd rect (at 1.1375 -0.25 180) (size 0.675 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U2-Pad10)"))
    (pad 9 smd rect (at 1.1375 0.25 180) (size 0.675 0.4) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(TP5-Pad1)"))
    (pad 8 smd custom (at 1.1375 0.75 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.3375 -0.2) (xy 0.3375 -0.2) (xy 0.3375 0.2) (xy -0.0875 0.2) (xy -0.3375 -0.05)
) (width 0))
      ))
    (pad 7 smd custom (at 0.5 0.8875 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.2 -0.3375) (xy -0.05 -0.3375) (xy 0.2 -0.0875) (xy 0.2 0.3375) (xy -0.2 0.3375)
) (width 0))
      ))
    (pad 6 smd rect (at 0 0.8875 180) (size 0.4 0.675) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd custom (at -0.5 0.8875 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.2 -0.0875) (xy 0.05 -0.3375) (xy 0.2 -0.3375) (xy 0.2 0.3375) (xy -0.2 0.3375)
) (width 0))
      ))
    (pad 4 smd custom (at -1.1375 0.75 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(TP4-Pad1)")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.3375 -0.2) (xy 0.3375 -0.2) (xy 0.3375 -0.05) (xy 0.0875 0.2) (xy -0.3375 0.2)
) (width 0))
      ))
    (pad 3 smd rect (at -1.1375 0.25 180) (size 0.675 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U2-Pad3)"))
    (pad 2 smd rect (at -1.1375 -0.25 180) (size 0.675 0.4) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U2-Pad2)"))
    (pad 1 smd custom (at -1.1375 -0.75 180) (size 0.4 0.4) (layers F.Cu F.Paste F.Mask)
      (net 33 IO22)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
           (xy -0.3375 -0.2) (xy 0.0875 -0.2) (xy 0.3375 0.05) (xy 0.3375 0.2) (xy -0.3375 0.2)
) (width 0))
      ))
    (model ${KISYS3DMOD}/Package_LGA.3dshapes/LGA-14_3x2.5mm_P0.5mm_LayoutBorder3x4y.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 160 75.4 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C8 (at 0 -1.1 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 164.65 88.29 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C7 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 169.35 85.25 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C6 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 168.85 98.53)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP5 (at 0 1.648) (layer B.Fab))
    (fp_text value IO14 (at 0 -1.75) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 40 "Net-(TP5-Pad1)"))
  )
  (module magic-wand:rod_connector (layer B.Cu) (tedit 5CF9D111)
    (at 169 56.2 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J2 (at 0 -6.15) (layer B.SilkS))
    (fp_text value LEDS (at 0 -4.7) (layer B.Fab))
    (pad 1 smd rect (at 0 7.5 180) (size 4 8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.75 -1.75 180) (size 1.5 4) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.25 -1.75 180) (size 1.5 4) (layers B.Cu B.Paste B.Mask)
      (net 30 IO32))
    (pad 3 smd rect (at 1.25 -1.75 180) (size 1.5 4) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at 3.75 -1.75 180) (size 1.5 4) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(J2-Pad4)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 177.15 72.49)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 0 1.648) (layer B.Fab))
    (fp_text value IO4 (at 0 -1.75) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 29 "Net-(Q1-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 166.58 92.44)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP8 (at 0 1.648) (layer B.Fab))
    (fp_text value IO22 (at -3.08 0.06) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 33 IO22))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 170.38 83.11)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP7 (at 0 1.648) (layer B.Fab))
    (fp_text value IO21 (at -2.98 -0.01) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 31 IO21))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 169 91.5)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP6 (at 0 1.648) (layer B.Fab))
    (fp_text value IO25 (at 3 0) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 34 IO25))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 170.35 86.25)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 1.648) (layer B.Fab))
    (fp_text value IO15 (at 2.9 0) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 39 "Net-(TP4-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 169.03 125.39)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at 0 1.648) (layer B.Fab))
    (fp_text value VUSB (at 3.42 0.01) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 43 VUSB))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 167.68 74.18)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at 0 1.648) (layer B.Fab))
    (fp_text value IO13 (at 0 -1.75) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 15 "Net-(J2-Pad3)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 174.51 82.78)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP9 (at 0 1.648) (layer B.Fab))
    (fp_text value IO23 (at -0.89 -1.58) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 32 IO23))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 164.77 70.59)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP10 (at 0 1.648) (layer B.Fab))
    (fp_text value IO32 (at 0 -1.75) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 30 IO32))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 171.49 106.06)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP12 (at 0 1.648) (layer B.Fab))
    (fp_text value VBAT (at -2.84 -0.01) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 23 "Net-(C5-Pad1)"))
  )
  (module TestPoint:TestPoint_Pad_D1.5mm (layer B.Cu) (tedit 5A0F774F)
    (at 172.19 102.26)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP11 (at 0 1.648) (layer B.Fab))
    (fp_text value +3V3 (at 3.16 -0.01) (layer B.SilkS))
    (fp_text user %R (at 0 1.65) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 12 +3V3))
  )
  (module magic-wand:SMD_2.54_CONN_01x06 (layer B.Cu) (tedit 5CECA851)
    (at 169 121)
    (fp_text reference J4 (at 0 -2) (layer B.SilkS))
    (fp_text value CONN_PROG (at 0 2.75) (layer B.Fab))
    (pad 6 smd rect (at 6.35 0) (size 1.524 2) (layers B.Cu B.Paste B.Mask)
      (net 12 +3V3))
    (pad 5 smd rect (at 3.81 0) (size 1.524 2) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 1.27 0) (size 1.524 2) (layers B.Cu B.Paste B.Mask)
      (net 38 IO0))
    (pad 3 smd rect (at -1.27 0) (size 1.524 2) (layers B.Cu B.Paste B.Mask)
      (net 37 EN))
    (pad 2 smd rect (at -3.81 0) (size 1.524 2) (layers B.Cu B.Paste B.Mask)
      (net 36 TX))
    (pad 1 smd rect (at -6.35 0) (size 1.524 2) (layers B.Cu B.Paste B.Mask)
      (net 35 RX))
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 169 53.25 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 43 VUSB))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 172.05 108.1 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0.075 -1.575 90) (layer F.SilkS))
    (fp_text value C (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 23 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 172.05 103 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value C (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 166 108.125 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 1.35 270) (layer F.SilkS))
    (fp_text value C (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 VUSB))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 166.05 103 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 1.6 270) (layer F.SilkS))
    (fp_text value C (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 VUSB))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 160 71.125 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.15 90) (layer F.SilkS))
    (fp_text value C (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal (layer F.Cu) (tedit 5B7745C6)
    (at 176 118 180)
    (descr "JST PH series connector, S2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (fp_text reference J3 (at 0.99 -2.28 180) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1 7.45 180) (layer F.Fab))
    (fp_text user %R (at 1 2.5 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 2 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 23 "Net-(C5-Pad1)"))
    (pad 1 thru_hole roundrect (at 0 0 180) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S2B-PH-K_1x02_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_USB:USB_Micro-B_Molex_47346-0001 (layer F.Cu) (tedit 5A1DC0BD)
    (at 169 125.35)
    (descr "Micro USB B receptable with flange, bottom-mount, SMD, right-angle (http://www.molex.com/pdm_docs/sd/473460001_sd.pdf)")
    (tags "Micro B USB SMD")
    (attr smd)
    (fp_text reference J1 (at 0 -3.3 180) (layer F.SilkS))
    (fp_text value USB_B_Micro (at 0 4.6 180) (layer F.Fab))
    (fp_text user %R (at 0 1.2) (layer F.Fab))
    (fp_text user "PCB Edge" (at 0 2.67 180) (layer Dwgs.User))
    (pad 6 smd rect (at 0.84 1.2) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -0.84 1.2) (size 1.175 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.91 1.2) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.91 1.2) (size 2.375 1.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.4625 -1.1) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.4625 -1.1) (size 1.475 2.1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.3 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J1-Pad4)"))
    (pad 3 smd rect (at 0 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-Pad3)"))
    (pad 2 smd rect (at -0.65 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-Pad2)"))
    (pad 1 smd rect (at -1.3 -1.46) (size 0.45 1.38) (layers F.Cu F.Paste F.Mask)
      (net 43 VUSB))
    (model ${KISYS3DMOD}/Connector_USB.3dshapes/USB_Micro-B_Molex_47346-0001.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 169 108 180)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at 0 -2.9 180) (layer F.SilkS))
    (fp_text value MCP73811T-420I-OT (at 0 2.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 43 VUSB))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(C5-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 43 VUSB))
    (pad 5 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 43 VUSB))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer F.Cu) (tedit 5A02FF57)
    (at 168.987001 103)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at 0 -2.9) (layer F.SilkS))
    (fp_text value AP2112K-3.3 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U3-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 43 VUSB))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 43 VUSB))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 160 65.125 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 2.875 0 270) (layer F.SilkS))
    (fp_text value R (at 0 1.43 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 +3V3))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 EN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module magic-wand:ESP32_micro (layer F.Cu) (tedit 5B87E20E)
    (at 169 70)
    (fp_text reference U1 (at 7.6 -9.25) (layer F.SilkS))
    (fp_text value ESP32-WROOM-32 (at 0 -2.3) (layer F.Fab))
    (pad 38 smd rect (at 6.5 -6.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd rect (at 6.5 -5.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 IO23))
    (pad 36 smd rect (at 6.5 -4.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 IO22))
    (pad 35 smd rect (at 6.5 -3.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 TX))
    (pad 34 smd rect (at 6.5 -2.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 RX))
    (pad 33 smd rect (at 6.5 -1.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 IO21))
    (pad 32 smd rect (at 6.5 -0.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(U1-Pad32)"))
    (pad 31 smd rect (at 6.5 0.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U1-Pad31)"))
    (pad 30 smd rect (at 6.5 1.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U1-Pad30)"))
    (pad 29 smd rect (at 6.5 2.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U1-Pad29)"))
    (pad 28 smd rect (at 6.5 3.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(U1-Pad28)"))
    (pad 27 smd rect (at 6.5 4.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(U1-Pad27)"))
    (pad 26 smd rect (at 6.5 5.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(Q1-Pad1)"))
    (pad 25 smd rect (at 6.5 6.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 IO0))
    (pad 24 smd rect (at 6.5 7.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(U1-Pad24)"))
    (pad 16 smd rect (at -3.5 9.2 90) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J2-Pad3)"))
    (pad 23 smd rect (at 3.5 9.2 90) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(TP4-Pad1)"))
    (pad 17 smd rect (at -2.5 9.2 90) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(U1-Pad17)"))
    (pad 18 smd rect (at -1.5 9.2 90) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(U1-Pad18)"))
    (pad 19 smd rect (at -0.5 9.2 90) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 0.5 9.2 90) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(U1-Pad20)"))
    (pad 21 smd rect (at 1.5 9.2 90) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad21)"))
    (pad 22 smd rect (at 2.5 9.2 90) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad22)"))
    (pad 2 smd rect (at -6.5 -5.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 +3V3))
    (pad 10 smd rect (at -6.5 2.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 IO25))
    (pad 8 smd rect (at -6.5 0.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 IO32))
    (pad 9 smd rect (at -6.5 1.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad9)"))
    (pad 15 smd rect (at -6.5 7.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -6.5 3.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad11)"))
    (pad 14 smd rect (at -6.5 6.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U1-Pad14)"))
    (pad 13 smd rect (at -6.5 5.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(TP5-Pad1)"))
    (pad 6 smd rect (at -6.5 -1.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U1-Pad6)"))
    (pad 3 smd rect (at -6.5 -4.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 EN))
    (pad 5 smd rect (at -6.5 -2.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U1-Pad5)"))
    (pad 1 smd rect (at -6.5 -6.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -6.5 -3.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U1-Pad4)"))
    (pad 7 smd rect (at -6.5 -0.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U1-Pad7)"))
    (pad 12 smd rect (at -6.5 4.5) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U1-Pad12)"))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/ESP32-WROOM-32.wrl
      (offset (xyz 0 -0.45 0.5))
      (scale (xyz 0.6 0.8100000000000001 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 3V3 (at 175.35 122.9) (layer B.SilkS))
  (gr_text GND (at 172.81 122.9) (layer B.SilkS))
  (gr_text IO0 (at 170.27 122.9) (layer B.SilkS))
  (gr_text EN (at 167.75 122.9) (layer B.SilkS))
  (gr_text TX (at 165.2 122.9) (layer B.SilkS))
  (gr_text RX (at 162.6 122.9) (layer B.SilkS))
  (gr_line (start 179 81) (end 179 56) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176 81) (end 179 81) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176 85.5) (end 176 81) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179 85.5) (end 176 85.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 169 48) (end 173 48) (angle -180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 173 48) (end 173 53) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 165 53) (end 165 48) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 176 56) (end 179 56) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 176 53) (end 176 56) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 162 53) (end 162 56) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159 56) (end 162 56) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159 128) (end 159 56) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179 128) (end 159 128) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179 85.5) (end 179 128) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.9 63) (xy 179.2 63) (xy 179 128) (xy 159 128)
      )
    )
  )
  (zone (net 12) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.2 63) (xy 158.9 63) (xy 159 128) (xy 179 128)
      )
    )
  )
)
