(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 47)
    (no_connects 0)
    (area 112.249761 89.840999 179.531001 114.767)
    (thickness 1.6)
    (drawings 25)
    (tracks 276)
    (zones 0)
    (modules 19)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.2)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(C3-Pad1)")
  (net 5 VCC)
  (net 6 "Net-(D1-Pad1)")
  (net 7 "Net-(D2-Pad1)")
  (net 8 "Net-(P1-Pad1)")
  (net 9 TXD)
  (net 10 RXD)
  (net 11 ~RTS)
  (net 12 ~CTS)
  (net 13 RST)
  (net 14 Vout)
  (net 15 "Net-(R1-Pad2)")
  (net 16 "Net-(R2-Pad2)")
  (net 17 "Net-(R3-Pad1)")
  (net 18 "Net-(R4-Pad1)")
  (net 19 ~DTR)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R4-Pad1)")
    (add_net RST)
    (add_net RXD)
    (add_net TXD)
    (add_net VCC)
    (add_net Vout)
    (add_net ~CTS)
    (add_net ~DTR)
    (add_net ~RTS)
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5786AD10)
    (at 132.08 101.6 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -1.778 -2.286 360) (layer F.SilkS))
    (fp_text value 47pF (at -3.302 -3.048 360) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5786BCA3)
    (at 127 109.22 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 2.794 -2.54 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.27 -3.556 180) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5786ACEF)
    (at 127 101.6 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 0 3.048 360) (layer F.SilkS))
    (fp_text value 47pF (at -2.032 3.302 360) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 5786ACF9)
    (at 120.65 110.49 180)
    (attr smd)
    (fp_text reference C4 (at 4.064 1.016 180) (layer F.SilkS))
    (fp_text value 10uF (at 3.048 -2.286 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 1.651 0 180) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5786AD0A)
    (at 132.08 109.22 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -4.318 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 2.54 3.048 180) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5786AE21)
    (at 146.05 110.49 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at -1.524 -2.286 360) (layer F.SilkS))
    (fp_text value LED (at -3.556 0.254 360) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 5786AE25)
    (at 138.43 110.49 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at -1.778 -2.286 360) (layer F.SilkS))
    (fp_text value LED (at -3.302 -2.54 360) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Connect:USB_Micro-B_10103594-0001LF (layer F.Cu) (tedit 5786AE37)
    (at 118.11 102.87 270)
    (descr "Micro USB Type B 10103594-0001LF")
    (tags "USB USB_B USB_micro USB_OTG")
    (attr smd)
    (fp_text reference P1 (at -4.826 -0.254 360) (layer F.SilkS))
    (fp_text value Micro-USB (at -8.382 2.286 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.3 -1.5) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at -0.65 -1.5) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -0.0009 -1.5) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (pad 4 smd rect (at 0.65 -1.5) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.3 -1.5) (size 1.65 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.425 -1.625) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.425 -1.625) (size 1.5 1.1) (drill oval 1.05 0.65) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at -2.725 1.375) (size 1.7 1.2) (drill oval 1.2 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 2.725 1.375) (size 1.7 1.2) (drill oval 1.2 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 smd rect (at -0.9625 1.625) (size 2.5 1.425) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 0.9625 1.625) (size 2.5 1.425) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Angled_1x07 (layer F.Cu) (tedit 5786AF3C)
    (at 168.656 94.996)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -0.508 -3.048) (layer F.SilkS))
    (fp_text value CONN_01X07 (at -2.032 -2.286) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 RST))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 RXD))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 TXD))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 Vout))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 ~CTS))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 ~RTS))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x07.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5786AD3B)
    (at 143.51 101.6 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 4.064 2.032 180) (layer F.SilkS))
    (fp_text value 2K2 (at 5.334 2.286 180) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5786AD18)
    (at 138.43 101.6 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 4.318 0 180) (layer F.SilkS))
    (fp_text value 2K2 (at 5.842 0.254 180) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5786ACE4)
    (at 127 93.98 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 2.54 360) (layer F.SilkS))
    (fp_text value 27R (at -1.778 2.54 360) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5786ACCE)
    (at 132.08 93.98 270)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at -0.762 -2.286 360) (layer F.SilkS))
    (fp_text value 27R (at -2.286 -2.794 360) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module NR_Footprints:Polyfuse_Littelfuse_1206L025 (layer F.Cu) (tedit 5786AA96)
    (at 121.92 95.25 180)
    (fp_text reference R5 (at 2.794 2.032 180) (layer F.SilkS))
    (fp_text value "Littelfuse 1206L050" (at 1.8 -2 180) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 2 smd rect (at 2.8 0 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P1-Pad1)"))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5786AD40)
    (at 140.97 92.71)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 4.572 -1.27) (layer F.SilkS))
    (fp_text value 10K (at 5.08 0.254) (layer F.SilkS))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 19 ~DTR))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5786C1CD)
    (at 157.988 104.648 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 2.286 2.286 180) (layer F.SilkS))
    (fp_text value 10K (at -2.286 -2.286 180) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 14 Vout))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 RST))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPDT_PCM12 (layer F.Cu) (tedit 5786AE1D)
    (at 156.21 110.998)
    (descr "Ultraminiature Surface Mount Slide Switch")
    (attr smd)
    (fp_text reference SW1 (at -1.016 -3.302) (layer F.SilkS))
    (fp_text value SWITCH_SPDT (at -5.588 2.794) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -1.5 0.325) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.5 0.325) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -2.25 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 Vout))
    (pad 2 smd rect (at 0.75 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 2.25 -1.425) (size 0.7 1.5) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad "" smd rect (at -3.65 1.425) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.65 1.425) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at 3.65 -0.775) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
    (pad "" smd rect (at -3.65 -0.775) (size 1 0.8) (layers F.Cu F.Paste F.Mask))
  )
  (module FT231X_Breakout:SSOP-20_3.9x8.7mm_Pitch0.635mm (layer F.Cu) (tedit 5786C1DA)
    (at 154.432 96.012 180)
    (descr "SSOP20: plastic shrink small outline package; 24 leads; body width 3.9 mm; lead pitch 0.635; (see FT231XS datasheet)")
    (tags "SSOP 0.635")
    (attr smd)
    (fp_text reference U1 (at -4.826 3.81 180) (layer F.SilkS))
    (fp_text value FT231X (at 0 4.572 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.6 -2.7925 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 19 ~DTR))
    (pad 2 smd rect (at -2.6 -2.1575 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 ~RTS))
    (pad 3 smd rect (at -2.6 -1.5225 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at -2.6 -0.8875 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 RXD))
    (pad 5 smd rect (at -2.6 -0.2525 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.6 0.3825 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at -2.6 1.0175 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -2.6 1.6525 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -2.6 2.2875 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 ~CTS))
    (pad 10 smd rect (at -2.6 2.9225 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(R2-Pad2)"))
    (pad 11 smd rect (at 2.5 2.9225 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R4-Pad1)"))
    (pad 12 smd rect (at 2.5 2.2875 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R3-Pad1)"))
    (pad 13 smd rect (at 2.5 1.6525 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 14 smd rect (at 2.5 1.0175 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 15 smd rect (at 2.5 0.3825 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 VCC))
    (pad 16 smd rect (at 2.5 -0.2525 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 17 smd rect (at 2.5 -0.8875 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad2)"))
    (pad 18 smd rect (at 2.5 -1.5225 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 2.5 -2.1575 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 2.5 -2.7925 180) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 TXD))
    (model Housings_SSOP.3dshapes/SSOP-24_3.9x8.7mm_Pitch0.635mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module FT231X_Breakout:SOT23_FET (layer F.Cu) (tedit 5786C220)
    (at 149.86 106.172)
    (attr smd)
    (fp_text reference Q1 (at -2.794 -1.778) (layer Eco1.User))
    (fp_text value 2N7002 (at 0 1.9) (layer Eco1.User) hide)
    (pad 2 smd rect (at -1.1 -2.6) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 ~DTR))
    (pad 1 smd rect (at 1.1 -2.6) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 0 0) (size 2.8 1.4) (layers F.Cu F.Paste F.Mask)
      (net 13 RST))
  )
  (gr_text Drain (at 146.05 106.172) (layer F.SilkS))
  (gr_text 2N7002 (at 148.59 101.854) (layer F.SilkS))
  (gr_text "OSH\nMIT License" (at 164.846 112.014) (layer B.SilkS))
  (gr_text 3V3 (at 149.86 112.776) (layer F.SilkS))
  (gr_text 5V (at 162.56 112.776) (layer F.SilkS))
  (gr_text TX (at 135.89 112.522) (layer F.SilkS))
  (gr_text RX (at 143.51 112.522) (layer F.SilkS))
  (gr_text "RupTek\n13-Jul-16\nv1.0" (at 124.968 93.218) (layer B.SilkS))
  (gr_text RupTek (at 118.11 91.44) (layer F.SilkS))
  (gr_text ~RTS (at 164.719 110.49) (layer F.SilkS))
  (gr_text GND (at 164.846 107.823) (layer F.SilkS))
  (gr_text ~CTS (at 164.719 105.41) (layer F.SilkS))
  (gr_text Vout (at 164.465 102.743) (layer F.SilkS))
  (gr_text TXD (at 164.973 100.203) (layer F.SilkS))
  (gr_text RXD (at 164.973 97.536) (layer F.SilkS))
  (gr_text DTR (at 163.576 95.25) (layer F.SilkS))
  (gr_line (start 114.554 114.554) (end 114.554 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.704 114.554) (end 114.554 114.554) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.704 89.916) (end 171.704 114.554) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.554 89.916) (end 171.704 89.916) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114.554 114.3) (end 114.554 89.916) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.554 89.916) (xy 171.704 89.916) (xy 171.704 114.554) (xy 114.554 114.554)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.062 90.424) (xy 170.942 90.424) (xy 171.196 114.046) (xy 115.062 114.046)
      )
    )
  )
)
